(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (title_block
    (title "Board Drawing")
    (date "16. 04. 2023")
    (comment 1 "${ProjectNumber}")
    (comment 2 "${ProjectTitle}")
    (comment 3 "${ProjectAuthor}")
    (comment 4 "${ProjectVariant}")
    (comment 5 "${ProjectDate}")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user "Test.Points")
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 86 79)
    (grid_origin 86 79.000001)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Fabrication/Gerber/")
    )
  )
  (property "ProjectAuthor" "René Široký")
  (property "ProjectDate" "21. 9. 2022")
  (property "ProjectNumber" "W220921.01")
  (property "ProjectTitle" "TMDSEMU110-U Debug Probe SWD Adapter")
  (property "ProjectVariant" "Default")
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3.3V")
  (net 3 "/tRX")
  (net 4 "/TMS{slash}SWDIO")
  (net 5 "/TCK{slash}SWCLK")
  (net 6 "/TDO{slash}SWO")
  (net 7 "unconnected-(J1-Pad14)")
  (net 8 "/nRESET")
  (net 9 "/tTX")
  (net 10 "unconnected-(J1-Pad18)")
  (net 11 "/nTRST")
  (net 12 "/TDI")
  (net 13 "unconnected-(J1-Pad4)")
  (net 14 "unconnected-(J1-Pad6)")
  (net 15 "unconnected-(J2-Pad9)")
  (net 16 "unconnected-(J1-Pad9)")
  (net 17 "unconnected-(J1-Pad13)")
  (net 18 "unconnected-(J1-Pad17)")
  (net 19 "unconnected-(J1-Pad19)")
  (net 20 "unconnected-(J2-Pad7)")
  (net 21 "/TGTSUPPLYOUT")
  (net 22 "unconnected-(J2-Pad8)")
  (net 23 "unconnected-(J2-Pad10)")
  (net 24 "unconnected-(J2-Pad11)")
  (net 25 "Net-(PTC1-Pad2)")
  (net 26 "Net-(LD1-PadA)")
  (net 27 "unconnected-(P1-Pad7)")
  (net 28 "unconnected-(P2-Pad3)")
  (net 29 "unconnected-(P2-Pad4)")
  (net 30 "unconnected-(U1-NC-Pad4)")
  (footprint "SOT,TO,SC:SOT23-5" (layer "F.Cu")
    (at 100.4 68.2 -90)
    (descr "Small Outline Transistor, SOT-23 Type, 0.95 mm pitch; 5 pin, 2.90 mm L X 1.30 mm W X 1.10 mm H body")
    (property "Manufacturer" "Analog Devices")
    (property "Manufacturer Part Number" "MAX40203AUK+T")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ideal Diode, 1.2 to 5.5V, 1A")
    (property "ki_keywords" "Diode")
    (attr smd)
    (fp_text reference "U1" (at -1.9 -1.5) (layer "F.SilkS"))
    (fp_text value "MAX40203" (at 0 0.2 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.15 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 1.1) (size 0.95 0.621) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2496006441)
      (net 21 "/TGTSUPPLYOUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0 1.1) (size 0.95 0.621) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2496006441)
      (net 1 "GND") (pinfunction "GND") (pintype "passive") (zone_connect 2))
    (pad "3" smd roundrect (at 0.95 1.1) (size 0.95 0.621) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2496006441)
      (net 21 "/TGTSUPPLYOUT") (pinfunction "EN") (pintype "passive"))
    (pad "4" smd roundrect (at 0.95 -1.1) (size 0.95 0.621) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2496006441)
      (net 30 "unconnected-(U1-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at -0.95 -1.1) (size 0.95 0.621) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2496006441)
      (net 25 "Net-(PTC1-Pad2)") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/SOT,TO,SC/SOT23-5.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PTC_Fuses:PTCF_1206_3216" (layer "F.Cu")
    (at 104.8 68.5 180)
    (descr "PTC, Fuse; 3.20 mm L X 1.60 mm W body")
    (property "Manufacturer" "Littlefuse")
    (property "Manufacturer Part Number" "1206L050YR")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "PTC Fuse SMD Size 1206, Fuse 500mA Hold, 1A Trip, 6V, 0.7R")
    (property "ki_keywords" "PTC Fuses")
    (attr smd)
    (fp_text reference "PTC1" (at 0 1.599999 180) (layer "F.SilkS"))
    (fp_text value "500mA" (at 0 0.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.15 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.525 0 180) (size 0.962 1.712) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 1.525 0 180) (size 0.962 1.712) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(PTC1-Pad2)") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/PTC_Fuses/PTCF_1206_3216.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED:LEDC_0603_1608_G" (layer "F.Cu")
    (at 108.8 67.3)
    (descr "LED, Chip; 1.60 mm L X 0.80 mm W body, GREEN")
    (property "Manufacturer" "Kingbright")
    (property "Manufacturer Part Number" "KPT-1608SGC")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "LED SMD Size 0603, Green 568nm, 2.2V, 20mA")
    (property "ki_keywords" "LED Diode")
    (attr smd)
    (fp_text reference "LD1" (at 0 -1.2) (layer "F.SilkS"))
    (fp_text value "KPT-1608SGC" (at 0 0.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 0.025) (layer "F.Fab"))
    (pad "A" smd rect (at 0.8 0) (size 0.712 0.912) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(LD1-PadA)") (pinfunction "A") (pintype "passive"))
    (pad "C" smd rect (at -0.8 0) (size 0.712 0.912) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/LED/LEDC_0603_1608_G.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors:P_THT_IDC-10-V" (layer "F.Cu")
    (at 123 73 180)
    (descr "THT 2.54mm Box Header, Double Row, Vertical")
    (property "Manufacturer" "Multicomp")
    (property "Manufacturer Part Number" "MC-254-10-00-ST-DIP")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "THT 10P 2.54mm 250V 3A Box Header, Double Row, Vertical")
    (property "ki_keywords" "Connector")
    (attr through_hole)
    (fp_text reference "P1" (at -4.6 3.4 unlocked) (layer "F.SilkS"))
    (fp_text value "IDC-10P-V" (at -2.5 0.2 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.5 -0.15 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "/TMS{slash}SWDIO") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "/TCK{slash}SWCLK") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "6" thru_hole circle (at 5.08 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "/TDO{slash}SWO") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(P1-Pad7)") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at 7.62 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "/TDI") (pintype "passive"))
    (pad "9" thru_hole circle (at 10.16 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "/nTRST") (pintype "passive"))
    (pad "10" thru_hole circle (at 10.16 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "/nRESET") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connectors/P_THT_IDC-10-V.STEP"
      (offset (xyz 10.16 0 2.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors:RESC_0603_1608X45" (layer "F.Cu")
    (at 108.8 68.9 180)
    (descr "Resistor, Chip; 1.60 mm L X 0.80 mm W X 0.45 mm H body")
    (property "Manufacturer" "Generic")
    (property "Manufacturer Part Number" "1k 1%")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor SMD Size 0603, 0.1W")
    (property "ki_keywords" "Resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.1 1.9 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 0.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8 0 180) (size 0.712 0.912) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(LD1-PadA)") (pintype "passive"))
    (pad "2" smd rect (at 0.8 0 180) (size 0.712 0.912) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Resistors/RESC_0603_1608X45.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors:P_THT_IDC-10-V" (layer "F.Cu")
    (at 102 73 180)
    (descr "THT 2.54mm Box Header, Double Row, Vertical")
    (property "Manufacturer" "Multicomp")
    (property "Manufacturer Part Number" "MC-254-10-00-ST-DIP")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "THT 10P 2.54mm 250V 3A Box Header, Double Row, Vertical")
    (property "ki_keywords" "Connector")
    (attr through_hole)
    (fp_text reference "P2" (at 14.7 3.4 unlocked) (layer "F.SilkS"))
    (fp_text value "IDC-10P-V" (at -2.5 0.2 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.5 -0.15 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 3 "/tRX") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "/tTX") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(P2-Pad3)") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 2.54 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(P2-Pad4)") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "6" thru_hole circle (at 5.08 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "/nRESET") (pintype "passive"))
    (pad "8" thru_hole circle (at 7.62 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "/TDO{slash}SWO") (pintype "passive"))
    (pad "9" thru_hole circle (at 10.16 0 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "/TMS{slash}SWDIO") (pintype "passive"))
    (pad "10" thru_hole circle (at 10.16 -2.54 180) (size 1.65 1.65) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "/TCK{slash}SWCLK") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connectors/P_THT_IDC-10-V.STEP"
      (offset (xyz 10.16 0 2.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors:J_THT_WR-PHD_62202021821" locked (layer "B.Cu")
    (at 123 69.27 180)
    (descr "THT 1.27mm WR-PHD THT Straight Dual Socket Header")
    (property "Manufacturer" "Würth Elektronik")
    (property "Manufacturer Part Number" "62202021821")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "THT 20P 1.27mm WR-PHD 1.27 mm Dual Socket Header Vertical")
    (property "ki_keywords" "Connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.6 unlocked) (layer "B.SilkS"))
    (fp_text value "62202021821" (at 0 -1.55 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 4 "/TMS{slash}SWDIO") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 11 "/nTRST") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 1.27 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 12 "/TDI") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 1.27 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(J1-Pad4)") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle locked (at 2.54 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(J1-Pad6)") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle locked (at 3.81 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 6 "/TDO{slash}SWO") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 3.81 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 5.08 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J1-Pad9)") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle locked (at 5.08 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 6.35 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 5 "/TCK{slash}SWCLK") (pintype "passive"))
    (pad "12" thru_hole circle locked (at 6.35 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 7.62 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J1-Pad13)") (pintype "passive+no_connect"))
    (pad "14" thru_hole circle locked (at 7.62 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(J1-Pad14)") (pintype "passive+no_connect"))
    (pad "15" thru_hole circle locked (at 8.89 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 8 "/nRESET") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 8.89 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "17" thru_hole circle locked (at 10.16 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J1-Pad17)") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle locked (at 10.16 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J1-Pad18)") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle locked (at 11.43 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J1-Pad19)") (pintype "passive+no_connect"))
    (pad "20" thru_hole circle locked (at 11.43 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connectors/J_THT_WR-PHD_62202021821.STEP"
      (offset (xyz 5.7 0.64 2.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors:J_THT_WR-PHD_62201421821" locked (layer "B.Cu")
    (at 97.5 69.27 180)
    (descr "THT 1.27mm WR-PHD THT Straight Dual Socket Header")
    (property "Manufacturer" "Würth Elektronik")
    (property "Manufacturer Part Number" "62201421821")
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "THT 14P 1.27mm WR-PHD 1.27 mm Dual Socket Header Vertical")
    (property "ki_keywords" "Connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.6 unlocked) (layer "B.SilkS"))
    (fp_text value "62201421821" (at 0 -1.55 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 1.27 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 21 "/TGTSUPPLYOUT") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 1.27 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 21 "/TGTSUPPLYOUT") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.54 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 3.81 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J2-Pad7)") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle locked (at 3.81 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(J2-Pad8)") (pintype "passive+no_connect"))
    (pad "9" thru_hole circle locked (at 5.08 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(J2-Pad9)") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle locked (at 5.08 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(J2-Pad10)") (pintype "passive+no_connect"))
    (pad "11" thru_hole circle locked (at 6.35 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(J2-Pad11)") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle locked (at 6.35 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 3 "/tRX") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 7.62 1.27 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "14" thru_hole circle locked (at 7.62 0 180) (size 1.05 1.05) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 9 "/tTX") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connectors/J_THT_WR-PHD_62201421821.STEP"
      (offset (xyz 3.8 0.64 2.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_PCB_Graphics:LOGO_WiSER_Mask" (layer "B.Cu")
    (at 106.2 68.8 180)
    (property "Sheetfile" "W220921.01.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Logo WiSER")
    (property "ki_keywords" "Logo")
    (zone_connect 0)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Logo1" (at -0.1 -0.15) (layer "B.SilkS") hide)
    (fp_text value "WiSER" (at 0.65 -0.15) (layer "B.SilkS") hide)
  )
  (gr_line (start 86 65.000001) (end 129 65.000001)
    (layer "Edge.Cuts"))
  (gr_line (start 129 79.000001) (end 86 79.000001)
    (layer "Edge.Cuts"))
  (gr_line (start 86 79.000001) (end 86 65.000001)
    (layer "Edge.Cuts"))
  (gr_line (start 129 65.000001) (end 129 79.000001)
    (layer "Edge.Cuts"))
  (gr_text "DEBUG" (at 120.3 67.1) (layer "B.SilkS"))
  (gr_text "TMDSEMU110-U Debug Probe SWD Adapter" (at 128.1 78.5) (layer "B.SilkS"))
  (gr_text "AUX" (at 95.5 67.1) (layer "B.SilkS"))
  (gr_text "JTAG-STM" (at 111.8 67.6) (layer "F.SilkS"))
  (gr_text "LINET" (at 92.6 67.6) (layer "F.SilkS"))
  (gr_text "${COMMENT1}" (at 86.5 71 -90) (layer "B.Mask"))
  (zone (net 8) (net_name "/nRESET") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.802409 67.14383)
        (xy 113.888589 67.274037)
        (xy 113.881043 67.387852)
        (xy 113.812661 67.50209)
        (xy 113.716337 67.633565)
        (xy 113.624963 67.799091)
        (xy 114.110707 68.000707)
        (xy 114.481231 67.628769)
        (xy 114.341305 67.479592)
        (xy 114.250047 67.366272)
        (xy 114.175012 67.264904)
        (xy 114.083754 67.151585)
        (xy 113.94383 67.002409)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.75 69.025)
        (xy 97.801003 68.85959)
        (xy 97.852007 68.710681)
        (xy 97.90301 68.578272)
        (xy 97.954014 68.462363)
        (xy 98.005018 68.362954)
        (xy 97.5 67.999)
        (xy 96.994982 68.362954)
        (xy 97.045985 68.462363)
        (xy 97.096989 68.578272)
        (xy 97.147992 68.710681)
        (xy 97.198996 68.85959)
        (xy 97.25 69.025)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.288 69.15)
        (xy 107.3592 69.158479)
        (xy 107.4304 69.173319)
        (xy 107.501599 69.19452)
        (xy 107.572799 69.22208)
        (xy 107.644 69.256)
        (xy 108.001 68.9)
        (xy 107.644 68.544)
        (xy 107.572799 68.577919)
        (xy 107.501599 68.605479)
        (xy 107.4304 68.62668)
        (xy 107.3592 68.64152)
        (xy 107.288 68.65)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.98 68.245)
        (xy 95.971297 68.457237)
        (xy 95.94449 68.606173)
        (xy 95.898531 68.7314)
        (xy 95.832371 68.872508)
        (xy 95.744963 69.069091)
        (xy 96.23 69.271)
        (xy 96.715037 69.069091)
        (xy 96.627628 68.872508)
        (xy 96.561468 68.7314)
        (xy 96.515509 68.606173)
        (xy 96.488702 68.457237)
        (xy 96.48 68.245)
      )
    )
  )
  (zone (net 4) (net_name "/TMS{slash}SWDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.847627 73.866205)
        (xy 92.68039 73.632931)
        (xy 92.643386 73.426393)
        (xy 92.665457 73.218299)
        (xy 92.675447 72.98036)
        (xy 92.602201 72.684286)
        (xy 91.839293 72.999293)
        (xy 91.524286 73.762201)
        (xy 91.82036 73.835447)
        (xy 92.058299 73.825457)
        (xy 92.266393 73.803386)
        (xy 92.472931 73.84039)
        (xy 92.706205 74.007627)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 120.21 66.975)
        (xy 120.201297 67.187237)
        (xy 120.17449 67.336173)
        (xy 120.128531 67.4614)
        (xy 120.062371 67.602508)
        (xy 119.974963 67.799091)
        (xy 120.46 68.001)
        (xy 120.945037 67.799091)
        (xy 120.857628 67.602508)
        (xy 120.791468 67.4614)
        (xy 120.745509 67.336173)
        (xy 120.718702 67.187237)
        (xy 120.71 66.975)
      )
    )
  )
  (zone (net 8) (net_name "/nRESET") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.973795 76.547627)
        (xy 112.207068 76.38039)
        (xy 112.413606 76.343386)
        (xy 112.621699 76.365457)
        (xy 112.859638 76.375447)
        (xy 113.155714 76.302201)
        (xy 112.840707 75.539293)
        (xy 112.077799 75.224286)
        (xy 112.004551 75.52036)
        (xy 112.014541 75.758299)
        (xy 112.036613 75.966393)
        (xy 111.999609 76.172931)
        (xy 111.832373 76.406205)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.075 67.163)
        (xy 106.0288 67.286919)
        (xy 105.9826 67.396979)
        (xy 105.9364 67.49318)
        (xy 105.8902 67.57552)
        (xy 105.844 67.644)
        (xy 106.325 68.501)
        (xy 106.806 67.644)
        (xy 106.7598 67.57552)
        (xy 106.7136 67.49318)
        (xy 106.6674 67.396979)
        (xy 106.6212 67.286919)
        (xy 106.575 67.163)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.67 71.675)
        (xy 96.637521 71.947082)
        (xy 96.552075 72.124165)
        (xy 96.431648 72.266135)
        (xy 96.294228 72.432879)
        (xy 96.157799 72.684286)
        (xy 96.92 73.001)
        (xy 97.682201 72.684286)
        (xy 97.545771 72.432879)
        (xy 97.40835 72.266135)
        (xy 97.287924 72.124165)
        (xy 97.202478 71.947082)
        (xy 97.17 71.675)
      )
    )
  )
  (zone (net 4) (net_name "/TMS{slash}SWDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.133795 76.547627)
        (xy 122.367068 76.38039)
        (xy 122.573606 76.343386)
        (xy 122.781699 76.365457)
        (xy 123.019638 76.375447)
        (xy 123.315714 76.302201)
        (xy 123.000707 75.539293)
        (xy 122.237799 75.224286)
        (xy 122.164551 75.52036)
        (xy 122.174541 75.758299)
        (xy 122.196613 75.966393)
        (xy 122.159609 76.172931)
        (xy 121.992373 76.406205)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.25 68.245)
        (xy 97.241297 68.457237)
        (xy 97.21449 68.606173)
        (xy 97.168531 68.7314)
        (xy 97.102371 68.872508)
        (xy 97.014963 69.069091)
        (xy 97.5 69.271)
        (xy 97.985037 69.069091)
        (xy 97.897628 68.872508)
        (xy 97.831468 68.7314)
        (xy 97.785509 68.606173)
        (xy 97.758702 68.457237)
        (xy 97.75 68.245)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.880958 71.765488)
        (xy 123.636421 71.91639)
        (xy 123.391884 72.032792)
        (xy 123.147347 72.114695)
        (xy 122.90281 72.162097)
        (xy 122.658274 72.175)
        (xy 122.999293 73.000707)
        (xy 123.824999 73.341726)
        (xy 123.906901 73.028189)
        (xy 123.988804 72.749152)
        (xy 124.070706 72.504615)
        (xy 124.152609 72.294578)
        (xy 124.234512 72.119042)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.0855 68.9)
        (xy 99.992399 68.895159)
        (xy 99.899299 68.886689)
        (xy 99.806198 68.87459)
        (xy 99.713098 68.85886)
        (xy 99.619998 68.8395)
        (xy 99.299 69.15)
        (xy 99.619998 69.4605)
        (xy 99.713098 69.441139)
        (xy 99.806198 69.425409)
        (xy 99.899299 69.41331)
        (xy 99.992399 69.40484)
        (xy 100.0855 69.4)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.33253 66.913917)
        (xy 96.146697 67.1031)
        (xy 96.021982 67.246424)
        (xy 95.931426 67.383672)
        (xy 95.848072 67.554633)
        (xy 95.744963 67.799091)
        (xy 96.229293 68.000707)
        (xy 96.755 68)
        (xy 96.722859 67.807522)
        (xy 96.655823 67.658142)
        (xy 96.597964 67.531747)
        (xy 96.593359 67.408226)
        (xy 96.686083 67.26747)
      )
    )
  )
  (zone (net 8) (net_name "/nRESET") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.387627 73.866205)
        (xy 95.22039 73.632931)
        (xy 95.183386 73.426393)
        (xy 95.205457 73.218299)
        (xy 95.215447 72.98036)
        (xy 95.142201 72.684286)
        (xy 94.379293 72.999293)
        (xy 94.064286 73.762201)
        (xy 94.36036 73.835447)
        (xy 94.598299 73.825457)
        (xy 94.806393 73.803386)
        (xy 95.012931 73.84039)
        (xy 95.246205 74.007627)
      )
    )
  )
  (zone (net 11) (net_name "/nTRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.706205 71.992373)
        (xy 113.472931 72.159609)
        (xy 113.266393 72.196613)
        (xy 113.058299 72.174541)
        (xy 112.82036 72.164551)
        (xy 112.524286 72.237799)
        (xy 112.839293 73.000707)
        (xy 113.602201 73.315714)
        (xy 113.675447 73.019638)
        (xy 113.665457 72.781699)
        (xy 113.643386 72.573606)
        (xy 113.68039 72.367068)
        (xy 113.847627 72.133795)
      )
    )
  )
  (zone (net 12) (net_name "/TDI") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.246205 74.532373)
        (xy 116.012931 74.699609)
        (xy 115.806393 74.736613)
        (xy 115.598299 74.714541)
        (xy 115.36036 74.704551)
        (xy 115.064286 74.777799)
        (xy 115.379293 75.540707)
        (xy 116.142201 75.855714)
        (xy 116.215447 75.559638)
        (xy 116.205457 75.321699)
        (xy 116.183386 75.113606)
        (xy 116.22039 74.907068)
        (xy 116.387627 74.673795)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.232236 70.078683)
        (xy 95.155112 69.956605)
        (xy 95.173301 69.852062)
        (xy 95.251332 69.747781)
        (xy 95.353734 69.626487)
        (xy 95.445037 69.470909)
        (xy 94.959293 69.269293)
        (xy 94.474963 69.470909)
        (xy 94.55817 69.720449)
        (xy 94.597091 69.911199)
        (xy 94.634779 70.073311)
        (xy 94.714292 70.236939)
        (xy 94.878683 70.432236)
      )
    )
  )
  (zone (net 25) (net_name "Net-(PTC1-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.2855 67)
        (xy 102.192399 66.995159)
        (xy 102.099299 66.986689)
        (xy 102.006198 66.97459)
        (xy 101.913098 66.95886)
        (xy 101.819998 66.9395)
        (xy 101.499 67.25)
        (xy 101.819998 67.5605)
        (xy 101.913098 67.541139)
        (xy 102.006198 67.525409)
        (xy 102.099299 67.51331)
        (xy 102.192399 67.50484)
        (xy 102.2855 67.5)
      )
    )
  )
  (zone (net 11) (net_name "/nTRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.862115 70.279307)
        (xy 122.99818 70.129828)
        (xy 123.082882 70.013144)
        (xy 123.150462 69.907392)
        (xy 123.235164 69.790708)
        (xy 123.371231 69.641231)
        (xy 123.000707 69.269293)
        (xy 122.514963 69.470909)
        (xy 122.611333 69.640395)
        (xy 122.716145 69.773901)
        (xy 122.793345 69.889361)
        (xy 122.806879 70.00471)
        (xy 122.720693 70.137885)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.75 70.295)
        (xy 97.758702 70.082762)
        (xy 97.785509 69.933826)
        (xy 97.831468 69.808599)
        (xy 97.897628 69.667491)
        (xy 97.985037 69.470909)
        (xy 97.5 69.269)
        (xy 97.014963 69.470909)
        (xy 97.102371 69.667491)
        (xy 97.168531 69.808599)
        (xy 97.21449 69.933826)
        (xy 97.241297 70.082762)
        (xy 97.25 70.295)
      )
    )
  )
  (zone (net 26) (net_name "Net-(LD1-PadA)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 109.35 68.088)
        (xy 109.3288 68.17192)
        (xy 109.3076 68.24948)
        (xy 109.286399 68.320679)
        (xy 109.265199 68.385519)
        (xy 109.244 68.444)
        (xy 109.6 68.901)
        (xy 109.956 68.444)
        (xy 109.9348 68.385519)
        (xy 109.9136 68.320679)
        (xy 109.892399 68.24948)
        (xy 109.871199 68.17192)
        (xy 109.85 68.088)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.0855 67)
        (xy 99.992399 66.995159)
        (xy 99.899299 66.986689)
        (xy 99.806198 66.97459)
        (xy 99.713098 66.95886)
        (xy 99.619998 66.9395)
        (xy 99.299 67.25)
        (xy 99.619998 67.5605)
        (xy 99.713098 67.541139)
        (xy 99.806198 67.525409)
        (xy 99.899299 67.51331)
        (xy 99.992399 67.50484)
        (xy 100.0855 67.5)
      )
    )
  )
  (zone (net 12) (net_name "/TDI") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.867885 66.990693)
        (xy 121.731818 67.14017)
        (xy 121.647116 67.256854)
        (xy 121.579536 67.362606)
        (xy 121.494834 67.47929)
        (xy 121.358769 67.628769)
        (xy 121.729293 68.000707)
        (xy 122.215037 67.799091)
        (xy 122.118665 67.629603)
        (xy 122.013853 67.496097)
        (xy 121.936653 67.380637)
        (xy 121.92312 67.265288)
        (xy 122.009307 67.132115)
      )
    )
  )
  (zone (net 8) (net_name "/nRESET") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.832373 74.673795)
        (xy 111.999609 74.907068)
        (xy 112.036613 75.113606)
        (xy 112.014541 75.321699)
        (xy 112.004551 75.559638)
        (xy 112.077799 75.855714)
        (xy 112.840707 75.540707)
        (xy 113.155714 74.777799)
        (xy 112.859638 74.704551)
        (xy 112.621699 74.714541)
        (xy 112.413606 74.736613)
        (xy 112.207068 74.699609)
        (xy 111.973795 74.532373)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.48 69.025)
        (xy 96.488702 68.812762)
        (xy 96.515509 68.663826)
        (xy 96.561468 68.538599)
        (xy 96.627628 68.397491)
        (xy 96.715037 68.200909)
        (xy 96.23 67.999)
        (xy 95.744963 68.200909)
        (xy 95.832371 68.397491)
        (xy 95.898531 68.538599)
        (xy 95.94449 68.663826)
        (xy 95.971297 68.812762)
        (xy 95.98 69.025)
      )
    )
  )
  (zone (net 21) (net_name "/TGTSUPPLYOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.5145 67.5)
        (xy 98.6076 67.50484)
        (xy 98.7007 67.51331)
        (xy 98.793801 67.525409)
        (xy 98.886901 67.541139)
        (xy 98.980002 67.5605)
        (xy 99.301 67.25)
        (xy 98.980002 66.9395)
        (xy 98.886901 66.95886)
        (xy 98.793801 66.97459)
        (xy 98.7007 66.986689)
        (xy 98.6076 66.995159)
        (xy 98.5145 67)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.575 69.837)
        (xy 106.6212 69.71308)
        (xy 106.6674 69.60302)
        (xy 106.7136 69.506819)
        (xy 106.7598 69.424479)
        (xy 106.806 69.356)
        (xy 106.325 68.499)
        (xy 105.844 69.356)
        (xy 105.8902 69.424479)
        (xy 105.9364 69.506819)
        (xy 105.9826 69.60302)
        (xy 106.0288 69.71308)
        (xy 106.075 69.837)
      )
    )
  )
  (zone (net 26) (net_name "Net-(LD1-PadA)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 109.85 68.112)
        (xy 109.871199 68.028079)
        (xy 109.892399 67.950519)
        (xy 109.9136 67.87932)
        (xy 109.9348 67.81448)
        (xy 109.956 67.756)
        (xy 109.6 67.299)
        (xy 109.244 67.756)
        (xy 109.265199 67.81448)
        (xy 109.286399 67.87932)
        (xy 109.3076 67.950519)
        (xy 109.3288 68.028079)
        (xy 109.35 68.112)
      )
    )
  )
  (zone (net 25) (net_name "Net-(PTC1-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.277105 67.530659)
        (xy 102.380483 67.727661)
        (xy 102.483862 67.938523)
        (xy 102.587242 68.163246)
        (xy 102.690621 68.401828)
        (xy 102.794 68.654271)
        (xy 103.275707 68.500707)
        (xy 103.253536 67.644)
        (xy 103.12896 67.57834)
        (xy 103.004385 67.498821)
        (xy 102.879809 67.405443)
        (xy 102.755234 67.298204)
        (xy 102.630659 67.177105)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (name "GND_TOP") (hatch none 0.5)
    (connect_pads (clearance 0.16))
    (min_thickness 0.16) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.16) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 129 79.000001)
        (xy 86 79.000001)
        (xy 86 65.000001)
        (xy 129 65.000001)
      )
    )
  )
  (zone (net 3) (net_name "/tRX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.871554 72.012976)
        (xy 100.932243 72.196948)
        (xy 100.992932 72.42181)
        (xy 101.053621 72.68756)
        (xy 101.11431 72.994198)
        (xy 101.175 73.341726)
        (xy 102.000707 73.000707)
        (xy 102.341726 72.175)
        (xy 102.075975 72.196087)
        (xy 101.810225 72.176287)
        (xy 101.544476 72.115598)
        (xy 101.278726 72.01402)
        (xy 101.012976 71.871554)
      )
    )
  )
  (zone (net 9) (net_name "/tTX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.127002 70.151266)
        (xy 90.040658 70.014614)
        (xy 90.060978 69.897583)
        (xy 90.148273 69.780841)
        (xy 90.262855 69.645059)
        (xy 90.365037 69.470909)
        (xy 89.879293 69.269293)
        (xy 89.508769 69.641231)
        (xy 89.640559 69.791185)
        (xy 89.717707 69.911644)
        (xy 89.77664 70.022273)
        (xy 89.853788 70.142733)
        (xy 89.98558 70.292688)
      )
    )
  )
  (zone (net 9) (net_name "/tTX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.992373 74.673795)
        (xy 101.159609 74.907068)
        (xy 101.196613 75.113606)
        (xy 101.174541 75.321699)
        (xy 101.164551 75.559638)
        (xy 101.237799 75.855714)
        (xy 102.000707 75.540707)
        (xy 102.315714 74.777799)
        (xy 102.019638 74.704551)
        (xy 101.781699 74.714541)
        (xy 101.573606 74.736613)
        (xy 101.367068 74.699609)
        (xy 101.133795 74.532373)
      )
    )
  )
  (zone (net 6) (net_name "/TDO{slash}SWO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.41166 76.370238)
        (xy 95.245436 76.14344)
        (xy 95.20188 75.943675)
        (xy 95.21449 75.742714)
        (xy 95.216764 75.512327)
        (xy 95.142201 75.224286)
        (xy 94.379293 75.539293)
        (xy 94.38 76.365)
        (xy 94.615191 76.349629)
        (xy 94.796377 76.324755)
        (xy 94.948992 76.322232)
        (xy 95.098468 76.373915)
        (xy 95.270238 76.51166)
      )
    )
  )
  (zone (net 5) (net_name "/TCK{slash}SWCLK") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 119.452373 74.673795)
        (xy 119.619609 74.907068)
        (xy 119.656613 75.113606)
        (xy 119.634541 75.321699)
        (xy 119.624551 75.559638)
        (xy 119.697799 75.855714)
        (xy 120.460707 75.540707)
        (xy 120.775714 74.777799)
        (xy 120.479638 74.704551)
        (xy 120.241699 74.714541)
        (xy 120.033606 74.736613)
        (xy 119.827068 74.699609)
        (xy 119.593795 74.532373)
      )
    )
  )
  (zone (net 5) (net_name "/TCK{slash}SWCLK") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.314125 67.155546)
        (xy 116.400433 67.282865)
        (xy 116.39892 67.395085)
        (xy 116.339338 67.507999)
        (xy 116.251435 67.637402)
        (xy 116.164963 67.799091)
        (xy 116.650707 68.000707)
        (xy 117.021231 67.628769)
        (xy 116.877342 67.479789)
        (xy 116.779581 67.369885)
        (xy 116.697195 67.273007)
        (xy 116.599433 67.163104)
        (xy 116.455546 67.014125)
      )
    )
  )
  (zone (net 6) (net_name "/TDO{slash}SWO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 119.35617 67.002409)
        (xy 119.216244 67.151585)
        (xy 119.124986 67.264904)
        (xy 119.049951 67.366272)
        (xy 118.958693 67.479592)
        (xy 118.818769 67.628769)
        (xy 119.189293 68.000707)
        (xy 119.675037 67.799091)
        (xy 119.583661 67.633565)
        (xy 119.487337 67.50209)
        (xy 119.418956 67.387852)
        (xy 119.41141 67.274037)
        (xy 119.497591 67.14383)
      )
    )
  )
  (zone (net 3) (net_name "/tRX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.25 70.295)
        (xy 91.273335 70.074988)
        (xy 91.335407 69.929457)
        (xy 91.424316 69.811524)
        (xy 91.528159 69.674303)
        (xy 91.635037 69.470909)
        (xy 91.15 69.269)
        (xy 90.664963 69.470909)
        (xy 90.77184 69.674303)
        (xy 90.875683 69.811524)
        (xy 90.964591 69.929457)
        (xy 91.026664 70.074988)
        (xy 91.05 70.295)
      )
    )
  )
  (zone (net 6) (net_name "/TDO{slash}SWO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 117.053795 76.547627)
        (xy 117.287068 76.38039)
        (xy 117.493606 76.343386)
        (xy 117.701699 76.365457)
        (xy 117.939638 76.375447)
        (xy 118.235714 76.302201)
        (xy 117.920707 75.539293)
        (xy 117.157799 75.224286)
        (xy 117.084551 75.52036)
        (xy 117.094541 75.758299)
        (xy 117.116613 75.966393)
        (xy 117.079609 76.172931)
        (xy 116.912373 76.406205)
      )
    )
  )
  (zone (net 4) (net_name "/TMS{slash}SWDIO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.87238 68.730958)
        (xy 123.802904 68.592274)
        (xy 123.733428 68.42809)
        (xy 123.663951 68.238406)
        (xy 123.594475 68.023222)
        (xy 123.525 67.782538)
        (xy 122.999293 67.999293)
        (xy 122.782538 68.525)
        (xy 122.972222 68.543475)
        (xy 123.161906 68.587451)
        (xy 123.35159 68.656928)
        (xy 123.541274 68.751904)
        (xy 123.730958 68.87238)
      )
    )
  )
  (zone (net 6) (net_name "/TDO{slash}SWO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 118.927627 76.406205)
        (xy 118.76039 76.172931)
        (xy 118.723386 75.966393)
        (xy 118.745457 75.758299)
        (xy 118.755447 75.52036)
        (xy 118.682201 75.224286)
        (xy 117.919293 75.539293)
        (xy 117.604286 76.302201)
        (xy 117.90036 76.375447)
        (xy 118.138299 76.365457)
        (xy 118.346393 76.343386)
        (xy 118.552931 76.38039)
        (xy 118.786205 76.547627)
      )
    )
  )
  (zone (net 4) (net_name "/TMS{slash}SWDIO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.866205 74.532373)
        (xy 123.632931 74.699609)
        (xy 123.426393 74.736613)
        (xy 123.218299 74.714541)
        (xy 122.98036 74.704551)
        (xy 122.684286 74.777799)
        (xy 122.999293 75.540707)
        (xy 123.762201 75.855714)
        (xy 123.835447 75.559638)
        (xy 123.825457 75.321699)
        (xy 123.803386 75.113606)
        (xy 123.84039 74.907068)
        (xy 124.007627 74.673795)
      )
    )
  )
  (zone (net 5) (net_name "/TCK{slash}SWCLK") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.706205 74.532373)
        (xy 92.472931 74.699609)
        (xy 92.266393 74.736613)
        (xy 92.058299 74.714541)
        (xy 91.82036 74.704551)
        (xy 91.524286 74.777799)
        (xy 91.839293 75.540707)
        (xy 92.602201 75.855714)
        (xy 92.675447 75.559638)
        (xy 92.665457 75.321699)
        (xy 92.643386 75.113606)
        (xy 92.68039 74.907068)
        (xy 92.847627 74.673795)
      )
    )
  )
)
