(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.599998)
  )
  (paper "A4")
  (title_block
    (title "STEPPER")
    (date "2022-06-23")
    (rev "v1.1")
    (company "EPAK GmbH")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power "In1_GND.Cu")
    (2 "In2.Cu" signal "In2_Signal1_Cu")
    (3 "In3.Cu" power "In3_Power_Cu")
    (4 "In4.Cu" power "In4_Power_Cu")
    (5 "In5.Cu" signal "In5_Signal2_Cu")
    (6 "In6.Cu" power "In6_GND_Cu")
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In3.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 4" (type "prepreg") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In4.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 5" (type "core") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In5.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 6" (type "prepreg") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In6.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 7" (type "core") (thickness 0.185714) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 104 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0001000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Fertigungsunterlagen/02 Gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/Motor1/VMOT")
  (footprint "0_EPAK:CP_Rad_D8_H6" (layer "B.Cu")
    (at 117.25 95.25 -90)
    (property "Comments" "wird beigestellt")
    (property "Manufac" "KEMET")
    (property "Params" "50mR 63V 125°C 2000h")
    (property "PartNr" "A759KC226M1JAAE054 ")
    (property "Place" "YES")
    (property "Sheetfile" "stepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C101" (at -4.75 0 unlocked) (layer "B.SilkS") hide)
    (fp_text value "22u" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -1.75 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "/Motor1/VMOT") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${EPAK_3DMOD}/Capacitors_ThroughHole.3dshapes/CP_Rad_D8_H6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_EPAK:CP_Rad_D8_H6" (layer "B.Cu")
    (at 238.75 95.25 -90)
    (property "Comments" "wird beigestellt")
    (property "Manufac" "KEMET")
    (property "Params" "50mR 63V 125°C 2000h")
    (property "PartNr" "A759KC226M1JAAE054 ")
    (property "Place" "YES")
    (property "Sheetfile" "stepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C102" (at -4.75 0 unlocked) (layer "B.SilkS") hide)
    (fp_text value "22u" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -1.75 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "/Motor1/VMOT") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive") (zone_connect 1))
    (model "${EPAK_3DMOD}/Capacitors_ThroughHole.3dshapes/CP_Rad_D8_H6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_EPAK:CP_Rad_D8_H6" (layer "B.Cu")
    (at 108.5 95.25 -90)
    (property "Comments" "wird beigestellt")
    (property "Manufac" "KEMET")
    (property "Params" "50mR 63V 125°C 2000h")
    (property "PartNr" "A759KC226M1JAAE054 ")
    (property "Place" "YES")
    (property "Sheetfile" "motordriver.kicad_sch")
    (property "Sheetname" "Motor4")
    (attr through_hole)
    (fp_text reference "C708" (at -4.75 0 unlocked) (layer "B.SilkS") hide)
    (fp_text value "22u" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -1.75 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "/Motor1/VMOT") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${EPAK_3DMOD}/Capacitors_ThroughHole.3dshapes/CP_Rad_D8_H6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_EPAK:CP_Rad_D8_H6" (layer "B.Cu")
    (at 176.25 95.25 180)
    (property "Comments" "wird beigestellt")
    (property "Manufac" "KEMET")
    (property "Params" "50mR 63V 125°C 2000h")
    (property "PartNr" "A759KC226M1JAAE054 ")
    (property "Place" "YES")
    (property "Sheetfile" "motordriver.kicad_sch")
    (property "Sheetname" "Motor3")
    (attr through_hole)
    (fp_text reference "C311" (at 5 0 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "22u" (at 0 0 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -1.75 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "/Motor1/VMOT") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${EPAK_3DMOD}/Capacitors_ThroughHole.3dshapes/CP_Rad_D8_H6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_EPAK:CP_Rad_D8_H6" (layer "B.Cu")
    (at 247.75 95.25 -90)
    (property "Comments" "wird beigestellt")
    (property "Manufac" "KEMET")
    (property "Params" "50mR 63V 125°C 2000h")
    (property "PartNr" "A759KC226M1JAAE054 ")
    (property "Place" "YES")
    (property "Sheetfile" "motordriver.kicad_sch")
    (property "Sheetname" "Motor1")
    (attr through_hole)
    (fp_text reference "C511" (at -4.75 0 unlocked) (layer "B.SilkS") hide)
    (fp_text value "22u" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -1.75 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "/Motor1/VMOT") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${EPAK_3DMOD}/Capacitors_ThroughHole.3dshapes/CP_Rad_D8_H6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 104 67) (end 252 100)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 1) (net_name "GND") (layers "In1.Cu" "In6.Cu") (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.25))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.4) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 104 100)
        (xy 252 100)
        (xy 252 67)
        (xy 104 67)
      )
    )
  )
)
