(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(layers
		(0 "F.Cu" signal "M1")
		(31 "B.Cu" signal "M2")
		(38 "B.Mask" user "BSM")
		(39 "F.Mask" user "TSM")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
	)
	(setup
		(stackup
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 101.6 63.5)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "AVDD")
	(footprint "Capacitor_SMD:C_01005_0402Metric"
		(layer "F.Cu")
		(at 101.6 63.1)
		(descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "SMD1"
			(at 0 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_01005_0402Metric"
			(at 0 1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_01005_0402Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.275 0)
			(size 0.27 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.275 0)
			(size 0.27 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.25 0)
			(size 0.4 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "AVDD")
		)
		(pad "2" smd roundrect
			(at 0.25 0)
			(size 0.4 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_01005_0402Metric"
		(layer "B.Cu")
		(at 101.6 63.9 180)
		(descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "SMD2"
			(at 0 1 180)
			(layer "B.SilkS")
		)
		(property "Value" "C_01005_0402Metric"
			(at 0 -1 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_01005_0402Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.25 0 180)
			(size 0.4 0.3)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(pad "2" smd roundrect
			(at 0.25 0 180)
			(size 0.4 0.3)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "AVDD")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 99.6 64.5)
		(end 103.6 64.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.6 62.5)
		(end 99.6 64.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.6 62.5)
		(end 103.6 62.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.6 62.5)
		(end 103.6 64.5)
		(layer "Edge.Cuts")
	)
)