(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 6.338)
		(legacy_teardrops no)
	)
	(paper "USLedger")
	(layers
		(0 "F.Cu" signal "F.Cu - hs signal")
		(4 "In1.Cu" power "In1.Cu - AGND")
		(6 "In2.Cu" power "In2.Cu - VCC_3V3")
		(8 "In3.Cu" signal "In3.Cu - h signal")
		(10 "In4.Cu" signal "In4.Cu - v signal")
		(12 "In5.Cu" power "In5.Cu - VCC_5V")
		(14 "In6.Cu" signal "In6.Cu - x signal")
		(2 "B.Cu" signal "B.Cu - signal")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "prepreg")
				(thickness 0.48)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "core")
				(thickness 0.48)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In5.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 6"
				(type "prepreg")
				(thickness 0.274)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In6.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 7"
				(type "core")
				(thickness 0.274)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 86 194)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-Pad1)")
	(net 2 "unconnected-(J1-Pad2)")
	(net 3 "unconnected-(J1-Pad3)")
	(net 4 "unconnected-(J1-Pad4)")
	(net 5 "unconnected-(J1-Pad95)")
	(net 6 "unconnected-(J1-Pad96)")
	(net 7 "unconnected-(J1-Pad97)")
	(net 8 "unconnected-(J1-Pad98)")
	(net 9 "unconnected-(J1-Pad99)")
	(net 10 "unconnected-(J1-Pad100)")
	(net 11 "MIM0_ADC0_BIAS_REF_CON")
	(net 12 "MIM0_ADC0_BIAS_ELEC_CON")
	(net 13 "MIM0_ADC0_REF_ELEC_CON")
	(net 14 "MIM0_ADC0_IN1P_CON")
	(net 15 "MIM0_ADC0_IN2P_CON")
	(net 16 "MIM0_ADC0_IN3P_CON")
	(net 17 "MIM0_ADC0_IN4P_CON")
	(net 18 "MIM0_ADC0_IN5P_CON")
	(net 19 "MIM0_ADC0_IN6P_CON")
	(net 20 "MIM0_ADC0_IN7P_CON")
	(net 21 "MIM0_ADC0_IN8P_CON")
	(net 22 "MIM0_ADC1_IN8P_CON")
	(net 23 "MIM0_ADC1_IN7P_CON")
	(net 24 "MIM0_ADC1_IN6P_CON")
	(net 25 "MIM0_ADC1_IN5P_CON")
	(net 26 "MIM0_ADC1_IN4P_CON")
	(net 27 "MIM0_ADC1_IN3P_CON")
	(net 28 "MIM0_ADC1_IN2P_CON")
	(net 29 "MIM0_ADC1_IN1P_CON")
	(net 30 "MIM0_ADC1_REF_ELEC_CON")
	(net 31 "MIM0_ADC1_BIAS_ELEC_CON")
	(net 32 "MIM0_ADC1_BIAS_REF_CON")
	(net 33 "MIM1_ADC0_BIAS_REF_CON")
	(net 34 "MIM1_ADC0_BIAS_ELEC_CON")
	(net 35 "MIM1_ADC0_REF_ELEC_CON")
	(net 36 "MIM1_ADC0_IN1P_CON")
	(net 37 "MIM1_ADC0_IN2P_CON")
	(net 38 "MIM1_ADC0_IN3P_CON")
	(net 39 "MIM1_ADC0_IN4P_CON")
	(net 40 "MIM1_ADC0_IN5P_CON")
	(net 41 "MIM1_ADC0_IN6P_CON")
	(net 42 "MIM1_ADC0_IN7P_CON")
	(net 43 "MIM1_ADC0_IN8P_CON")
	(net 44 "MIM1_ADC1_IN8P_CON")
	(net 45 "MIM1_ADC1_IN7P_CON")
	(net 46 "MIM1_ADC1_IN6P_CON")
	(net 47 "MIM1_ADC1_IN5P_CON")
	(net 48 "MIM1_ADC1_IN4P_CON")
	(net 49 "MIM1_ADC1_IN3P_CON")
	(net 50 "MIM1_ADC1_IN2P_CON")
	(net 51 "MIM1_ADC1_IN1P_CON")
	(net 52 "MIM1_ADC1_REF_ELEC_CON")
	(net 53 "MIM1_ADC1_BIAS_ELEC_CON")
	(net 54 "MIM1_ADC1_BIAS_REF_CON")
	(net 55 "unconnected-(J10-Pad1)")
	(net 56 "unconnected-(J10-Pad2)")
	(net 57 "unconnected-(J10-Pad3)")
	(net 58 "unconnected-(J10-Pad4)")
	(net 59 "unconnected-(J10-Pad95)")
	(net 60 "unconnected-(J10-Pad96)")
	(net 61 "unconnected-(J10-Pad97)")
	(net 62 "unconnected-(J10-Pad98)")
	(net 63 "unconnected-(J10-Pad99)")
	(net 64 "unconnected-(J10-Pad100)")
	(net 65 "AGND")
	(footprint "mi32-main-footprints:hirose-100-pin-receptacle-DF40HC-3.0-100DS-0.4V-58"
		(locked yes)
		(layer "F.Cu")
		(at 117 162 90)
		(descr "DF40HC(3.0)-100DS-0.4V(58)-1")
		(tags "Connector")
		(property "Reference" "J1"
			(at 0 0.455 90)
			(layer "F.SilkS")
		)
		(property "Value" "DF40HC(3.0)-100DS-0.4V(58)"
			(at 0 0.455 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" "Good"
			(at 279 45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "HRS"
			(at 279 45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "DF40C-100DS-0.4V(51)"
			(at 279 45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" "None"
			(at 279 45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" "$1.36 USD"
			(at 279 45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "MIM 0 Connectors")
		(sheetfile "mi32_main_mim0_analog_connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.455 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -9.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "unconnected-(J1-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -9.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "unconnected-(J1-Pad2)")
			(pinfunction "2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -9.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(J1-Pad3)")
			(pinfunction "3")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at -9.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(J1-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -9 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -9 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -8.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -8.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -8.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "MIM0_ADC0_BIAS_REF_CON")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -8.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "MIM0_ADC0_BIAS_REF_CON")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -7.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "MIM0_ADC0_BIAS_ELEC_CON")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -7.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "MIM0_ADC0_BIAS_ELEC_CON")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -7.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "MIM0_ADC0_REF_ELEC_CON")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -7.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "MIM0_ADC0_REF_ELEC_CON")
			(pinfunction "14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -7 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -7 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -6.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "MIM0_ADC0_IN1P_CON")
			(pinfunction "17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -6.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "MIM0_ADC0_IN1P_CON")
			(pinfunction "18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -6.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -6.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -5.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "MIM0_ADC0_IN2P_CON")
			(pinfunction "21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -5.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "MIM0_ADC0_IN2P_CON")
			(pinfunction "22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -5.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -5.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -5 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "MIM0_ADC0_IN3P_CON")
			(pinfunction "25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at -5 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "MIM0_ADC0_IN3P_CON")
			(pinfunction "26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at -4.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -4.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -4.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "MIM0_ADC0_IN4P_CON")
			(pinfunction "29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -4.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "MIM0_ADC0_IN4P_CON")
			(pinfunction "30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -3.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -3.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at -3.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "MIM0_ADC0_IN5P_CON")
			(pinfunction "33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at -3.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "MIM0_ADC0_IN5P_CON")
			(pinfunction "34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at -3 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at -3 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -2.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "MIM0_ADC0_IN6P_CON")
			(pinfunction "37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -2.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "MIM0_ADC0_IN6P_CON")
			(pinfunction "38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -2.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at -2.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "40")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at -1.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "MIM0_ADC0_IN7P_CON")
			(pinfunction "41")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at -1.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "MIM0_ADC0_IN7P_CON")
			(pinfunction "42")
			(pintype "passive")
		)
		(pad "43" smd rect
			(at -1.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "43")
			(pintype "passive")
		)
		(pad "44" smd rect
			(at -1.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "44")
			(pintype "passive")
		)
		(pad "45" smd rect
			(at -1 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "MIM0_ADC0_IN8P_CON")
			(pinfunction "45")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at -1 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "MIM0_ADC0_IN8P_CON")
			(pinfunction "46")
			(pintype "passive")
		)
		(pad "47" smd rect
			(at -0.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "47")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at -0.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "48")
			(pintype "passive")
		)
		(pad "49" smd rect
			(at -0.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "49")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at -0.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "50")
			(pintype "passive")
		)
		(pad "51" smd rect
			(at 0.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "51")
			(pintype "passive")
		)
		(pad "52" smd rect
			(at 0.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "52")
			(pintype "passive")
		)
		(pad "53" smd rect
			(at 0.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "MIM0_ADC1_IN8P_CON")
			(pinfunction "53")
			(pintype "passive")
		)
		(pad "54" smd rect
			(at 0.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "MIM0_ADC1_IN8P_CON")
			(pinfunction "54")
			(pintype "passive")
		)
		(pad "55" smd rect
			(at 1 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "55")
			(pintype "passive")
		)
		(pad "56" smd rect
			(at 1 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "56")
			(pintype "passive")
		)
		(pad "57" smd rect
			(at 1.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "MIM0_ADC1_IN7P_CON")
			(pinfunction "57")
			(pintype "passive")
		)
		(pad "58" smd rect
			(at 1.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "MIM0_ADC1_IN7P_CON")
			(pinfunction "58")
			(pintype "passive")
		)
		(pad "59" smd rect
			(at 1.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "59")
			(pintype "passive")
		)
		(pad "60" smd rect
			(at 1.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "60")
			(pintype "passive")
		)
		(pad "61" smd rect
			(at 2.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "MIM0_ADC1_IN6P_CON")
			(pinfunction "61")
			(pintype "passive")
		)
		(pad "62" smd rect
			(at 2.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "MIM0_ADC1_IN6P_CON")
			(pinfunction "62")
			(pintype "passive")
		)
		(pad "63" smd rect
			(at 2.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "63")
			(pintype "passive")
		)
		(pad "64" smd rect
			(at 2.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "64")
			(pintype "passive")
		)
		(pad "65" smd rect
			(at 3 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "MIM0_ADC1_IN5P_CON")
			(pinfunction "65")
			(pintype "passive")
		)
		(pad "66" smd rect
			(at 3 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "MIM0_ADC1_IN5P_CON")
			(pinfunction "66")
			(pintype "passive")
		)
		(pad "67" smd rect
			(at 3.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "67")
			(pintype "passive")
		)
		(pad "68" smd rect
			(at 3.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "68")
			(pintype "passive")
		)
		(pad "69" smd rect
			(at 3.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "MIM0_ADC1_IN4P_CON")
			(pinfunction "69")
			(pintype "passive")
		)
		(pad "70" smd rect
			(at 3.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "MIM0_ADC1_IN4P_CON")
			(pinfunction "70")
			(pintype "passive")
		)
		(pad "71" smd rect
			(at 4.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "71")
			(pintype "passive")
		)
		(pad "72" smd rect
			(at 4.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "72")
			(pintype "passive")
		)
		(pad "73" smd rect
			(at 4.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "MIM0_ADC1_IN3P_CON")
			(pinfunction "73")
			(pintype "passive")
		)
		(pad "74" smd rect
			(at 4.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "MIM0_ADC1_IN3P_CON")
			(pinfunction "74")
			(pintype "passive")
		)
		(pad "75" smd rect
			(at 5 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "75")
			(pintype "passive")
		)
		(pad "76" smd rect
			(at 5 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "76")
			(pintype "passive")
		)
		(pad "77" smd rect
			(at 5.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "MIM0_ADC1_IN2P_CON")
			(pinfunction "77")
			(pintype "passive")
		)
		(pad "78" smd rect
			(at 5.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "MIM0_ADC1_IN2P_CON")
			(pinfunction "78")
			(pintype "passive")
		)
		(pad "79" smd rect
			(at 5.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "79")
			(pintype "passive")
		)
		(pad "80" smd rect
			(at 5.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "80")
			(pintype "passive")
		)
		(pad "81" smd rect
			(at 6.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "MIM0_ADC1_IN1P_CON")
			(pinfunction "81")
			(pintype "passive")
		)
		(pad "82" smd rect
			(at 6.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "MIM0_ADC1_IN1P_CON")
			(pinfunction "82")
			(pintype "passive")
		)
		(pad "83" smd rect
			(at 6.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "83")
			(pintype "passive")
		)
		(pad "84" smd rect
			(at 6.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "84")
			(pintype "passive")
		)
		(pad "85" smd rect
			(at 7 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "MIM0_ADC1_REF_ELEC_CON")
			(pinfunction "85")
			(pintype "passive")
		)
		(pad "86" smd rect
			(at 7 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "MIM0_ADC1_REF_ELEC_CON")
			(pinfunction "86")
			(pintype "passive")
		)
		(pad "87" smd rect
			(at 7.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "MIM0_ADC1_BIAS_ELEC_CON")
			(pinfunction "87")
			(pintype "passive")
		)
		(pad "88" smd rect
			(at 7.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "MIM0_ADC1_BIAS_ELEC_CON")
			(pinfunction "88")
			(pintype "passive")
		)
		(pad "89" smd rect
			(at 7.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "MIM0_ADC1_BIAS_REF_CON")
			(pinfunction "89")
			(pintype "passive")
		)
		(pad "90" smd rect
			(at 7.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "MIM0_ADC1_BIAS_REF_CON")
			(pinfunction "90")
			(pintype "passive")
		)
		(pad "91" smd rect
			(at 8.2 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "91")
			(pintype "passive")
		)
		(pad "92" smd rect
			(at 8.2 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "92")
			(pintype "passive")
		)
		(pad "93" smd rect
			(at 8.6 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "93")
			(pintype "passive")
		)
		(pad "94" smd rect
			(at 8.6 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "AGND")
			(pinfunction "94")
			(pintype "passive")
		)
		(pad "95" smd rect
			(at 9 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(J1-Pad95)")
			(pinfunction "95")
			(pintype "passive+no_connect")
		)
		(pad "96" smd rect
			(at 9 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(J1-Pad96)")
			(pinfunction "96")
			(pintype "passive+no_connect")
		)
		(pad "97" smd rect
			(at 9.4 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(J1-Pad97)")
			(pinfunction "97")
			(pintype "passive+no_connect")
		)
		(pad "98" smd rect
			(at 9.4 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(J1-Pad98)")
			(pinfunction "98")
			(pintype "passive+no_connect")
		)
		(pad "99" smd rect
			(at 9.8 1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(J1-Pad99)")
			(pinfunction "99")
			(pintype "passive+no_connect")
		)
		(pad "100" smd rect
			(at 9.8 -1.54 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(J1-Pad100)")
			(pinfunction "100")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${MI32_3D_MODELS}/hirose-100-pin-receptacle-DF40HC-3.0-100DS-0.4V-58.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.6 167.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at -2.61 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "MIM1_ADC0_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "MIM0_ADC1_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.64 160.7)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 2.29 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 52 "MIM1_ADC1_REF_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "MIM1_ADC0_REF_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.61 166.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 2.7 -0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "MIM1_ADC1_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "MIM1_ADC0_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.62 155.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at -2.4 -0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "MIM1_ADC0_BIAS_REF_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "MIM0_ADC1_BIAS_REF_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.63 157.1)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 2.49 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "MIM0_ADC1_BIAS_REF_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "MIM0_ADC0_BIAS_REF_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mi32-main-footprints:hirose-100-pin-receptacle-DF40HC-3.0-100DS-0.4V-58"
		(locked yes)
		(layer "B.Cu")
		(at 117 162 -90)
		(descr "DF40HC(3.0)-100DS-0.4V(58)-1")
		(tags "Connector")
		(property "Reference" "J10"
			(at 0 -0.455 90)
			(layer "B.SilkS")
		)
		(property "Value" "DF40HC(3.0)-100DS-0.4V(58)"
			(at 0 -0.455 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" "Good"
			(at -45 279 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "HRS"
			(at -45 279 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "DF40C-100DS-0.4V(51)"
			(at -45 279 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PACKAGE" "None"
			(at -45 279 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PRICE" "$1.36 USD"
			(at -45 279 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "MIM 1 Connectors")
		(sheetfile "mi32_main_mim1_analog_connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.455 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -9.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 55 "unconnected-(J10-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -9.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "unconnected-(J10-Pad2)")
			(pinfunction "2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -9.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 57 "unconnected-(J10-Pad3)")
			(pinfunction "3")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at -9.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "unconnected-(J10-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -9 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -9 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -8.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -8.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -8.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "MIM1_ADC0_BIAS_REF_CON")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -8.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "MIM1_ADC0_BIAS_REF_CON")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -7.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "MIM1_ADC0_BIAS_ELEC_CON")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -7.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "MIM1_ADC0_BIAS_ELEC_CON")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -7.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "MIM1_ADC0_REF_ELEC_CON")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -7.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "MIM1_ADC0_REF_ELEC_CON")
			(pinfunction "14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -7 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -7 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -6.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "MIM1_ADC0_IN1P_CON")
			(pinfunction "17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -6.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "MIM1_ADC0_IN1P_CON")
			(pinfunction "18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -6.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -6.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -5.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "MIM1_ADC0_IN2P_CON")
			(pinfunction "21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -5.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "MIM1_ADC0_IN2P_CON")
			(pinfunction "22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -5.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -5.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -5 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "MIM1_ADC0_IN3P_CON")
			(pinfunction "25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at -5 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "MIM1_ADC0_IN3P_CON")
			(pinfunction "26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at -4.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -4.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -4.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "MIM1_ADC0_IN4P_CON")
			(pinfunction "29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -4.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "MIM1_ADC0_IN4P_CON")
			(pinfunction "30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -3.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -3.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at -3.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "MIM1_ADC0_IN5P_CON")
			(pinfunction "33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at -3.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "MIM1_ADC0_IN5P_CON")
			(pinfunction "34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at -3 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at -3 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -2.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "MIM1_ADC0_IN6P_CON")
			(pinfunction "37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -2.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "MIM1_ADC0_IN6P_CON")
			(pinfunction "38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -2.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at -2.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "40")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at -1.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "MIM1_ADC0_IN7P_CON")
			(pinfunction "41")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at -1.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "MIM1_ADC0_IN7P_CON")
			(pinfunction "42")
			(pintype "passive")
		)
		(pad "43" smd rect
			(at -1.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "43")
			(pintype "passive")
		)
		(pad "44" smd rect
			(at -1.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "44")
			(pintype "passive")
		)
		(pad "45" smd rect
			(at -1 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "MIM1_ADC0_IN8P_CON")
			(pinfunction "45")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at -1 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "MIM1_ADC0_IN8P_CON")
			(pinfunction "46")
			(pintype "passive")
		)
		(pad "47" smd rect
			(at -0.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "47")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at -0.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "48")
			(pintype "passive")
		)
		(pad "49" smd rect
			(at -0.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "49")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at -0.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "50")
			(pintype "passive")
		)
		(pad "51" smd rect
			(at 0.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "51")
			(pintype "passive")
		)
		(pad "52" smd rect
			(at 0.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "52")
			(pintype "passive")
		)
		(pad "53" smd rect
			(at 0.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 44 "MIM1_ADC1_IN8P_CON")
			(pinfunction "53")
			(pintype "passive")
		)
		(pad "54" smd rect
			(at 0.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 44 "MIM1_ADC1_IN8P_CON")
			(pinfunction "54")
			(pintype "passive")
		)
		(pad "55" smd rect
			(at 1 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "55")
			(pintype "passive")
		)
		(pad "56" smd rect
			(at 1 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "56")
			(pintype "passive")
		)
		(pad "57" smd rect
			(at 1.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "MIM1_ADC1_IN7P_CON")
			(pinfunction "57")
			(pintype "passive")
		)
		(pad "58" smd rect
			(at 1.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "MIM1_ADC1_IN7P_CON")
			(pinfunction "58")
			(pintype "passive")
		)
		(pad "59" smd rect
			(at 1.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "59")
			(pintype "passive")
		)
		(pad "60" smd rect
			(at 1.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "60")
			(pintype "passive")
		)
		(pad "61" smd rect
			(at 2.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "MIM1_ADC1_IN6P_CON")
			(pinfunction "61")
			(pintype "passive")
		)
		(pad "62" smd rect
			(at 2.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "MIM1_ADC1_IN6P_CON")
			(pinfunction "62")
			(pintype "passive")
		)
		(pad "63" smd rect
			(at 2.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "63")
			(pintype "passive")
		)
		(pad "64" smd rect
			(at 2.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "64")
			(pintype "passive")
		)
		(pad "65" smd rect
			(at 3 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "MIM1_ADC1_IN5P_CON")
			(pinfunction "65")
			(pintype "passive")
		)
		(pad "66" smd rect
			(at 3 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "MIM1_ADC1_IN5P_CON")
			(pinfunction "66")
			(pintype "passive")
		)
		(pad "67" smd rect
			(at 3.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "67")
			(pintype "passive")
		)
		(pad "68" smd rect
			(at 3.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "68")
			(pintype "passive")
		)
		(pad "69" smd rect
			(at 3.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "MIM1_ADC1_IN4P_CON")
			(pinfunction "69")
			(pintype "passive")
		)
		(pad "70" smd rect
			(at 3.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "MIM1_ADC1_IN4P_CON")
			(pinfunction "70")
			(pintype "passive")
		)
		(pad "71" smd rect
			(at 4.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "71")
			(pintype "passive")
		)
		(pad "72" smd rect
			(at 4.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "72")
			(pintype "passive")
		)
		(pad "73" smd rect
			(at 4.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "MIM1_ADC1_IN3P_CON")
			(pinfunction "73")
			(pintype "passive")
		)
		(pad "74" smd rect
			(at 4.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "MIM1_ADC1_IN3P_CON")
			(pinfunction "74")
			(pintype "passive")
		)
		(pad "75" smd rect
			(at 5 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "75")
			(pintype "passive")
		)
		(pad "76" smd rect
			(at 5 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "76")
			(pintype "passive")
		)
		(pad "77" smd rect
			(at 5.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "MIM1_ADC1_IN2P_CON")
			(pinfunction "77")
			(pintype "passive")
		)
		(pad "78" smd rect
			(at 5.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "MIM1_ADC1_IN2P_CON")
			(pinfunction "78")
			(pintype "passive")
		)
		(pad "79" smd rect
			(at 5.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "79")
			(pintype "passive")
		)
		(pad "80" smd rect
			(at 5.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "80")
			(pintype "passive")
		)
		(pad "81" smd rect
			(at 6.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "MIM1_ADC1_IN1P_CON")
			(pinfunction "81")
			(pintype "passive")
		)
		(pad "82" smd rect
			(at 6.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "MIM1_ADC1_IN1P_CON")
			(pinfunction "82")
			(pintype "passive")
		)
		(pad "83" smd rect
			(at 6.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "83")
			(pintype "passive")
		)
		(pad "84" smd rect
			(at 6.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "84")
			(pintype "passive")
		)
		(pad "85" smd rect
			(at 7 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "MIM1_ADC1_REF_ELEC_CON")
			(pinfunction "85")
			(pintype "passive")
		)
		(pad "86" smd rect
			(at 7 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "MIM1_ADC1_REF_ELEC_CON")
			(pinfunction "86")
			(pintype "passive")
		)
		(pad "87" smd rect
			(at 7.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "MIM1_ADC1_BIAS_ELEC_CON")
			(pinfunction "87")
			(pintype "passive")
		)
		(pad "88" smd rect
			(at 7.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "MIM1_ADC1_BIAS_ELEC_CON")
			(pinfunction "88")
			(pintype "passive")
		)
		(pad "89" smd rect
			(at 7.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 54 "MIM1_ADC1_BIAS_REF_CON")
			(pinfunction "89")
			(pintype "passive")
		)
		(pad "90" smd rect
			(at 7.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 54 "MIM1_ADC1_BIAS_REF_CON")
			(pinfunction "90")
			(pintype "passive")
		)
		(pad "91" smd rect
			(at 8.2 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "91")
			(pintype "passive")
		)
		(pad "92" smd rect
			(at 8.2 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "92")
			(pintype "passive")
		)
		(pad "93" smd rect
			(at 8.6 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "93")
			(pintype "passive")
		)
		(pad "94" smd rect
			(at 8.6 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "AGND")
			(pinfunction "94")
			(pintype "passive")
		)
		(pad "95" smd rect
			(at 9 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "unconnected-(J10-Pad95)")
			(pinfunction "95")
			(pintype "passive+no_connect")
		)
		(pad "96" smd rect
			(at 9 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "unconnected-(J10-Pad96)")
			(pinfunction "96")
			(pintype "passive+no_connect")
		)
		(pad "97" smd rect
			(at 9.4 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "unconnected-(J10-Pad97)")
			(pinfunction "97")
			(pintype "passive+no_connect")
		)
		(pad "98" smd rect
			(at 9.4 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "unconnected-(J10-Pad98)")
			(pinfunction "98")
			(pintype "passive+no_connect")
		)
		(pad "99" smd rect
			(at 9.8 -1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "unconnected-(J10-Pad99)")
			(pinfunction "99")
			(pintype "passive+no_connect")
		)
		(pad "100" smd rect
			(at 9.8 1.54 270)
			(size 0.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "unconnected-(J10-Pad100)")
			(pinfunction "100")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${MI32_3D_MODELS}/hirose-100-pin-receptacle-DF40HC-3.0-100DS-0.4V-58.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.62 163.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 2.51 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "MIM0_ADC1_REF_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "MIM0_ADC0_REF_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.61 168.7 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 2.6 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "MIM0_ADC1_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "MIM0_ADC0_BIAS_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.62 161.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -2.31 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "MIM1_ADC0_REF_ELEC_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "MIM0_ADC1_REF_ELEC_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(placed yes)
		(layer "B.Cu")
		(at 125.607448 154.711158)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 2.29 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0R"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Electrode Connector")
		(sheetfile "electrode_connector.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "MIM1_ADC1_BIAS_REF_CON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "MIM1_ADC0_BIAS_REF_CON")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 86.6 131)
		(end 86.6 193)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 86.6 131)
		(mid 86.892893 130.292893)
		(end 87.6 130)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.6 194)
		(end 133 194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133 130)
		(end 133 194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.6 130)
		(end 133 130)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 87.6 194)
		(mid 86.892893 193.707107)
		(end 86.6 193)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
