(kicad_pcb
	(version 20240225)
	(generator "pcbnew")
	(generator_version "8.99")
	(general
		(thickness 2.93)
		(legacy_teardrops no)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.7)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.7)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010f0_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "production/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(footprint "0IBF_IC_spezial:SO-8_3.9x4.9mm_P1.27mm_IBF"
		(layer "B.Cu")
		(at 69 -14 -90)
		(descr "SO8, IBFEEW standard")
		(tags "SOIC SO8")
		(property "Reference" "IC5"
			(at 0 3.4 -90)
			(layer "B.SilkS")
		)
		(property "Value" "AD8418AWBRZ"
			(at 0 -3.4 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "0IBF_IC_spezial:SO-8_3.9x4.9mm_P1.27mm_IBF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "OPV, current sense over the TOP OPV, differential amplifier, high common mode range  (70V) / Gain=20 / bis 250kHz SO8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "AD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "AD8418AWBRZ"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "RS" "798-9903"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Farnell" "2383472"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "mouser" "584-AD8418AWBRZ "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "digikey" "505-AD8418AWBRZ-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Alternative" "AD8418AWHRZ"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.2 0)
			(layer "B.Fab")
		)
		(pad "2" smd roundrect
			(at -2.575 0.635 270)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "gnd")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.575 -0.635 270)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "ref2")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 110.5 -95)
		(end 104 -101.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110.5 -1.27)
		(end 110.5 -95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 5 -97.5)
		(end 8 -101.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 -1.27)
		(end 71.12 -1.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 -95)
		(end 2 -97.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 5 -97.5)
		(end 2 -97.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 71.12 -1.27)
		(end 110.5 -1.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 -95)
		(end 0 -1.27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104 -101.2)
		(end 8 -101.2)
		(layer "Edge.Cuts")
	)
	(gr_text "TOP"
		(at -14.3 50.65 0)
		(layer "F.Cu")
	)
	(gr_text "Pumpensteuerung SEQU\nBedienteil 140mm v31a"
		(at -5.25 52.1 0)
		(layer "F.Cu")
	)
	(gr_text "compare GND zone fill around both PAD4 on both AD8418:\n- these pin is unconnected in eeschema (not available in the symbol)\n- on one footprint pad 4 is leaved unconnected\n- on the other footprint pad4 is overflooded with copper"
		(at 8.6 34 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(name "gnd")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 0.23)
		)
		(polygon
			(pts
				(xy 55.242749 -5.605916) (xy 95.722142 -5.547992) (xy 95.74 -34.12555) (xy 55.180826 -34.138786)
			)
		)
	)
)
