(kicad_pcb
	(version 20240225)
	(generator "pcbnew")
	(generator_version "8.99")
	(general
		(thickness 0.122)
		(legacy_teardrops yes)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0455)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.012)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.025)
				(material "FR4")
				(epsilon_r 3.3)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.012)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0275)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 65.228337 169.967332)
		(grid_origin 65.228337 169.967332)
		(pcbplotparams
			(layerselection 0x00012fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(subtractmaskfromsilk no)
			(outputformat 3)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerber/")
		)
	)
	(net 0 "")
	(net 1 "/D_CLK_N")
	(net 2 "/D_CLK_P")
	(net 3 "/D_D0_N")
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 293.728337 135.967332 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "REF**"
			(at 0 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "R_0201_0603Metric"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0201_0603Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/D_CLK_N")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/D_CLK_P")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "B.Cu")
		(at 296.487546 170.44068 -65)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "REF**"
			(at 0 1.05 115)
			(layer "B.SilkS")
		)
		(property "Value" "R_0201_0603Metric"
			(at 0 -1.05 115)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0201_0603Metric"
			(at 0 0 115)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 115)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 115)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.680001 115)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345001 -0.000001 295)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345001 0.000001 295)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.319999 0.000001 295)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/D_CLK_N")
		)
		(pad "2" smd roundrect
			(at 0.319999 -0.000001 295)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/D_CLK_P")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 289.228337 127.967332)
		(end 313.228337 177.467332)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 3)
		(net_name "/D_D0_N")
		(layer "F.Cu")
		(name "$teardrop_track$")
		(hatch edge 0.5)
		(priority 30093)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 70.857645 167.377956) (xy 70.843 167.314628) (xy 70.628337 167.282628) (xy 70.627363 167.397853)
				(xy 70.709654 167.478945)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/D_D0_N")
		(layer "F.Cu")
		(name "$teardrop_track$")
		(hatch edge 0.5)
		(priority 30094)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 70.857645 167.377956) (xy 70.843 167.314628) (xy 70.628337 167.282628) (xy 70.627363 167.397853)
				(xy 70.709654 167.478945)
			)
		)
	)
)
