(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (3 "In3.Cu" signal)
    (4 "In4.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ".")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/rasp_cm/HDMI_CK_N")
  (net 3 "/rasp_cm/HDMI_CK_P")
  (net 4 "/hdmi_conn/HDMI_D0_N")
  (net 5 "/hdmi_conn/HDMI_D0_P")
  (net 6 "/hdmi_conn/HDMI_D1_N")
  (net 7 "/hdmi_conn/HDMI_D1_P")
  (net 8 "/hdmi_conn/HDMI_D2_N")
  (net 9 "/hdmi_conn/HDMI_D2_P")
  (net 10 "/hdmi_conn/HDMI_CEC")
  (net 11 "/hdmi_conn/HDMI_SDA")
  (net 12 "/hdmi_conn/HDMI_SCL")
  (net 13 "/hdmi_conn/HDMI_HPD")
  (net 14 "+5V")
  (footprint "FS-Diode:TestFootprint" (layer "F.Cu")
    (at 22.8 18.07 180)
    (property "Reference" "U13" (at 0 1.8 180) (layer "F.SilkS"))
    (property "Value" "TestFootprint" (at 0 -1.7 180) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (clearance 0.12)
    (attr smd)
    (pad "1" smd rect (at -2.575 0.65 180) (size 0.45 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/hdmi_conn/HDMI_D2_P")
    )
    (pad "2" smd rect (at -2 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/hdmi_conn/HDMI_D2_N")
    )
    (pad "3" smd rect (at -1.5 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at -1 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/hdmi_conn/HDMI_D1_P")
    )
    (pad "5" smd rect (at -0.5 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/hdmi_conn/HDMI_D1_N")
    )
    (pad "6" smd rect (at 0 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/hdmi_conn/HDMI_SCL")
    )
    (pad "7" smd rect (at 0.5 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/hdmi_conn/HDMI_D0_P")
    )
    (pad "8" smd rect (at 1 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/hdmi_conn/HDMI_D0_N")
    )
    (pad "9" smd rect (at 1.5 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/hdmi_conn/HDMI_HPD")
    )
    (pad "10" smd rect (at 2 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/rasp_cm/HDMI_CK_P")
    )
    (pad "11" smd rect (at 2.5 0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/rasp_cm/HDMI_CK_N")
    )
    (pad "12" smd rect (at 2.25 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (pad "13" smd rect (at 1.5 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+5V")
    )
    (pad "14" smd rect (at 0.75 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (pad "15" smd rect (at 0 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/hdmi_conn/HDMI_SDA")
    )
    (pad "16" smd rect (at -0.75 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (pad "17" smd rect (at -1.5 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/hdmi_conn/HDMI_CEC")
    )
    (pad "18" smd rect (at -2.25 -0.65 180) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.5 16)
        (xy 19.5 21)
        (xy 26.5 21)
        (xy 26.5 16)
      )
    )
  )
)
