(kicad_pcb (version 20240108) (generator "pcbnew")
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (44 "Edge.Cuts" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (allow_soldermask_bridges_in_footprints no)
  )
  (net 0 "")
  (net 1 "Net1")
  (net_class "Default" ""
    (clearance 0.1)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (gr_arc
    (start 105 100)
    (mid 103.535534 103.535534)
    (end 100 105)
    (layer "Edge.Cuts")
  )
)
