(kicad_pcb
	(version 20241007)
	(generator "pcbnew")
	(generator_version "8.99")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x000010fc_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(IC4-OB2-Pad23)")
	(net 2 "Net-(IC4-VS{slash}VSA{slash}VSB-Pad30)")
	(net 3 "unconnected-(IC4-BRA-Pad9)")
	(net 4 "unconnected-(IC4-SRB-Pad22)")
	(net 5 "+3V3")
	(net 6 "Net-(IC4-OB1-Pad26)")
	(net 7 "unconnected-(IC4-VHS-Pad35)")
	(net 8 "unconnected-(IC4-BRB-Pad25)")
	(net 9 "Net-(IC4-OA2-Pad10)")
	(net 10 "Net-(IC4-OA1-Pad2)")
	(net 11 "Net-(IC4-GND-Pad17)")
	(net 12 "unconnected-(IC4-5V_OUT-Pad13)")
	(net 13 "unconnected-(IC4-CLK-Pad21)")
	(net 14 "unconnected-(IC4-Vcc_IO-Pad40)")
	(net 15 "unconnected-(IC4-SRA-Pad12)")
	(net 16 "unconnected-(IC4-TEST_SE-Pad43)")
	(net 17 "unconnected-(R10-Pad1)")
	(net 18 "unconnected-(R11-Pad1)")
	(net 19 "unconnected-(R12-Pad1)")
	(net 20 "unconnected-(R13-Pad1)")
	(net 21 "Net-(R14-Pad1)")
	(net 22 "Net-(R15-Pad1)")
	(net 23 "SPI1_MOSI")
	(net 24 "SPI1_MISO")
	(net 25 "SPI1_SCK")
	(net 26 "SPI1_SSEL")
	(net 27 "PWM_MCOA1")
	(net 28 "unconnected-(IC4-SG_TST-Pad38)")
	(net 29 "IO_P1_1")
	(net 30 "IO_P1_0")
	(net 31 "unconnected-(IC4-TEST_ANA-Pad37)")
	(footprint "Package_QFP:TQFP-44_10x10mm_P0.8mm"
		(layer "F.Cu")
		(at 52.2 -39.4)
		(descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "IC4"
			(at 0 -7.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "TMC261C-PA"
			(at 0 7.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" "3529989"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Trinamic"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "TMC261C-PA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reichelt" "TMC261C-PA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" "1460-1043-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" "700-TMC261C-PA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Package_QFP:TQFP-44_10x10mm_P0.8mm")
		(sheetname "/Schrittmotor/")
		(sheetfile "Schrittmotor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5.7 -4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -5.7 -3.2)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC4-OA1-Pad2)")
			(pinfunction "OA1")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -5.7 -2.4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC4-OA1-Pad2)")
			(pinfunction "OA1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -5.7 -1.6)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC4-VS{slash}VSA{slash}VSB-Pad30)")
			(pinfunction "VS/VSA/VSB")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -5.7 -0.8)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC4-OA2-Pad10)")
			(pinfunction "OA2")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -5.7 0)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC4-OA2-Pad10)")
			(pinfunction "OA2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -5.7 0.8)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC4-OA1-Pad2)")
			(pinfunction "OA1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -5.7 1.6)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC4-OA1-Pad2)")
			(pinfunction "OA1")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -5.7 2.4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(IC4-BRA-Pad9)")
			(pinfunction "BRA")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -5.7 3.2)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC4-OA2-Pad10)")
			(pinfunction "OA2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -5.7 4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC4-OA2-Pad10)")
			(pinfunction "OA2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -4 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(IC4-SRA-Pad12)")
			(pinfunction "SRA")
			(pintype "input")
		)
		(pad "13" smd rect
			(at -3.2 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(IC4-5V_OUT-Pad13)")
			(pinfunction "5V_OUT")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -2.4 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "SPI1_MOSI")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "15" smd rect
			(at -1.6 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "SPI1_MISO")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "16" smd rect
			(at -0.8 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "SPI1_SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 0 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC4-GND-Pad17)")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "18" smd rect
			(at 0.8 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "SPI1_SSEL")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "19" smd rect
			(at 1.6 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "PWM_MCOA1")
			(pinfunction "~{ENABLE}")
			(pintype "input")
		)
		(pad "20" smd rect
			(at 2.4 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "21" smd rect
			(at 3.2 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(IC4-CLK-Pad21)")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "22" smd rect
			(at 4 5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(IC4-SRB-Pad22)")
			(pinfunction "SRB")
			(pintype "input")
		)
		(pad "23" smd rect
			(at 5.7 4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC4-OB2-Pad23)")
			(pinfunction "OB2")
			(pintype "output")
		)
		(pad "24" smd rect
			(at 5.7 3.2)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC4-OB2-Pad23)")
			(pinfunction "OB2")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 5.7 2.4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(IC4-BRB-Pad25)")
			(pinfunction "BRB")
			(pintype "input")
		)
		(pad "26" smd rect
			(at 5.7 1.6)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(IC4-OB1-Pad26)")
			(pinfunction "OB1")
			(pintype "output")
		)
		(pad "27" smd rect
			(at 5.7 0.8)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(IC4-OB1-Pad26)")
			(pinfunction "OB1")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 5.7 0)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC4-OB2-Pad23)")
			(pinfunction "OB2")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 5.7 -0.8)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC4-OB2-Pad23)")
			(pinfunction "OB2")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 5.7 -1.6)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC4-VS{slash}VSA{slash}VSB-Pad30)")
			(pinfunction "VS/VSA/VSB")
			(pintype "input")
		)
		(pad "31" smd rect
			(at 5.7 -2.4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(IC4-OB1-Pad26)")
			(pinfunction "OB1")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 5.7 -3.2)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(IC4-OB1-Pad26)")
			(pinfunction "OB1")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 5.7 -4)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "34" smd rect
			(at 4 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "35" smd rect
			(at 3.2 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(IC4-VHS-Pad35)")
			(pinfunction "VHS")
			(pintype "input")
		)
		(pad "36" smd rect
			(at 2.4 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC4-VS{slash}VSA{slash}VSB-Pad30)")
			(pinfunction "VS/VSA/VSB")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 1.6 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(IC4-TEST_ANA-Pad37)")
			(pinfunction "TEST_ANA")
			(pintype "input")
		)
		(pad "38" smd rect
			(at 0.8 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(IC4-SG_TST-Pad38)")
			(pinfunction "SG_TST")
			(pintype "output")
		)
		(pad "39" smd rect
			(at 0 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC4-GND-Pad17)")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "40" smd rect
			(at -0.8 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(IC4-Vcc_IO-Pad40)")
			(pinfunction "Vcc_IO")
			(pintype "input")
		)
		(pad "41" smd rect
			(at -1.6 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "IO_P1_1")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "42" smd rect
			(at -2.4 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "IO_P1_0")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "43" smd rect
			(at -3.2 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(IC4-TEST_SE-Pad43)")
			(pinfunction "TEST_SE")
			(pintype "input")
		)
		(pad "44" smd rect
			(at -4 -5.7 90)
			(size 1.5 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC4-GND-Pad17)")
			(pinfunction "GND")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 21.2 -93.2 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R15"
			(at 3.7 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 114.4 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 22 "Net-(R15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 29 "IO_P1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 33.2 -93.2625 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R12"
			(at 3.8625 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 126.4625 -60.0625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 19 "unconnected-(R12-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 24 "SPI1_MISO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 35.6 -93.2625 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R11"
			(at 3.8625 0.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 128.8625 -57.6625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 18 "unconnected-(R11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 25 "SPI1_SCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 28.4 -93.2625 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R14"
			(at 3.8625 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 121.6625 -64.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 21 "Net-(R14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 30 "IO_P1_0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 30.8 -93.2625 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R13"
			(at 5.1625 -0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 124.0625 -62.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 20 "unconnected-(R13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 23 "SPI1_MOSI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 37.8 -93.2625 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R10"
			(at 4.7125 0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at 131.0625 -55.4625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 17 "unconnected-(R10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 26 "SPI1_SSEL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 26 -93.2625 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R18"
			(at -4.9625 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at -67.2625 -119.2625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 21 "Net-(R14-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0IBF_RCL:R_1206_3216Metric"
		(layer "F.Cu")
		(at 23.6 -93.2625 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal")
		(tags "resistor")
		(property "Reference" "R19"
			(at -3.7625 -0.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "0IBF_RCL:R_1206_3216Metric"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternative" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Bemerkung" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Farnell" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "RS" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "digikey" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "mouser" ""
			(at -69.6625 -116.8625 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "0IBF_RCL:R* Resistor_THT:R_Axial_*")
		(sheetname "/Anschluss/")
		(sheetfile "Anschluss.kicad_sch")
		(attr smd)
		(fp_text user "FP:R1206"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.08888888889)
			(net 22 "Net-(R15-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start -9.3 -102.7)
		(end 235.1 -10.4)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "DRC-check: front soldermask bridges items with different nets"
		(at -66.1 -108 0)
		(layer "F.SilkS")
	)
	(gr_text "The DRC-check {dblquote}front soldermask bridges items with different nets{dblquote} \ndoesn't looks for the newly introduced feature to have tracks with integrated soldermask removing."
		(at 51.4 -79 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
