(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Jumper:Jumper_3_Bridged12"
			(pin_names
				(offset 0) hide)
			(exclude_from_sim yes)
			(in_bom no)
			(on_board yes)
			(property "Reference" "JP"
				(at -2.54 -2.54 0)
			)
			(property "Value" "Jumper_3_Bridged12"
				(at 0 2.794 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Jumper, 3-pole, pins 1+2 closed/bridged"
				(at 0 0 0)
			)
			(property "ki_keywords" "Jumper SPDT"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Jumper* TestPoint*3Pads* TestPoint*Bridge*"
				(at 0 0 0)
			)
			(symbol "Jumper_3_Bridged12_0_0"
				(circle
					(center -3.302 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 3.302 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
			)
			(symbol "Jumper_3_Bridged12_0_1"
				(arc
					(start -0.254 0.508)
					(mid -1.651 0.9912)
					(end -3.048 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Jumper_3_Bridged12_1_1"
				(pin passive line
					(at -6.35 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "C")
					(number "2")
				)
				(pin passive line
					(at 6.35 0 180)
					(length 2.54)
					(name "B")
					(number "3")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(wire
		(pts
			(xy 139.7 49.53) (xy 149.86 49.53)
		)
	)
	(wire
		(pts
			(xy 149.86 38.1) (xy 146.05 38.1)
		)
	)
	(wire
		(pts
			(xy 149.86 40.64) (xy 149.86 38.1)
		)
	)
	(wire
		(pts
			(xy 132.08 40.64) (xy 132.08 38.1)
		)
	)
	(wire
		(pts
			(xy 149.86 49.53) (xy 149.86 48.26)
		)
	)
	(wire
		(pts
			(xy 139.7 41.91) (xy 139.7 49.53)
		)
	)
	(wire
		(pts
			(xy 132.08 38.1) (xy 133.35 38.1)
		)
	)
	(symbol
		(lib_id "Jumper:Jumper_3_Bridged12")
		(at 139.7 38.1 0)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "JP1"
			(at 139.7 31.75 0)
		)
		(property "Value" "Jumper_3_Bridged12"
			(at 139.7 34.29 0)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 139.7 38.1 0)
		)
		(property "Datasheet" "~"
			(at 139.7 38.1 0)
		)
		(property "Description" "Jumper, 3-pole, pins 1+2 closed/bridged"
			(at 139.7 38.1 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "JP1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 132.08 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 132.08 46.99 0)
		)
		(property "Value" "GND"
			(at 132.08 45.72 0)
		)
		(property "Footprint" ""
			(at 132.08 40.64 0)
		)
		(property "Datasheet" ""
			(at 132.08 40.64 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 132.08 40.64 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 149.86 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 152.4 43.1799 0)
		)
		(property "Value" "R"
			(at 152.4 45.7199 0)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 148.082 44.45 90)
		)
		(property "Datasheet" "~"
			(at 149.86 44.45 0)
		)
		(property "Description" "Resistor"
			(at 149.86 44.45 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
