(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 4.69)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "/BUZZ")
	(net 2 "GND")
	(net 3 "VDD")
	(net 4 "+5V")
	(net 5 "Net-(U1-VINT)")
	(net 6 "Net-(U1-VCP)")
	(net 7 "/G2_OUT")
	(net 8 "/G1_OUT")
	(net 9 "Net-(U2-VINT)")
	(net 10 "Net-(U2-VCP)")
	(net 11 "/A1_OUT")
	(net 12 "/A2_OUT")
	(net 13 "/B1_OUT")
	(net 14 "/B2_OUT")
	(net 15 "Net-(D1-A)")
	(net 16 "Net-(D2-A)")
	(net 17 "Net-(D3-A)")
	(net 18 "Net-(D4-A)")
	(net 19 "unconnected-(J1-D+-PadA6)")
	(net 20 "unconnected-(J1-D--PadA7)")
	(net 21 "unconnected-(J1-D+-PadB6)")
	(net 22 "/CC1")
	(net 23 "unconnected-(J1-D--PadB7)")
	(net 24 "unconnected-(J1-SBU2-PadB8)")
	(net 25 "unconnected-(J1-SBU1-PadA8)")
	(net 26 "/CC2")
	(net 27 "/RX0")
	(net 28 "/TX0")
	(net 29 "/SWDIO0")
	(net 30 "unconnected-(J2-~{RESET}-Pad3)")
	(net 31 "unconnected-(J3-~{RESET}-Pad3)")
	(net 32 "/TX1")
	(net 33 "/RX1")
	(net 34 "/SWDIO1")
	(net 35 "Net-(U1-AOUT2)")
	(net 36 "Net-(U2-AOUT2)")
	(net 37 "Net-(U2-BOUT2)")
	(net 38 "/MUSIC2")
	(net 39 "/SPD--")
	(net 40 "/RUN")
	(net 41 "/SPD++")
	(net 42 "/MUSIC")
	(net 43 "/SDA")
	(net 44 "/SCL")
	(net 45 "unconnected-(U1-~{FAULT}-Pad8)")
	(net 46 "/PWM_G2")
	(net 47 "/PWM_G1")
	(net 48 "/PWM_A1")
	(net 49 "/PWM_B2")
	(net 50 "/PWM_A2")
	(net 51 "/PWM_B1")
	(net 52 "unconnected-(U2-~{FAULT}-Pad8)")
	(net 53 "unconnected-(U3-PD2-Pad16)")
	(net 54 "unconnected-(U3-PD7-Pad1)")
	(net 55 "unconnected-(U4-PA2-Pad3)")
	(net 56 "unconnected-(U4-PD7-Pad1)")
	(net 57 "/LED2")
	(net 58 "unconnected-(U4-PC3-Pad10)")
	(net 59 "/LED4")
	(net 60 "unconnected-(U4-PD0-Pad5)")
	(net 61 "unconnected-(U4-PD3-Pad17)")
	(net 62 "/LED1")
	(net 63 "unconnected-(U4-PC0-Pad7)")
	(net 64 "/LED3")
	(net 65 "/SLEEP_PH")
	(net 66 "/SLEEP_G")
	(net 67 "unconnected-(H5-Pad1)")
	(net 68 "unconnected-(H6-Pad1)")
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 167.325 88.775 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 199.7 135.755 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 172.025 72.55)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:SMMS0650-101M"
		(layer "F.Cu")
		(at 148.025 95.525)
		(property "Reference" "L2"
			(at 0.45 -2.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMMS0650-101M"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:SMMS0650-101M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2894722"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U2-AOUT2)")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/A2_OUT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Chilisin_BMRx00060630.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 68.276649 114.649061 70)
		(property "Reference" "G***"
			(at 0 0 70)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 70)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 70)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 70)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 70)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 123.47 96.045 70)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at 0 -1.65 70)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.65 70)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 70)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 70)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 70)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5878906"
			(at 0 0 70)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 70)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 70)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 70)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:Cap_Touch_10mm"
		(layer "F.Cu")
		(at 172.175 116.2 90)
		(property "Reference" "TP5"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SPD+"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:Cap_Touch_10mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at 0 0 90)
			(size 1.524 1.524)
			(layers "F.Cu")
			(net 41 "/SPD++")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.762 -0.512) (xy -0.74297 -0.607671) (xy -0.688777 -0.688777) (xy -0.607671 -0.74297) (xy -0.512 -0.762)
						(xy 0.512 -0.762) (xy 0.607671 -0.74297) (xy 0.688777 -0.688777) (xy 0.74297 -0.607671) (xy 0.762 -0.512)
						(xy 0.762 0.512) (xy 0.74297 0.607671) (xy 0.688777 0.688777) (xy 0.607671 0.74297) (xy 0.512 0.762)
						(xy -0.512 0.762) (xy -0.607671 0.74297) (xy -0.688777 0.688777) (xy -0.74297 0.607671) (xy -0.762 0.512)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(arc
							(start -5 2)
							(mid -4.12132 4.12132)
							(end -2 5)
						)
						(arc
							(start 2 5)
							(mid 4.12132 4.12132)
							(end 5 2)
						)
						(arc
							(start 5 -2)
							(mid 4.12132 -4.12132)
							(end 2 -5)
						)
						(arc
							(start -2 -5)
							(mid -4.12132 -4.12132)
							(end -5 -2)
						)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
				"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu" "B.Cu"
			)
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 166.97502 114.197196) (xy 166.97738 114.028852) (xy 166.978618 114.009263) (xy 167.016315 113.674692)
					(xy 167.020071 113.652581) (xy 167.094991 113.324335) (xy 167.1012 113.302783) (xy 167.212401 112.984989)
					(xy 167.220984 112.964268) (xy 167.367067 112.660923) (xy 167.377916 112.641294) (xy 167.557045 112.356212)
					(xy 167.570024 112.33792) (xy 167.779945 112.074687) (xy 167.79489 112.057964) (xy 168.032964 111.81989)
					(xy 168.049687 111.804945) (xy 168.31292 111.595024) (xy 168.331212 111.582045) (xy 168.616294 111.402916)
					(xy 168.635923 111.392067) (xy 168.939268 111.245984) (xy 168.959989 111.237401) (xy 169.277783 111.1262)
					(xy 169.299335 111.119991) (xy 169.627581 111.045071) (xy 169.649692 111.041315) (xy 169.984263 111.003618)
					(xy 170.003852 111.00238) (xy 170.172196 111.00002) (xy 170.175 111) (xy 174.175 111) (xy 174.177804 111.00002)
					(xy 174.346148 111.00238) (xy 174.365737 111.003618) (xy 174.700308 111.041315) (xy 174.722419 111.045071)
					(xy 175.050665 111.119991) (xy 175.072217 111.1262) (xy 175.390011 111.237401) (xy 175.410732 111.245984)
					(xy 175.714077 111.392067) (xy 175.733706 111.402916) (xy 176.018788 111.582045) (xy 176.03708 111.595024)
					(xy 176.300313 111.804945) (xy 176.317036 111.81989) (xy 176.55511 112.057964) (xy 176.570055 112.074687)
					(xy 176.779976 112.33792) (xy 176.792955 112.356212) (xy 176.972084 112.641294) (xy 176.982933 112.660923)
					(xy 177.129016 112.964268) (xy 177.137599 112.984989) (xy 177.2488 113.302783) (xy 177.255009 113.324335)
					(xy 177.329929 113.652581) (xy 177.333685 113.674692) (xy 177.371382 114.009263) (xy 177.37262 114.028852)
					(xy 177.37498 114.197196) (xy 177.375 114.2) (xy 177.375 118.2) (xy 177.37498 118.202804) (xy 177.37262 118.371148)
					(xy 177.371382 118.390737) (xy 177.333685 118.725308) (xy 177.329929 118.747419) (xy 177.255009 119.075665)
					(xy 177.2488 119.097217) (xy 177.137599 119.415011) (xy 177.129016 119.435732) (xy 176.982933 119.739077)
					(xy 176.972084 119.758707) (xy 176.792955 120.043788) (xy 176.779976 120.062079) (xy 176.570055 120.325312)
					(xy 176.55511 120.342035) (xy 176.317035 120.58011) (xy 176.300312 120.595055) (xy 176.037079 120.804976)
					(xy 176.018788 120.817955) (xy 175.733707 120.997084) (xy 175.714077 121.007933) (xy 175.410732 121.154016)
					(xy 175.390011 121.162599) (xy 175.072217 121.2738) (xy 175.050665 121.280009) (xy 174.722419 121.354929)
					(xy 174.700308 121.358685) (xy 174.365737 121.396382) (xy 174.346148 121.39762) (xy 174.177804 121.39998)
					(xy 174.175 121.4) (xy 170.175 121.4) (xy 170.172196 121.39998) (xy 170.003852 121.39762) (xy 169.984263 121.396382)
					(xy 169.649692 121.358685) (xy 169.627581 121.354929) (xy 169.299335 121.280009) (xy 169.277783 121.2738)
					(xy 168.959989 121.162599) (xy 168.939268 121.154016) (xy 168.635923 121.007933) (xy 168.616293 120.997084)
					(xy 168.331212 120.817955) (xy 168.312921 120.804976) (xy 168.049688 120.595055) (xy 168.032965 120.58011)
					(xy 167.79489 120.342035) (xy 167.779945 120.325312) (xy 167.570024 120.062079) (xy 167.557045 120.043788)
					(xy 167.377916 119.758707) (xy 167.367067 119.739077) (xy 167.220984 119.435732) (xy 167.212401 119.415011)
					(xy 167.1012 119.097217) (xy 167.094991 119.075665) (xy 167.020071 118.747419) (xy 167.016315 118.725308)
					(xy 166.978618 118.390737) (xy 166.97738 118.371148) (xy 166.97502 118.202804) (xy 166.975 118.2)
					(xy 166.975 114.2)
				)
			)
		)
	)
	(footprint "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 183.475 101.38 90)
		(descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
		(tags "tag connect programming header pogo pins")
		(property "Reference" "J2"
			(at 0 2.7 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PROG"
			(at 0 -2.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin, no legs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TC2030*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "KEEPOUT"
			(at 0 0 90)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.54 0 90)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 -1.016 90)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 1.016 90)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" connect circle
			(at -1.27 0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" connect circle
			(at -1.27 -0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 29 "/SWDIO0")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "3" connect circle
			(at 0 0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 30 "unconnected-(J2-~{RESET}-Pad3)")
			(pinfunction "~{RESET}")
			(pintype "open_collector+no_connect")
		)
		(pad "4" connect circle
			(at 0 -0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 27 "/RX0")
			(pinfunction "SWCLK")
			(pintype "output")
		)
		(pad "5" connect circle
			(at 1.27 0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" connect circle
			(at 1.27 -0.635 90)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 28 "/TX0")
			(pinfunction "SWO")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 182.84 100.11) (xy 182.84 102.65) (xy 184.11 102.65) (xy 184.11 100.11)
				)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 142.175 116.2 90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 167.325 83.275 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C50254"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "Net-(U1-VINT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 68.332064 72.343479 4)
		(property "Reference" "G***"
			(at 0 0 4)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 4)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 4)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 4)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 4)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:Cap_Touch_10mm"
		(layer "F.Cu")
		(at 172.5 72.5 90)
		(property "Reference" "TP6"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MUSIC"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:Cap_Touch_10mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at 0 0 90)
			(size 1.524 1.524)
			(layers "F.Cu")
			(net 42 "/MUSIC")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.762 -0.512) (xy -0.74297 -0.607671) (xy -0.688777 -0.688777) (xy -0.607671 -0.74297) (xy -0.512 -0.762)
						(xy 0.512 -0.762) (xy 0.607671 -0.74297) (xy 0.688777 -0.688777) (xy 0.74297 -0.607671) (xy 0.762 -0.512)
						(xy 0.762 0.512) (xy 0.74297 0.607671) (xy 0.688777 0.688777) (xy 0.607671 0.74297) (xy 0.512 0.762)
						(xy -0.512 0.762) (xy -0.607671 0.74297) (xy -0.688777 0.688777) (xy -0.74297 0.607671) (xy -0.762 0.512)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(arc
							(start -5 2)
							(mid -4.12132 4.12132)
							(end -2 5)
						)
						(arc
							(start 2 5)
							(mid 4.12132 4.12132)
							(end 5 2)
						)
						(arc
							(start 5 -2)
							(mid 4.12132 -4.12132)
							(end 2 -5)
						)
						(arc
							(start -2 -5)
							(mid -4.12132 -4.12132)
							(end -5 -2)
						)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
				"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu" "B.Cu"
			)
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 167.30002 70.497196) (xy 167.30238 70.328852) (xy 167.303618 70.309263) (xy 167.341315 69.974692)
					(xy 167.345071 69.952581) (xy 167.419991 69.624335) (xy 167.4262 69.602783) (xy 167.537401 69.284989)
					(xy 167.545984 69.264268) (xy 167.692067 68.960923) (xy 167.702916 68.941294) (xy 167.882045 68.656212)
					(xy 167.895024 68.63792) (xy 168.104945 68.374687) (xy 168.11989 68.357964) (xy 168.357964 68.11989)
					(xy 168.374687 68.104945) (xy 168.63792 67.895024) (xy 168.656212 67.882045) (xy 168.941294 67.702916)
					(xy 168.960923 67.692067) (xy 169.264268 67.545984) (xy 169.284989 67.537401) (xy 169.602783 67.4262)
					(xy 169.624335 67.419991) (xy 169.952581 67.345071) (xy 169.974692 67.341315) (xy 170.309263 67.303618)
					(xy 170.328852 67.30238) (xy 170.497196 67.30002) (xy 170.5 67.3) (xy 174.5 67.3) (xy 174.502804 67.30002)
					(xy 174.671148 67.30238) (xy 174.690737 67.303618) (xy 175.025308 67.341315) (xy 175.047419 67.345071)
					(xy 175.375665 67.419991) (xy 175.397217 67.4262) (xy 175.715011 67.537401) (xy 175.735732 67.545984)
					(xy 176.039077 67.692067) (xy 176.058706 67.702916) (xy 176.343788 67.882045) (xy 176.36208 67.895024)
					(xy 176.625313 68.104945) (xy 176.642036 68.11989) (xy 176.88011 68.357964) (xy 176.895055 68.374687)
					(xy 177.104976 68.63792) (xy 177.117955 68.656212) (xy 177.297084 68.941294) (xy 177.307933 68.960923)
					(xy 177.454016 69.264268) (xy 177.462599 69.284989) (xy 177.5738 69.602783) (xy 177.580009 69.624335)
					(xy 177.654929 69.952581) (xy 177.658685 69.974692) (xy 177.696382 70.309263) (xy 177.69762 70.328852)
					(xy 177.69998 70.497196) (xy 177.7 70.5) (xy 177.7 74.5) (xy 177.69998 74.502804) (xy 177.69762 74.671148)
					(xy 177.696382 74.690737) (xy 177.658685 75.025308) (xy 177.654929 75.047419) (xy 177.580009 75.375665)
					(xy 177.5738 75.397217) (xy 177.462599 75.715011) (xy 177.454016 75.735732) (xy 177.307933 76.039077)
					(xy 177.297084 76.058707) (xy 177.117955 76.343788) (xy 177.104976 76.362079) (xy 176.895055 76.625312)
					(xy 176.88011 76.642035) (xy 176.642035 76.88011) (xy 176.625312 76.895055) (xy 176.362079 77.104976)
					(xy 176.343788 77.117955) (xy 176.058707 77.297084) (xy 176.039077 77.307933) (xy 175.735732 77.454016)
					(xy 175.715011 77.462599) (xy 175.397217 77.5738) (xy 175.375665 77.580009) (xy 175.047419 77.654929)
					(xy 175.025308 77.658685) (xy 174.690737 77.696382) (xy 174.671148 77.69762) (xy 174.502804 77.69998)
					(xy 174.5 77.7) (xy 170.5 77.7) (xy 170.497196 77.69998) (xy 170.328852 77.69762) (xy 170.309263 77.696382)
					(xy 169.974692 77.658685) (xy 169.952581 77.654929) (xy 169.624335 77.580009) (xy 169.602783 77.5738)
					(xy 169.284989 77.462599) (xy 169.264268 77.454016) (xy 168.960923 77.307933) (xy 168.941293 77.297084)
					(xy 168.656212 77.117955) (xy 168.637921 77.104976) (xy 168.374688 76.895055) (xy 168.357965 76.88011)
					(xy 168.11989 76.642035) (xy 168.104945 76.625312) (xy 167.895024 76.362079) (xy 167.882045 76.343788)
					(xy 167.702916 76.058707) (xy 167.692067 76.039077) (xy 167.545984 75.735732) (xy 167.537401 75.715011)
					(xy 167.4262 75.397217) (xy 167.419991 75.375665) (xy 167.345071 75.047419) (xy 167.341315 75.025308)
					(xy 167.303618 74.690737) (xy 167.30238 74.671148) (xy 167.30002 74.502804) (xy 167.3 74.5) (xy 167.3 70.5)
				)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 157.175 116.2)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
		(layer "F.Cu")
		(at 210.8 131.56 90)
		(descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
		(tags "usb usb-c 2.0 pd")
		(property "Reference" "J1"
			(at 0 -5.645 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 0 5.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C165948"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.6 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.6 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -3.25 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd rect
			(at -2.45 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd rect
			(at -1.25 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(pad "A7" smd rect
			(at 0.25 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "unconnected-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "A8" smd rect
			(at 1.25 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd rect
			(at 2.45 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd rect
			(at 3.25 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd rect
			(at 3.25 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd rect
			(at 2.45 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd rect
			(at 1.75 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J1-D+-PadB6)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(pad "B7" smd rect
			(at -0.75 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "unconnected-(J1-D--PadB7)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "B8" smd rect
			(at -1.75 -4.045 90)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd rect
			(at -2.45 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd rect
			(at -3.25 -4.045 90)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.13 90)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.05 90)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.13 90)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.05 90)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 144.000372 47.772317)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 97.168267 146.292261 30)
		(property "Reference" "G***"
			(at 0 0 30)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 30)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 210.04 138.46 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5k1"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23186"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/CC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.175 110.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23192"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/SPD++")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 165.325 87.525 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C15195"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-VCP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.9125 76.3 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "180R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25270"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 64 "/LED3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:tooling_hole"
		(layer "F.Cu")
		(at 201 145 180)
		(property "Reference" "H9"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Tooling"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:tooling_hole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 1.152)
			(layers "*.Mask")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 200.834222 145.726321) (xy 200.676757 145.671222) (xy 200.5355 145.582464) (xy 200.417536 145.4645)
					(xy 200.328778 145.323243) (xy 200.273679 145.165778) (xy 200.255 145) (xy 200.273679 144.834222)
					(xy 200.328778 144.676757) (xy 200.417536 144.5355) (xy 200.5355 144.417536) (xy 200.676757 144.328778)
					(xy 200.834222 144.273679) (xy 201 144.255) (xy 201.165778 144.273679) (xy 201.323243 144.328778)
					(xy 201.4645 144.417536) (xy 201.582464 144.5355) (xy 201.671222 144.676757) (xy 201.726321 144.834222)
					(xy 201.745 145) (xy 201.726321 145.165778) (xy 201.671222 145.323243) (xy 201.582464 145.4645)
					(xy 201.4645 145.582464) (xy 201.323243 145.671222) (xy 201.165778 145.726321) (xy 201 145.745)
				)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 94.166367 43.553772 25)
		(property "Reference" "G***"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:NetTie_1.25mm"
		(layer "F.Cu")
		(at 135.02 85.21)
		(property "Reference" "NT1"
			(at 0.135 -1.585 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PWM_G"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:NetTie_1.25mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(net_tie_pad_groups "1, 2")
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -0.875 0)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 7 "/G2_OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd oval
			(at 0.875 0)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 8 "/G1_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 178.4 98.37)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 71.68 58 25)
		(property "Reference" "G***"
			(at 5 0.999999 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 172.175 116.2 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 167.325 101.5 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 193.35 142.95 -30)
		(property "Reference" "G***"
			(at 0 0 150)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 150)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 202.94 127.46 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 148.804147 43.443134)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 211.445993 64.666224)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 110.275 102.875)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H6"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M2.5"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(H6-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 167.325 96 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C50254"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 9 "Net-(U2-VINT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 95.85 92.95 -45)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -1.65 -45)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.65 -45)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5878906"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.937501 0 315)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.937501 0 315)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 208.91 118.38 -15)
		(property "Reference" "G***"
			(at 0 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 165)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 190.46093 43.808548)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 178.4 96.9)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 114.931282 73.581281 -15)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -0.000001 -1.65 -15)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0.000001 1.65 -15)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -15)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -15)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -15)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5878906"
			(at 0 0 -15)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -15)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 345)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 345)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 157.985 70.612)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25890"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:Cap_Touch_10mm"
		(layer "F.Cu")
		(at 142.175 116.2 90)
		(property "Reference" "TP3"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SPD-"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:Cap_Touch_10mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at 0 0 90)
			(size 1.524 1.524)
			(layers "F.Cu")
			(net 39 "/SPD--")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.762 -0.512) (xy -0.74297 -0.607671) (xy -0.688777 -0.688777) (xy -0.607671 -0.74297) (xy -0.512 -0.762)
						(xy 0.512 -0.762) (xy 0.607671 -0.74297) (xy 0.688777 -0.688777) (xy 0.74297 -0.607671) (xy 0.762 -0.512)
						(xy 0.762 0.512) (xy 0.74297 0.607671) (xy 0.688777 0.688777) (xy 0.607671 0.74297) (xy 0.512 0.762)
						(xy -0.512 0.762) (xy -0.607671 0.74297) (xy -0.688777 0.688777) (xy -0.74297 0.607671) (xy -0.762 0.512)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(arc
							(start -5 2)
							(mid -4.12132 4.12132)
							(end -2 5)
						)
						(arc
							(start 2 5)
							(mid 4.12132 4.12132)
							(end 5 2)
						)
						(arc
							(start 5 -2)
							(mid 4.12132 -4.12132)
							(end 2 -5)
						)
						(arc
							(start -2 -5)
							(mid -4.12132 -4.12132)
							(end -5 -2)
						)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
				"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu" "B.Cu"
			)
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.97502 114.197196) (xy 136.97738 114.028852) (xy 136.978618 114.009263) (xy 137.016315 113.674692)
					(xy 137.020071 113.652581) (xy 137.094991 113.324335) (xy 137.1012 113.302783) (xy 137.212401 112.984989)
					(xy 137.220984 112.964268) (xy 137.367067 112.660923) (xy 137.377916 112.641294) (xy 137.557045 112.356212)
					(xy 137.570024 112.33792) (xy 137.779945 112.074687) (xy 137.79489 112.057964) (xy 138.032964 111.81989)
					(xy 138.049687 111.804945) (xy 138.31292 111.595024) (xy 138.331212 111.582045) (xy 138.616294 111.402916)
					(xy 138.635923 111.392067) (xy 138.939268 111.245984) (xy 138.959989 111.237401) (xy 139.277783 111.1262)
					(xy 139.299335 111.119991) (xy 139.627581 111.045071) (xy 139.649692 111.041315) (xy 139.984263 111.003618)
					(xy 140.003852 111.00238) (xy 140.172196 111.00002) (xy 140.175 111) (xy 144.175 111) (xy 144.177804 111.00002)
					(xy 144.346148 111.00238) (xy 144.365737 111.003618) (xy 144.700308 111.041315) (xy 144.722419 111.045071)
					(xy 145.050665 111.119991) (xy 145.072217 111.1262) (xy 145.390011 111.237401) (xy 145.410732 111.245984)
					(xy 145.714077 111.392067) (xy 145.733706 111.402916) (xy 146.018788 111.582045) (xy 146.03708 111.595024)
					(xy 146.300313 111.804945) (xy 146.317036 111.81989) (xy 146.55511 112.057964) (xy 146.570055 112.074687)
					(xy 146.779976 112.33792) (xy 146.792955 112.356212) (xy 146.972084 112.641294) (xy 146.982933 112.660923)
					(xy 147.129016 112.964268) (xy 147.137599 112.984989) (xy 147.2488 113.302783) (xy 147.255009 113.324335)
					(xy 147.329929 113.652581) (xy 147.333685 113.674692) (xy 147.371382 114.009263) (xy 147.37262 114.028852)
					(xy 147.37498 114.197196) (xy 147.375 114.2) (xy 147.375 118.2) (xy 147.37498 118.202804) (xy 147.37262 118.371148)
					(xy 147.371382 118.390737) (xy 147.333685 118.725308) (xy 147.329929 118.747419) (xy 147.255009 119.075665)
					(xy 147.2488 119.097217) (xy 147.137599 119.415011) (xy 147.129016 119.435732) (xy 146.982933 119.739077)
					(xy 146.972084 119.758707) (xy 146.792955 120.043788) (xy 146.779976 120.062079) (xy 146.570055 120.325312)
					(xy 146.55511 120.342035) (xy 146.317035 120.58011) (xy 146.300312 120.595055) (xy 146.037079 120.804976)
					(xy 146.018788 120.817955) (xy 145.733707 120.997084) (xy 145.714077 121.007933) (xy 145.410732 121.154016)
					(xy 145.390011 121.162599) (xy 145.072217 121.2738) (xy 145.050665 121.280009) (xy 144.722419 121.354929)
					(xy 144.700308 121.358685) (xy 144.365737 121.396382) (xy 144.346148 121.39762) (xy 144.177804 121.39998)
					(xy 144.175 121.4) (xy 140.175 121.4) (xy 140.172196 121.39998) (xy 140.003852 121.39762) (xy 139.984263 121.396382)
					(xy 139.649692 121.358685) (xy 139.627581 121.354929) (xy 139.299335 121.280009) (xy 139.277783 121.2738)
					(xy 138.959989 121.162599) (xy 138.939268 121.154016) (xy 138.635923 121.007933) (xy 138.616293 120.997084)
					(xy 138.331212 120.817955) (xy 138.312921 120.804976) (xy 138.049688 120.595055) (xy 138.032965 120.58011)
					(xy 137.79489 120.342035) (xy 137.779945 120.325312) (xy 137.570024 120.062079) (xy 137.557045 120.043788)
					(xy 137.377916 119.758707) (xy 137.367067 119.739077) (xy 137.220984 119.435732) (xy 137.212401 119.415011)
					(xy 137.1012 119.097217) (xy 137.094991 119.075665) (xy 137.020071 118.747419) (xy 137.016315 118.725308)
					(xy 136.978618 118.390737) (xy 136.97738 118.371148) (xy 136.97502 118.202804) (xy 136.975 118.2)
					(xy 136.975 114.2)
				)
			)
		)
	)
	(footprint "cust_fp:tooling_hole"
		(layer "F.Cu")
		(at 84 146 180)
		(property "Reference" "H7"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Tooling"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:tooling_hole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 1.152)
			(layers "*.Mask")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 83.834222 146.726321) (xy 83.676757 146.671222) (xy 83.5355 146.582464) (xy 83.417536 146.4645)
					(xy 83.328778 146.323243) (xy 83.273679 146.165778) (xy 83.255 146) (xy 83.273679 145.834222) (xy 83.328778 145.676757)
					(xy 83.417536 145.5355) (xy 83.5355 145.417536) (xy 83.676757 145.328778) (xy 83.834222 145.273679)
					(xy 84 145.255) (xy 84.165778 145.273679) (xy 84.323243 145.328778) (xy 84.4645 145.417536) (xy 84.582464 145.5355)
					(xy 84.671222 145.676757) (xy 84.726321 145.834222) (xy 84.745 146) (xy 84.726321 146.165778) (xy 84.671222 146.323243)
					(xy 84.582464 146.4645) (xy 84.4645 146.582464) (xy 84.323243 146.671222) (xy 84.165778 146.726321)
					(xy 84 146.745)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 142.175 110.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23192"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/SPD--")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:Cap_Touch_10mm"
		(layer "F.Cu")
		(at 157.175 116.2 90)
		(property "Reference" "TP4"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RUN"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:Cap_Touch_10mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at 0 0 90)
			(size 1.524 1.524)
			(layers "F.Cu")
			(net 40 "/RUN")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.762 -0.512) (xy -0.74297 -0.607671) (xy -0.688777 -0.688777) (xy -0.607671 -0.74297) (xy -0.512 -0.762)
						(xy 0.512 -0.762) (xy 0.607671 -0.74297) (xy 0.688777 -0.688777) (xy 0.74297 -0.607671) (xy 0.762 -0.512)
						(xy 0.762 0.512) (xy 0.74297 0.607671) (xy 0.688777 0.688777) (xy 0.607671 0.74297) (xy 0.512 0.762)
						(xy -0.512 0.762) (xy -0.607671 0.74297) (xy -0.688777 0.688777) (xy -0.74297 0.607671) (xy -0.762 0.512)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(arc
							(start -5 2)
							(mid -4.12132 4.12132)
							(end -2 5)
						)
						(arc
							(start 2 5)
							(mid 4.12132 4.12132)
							(end 5 2)
						)
						(arc
							(start 5 -2)
							(mid 4.12132 -4.12132)
							(end 2 -5)
						)
						(arc
							(start -2 -5)
							(mid -4.12132 -4.12132)
							(end -5 -2)
						)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
				"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu" "B.Cu"
			)
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 151.97502 114.197196) (xy 151.97738 114.028852) (xy 151.978618 114.009263) (xy 152.016315 113.674692)
					(xy 152.020071 113.652581) (xy 152.094991 113.324335) (xy 152.1012 113.302783) (xy 152.212401 112.984989)
					(xy 152.220984 112.964268) (xy 152.367067 112.660923) (xy 152.377916 112.641294) (xy 152.557045 112.356212)
					(xy 152.570024 112.33792) (xy 152.779945 112.074687) (xy 152.79489 112.057964) (xy 153.032964 111.81989)
					(xy 153.049687 111.804945) (xy 153.31292 111.595024) (xy 153.331212 111.582045) (xy 153.616294 111.402916)
					(xy 153.635923 111.392067) (xy 153.939268 111.245984) (xy 153.959989 111.237401) (xy 154.277783 111.1262)
					(xy 154.299335 111.119991) (xy 154.627581 111.045071) (xy 154.649692 111.041315) (xy 154.984263 111.003618)
					(xy 155.003852 111.00238) (xy 155.172196 111.00002) (xy 155.175 111) (xy 159.175 111) (xy 159.177804 111.00002)
					(xy 159.346148 111.00238) (xy 159.365737 111.003618) (xy 159.700308 111.041315) (xy 159.722419 111.045071)
					(xy 160.050665 111.119991) (xy 160.072217 111.1262) (xy 160.390011 111.237401) (xy 160.410732 111.245984)
					(xy 160.714077 111.392067) (xy 160.733706 111.402916) (xy 161.018788 111.582045) (xy 161.03708 111.595024)
					(xy 161.300313 111.804945) (xy 161.317036 111.81989) (xy 161.55511 112.057964) (xy 161.570055 112.074687)
					(xy 161.779976 112.33792) (xy 161.792955 112.356212) (xy 161.972084 112.641294) (xy 161.982933 112.660923)
					(xy 162.129016 112.964268) (xy 162.137599 112.984989) (xy 162.2488 113.302783) (xy 162.255009 113.324335)
					(xy 162.329929 113.652581) (xy 162.333685 113.674692) (xy 162.371382 114.009263) (xy 162.37262 114.028852)
					(xy 162.37498 114.197196) (xy 162.375 114.2) (xy 162.375 118.2) (xy 162.37498 118.202804) (xy 162.37262 118.371148)
					(xy 162.371382 118.390737) (xy 162.333685 118.725308) (xy 162.329929 118.747419) (xy 162.255009 119.075665)
					(xy 162.2488 119.097217) (xy 162.137599 119.415011) (xy 162.129016 119.435732) (xy 161.982933 119.739077)
					(xy 161.972084 119.758707) (xy 161.792955 120.043788) (xy 161.779976 120.062079) (xy 161.570055 120.325312)
					(xy 161.55511 120.342035) (xy 161.317035 120.58011) (xy 161.300312 120.595055) (xy 161.037079 120.804976)
					(xy 161.018788 120.817955) (xy 160.733707 120.997084) (xy 160.714077 121.007933) (xy 160.410732 121.154016)
					(xy 160.390011 121.162599) (xy 160.072217 121.2738) (xy 160.050665 121.280009) (xy 159.722419 121.354929)
					(xy 159.700308 121.358685) (xy 159.365737 121.396382) (xy 159.346148 121.39762) (xy 159.177804 121.39998)
					(xy 159.175 121.4) (xy 155.175 121.4) (xy 155.172196 121.39998) (xy 155.003852 121.39762) (xy 154.984263 121.396382)
					(xy 154.649692 121.358685) (xy 154.627581 121.354929) (xy 154.299335 121.280009) (xy 154.277783 121.2738)
					(xy 153.959989 121.162599) (xy 153.939268 121.154016) (xy 153.635923 121.007933) (xy 153.616293 120.997084)
					(xy 153.331212 120.817955) (xy 153.312921 120.804976) (xy 153.049688 120.595055) (xy 153.032965 120.58011)
					(xy 152.79489 120.342035) (xy 152.779945 120.325312) (xy 152.570024 120.062079) (xy 152.557045 120.043788)
					(xy 152.377916 119.758707) (xy 152.367067 119.739077) (xy 152.220984 119.435732) (xy 152.212401 119.415011)
					(xy 152.1012 119.097217) (xy 152.094991 119.075665) (xy 152.020071 118.747419) (xy 152.016315 118.725308)
					(xy 151.978618 118.390737) (xy 151.97738 118.371148) (xy 151.97502 118.202804) (xy 151.975 118.2)
					(xy 151.975 114.2)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.175 110.2)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23192"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/RUN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 206.803385 144.029592 -80)
		(property "Reference" "G***"
			(at 0 0 100)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 100)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 100)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 100)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 100)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 202.94 135.76 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 163.8 70.4 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25890"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 140.675 104.325 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 13 "/B1_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 14 "/B2_OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:FUET-1325"
		(layer "F.Cu")
		(at 182.9 86.3 -90)
		(property "Reference" "BZ1"
			(at 0 -0.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FUET-1325H"
			(at 0 1 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:FUET-1325"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2982583"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 7.6 270)
			(size 2.2 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/BUZZ")
			(pinfunction "+")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 0 -7.6 270)
			(size 2.2 2.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/cust_fp/buzzer_C391038.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 140.675 86.675 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "/G1_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "/G2_OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 80.809917 141.075188 -7)
		(property "Reference" "G***"
			(at 0 0 173)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 173)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 173)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 173)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 173)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:SMMS0650-101M"
		(layer "F.Cu")
		(at 148.025 104.325)
		(property "Reference" "L3"
			(at 0.45 -2.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMMS0650-101M"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:SMMS0650-101M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2894722"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "Net-(U2-BOUT2)")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/B2_OUT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Chilisin_BMRx00060630.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.395 69.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 72.5 130 7)
		(property "Reference" "G***"
			(at 5 1 7)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 7)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 7)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 7)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 7)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias_Larger"
		(layer "F.Cu")
		(at 159.325 86.025)
		(descr "HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U1"
			(at 0 -3.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DRV8833PWP"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias_Larger"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8833.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual H-Bridge Motor Driver, HTSSOP-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C50506"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "HTSSOP-16-1EP*4.4x5mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.58)
			(size 1.98 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd rect
			(at 0 0)
			(size 2.46 2.31)
			(layers "F.Mask")
		)
		(pad "" smd roundrect
			(at 0 0.58)
			(size 1.98 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/SLEEP_G")
			(pinfunction "~{SLEEP}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/G1_OUT")
			(pinfunction "AOUT1")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "AISEN")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U1-AOUT2)")
			(pinfunction "AOUT2")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U1-AOUT2)")
			(pinfunction "BOUT2")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "BISEN")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/G1_OUT")
			(pinfunction "BOUT1")
			(pintype "power_out")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U1-~{FAULT}-Pad8)")
			(pinfunction "~{FAULT}")
			(pintype "open_collector+no_connect")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/PWM_G1")
			(pinfunction "BIN1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/PWM_G2")
			(pinfunction "BIN2")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-VCP)")
			(pinfunction "VCP")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-VINT)")
			(pinfunction "VINT")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/PWM_G2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/PWM_G1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at -0.75 -1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.75 0)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.75 1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 2 3.5)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" smd rect
			(at 0 0)
			(size 3.4 5)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" thru_hole circle
			(at 0.75 -1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0.75 0)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0.75 1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.9125 79.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "180R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25270"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 59 "/LED4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 18 "Net-(D4-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 102.275 79.625)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H5"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M2.5"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(H5-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 165.325 100.25 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C15195"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U2-VCP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 80.1 47.5 -10)
		(property "Reference" "G***"
			(at 0 0 170)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 170)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 170)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 170)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 170)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.9125 70 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "180R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25270"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 62 "/LED1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "Net-(D3-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 144.000372 145 -3)
		(property "Reference" "G***"
			(at 0 0 177)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 177)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 177)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 177)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 177)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 140.675 95.525 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C13585"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 11 "/A1_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 12 "/A2_OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:NetTie_1.25mm"
		(layer "F.Cu")
		(at 134.965 94.06)
		(property "Reference" "NT2"
			(at 0.05 1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PWM_A"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:NetTie_1.25mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(net_tie_pad_groups "1, 2")
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -0.875 0)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 12 "/A2_OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd oval
			(at 0.875 0)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 11 "/A1_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 202.1025 131.46 180)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "500mA"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Fuse:Fuse_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C269104"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*polyfuse* *PTC*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
		(layer "F.Cu")
		(at 159.785 73.31 180)
		(descr "QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U4"
			(at 0 -2.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CH32V003FxUx"
			(at 0 2.83 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5299908"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*3x3mm*P0.4mm*EP1.65x1.65mm*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.45 -0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U4-PD7-Pad1)")
			(pinfunction "PD7")
			(pintype "bidirectional+no_connect")
		)
		(pad "2" smd roundrect
			(at -1.45 -0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/MUSIC")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -1.45 0 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U4-PA2-Pad3)")
			(pinfunction "PA2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -1.45 0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.45 0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(U4-PD0-Pad5)")
			(pinfunction "PD0")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" smd roundrect
			(at -0.8 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -0.4 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "unconnected-(U4-PC0-Pad7)")
			(pinfunction "PC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd roundrect
			(at 0 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/SDA")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 0.4 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/SCL")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 0.8 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U4-PC3-Pad10)")
			(pinfunction "PC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd roundrect
			(at 1.45 0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "/LED1")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 1.45 0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "/LED2")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 1.45 0 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/MUSIC2")
			(pinfunction "PC6")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 1.45 -0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "/LED3")
			(pinfunction "PC7")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 1.45 -0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/SWDIO1")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 0.8 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/BUZZ")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 0.4 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(U4-PD3-Pad17)")
			(pinfunction "PD3")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd roundrect
			(at 0 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "/LED4")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -0.4 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/RX1")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -0.8 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/TX1")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 0 0 180)
			(size 1.65 1.65)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_P0.4mm_EP1.85x1.85mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias_Larger"
		(layer "F.Cu")
		(at 159.325 98.75)
		(descr "HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U2"
			(at 0 -3.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DRV8833PWP"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias_Larger"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8833.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual H-Bridge Motor Driver, HTSSOP-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C50506"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "HTSSOP-16-1EP*4.4x5mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.58)
			(size 1.98 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd rect
			(at 0 0)
			(size 2.46 2.31)
			(layers "F.Mask")
		)
		(pad "" smd roundrect
			(at 0 0.58)
			(size 1.98 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/SLEEP_PH")
			(pinfunction "~{SLEEP}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/A1_OUT")
			(pinfunction "AOUT1")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "AISEN")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U2-AOUT2)")
			(pinfunction "AOUT2")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "Net-(U2-BOUT2)")
			(pinfunction "BOUT2")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "BISEN")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/B1_OUT")
			(pinfunction "BOUT1")
			(pintype "power_out")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U2-~{FAULT}-Pad8)")
			(pinfunction "~{FAULT}")
			(pintype "open_collector+no_connect")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/PWM_B1")
			(pinfunction "BIN1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/PWM_B2")
			(pinfunction "BIN2")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U2-VCP)")
			(pinfunction "VCP")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U2-VINT)")
			(pinfunction "VINT")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/PWM_A2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275)
			(size 1.575 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/PWM_A1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at -0.75 -1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.75 0)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.75 1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 2 3.5)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" smd rect
			(at 0 0)
			(size 3.4 5)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" thru_hole circle
			(at 0.75 -1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0.75 0)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0.75 1.5)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 205.1 50 10)
		(property "Reference" "G***"
			(at 0 0 10)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 210.04 124.66 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5k1"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23186"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/CC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:NetTie_1.25mm"
		(layer "F.Cu")
		(at 134.98 102.85 180)
		(property "Reference" "NT3"
			(at -0.16 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PWM_B"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:NetTie_1.25mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(net_tie_pad_groups "1, 2")
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -0.875 0 180)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 14 "/B2_OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd oval
			(at 0.875 0 180)
			(size 1.25 1.25)
			(layers "F.Cu")
			(net 13 "/B1_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.395 70.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 112.1 116.25 -165)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0.000001 -1.65 -165)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at -0.000001 1.65 -165)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -165)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -165)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -165)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5878906"
			(at 0 0 -165)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -165)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 195)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 195)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 182.5 145 -12)
		(property "Reference" "G***"
			(at 0 0 168)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 168)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 168)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 168)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 168)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "cust_fp:SMMS0650-101M"
		(layer "F.Cu")
		(at 148.025 86.675)
		(property "Reference" "L1"
			(at 0.45 -2.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMMS0650-101M"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:SMMS0650-101M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2894722"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U1-AOUT2)")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -3.025 0)
			(size 2.35 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/G2_OUT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Chilisin_BMRx00060630.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
		(layer "F.Cu")
		(at 176.59 101.41 180)
		(descr "QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U3"
			(at 0 -2.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CH32V003FxUx"
			(at 0 2.83 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C5299908"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*3x3mm*P0.4mm*EP1.65x1.65mm*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.41 180)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.45 -0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U3-PD7-Pad1)")
			(pinfunction "PD7")
			(pintype "bidirectional+no_connect")
		)
		(pad "2" smd roundrect
			(at -1.45 -0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/SPD--")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -1.45 0 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/RUN")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -1.45 0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.45 0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/SPD++")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -0.8 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -0.4 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/PWM_G2")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 0 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/SDA")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 0.4 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/SCL")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 0.8 1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/SLEEP_G")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 1.45 0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/PWM_A1")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 1.45 0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/PWM_A2")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 1.45 0 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/SLEEP_PH")
			(pinfunction "PC6")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 1.45 -0.4 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/PWM_B2")
			(pinfunction "PC7")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 1.45 -0.8 180)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/SWDIO0")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 0.8 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U3-PD2-Pad16)")
			(pinfunction "PD2")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd roundrect
			(at 0.4 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/PWM_G1")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 0 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/PWM_B1")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -0.4 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/RX0")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -0.8 -1.45 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/TX0")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 0 0 180)
			(size 1.65 1.65)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_P0.4mm_EP1.85x1.85mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "cust_fp:tooling_hole"
		(layer "F.Cu")
		(at 144 51 180)
		(property "Reference" "H8"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Tooling"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "cust_fp:tooling_hole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 1.152)
			(layers "*.Mask")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 143.834222 51.726321) (xy 143.676757 51.671222) (xy 143.5355 51.582464) (xy 143.417536 51.4645)
					(xy 143.328778 51.323243) (xy 143.273679 51.165778) (xy 143.255 51) (xy 143.273679 50.834222) (xy 143.328778 50.676757)
					(xy 143.417536 50.5355) (xy 143.5355 50.417536) (xy 143.676757 50.328778) (xy 143.834222 50.273679)
					(xy 144 50.255) (xy 144.165778 50.273679) (xy 144.323243 50.328778) (xy 144.4645 50.417536) (xy 144.582464 50.5355)
					(xy 144.671222 50.676757) (xy 144.726321 50.834222) (xy 144.745 51) (xy 144.726321 51.165778) (xy 144.671222 51.323243)
					(xy 144.582464 51.4645) (xy 144.4645 51.582464) (xy 144.323243 51.671222) (xy 144.165778 51.726321)
					(xy 144 51.745)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.9125 73.1 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "180R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C25270"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 57 "/LED2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 16 "Net-(D2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 159.875 79.4)
		(descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
		(tags "tag connect programming header pogo pins")
		(property "Reference" "J3"
			(at 0 2.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PROG"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin, no legs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TC2030*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "KEEPOUT"
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.54 0)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 -1.016)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 1.016)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" connect circle
			(at -1.27 0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" connect circle
			(at -1.27 -0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 34 "/SWDIO1")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "3" connect circle
			(at 0 0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 31 "unconnected-(J3-~{RESET}-Pad3)")
			(pinfunction "~{RESET}")
			(pintype "open_collector+no_connect")
		)
		(pad "4" connect circle
			(at 0 -0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 33 "/RX1")
			(pinfunction "SWCLK")
			(pintype "output")
		)
		(pad "5" connect circle
			(at 1.27 0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" connect circle
			(at 1.27 -0.635)
			(size 0.7874 0.7874)
			(layers "F.Cu" "F.Mask")
			(net 32 "/TX1")
			(pinfunction "SWO")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 161.145 78.765) (xy 158.605 78.765) (xy 158.605 80.035) (xy 161.145 80.035)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 163.675 73.4 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C23192"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "NorthPoleCircuit_PCB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/MUSIC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 76.210814 66.000348 -5)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 151.899223 47.053772 -170)
		(property "Reference" "G***"
			(at 0 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 71.5 46.5 -170)
		(property "Reference" "G***"
			(at 0 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 140.642762 136.767135 -170)
		(property "Reference" "G***"
			(at 0 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 140.847438 121.764942 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 208.5 143.5 165)
		(property "Reference" "G***"
			(at 0 0 165)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 165)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 165)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 165)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 165)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 108.362065 130.249456 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 71.5 143.5 -178)
		(property "Reference" "G***"
			(at 0 0 2)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 2)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 2)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 2)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 2)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 208.5 46.5 178)
		(property "Reference" "G***"
			(at 0 0 178)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 178)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 177.749884 46.808896 -5)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 125.373609 45.898665 5)
		(property "Reference" "G***"
			(at 0 0 5)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 5)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 5)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 5)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 5)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 201.4 122.53 -5)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 108.881266 139.379891 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 93 142 10)
		(property "Reference" "G***"
			(at 5 -1 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 140 101 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 202.733526 68.843479 175)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 75.96559 86 -170)
		(property "Reference" "G***"
			(at 0 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 76.231991 103.791865)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 139.998205 67.766949 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 152.45883 139.70659 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 95.992986 47.511263 175)
		(property "Reference" "G***"
			(at 5 -1 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 201.195877 109.142672 -2)
		(property "Reference" "G***"
			(at 0 0 178)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 178)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 178)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 204.705342 88.190926 10)
		(property "Reference" "G***"
			(at 5 -1 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 10)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 10)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 133.036437 83.537973 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 190 142.5 175)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 85.75 123.75 175)
		(property "Reference" "G***"
			(at 0 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 175)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "LOGO"
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 175)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 157.638176 130.286041 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_line
		(start 215 140)
		(end 215 50)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205 40)
		(end 75 40)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 215 140)
		(mid 212.071068 147.071068)
		(end 205 150)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 65 50)
		(mid 67.928932 42.928932)
		(end 75 40)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 75 150)
		(end 205 150)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 205 40)
		(mid 212.071068 42.928932)
		(end 215 50)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65 50)
		(end 65 140)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 75 150)
		(mid 67.928932 147.071068)
		(end 65 140)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_text "USB 2.0\nINPUT: 5V         0.5A  2.5W"
		(at 214.179764 131.582469 90)
		(layer "B.SilkS")
	)
	(gr_text "Electronics"
		(at 137 76.5 90)
		(layer "Cmts.User")
	)
	(gr_text "Decorations"
		(at 134 76.5 90)
		(layer "Cmts.User")
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 112.1 116.25) (xy 123.5 116.25)
		)
		(height 0)
		(gr_text "11,4000 mm"
			(locked yes)
			(at 117.8 115.1 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 123.47 96.045) (xy 123.47 102.875)
		)
		(height 13.22)
		(gr_text "6,8300 mm"
			(locked yes)
			(at 109.1 99.46 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 112.1 116.25) (xy 95.75 116.25)
		)
		(height 0)
		(gr_text "16,3500 mm"
			(locked yes)
			(at 103.925 115.1 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 123.500001 96.045) (xy 110.25 96.045)
		)
		(height -6.83)
		(gr_text "13,2500 mm"
			(locked yes)
			(at 116.875 101.725 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 95.75 116.25) (xy 95.75 92.95)
		)
		(height 0)
		(gr_text "23,3000 mm"
			(locked yes)
			(at 94.6 104.6 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 123.5 73.581281) (xy 123.5 96.045)
		)
		(height 0)
		(gr_text "22,4637 mm"
			(locked yes)
			(at 122.35 84.813141 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 102.275 79.625) (xy 95.75 79.625)
		)
		(height 0)
		(gr_text "6,5250 mm"
			(locked yes)
			(at 99.0125 78.475 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 114.931282 73.581281) (xy 95.75 73.581281)
		)
		(height 0.081281)
		(gr_text "19,1813 mm"
			(locked yes)
			(at 105.340641 72.35 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 124 96.045) (xy 124 116.25)
		)
		(height 0.499999)
		(gr_text "20,2050 mm"
			(locked yes)
			(at 122.260167 106.057666 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 95.75 92.95) (xy 95.75 79.625)
		)
		(height 6.525)
		(gr_text "13,3250 mm"
			(locked yes)
			(at 101.125 86.2875 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 114.931282 73.581281) (xy 123.5 73.581281)
		)
		(height -0.081281)
		(gr_text "8,5687 mm"
			(locked yes)
			(at 119.215641 72.35 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Cmts.User")
		(pts
			(xy 95.75 73.581281) (xy 95.75 93.232843)
		)
		(height 0)
		(gr_text "19,6516 mm"
			(locked yes)
			(at 94.6 83.407062 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 14)
		(net_name "/B2_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.6 103.6) (xy 139.6 102) (xy 141.8 102) (xy 141.8 102.4) (xy 142 102.6) (xy 146.2 102.6)
				(xy 146.2 106.1) (xy 144.1 106.1) (xy 143.6 105.6) (xy 143.6 103.7) (xy 143.5 103.6)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A2_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.6 96.2) (xy 139.6 97.8) (xy 141.8 97.8) (xy 141.8 97.4) (xy 142 97.2) (xy 146.2 97.2) (xy 146.2 93.7)
				(xy 144.1 93.7) (xy 143.6 94.2) (xy 143.6 96.1) (xy 143.5 96.2)
			)
		)
	)
	(zone
		(net 35)
		(net_name "Net-(U1-AOUT2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 149.8 88.4) (xy 152.4 88.4) (xy 152.4 86.6) (xy 157.4 86.6) (xy 157.4 85.2) (xy 152.4 85.2)
				(xy 152 84.8) (xy 149.8 84.8)
			)
		)
	)
	(zone
		(net 36)
		(net_name "Net-(U2-AOUT2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 149.9 95.5) (xy 152.2 95.5) (xy 152.2 97.8) (xy 152.5 98.1) (xy 157.3 98.1) (xy 157.3 98.6)
				(xy 150.2 98.6) (xy 149.9 98.3)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/A1_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.3 96.8) (xy 154.4 96.8) (xy 154.1 96.5) (xy 154.1 92.5) (xy 153.1 91.5) (xy 140.2 91.5)
				(xy 139.6 92.1) (xy 139.6 94.4) (xy 139.9 94.7) (xy 141.4 94.7) (xy 141.7 94.4) (xy 141.7 92.6)
				(xy 142.1 92.2) (xy 152.7 92.2) (xy 153.3 92.8) (xy 153.3 97.1) (xy 153.6 97.4) (xy 157.3 97.4)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.03 95.4) (xy 177.03 100.4) (xy 177.6 100.4) (xy 177.6 99.1) (xy 177.9 98.8) (xy 178.3 98.8)
				(xy 179.178 97.922) (xy 179.178 95.4)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159.775 67.636822) (xy 159.775 70.60206) (xy 160.375 71.2) (xy 160.375 72.44) (xy 160.8 72.44)
				(xy 160.8 71.14) (xy 161 70.94) (xy 161.3 70.94) (xy 161.91 70.33) (xy 161.91 67.640755)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.69 130.06) (xy 199.7 130.06) (xy 196.44 133.32) (xy 196.44 133.91) (xy 196.44 136.22) (xy 201.28 136.22)
				(xy 201.69 135.81)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VDD")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.84 134.96) (xy 205.24 134.96) (xy 205.74 134.46) (xy 207.54 134.46) (xy 207.54 133.56) (xy 201.84 133.56)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 161.4 86.6) (xy 166.2 86.6) (xy 166.4 86.8) (xy 166.4 87.8) (xy 166.5 87.9) (xy 168.2 87.9)
				(xy 168.2 86.3) (xy 167.9 86) (xy 161.5 86) (xy 161.4 86.1)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/B1_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.3 100.1) (xy 157.3 100.6) (xy 154.7 100.6) (xy 154.3 101) (xy 154.3 106.5) (xy 152.3 108.5)
				(xy 140.9 108.5) (xy 139.8 107.4) (xy 139.8 105.2) (xy 141.8 105.2) (xy 141.8 107) (xy 142.5 107.7)
				(xy 151.7 107.7) (xy 153.4 106) (xy 153.4 100.6) (xy 153.9 100.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VDD")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.84 128.06) (xy 205.14 128.06) (xy 205.74 128.66) (xy 207.54 128.66) (xy 207.54 129.56) (xy 201.84 129.56)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/G1_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.4 87.4) (xy 157.4 87.9) (xy 154.9 87.9) (xy 154.5 88.3) (xy 154.5 89.2) (xy 153 90.7) (xy 148.7 90.7)
				(xy 147.5 89.5) (xy 147.5 84.5) (xy 148.3 84.5) (xy 148.3 89.3) (xy 149 90) (xy 152.5 90) (xy 153.7 88.8)
				(xy 153.7 88) (xy 154.3 87.4)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 161.4 99.3) (xy 166.2 99.3) (xy 166.4 99.5) (xy 166.4 100.5) (xy 166.5 100.6) (xy 168.2 100.6)
				(xy 168.2 99) (xy 167.9 98.7) (xy 161.5 98.7) (xy 161.4 98.8)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VDD")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.84 129.56) (xy 201.84 133.56) (xy 203.74 133.56) (xy 203.74 129.56)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/G2_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.6 87.4) (xy 139.6 89) (xy 141.8 89) (xy 141.8 88.6) (xy 142 88.4) (xy 146.2 88.4) (xy 146.2 84.9)
				(xy 144.1 84.9) (xy 143.6 85.4) (xy 143.6 87.3) (xy 143.5 87.4)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/G1_OUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.4 84.2) (xy 157.4 84.6) (xy 141.8 84.6) (xy 141.6 84.8) (xy 141.6 85.8) (xy 139.6 85.8)
				(xy 139.6 84.2) (xy 139.8 84) (xy 157.2 84)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Net-(U2-BOUT2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 149.9 104.3) (xy 152.2 104.3) (xy 152.2 99.7) (xy 152.5 99.4) (xy 157.3 99.4) (xy 157.3 98.9)
				(xy 150.5 98.9) (xy 149.9 99.5)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 95.685878 62.336665)
					(mid 82.582284 103.57202)
					(end 113.833804 133.495274)
				)
				(arc
					(start 113.833804 133.495274)
					(mid 121.862563 133.801432)
					(end 129.542462 131.44053)
				)
				(arc
					(start 129.542462 131.44053)
					(mid 143.291541 127.677881)
					(end 157.423164 129.546551)
				)
				(arc
					(start 157.423164 129.546551)
					(mid 171.092457 130.117378)
					(end 182.852684 123.126495)
				)
				(arc
					(start 182.852684 123.126495)
					(mid 194.622642 103.904433)
					(end 198.155881 81.643799)
				)
				(arc
					(start 198.155881 81.643799)
					(mid 185.797483 61.572615)
					(end 162.227389 61.754491)
				)
				(arc
					(start 162.227389 61.754491)
					(mid 143.183688 66.513713)
					(end 124.474206 60.575022)
				)
				(arc
					(start 124.474206 60.575022)
					(mid 109.785897 56.649)
					(end 95.685878 62.336665)
				)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 56 36) (xy 221 36) (xy 221 155) (xy 56 155)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 56 36) (xy 221 36) (xy 221 155) (xy 56 155)
			)
		)
	)
)
