(kicad_pcb
	(version 20241228)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.25)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_000000a5)
			(plot_on_all_layers_selection 0x00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(Q1-Pad1)")
	(net 2 "Net-(R1-Pad1)")
	(net 3 "Net-(R2-Pad2)")
	(net 4 "/Col")
	(net 5 "/Base")
	(footprint "Package_TO_SOT_SMD:SOT-223"
		(layer "F.Cu")
		(at 164.025001 100.425001)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "Q1"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Q_NPN_Darlington_ECBC"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(Q1-Pad1)")
		)
		(pad "2" smd rect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/Col")
		)
		(pad "3" smd rect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/Base")
		)
		(pad "4" smd rect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/Col")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder"
		(layer "F.Cu")
		(at 161.8 107 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0425 0 180)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(R1-Pad1)")
		)
		(pad "2" smd rect
			(at 1.0425 0 180)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/Base")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder"
		(layer "F.Cu")
		(at 157.2 101.6 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0425 0 90)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/Base")
		)
		(pad "2" smd rect
			(at 1.0425 0 90)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(R2-Pad2)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder"
		(layer "F.Cu")
		(at 166.6 107)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "100R"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0425 0)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(R1-Pad1)")
		)
		(pad "2" smd rect
			(at 1.0425 0)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/Col")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder"
		(layer "F.Cu")
		(at 157.2 97.4 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0425 0 270)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(Q1-Pad1)")
		)
		(pad "2" smd rect
			(at 1.0425 0 270)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(R2-Pad2)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder"
		(layer "F.Cu")
		(at 166.6 110.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0425 0)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(R1-Pad1)")
		)
		(pad "2" smd rect
			(at 1.0425 0)
			(size 1.145 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(R2-Pad2)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 180 115)
		(end 180 90)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150 115)
		(end 180 115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180 90)
		(end 150 90)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150 90)
		(end 150 115)
		(layer "Edge.Cuts")
	)
	(zone
		(net 4)
		(net_name "/Col")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 154.2 94.5) (xy 169 94.5) (xy 165 110.1) (xy 154.2 110.1)
			)
		)
	)
	(embedded_fonts no)
)
