(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (grid_origin 114.3 66.802)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "+12V")
  (net 4 "Net-(F1-Pad2)")
  (net 5 "/PB0")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "/LED0")
  (net 8 "/LED1")
  (net 9 "/LED2")
  (net 10 "/LED3")
  (net 11 "/LED4")
  (net 12 "/LED5")
  (net 13 "/LED6")
  (net 14 "/LED7")
  (net 15 "/LED8")
  (net 16 "/LED9")
  (net 17 "/LED10")
  (net 18 "/LED11")
  (net 19 "/LED12")
  (net 20 "/LED13")
  (net 21 "/LED14")
  (net 22 "/LED15")
  (net 23 "/PB1")
  (net 24 "/PB2")
  (net 25 "/PB3")
  (net 26 "/PB4")
  (net 27 "/PB5")
  (net 28 "/PB6")
  (net 29 "/PB7")
  (net 30 "/PD0")
  (net 31 "/PD1")
  (net 32 "/PD2")
  (net 33 "/PD3")
  (net 34 "/PD4")
  (net 35 "/PD5")
  (net 36 "/PD6")
  (net 37 "/PD7")
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (at 149.3 82.802)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Reference" "C1" (at 1.25 -4.4 0) (layer "F.SilkS"))
    (property "Value" "CP" (at 1.25 4.4 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.25 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)")
    )
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 131.3625 76.802)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C2" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "C" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+12V")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 142.3625 76.802 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C3" (at 0 -1.65 180) (layer "F.SilkS"))
    (property "Value" "C" (at 0 1.65 180) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0.1324 0.034 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C3-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_VH_B2PS-VH_1x02_P3.96mm_Horizontal" (layer "F.Cu")
    (at 122.3 69.802 -90)
    (descr "JST VH series connector, B2PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (property "Reference" "J1" (at 1.98 -2.55 -90) (layer "F.SilkS"))
    (property "Value" "Conn_01x02_Male" (at 1.98 16.1 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.98 9.45 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(F1-Pad2)")
    )
    (pad "2" thru_hole circle (at 3.96 0 270) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_B2PS-VH_1x02_P3.96mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x16_P2.54mm_Horizontal" (layer "F.Cu")
    (at 197.3 83.802 90)
    (descr "Through hole angled pin header, 2x16, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x16 2.54mm double row")
    (property "Reference" "J2" (at 5.655 -2.27 90) (layer "F.SilkS"))
    (property "Value" "Conn_02x16_Odd_Even" (at 5.655 40.37 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 5.31 19.05 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/LED0")
    )
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/LED1")
    )
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/LED2")
    )
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/LED3")
    )
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/LED4")
    )
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "12" thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/LED5")
    )
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "14" thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/LED6")
    )
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "16" thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/LED7")
    )
    (pad "17" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "18" thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/LED8")
    )
    (pad "19" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "20" thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/LED9")
    )
    (pad "21" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "22" thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/LED10")
    )
    (pad "23" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "24" thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/LED11")
    )
    (pad "25" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "26" thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/LED12")
    )
    (pad "27" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "28" thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/LED13")
    )
    (pad "29" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "30" thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/LED14")
    )
    (pad "31" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V")
    )
    (pad "32" thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/LED15")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (at 131.3 71.802)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Reference" "U1" (at 0 -4.5 0) (layer "F.SilkS"))
    (property "Value" "NCP1117-12_SOT223" (at 0 4.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V")
    )
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V")
    )
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (at 149.3 76.802 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Reference" "U3" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (property "Value" "ATmega328P-PU" (at 3.81 35.35 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 3.81 16.51 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/PD0")
    )
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/PD1")
    )
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/PD2")
    )
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "/PD3")
    )
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/PD4")
    )
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C3-Pad2)")
    )
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND")
    )
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/PB6")
    )
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "/PB7")
    )
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/PD5")
    )
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/PD6")
    )
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/PD7")
    )
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/PB0")
    )
    (pad "15" thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/PB1")
    )
    (pad "16" thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/PB2")
    )
    (pad "17" thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/PB3")
    )
    (pad "18" thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/PB4")
    )
    (pad "19" thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/PB5")
    )
    (pad "20" thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C3-Pad2)")
    )
    (pad "21" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C3-Pad2)")
    )
    (pad "22" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND")
    )
    (pad "23" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "24" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "25" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "26" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "27" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "28" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (at 142.3 71.802)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Reference" "U2" (at 0 -4.5 0) (layer "F.SilkS"))
    (property "Value" "AP1117-50" (at 0 4.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C3-Pad2)")
    )
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C3-Pad2)")
    )
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_Littelfuse-LVR200" (layer "F.Cu")
    (at 139.3 82.802 180)
    (descr "Littelfuse, resettable fuse, PTC, polyswitch LVR200, Ih 2A, http://www.littelfuse.com/~/media/electronics/datasheets/resettable_ptcs/littelfuse_ptc_lvr_catalog_datasheet.pdf.pdf")
    (tags "LVR200 PTC resettable polyswitch ")
    (property "Reference" "F1" (at 6.3 -4.1 180) (layer "F.SilkS"))
    (property "Value" "Fuse" (at 5.5 4.2 180) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 6 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)")
    )
    (pad "2" thru_hole circle (at 11.4 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(F1-Pad2)")
    )
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_Littelfuse-LVR200.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 190.3 83.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q0" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/PB0")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/LED0")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 183.3 83.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q1" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/PB1")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/LED1")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 176.3 83.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q2" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PB2")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/LED2")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 169.3 83.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q3" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/PB3")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/LED3")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 162.3 83.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q4" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/PB4")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/LED4")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 195.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q5" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/PB5")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/LED5")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 199.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q6" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/PB6")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/LED6")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 203.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q7" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/PB7")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/LED7")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 207.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q8" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/PD0")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/LED8")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 211.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q9" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/PD1")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/LED9")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 215.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q10" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/PD2")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/LED10")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 219.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q11" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/PD3")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/LED11")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 223.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q12" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/PD4")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/LED12")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 227.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q13" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/PD5")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/LED13")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 231.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q14" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/PD6")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/LED14")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 235.3 74.802)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q15" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/PD7")
    )
    (pad "2" smd rect (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND")
    )
    (pad "3" smd rect (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LED15")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 187.3 83.802 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R0" (at 0 -1.65 -90) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "/PB0")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 173.3 83.802 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R2" (at 0 -1.65 -90) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 24 "/PB2")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 166.3 83.802 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R3" (at 0 -1.65 -90) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 25 "/PB3")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 159.3 83.8645 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R4" (at 0 -1.65 -90) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 26 "/PB4")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 195.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R5" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 27 "/PB5")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 199.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R6" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 28 "/PB6")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 203.3 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R7" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "/PB7")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 207.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R8" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "/PD0")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 211.3 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R9" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "/PD1")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 215.3 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R10" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "/PD2")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 219.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R11" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "/PD3")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 223.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R12" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 34 "/PD4")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 227.3 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R13" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 35 "/PD5")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 231.3 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R14" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 36 "/PD6")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 235.3625 69.802)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R15" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "/PD7")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.33x1.40mm_HandSolder" (layer "F.Cu")
    (at 180.3 83.802 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R1" (at 0 -1.65 -90) (layer "F.SilkS"))
    (property "Value" "R" (at 0 1.65 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "/PB1")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 1.325 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 244.3 66.802) (end 244.3 86.802)
    (layer "Edge.Cuts"))
  (gr_line (start 244.3 86.802) (end 114.3 86.802)
    (layer "Edge.Cuts"))
  (gr_line (start 114.3 66.802) (end 244.3 66.802)
    (layer "Edge.Cuts"))
  (gr_line (start 114.3 86.802) (end 114.3 66.802)
    (layer "Edge.Cuts"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 66.802)
        (xy 114.3 86.802)
        (xy 244.3 86.802)
        (xy 244.3 66.802)
      )
    )
  )
  (zone (net 3) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 66.802)
        (xy 114.3 86.802)
        (xy 244.3 86.802)
        (xy 244.3 66.802)
      )
    )
  )
)
