(kicad_pcb (version 20200119) (host pcbnew "(5.99.0-1404-g52d891940-dirty)")
  (general
    (thickness 4.62)
    (drawings 1)
    (tracks 5)
    (modules 1)
    (nets 1)
  )
  (page "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user)
    (33 "F.Adhes" user)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user)
    (37 "F.SilkS" user)
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user)
    (41 "Cmts.User" user)
    (42 "Eco1.User" user)
    (43 "Eco2.User" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user)
    (47 "F.CrtYd" user)
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.44) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "HAL lead-free")
      (dielectric_constraints no)
    )
    (last_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (max_error 0.005)
    (defaults
      (edge_clearance 0.01)
      (edge_cuts_line_width 0.05)
      (courtyard_line_width 0.05)
      (copper_line_width 0.2)
      (copper_text_dims (size 1.5 1.5) (thickness 0.3))
      (silk_line_width 0.12)
      (silk_text_dims (size 1 1) (thickness 0.15))
      (other_layers_line_width 0.1)
      (other_layers_text_dims (size 1 1) (thickness 0.15))
      (dimension_units 0)
      (dimension_precision 1)
    )
    (pad_size 1.5 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_7ffffff9)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.101600)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "${plot}")
    )
  )
  (net 0 "")
  (net_class "Default" "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "Housings_DIP:DIP-40_W15.24mm" (layer "F.Cu") (tedit 54130A77)
    (at 164.719 77.597)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference "U1" (at 0 -5.22) (layer "F.SilkS"))
    (fp_text value "DIP-40_W15.24mm${stuff}" (at 0 -3.72) (layer "F.Fab"))
    (fp_text user "field on copper" (at 7.85622 26.98242 unlocked) (layer "F.Cu"))
    (pad "40" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "39" thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "38" thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "37" thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "36" thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "35" thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "34" thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "33" thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "32" thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "31" thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "30" thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "29" thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "28" thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "27" thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "26" thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "25" thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "24" thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "23" thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "22" thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "21" thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "20" thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "19" thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "/Users/jeff/kicad/Package_QFP.3dshapes/HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm.wrl"
      (opacity 0.6500)      (offset (xyz 0 -13 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "/Users/jeff/kicad/Package_QFP.3dshapes/TQFP-48_7x7mm_P0.5mm.wrl"
      (opacity 0.2100)      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Text: ${LAYER} ${00000000-0000-0000-0000-00005e384273:REFERENCE}" (at 151.0919 104.5464) (layer "F.Cu"))
)
