(kicad_pcb (version 20210807) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "SERIAL PIC PROGRAMMER")
  )
  (layers
    (0 "F.Cu" signal "top_layer")
    (31 "B.Cu" signal "bottom_layer")
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 62.23 153.67)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/PC-CLOCK-OUT")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C9-Pad2)")
  (net 7 "Net-(D11-Pad1)")
  (net 8 "Net-(D11-Pad2)")
  (net 9 "Net-(Q1-Pad2)")
  (net 10 "Net-(Q3-Pad2)")
  (net 11 "Net-(R12-Pad1)")
  (net 12 "Net-(R13-Pad1)")
  (net 13 "Net-(R15-Pad1)")
  (net 14 "Net-(R16-Pad1)")
  (net 15 "Net-(R8-Pad1)")
  (net 16 "Net-(RV1-Pad2)")
  (net 17 "VCC")
  (net 18 "VPP")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(D4-Pad2)")
  (net 21 "Net-(D8-Pad2)")
  (net 22 "Net-(D9-Pad2)")
  (net 23 "Net-(D12-Pad2)")
  (net 24 "/pic_sockets/VCC_PIC")
  (net 25 "/CLOCK-RB6")
  (net 26 "/DATA-RB7")
  (net 27 "Net-(D2-Pad2)")
  (net 28 "Net-(D6-Pad2)")
  (net 29 "Net-(D10-Pad2)")
  (net 30 "unconnected-(J1-Pad1)")
  (net 31 "/PC-DATA-IN")
  (net 32 "/PC-DATA-OUT")
  (net 33 "/VPP_ON")
  (net 34 "Net-(Q2-Pad1)")
  (net 35 "unconnected-(J1-Pad2)")
  (net 36 "unconnected-(J1-Pad6)")
  (net 37 "unconnected-(J1-Pad9)")
  (net 38 "/VPP{slash}MCLR")
  (net 39 "unconnected-(P2-Pad2)")
  (net 40 "unconnected-(P2-Pad3)")
  (net 41 "unconnected-(P2-Pad4)")
  (net 42 "unconnected-(P2-Pad5)")
  (net 43 "unconnected-(P2-Pad6)")
  (net 44 "unconnected-(P2-Pad7)")
  (net 45 "unconnected-(P2-Pad9)")
  (net 46 "unconnected-(P2-Pad10)")
  (net 47 "unconnected-(P2-Pad11)")
  (net 48 "unconnected-(P2-Pad12)")
  (net 49 "unconnected-(P2-Pad13)")
  (net 50 "unconnected-(P2-Pad14)")
  (net 51 "unconnected-(P2-Pad15)")
  (net 52 "unconnected-(P2-Pad16)")
  (net 53 "unconnected-(P2-Pad17)")
  (net 54 "unconnected-(P2-Pad18)")
  (net 55 "unconnected-(P2-Pad21)")
  (net 56 "unconnected-(P2-Pad22)")
  (net 57 "unconnected-(P2-Pad23)")
  (net 58 "unconnected-(P2-Pad24)")
  (net 59 "unconnected-(P2-Pad25)")
  (net 60 "unconnected-(P2-Pad26)")
  (net 61 "unconnected-(P3-Pad2)")
  (net 62 "unconnected-(P3-Pad3)")
  (net 63 "unconnected-(P3-Pad4)")
  (net 64 "unconnected-(P3-Pad5)")
  (net 65 "unconnected-(P3-Pad6)")
  (net 66 "unconnected-(P3-Pad7)")
  (net 67 "unconnected-(P3-Pad9)")
  (net 68 "unconnected-(P3-Pad10)")
  (net 69 "unconnected-(P3-Pad13)")
  (net 70 "unconnected-(P3-Pad14)")
  (net 71 "unconnected-(P3-Pad15)")
  (net 72 "unconnected-(P3-Pad16)")
  (net 73 "unconnected-(P3-Pad17)")
  (net 74 "unconnected-(P3-Pad18)")
  (net 75 "unconnected-(P3-Pad19)")
  (net 76 "unconnected-(P3-Pad20)")
  (net 77 "unconnected-(P3-Pad21)")
  (net 78 "unconnected-(P3-Pad22)")
  (net 79 "unconnected-(P3-Pad23)")
  (net 80 "unconnected-(P3-Pad24)")
  (net 81 "unconnected-(P3-Pad25)")
  (net 82 "unconnected-(P3-Pad26)")
  (net 83 "unconnected-(P3-Pad27)")
  (net 84 "unconnected-(P3-Pad28)")
  (net 85 "unconnected-(P3-Pad29)")
  (net 86 "unconnected-(P3-Pad30)")
  (net 87 "unconnected-(P3-Pad33)")
  (net 88 "unconnected-(P3-Pad34)")
  (net 89 "unconnected-(P3-Pad35)")
  (net 90 "unconnected-(P3-Pad36)")
  (net 91 "unconnected-(P3-Pad37)")
  (net 92 "unconnected-(P3-Pad38)")
  (net 93 "unconnected-(U1-Pad7)")
  (net 94 "unconnected-(U4-Pad3)")
  (net 95 "unconnected-(U4-Pad4)")
  (net 96 "unconnected-(U5-Pad1)")
  (net 97 "unconnected-(U5-Pad2)")
  (net 98 "unconnected-(U5-Pad3)")
  (net 99 "unconnected-(U5-Pad6)")
  (net 100 "unconnected-(U5-Pad7)")
  (net 101 "unconnected-(U5-Pad8)")
  (net 102 "unconnected-(U5-Pad9)")
  (net 103 "unconnected-(U5-Pad10)")
  (net 104 "unconnected-(U5-Pad11)")
  (net 105 "unconnected-(U5-Pad15)")
  (net 106 "unconnected-(U5-Pad16)")
  (net 107 "unconnected-(U5-Pad17)")
  (net 108 "unconnected-(U5-Pad18)")
  (net 109 "unconnected-(U6-Pad2)")
  (net 110 "unconnected-(U6-Pad3)")
  (net 111 "unconnected-(U6-Pad5)")
  (footprint "Capacitor_THT:CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal" (layer "F.Cu")
    (tedit 5A533291)
    (at 110.49 78.867 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
    (tags "CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 12.5 -4.31 180) (layer "F.SilkS"))
    (fp_text value "100µF" (at 12.5 4.31 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.5 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 25 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal" (layer "F.Cu")
    (tedit 5A533291)
    (at 84.582 90.17)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
    (tags "CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 12.5 -4.31) (layer "F.SilkS"))
    (fp_text value "220uF" (at 12.5 4.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 25 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252FAB)
    (at 77.47 135.89)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P101" (at 6.13 -2.99) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at 8.03 -1.09) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252FB1)
    (at 158.75 135.89)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P102" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at 9.05 0.91) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252FB5)
    (at 229.87 135.89)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P103" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at -7.87 0.01) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252FA3)
    (at 229.87 44.45)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P104" (at -7.87 -1.65) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252F9E)
    (at 158.75 44.45)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P105" (at -6.75 -1.45) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (tedit 5B252F9A)
    (at 77.47 44.45)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P106" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "CONN_1" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (footprint "footprints:40tex-Ell600" (layer "F.Cu")
    (tedit 5D822BD5)
    (at 175.26 50.8)
    (descr "Support TEXTOOL Dil 40 pins, pads elliptiques, e=600 mils")
    (tags "DEV")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "P3" (at -6.66 -3.6 180) (layer "F.SilkS"))
    (fp_text value "SUPP40" (at -9.16 2.5 180) (layer "F.SilkS"))
    (pad "1" thru_hole oval locked (at 0 0 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/VPP{slash}MCLR") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 61 "unconnected-(P3-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 62 "unconnected-(P3-Pad3)") (pinfunction "3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 63 "unconnected-(P3-Pad4)") (pinfunction "4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 64 "unconnected-(P3-Pad5)") (pinfunction "5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 65 "unconnected-(P3-Pad6)") (pinfunction "6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 66 "unconnected-(P3-Pad7)") (pinfunction "7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 20.32 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 67 "unconnected-(P3-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" thru_hole oval locked (at 0 22.86 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 68 "unconnected-(P3-Pad10)") (pinfunction "10") (pintype "passive+no_connect"))
    (pad "11" thru_hole oval locked (at 0 25.4 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 0 27.94 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 30.48 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 69 "unconnected-(P3-Pad13)") (pinfunction "13") (pintype "passive+no_connect"))
    (pad "14" thru_hole oval locked (at 0 33.02 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 70 "unconnected-(P3-Pad14)") (pinfunction "14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 35.56 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 71 "unconnected-(P3-Pad15)") (pinfunction "15") (pintype "passive+no_connect"))
    (pad "16" thru_hole oval locked (at 0 38.1 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 72 "unconnected-(P3-Pad16)") (pinfunction "16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 40.64 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 73 "unconnected-(P3-Pad17)") (pinfunction "17") (pintype "passive+no_connect"))
    (pad "18" thru_hole oval locked (at 0 43.18 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 74 "unconnected-(P3-Pad18)") (pinfunction "18") (pintype "passive+no_connect"))
    (pad "19" thru_hole oval locked (at 0 45.72 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 75 "unconnected-(P3-Pad19)") (pinfunction "19") (pintype "passive+no_connect"))
    (pad "20" thru_hole oval locked (at 0 48.26 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 76 "unconnected-(P3-Pad20)") (pinfunction "20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval locked (at 15.24 48.26 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 77 "unconnected-(P3-Pad21)") (pinfunction "21") (pintype "passive+no_connect"))
    (pad "22" thru_hole oval locked (at 15.24 45.72 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 78 "unconnected-(P3-Pad22)") (pinfunction "22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 15.24 43.18 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 79 "unconnected-(P3-Pad23)") (pinfunction "23") (pintype "passive+no_connect"))
    (pad "24" thru_hole oval locked (at 15.24 40.64 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 80 "unconnected-(P3-Pad24)") (pinfunction "24") (pintype "passive+no_connect"))
    (pad "25" thru_hole oval locked (at 15.24 38.1 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 81 "unconnected-(P3-Pad25)") (pinfunction "25") (pintype "passive+no_connect"))
    (pad "26" thru_hole oval locked (at 15.24 35.56 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 82 "unconnected-(P3-Pad26)") (pinfunction "26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 15.24 33.02 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 83 "unconnected-(P3-Pad27)") (pinfunction "27") (pintype "passive+no_connect"))
    (pad "28" thru_hole oval locked (at 15.24 30.48 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 84 "unconnected-(P3-Pad28)") (pinfunction "28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval locked (at 15.24 27.94 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 85 "unconnected-(P3-Pad29)") (pinfunction "29") (pintype "passive+no_connect"))
    (pad "30" thru_hole oval locked (at 15.24 25.4 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 86 "unconnected-(P3-Pad30)") (pinfunction "30") (pintype "passive+no_connect"))
    (pad "31" thru_hole oval locked (at 15.24 22.86 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at 15.24 20.32 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "32") (pintype "passive"))
    (pad "33" thru_hole oval locked (at 15.24 17.78 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 87 "unconnected-(P3-Pad33)") (pinfunction "33") (pintype "passive+no_connect"))
    (pad "34" thru_hole oval locked (at 15.24 15.24 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 88 "unconnected-(P3-Pad34)") (pinfunction "34") (pintype "passive+no_connect"))
    (pad "35" thru_hole oval locked (at 15.24 12.7 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 89 "unconnected-(P3-Pad35)") (pinfunction "35") (pintype "passive+no_connect"))
    (pad "36" thru_hole oval locked (at 15.24 10.16 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 90 "unconnected-(P3-Pad36)") (pinfunction "36") (pintype "passive+no_connect"))
    (pad "37" thru_hole oval locked (at 15.24 7.62 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 91 "unconnected-(P3-Pad37)") (pinfunction "37") (pintype "passive+no_connect"))
    (pad "38" thru_hole oval locked (at 15.24 5.08 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 92 "unconnected-(P3-Pad38)") (pinfunction "38") (pintype "passive+no_connect"))
    (pad "39" thru_hole oval locked (at 15.24 2.54 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pinfunction "39") (pintype "passive"))
    (pad "40" thru_hole rect locked (at 15.24 0 270) (size 1.6 2.8) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pinfunction "40") (pintype "passive"))
    (pad "HOLE" thru_hole circle locked (at -6.35 45.72 270) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask))
    (pad "HOLE" thru_hole circle locked (at 21.59 -2.54 270) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/libs/3d_shapes/textool_40.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 179.07 120.65)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "U6" (at -3.67 2.55) (layer "F.SilkS"))
    (fp_text value "PIC_8_PINS" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "unconnected-(U6-Pad2)") (pinfunction "GP5/OSC1") (pintype "input+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "unconnected-(U6-Pad3)") (pinfunction "GP4/OSC2") (pintype "input+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/VPP{slash}MCLR") (pinfunction "GP3/MCLR") (pintype "input"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "unconnected-(U6-Pad5)") (pinfunction "GP2") (pintype "input+no_connect"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pinfunction "GP1") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pinfunction "GP0") (pintype "input"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 179.07 109.22)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "U1" (at -3.57 3.38) (layer "F.SilkS"))
    (fp_text value "24Cxx" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A0") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pinfunction "SCL") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "unconnected-(U1-Pad7)") (pinfunction "WP") (pintype "input+no_connect"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 110.49 57.15)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "LT1373" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)") (pinfunction "Vc") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(RV1-Pad2)") (pinfunction "FB+") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "unconnected-(U4-Pad3)") (pinfunction "FB-") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "unconnected-(U4-Pad4)") (pinfunction "S/S") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "Vin") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND_S") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D10-Pad2)") (pinfunction "Vsw") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-28_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 207.645 50.8)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "P2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "SUPP28" (at 3.81 35.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 16.51) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/VPP{slash}MCLR") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "unconnected-(P2-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "unconnected-(P2-Pad3)") (pinfunction "3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "unconnected-(P2-Pad4)") (pinfunction "4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "unconnected-(P2-Pad5)") (pinfunction "5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "unconnected-(P2-Pad6)") (pinfunction "6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "unconnected-(P2-Pad7)") (pinfunction "7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "unconnected-(P2-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "unconnected-(P2-Pad10)") (pinfunction "10") (pintype "passive+no_connect"))
    (pad "11" thru_hole oval locked (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "unconnected-(P2-Pad11)") (pinfunction "11") (pintype "passive+no_connect"))
    (pad "12" thru_hole oval locked (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "unconnected-(P2-Pad12)") (pinfunction "12") (pintype "passive+no_connect"))
    (pad "13" thru_hole oval locked (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "unconnected-(P2-Pad13)") (pinfunction "13") (pintype "passive+no_connect"))
    (pad "14" thru_hole oval locked (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "unconnected-(P2-Pad14)") (pinfunction "14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 7.62 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "unconnected-(P2-Pad15)") (pinfunction "15") (pintype "passive+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "unconnected-(P2-Pad16)") (pinfunction "16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 7.62 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "unconnected-(P2-Pad17)") (pinfunction "17") (pintype "passive+no_connect"))
    (pad "18" thru_hole oval locked (at 7.62 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "unconnected-(P2-Pad18)") (pinfunction "18") (pintype "passive+no_connect"))
    (pad "19" thru_hole oval locked (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "20") (pintype "passive"))
    (pad "21" thru_hole oval locked (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "unconnected-(P2-Pad21)") (pinfunction "21") (pintype "passive+no_connect"))
    (pad "22" thru_hole oval locked (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "unconnected-(P2-Pad22)") (pinfunction "22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "unconnected-(P2-Pad23)") (pinfunction "23") (pintype "passive+no_connect"))
    (pad "24" thru_hole oval locked (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "unconnected-(P2-Pad24)") (pinfunction "24") (pintype "passive+no_connect"))
    (pad "25" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "unconnected-(P2-Pad25)") (pinfunction "25") (pintype "passive+no_connect"))
    (pad "26" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "unconnected-(P2-Pad26)") (pinfunction "26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pinfunction "27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pinfunction "28") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-18_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 207.899 107.95)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "U5" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "PIC_18_PINS" (at 3.81 22.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 10.16) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "unconnected-(U5-Pad1)") (pinfunction "RA2") (pintype "bidirectional+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "unconnected-(U5-Pad2)") (pinfunction "RA3") (pintype "bidirectional+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "unconnected-(U5-Pad3)") (pinfunction "T0ckl") (pintype "output+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/VPP{slash}MCLR") (pinfunction "MCLR") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "unconnected-(U5-Pad6)") (pinfunction "RB0") (pintype "bidirectional+no_connect"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "unconnected-(U5-Pad7)") (pinfunction "RB1") (pintype "bidirectional+no_connect"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "unconnected-(U5-Pad8)") (pinfunction "RB2") (pintype "bidirectional+no_connect"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "unconnected-(U5-Pad9)") (pinfunction "RB3") (pintype "bidirectional+no_connect"))
    (pad "10" thru_hole oval locked (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "unconnected-(U5-Pad10)") (pinfunction "RB4") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole oval locked (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "unconnected-(U5-Pad11)") (pinfunction "RB5") (pintype "bidirectional+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pinfunction "ICSPC/RB6") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pinfunction "ICSPD/RB7") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "VDD") (pintype "power_in"))
    (pad "15" thru_hole oval locked (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "unconnected-(U5-Pad15)") (pinfunction "OSC2/CLKO") (pintype "output+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "unconnected-(U5-Pad16)") (pinfunction "OSC1/CLKI") (pintype "input+no_connect"))
    (pad "17" thru_hole oval locked (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "unconnected-(U5-Pad17)") (pinfunction "RA0") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole oval locked (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "unconnected-(U5-Pad18)") (pinfunction "RA1") (pintype "bidirectional+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 115.57 119.38 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "74HC125" (at 3.81 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R8-Pad1)") (pintype "tri_state"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad2)") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R12-Pad1)") (pintype "tri_state"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval locked (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R13-Pad1)") (pintype "tri_state"))
    (pad "9" thru_hole oval locked (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "/PC-DATA-IN") (pintype "tri_state"))
    (pad "12" thru_hole oval locked (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 118.237 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at -2.45 -0.163 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 121.92 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -2.75 0.12 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 111.887 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at -2.35 0.087 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 108.585 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at -2.25 -0.015 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 139.065 80.645)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at 10.435 0.155) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 115.316 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at -2.35 0.016 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 107.95 125.095 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at 3.81 -2.12 180) (layer "F.SilkS"))
    (fp_text value "BAT43" (at 3.81 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (tedit 5F95B7D9)
    (at 82.6 120.2 -90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -5.54 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "DB9-FEMAL" (at -5.54 18.61 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.54 14.025 -90) (layer "F.Fab"))
    (pad "0" thru_hole circle locked (at -18.04 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle locked (at 6.96 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J1-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J1-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/VPP_ON") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/PC-DATA-OUT") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J1-Pad6)") (pinfunction "P6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle locked (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/PC-CLOCK-OUT") (pinfunction "P7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/PC-DATA-IN") (pinfunction "P8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J1-Pad9)") (pinfunction "P9") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5E24ADA3)
    (at 142.24 97.79)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC307" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -3.56) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(Q3-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle locked (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5E24AD8A)
    (at 148.082 60.706 180)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC307" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -3.56) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q2-Pad1)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle locked (at 2.54 0 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "VPP") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5E24AD95)
    (at 146.05 69.85)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC237" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -3.56) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D11-Pad1)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle locked (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 152.4 68.58 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R18" (at 5.08 -2.31 90) (layer "F.SilkS"))
    (fp_text value "220" (at 5.08 2.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/VPP{slash}MCLR") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 114.3 48.26)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R10" (at 5.08 -2.31) (layer "F.SilkS"))
    (fp_text value "5,1K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 139.065 77.47)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at 5.08 -2.31) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(D8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.63 118.11)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 3.07 -0.01) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "/VPP_ON") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.63 114.554)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 2.97 -0.054) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "/VPP_ON") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.63 111.125)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 2.87 0.175) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/PC-DATA-OUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.63 107.823)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.31) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/PC-DATA-OUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.757 125.476)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 1.943 2.524) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/PC-CLOCK-OUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 139.7 54.61)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 -2.31) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "VPP") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 87.757 121.92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 3.143 -0.12) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/PC-CLOCK-OUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 158.115 102.235 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R21" (at 5.08 -2.31 180) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.31 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(D12-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 144.78 102.235 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R20" (at 5.08 -2.31 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 5.08 2.31 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 149.225 83.82 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R19" (at -2.675 1.72 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 5.08 2.31 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 156.21 68.58 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R17" (at 1.18 2.69 90) (layer "F.SilkS"))
    (fp_text value "22K" (at 5.08 2.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 118.11 75.184)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R16" (at 5.08 -2.31) (layer "F.SilkS"))
    (fp_text value "62K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "VPP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 118.11 78.74)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R15" (at -2.71 -0.14) (layer "F.SilkS"))
    (fp_text value "6.2K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 139.065 87.63)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R14" (at -3.165 -0.23) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(D9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 140.335 111.76 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R13" (at 5.08 -2.31 -90) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.31 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "/CLOCK-RB6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 139.065 91.059)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at -3.365 -0.159) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 135.255 121.92 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R12" (at 5.08 -2.31 90) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "/DATA-RB7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 156.21 77.47 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Champ4" "Low Current Led")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 1.27 -3.96 180) (layer "F.SilkS"))
    (fp_text value "RED-LED" (at 1.27 3.96 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 156.21 87.63 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Champ4" "GREEN LED")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D9" (at 1.27 -3.96 180) (layer "F.SilkS"))
    (fp_text value "GREEN-LED" (at 1.27 3.96 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 156.21 97.155 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D12" (at -3.69 0.555 180) (layer "F.SilkS"))
    (fp_text value "YELLOW-LED" (at 1.27 3.96 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(D12-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5A142A3B)
    (at 114.3 52.07)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at -2.6 0.03) (layer "F.SilkS"))
    (fp_text value "0" (at 2.5 2.91) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5A142A3B)
    (at 129.54 49.53)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 -2.91) (layer "F.SilkS"))
    (fp_text value "10nF" (at 2.5 2.91) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5A142A3B)
    (at 198.755 71.12 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "C7" (at 2.5 -2.91 -90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 2.5 2.91 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5A142A3B)
    (at 143.002 49.784)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at 2.5 -2.91) (layer "F.SilkS"))
    (fp_text value "220nF" (at 2.5 2.91) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "VPP") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5A142A3B)
    (at 196.85 112.395 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "pic_sockets.kicad_sch")
    (property "Sheetname" "pic_sockets")
    (attr through_hole)
    (fp_text reference "C6" (at 2.5 -2.91 -90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 2.5 2.91 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "/pic_sockets/VCC_PIC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 137.16 57.15 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D10" (at 6.35 -2.12 180) (layer "F.SilkS"))
    (fp_text value "SCHOTTKY" (at 6.35 2.12 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.65 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "VPP") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:RV2X4" (layer "F.Cu")
    (tedit 5F95B8F7)
    (at 127.635 90.805 180)
    (descr "Resistance variable / Potentiometre")
    (tags "R")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.54 -5.08 180) (layer "F.SilkS"))
    (fp_text value "1K" (at -1.651 5.461 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 13 "Net-(R15-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 2.54 180) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 16 "Net-(RV1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 5.08 180) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 14 "Net-(R16-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/libs/3d_shapes/adjustable_rx2v4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Altech:Altech_AK300_1x02_P5.00mm_45-Degree" (layer "F.Cu")
    (tedit 5C27907F)
    (at 81.8 60 -90)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 1.9 -7.9 -90) (layer "F.SilkS"))
    (fp_text value "CONN_2" (at 2.5 5.66 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 3.2 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "P1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 "Net-(D1-Pad2)") (pinfunction "PM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown" (layer "F.Cu")
    (tedit 5F95B99C)
    (at 96.52 71.12)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -4.22 -16.52) (layer "F.SilkS"))
    (fp_text value "7805" (at 2.54 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -20.58) (layer "F.Fab"))
    (pad "" thru_hole rect locked (at 2.54 -16.66) (size 10 8) (drill 3.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.905 3) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "VI") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.905 3) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.905 3) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5A14249F)
    (at 140.081 70.993 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R11" (at 6.993 -2.381 90) (layer "F.SilkS"))
    (fp_text value "22K" (at 5.08 2.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_THT:C_Axial_L12.0mm_D6.5mm_P20.00mm_Horizontal" (layer "F.Cu")
    (tedit 5A285655)
    (at 134.112 62.23 -90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 10 -4.31 -90) (layer "F.SilkS"))
    (fp_text value "22uF/25V" (at 10 4.31 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "VPP") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 20 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L12.0mm_D6.5mm_P20.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Radial_D7.8mm_P5.00mm_Fastron_07HCP" (layer "F.Cu")
    (tedit 5A142293)
    (at 125.73 62.23 -90)
    (descr "L, Radial series, Radial, pin pitch=5.00mm, , diameter=7.8mm, Fastron, 07HCP, http://www.abracon.com/Magnetics/radial/AISR875.pdf")
    (tags "L Radial series Radial pin pitch 5.00mm  diameter 7.8mm Fastron 07HCP")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at 2.5 -4.96 -90) (layer "F.SilkS"))
    (fp_text value "22uH" (at 2.5 4.96 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(D10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D7.8mm_P5.00mm_Fastron_07HCP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5A195B5A)
    (at 78.3 89.7 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 6.35 -2.12 90) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 6.35 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.65 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F)
    (at 148.082 97.79)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "pic_programmer.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.2)
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "JUMPER" (at 0 -1.9) (layer "B.Fab"))
    (pad "1" smd custom locked (at -0.725 0) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 17 "VCC") (pinfunction "1") (pintype "passive") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom locked (at 0.725 0) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 24 "/pic_sockets/VCC_PIC") (pinfunction "2") (pintype "passive") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (gr_line (start 73.66 139.7) (end 73.66 40.64) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 173.99 40.64) (end 233.68 40.64) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 73.66 40.64) (end 173.99 40.64) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 233.68 139.7) (end 73.66 139.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 233.68 40.64) (end 233.68 139.7) (layer "Edge.Cuts") (width 0.1))
  (gr_text "+8/12V" (at 81.5 55.5) (layer "F.Cu"))
  (gr_text "VCC ON" (at 162.9 99.1) (layer "F.Cu"))
  (gr_text "JP-CHARRAS" (at 94.615 137.16) (layer "F.Cu"))
  (gr_text "1=>>" (at 167.64 48.895) (layer "F.Cu"))
  (gr_text "PWR ON" (at 163.83 88.9) (layer "F.Cu"))
  (gr_text "PIC PROGRAMMER V03" (at 125.095 132.08) (layer "F.Cu"))
  (gr_text "1=>>" (at 200.66 107.95) (layer "F.Cu"))
  (gr_text "PIC 18 PINS" (at 211.455 132.715) (layer "F.Cu"))
  (gr_text "I2C PROM" (at 166.37 114.3) (layer "F.Cu"))
  (gr_text "VPP ON" (at 163.195 80.645) (layer "F.Cu"))
  (gr_text "1=>>" (at 171.45 109.22) (layer "F.Cu"))
  (gr_text "13V ADJUST" (at 123.19 95.25) (layer "F.Cu"))
  (gr_text "PIC 8 PINS" (at 183.515 132.08) (layer "F.Cu"))
  (gr_text "PIC 28 PINS" (at 212.725 45.085) (layer "F.Cu"))
  (gr_text "1=>>" (at 171.45 120.65) (layer "F.Cu"))
  (gr_text "PIC 40 PINS" (at 182.245 45.085) (layer "F.Cu"))
  (gr_text "1=>>" (at 202 48.7) (layer "F.Cu"))
  (gr_text "J-P CHARRAS" (at 94.615 137.16) (layer "B.Cu"))
  (gr_text "PIC PROGRAMMER V03" (at 124.46 134.62) (layer "B.Cu"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 223.52 138.43)
        (xy 232.41 128.905)
        (xy 232.41 53.975)
        (xy 219.71 41.91)
        (xy 81.28 41.91)
        (xy 74.295 48.895)
        (xy 74.295 127.635)
        (xy 86.36 138.43)
      )
    )
  )
)
