(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/left/P55")
  (net 2 "/left/P42")
  (net 3 "/left/P35")
  (net 4 "/left/P20")
  (net 5 "/left/P17")
  (net 6 "/left/P25")
  (net 7 "/left/APA_CI")
  (net 8 "/left/GND")
  (net 9 "/left/APA_DI")
  (net 10 "Net-(C217-Pad1)")
  (net 11 "Net-(C317-Pad1)")
  (net 12 "Net-(D201-Pad6)")
  (net 13 "Net-(D201-Pad5)")
  (net 14 "/left/SPI2_~{CS}")
  (net 15 "/left/SPI2_SCK")
  (net 16 "Net-(J208-Pad6)")
  (net 17 "Net-(J208-Pad7)")
  (net 18 "Net-(J208-Pad8)")
  (net 19 "/left/SD_DET")
  (net 20 "/left/SWDIO")
  (net 21 "/left/SWCLK")
  (net 22 "Net-(J215-PadB8)")
  (net 23 "Net-(J215-PadA5)")
  (net 24 "Net-(J215-PadA8)")
  (net 25 "Net-(U201-Pad61)")
  (net 26 "Net-(U201-Pad57)")
  (net 27 "Net-(U201-Pad54)")
  (net 28 "Net-(U201-Pad41)")
  (net 29 "Net-(U201-Pad40)")
  (net 30 "Net-(U201-Pad36)")
  (net 31 "Net-(U201-Pad9)")
  (net 32 "/left/NRST")
  (net 33 "/left/P26")
  (net 34 "/left/P58")
  (net 35 "/left/P56")
  (net 36 "/left/P21")
  (net 37 "/left/P59")
  (net 38 "/left/P15")
  (net 39 "/left/P16")
  (net 40 "/left/P23")
  (net 41 "/left/P22")
  (net 42 "Net-(U201-Pad8)")
  (net 43 "Net-(U201-Pad6)")
  (net 44 "/left/P30")
  (net 45 "/left/P14")
  (net 46 "/left/P27")
  (net 47 "/left/P28")
  (net 48 "/left/P43")
  (net 49 "/left/P34")
  (net 50 "/left/P33")
  (net 51 "/left/BOOT0")
  (net 52 "Net-(U201-Pad5)")
  (net 53 "/left/USART4_TX")
  (net 54 "/left/USART4_RX")
  (net 55 "/left/D-")
  (net 56 "Net-(U201-Pad4)")
  (net 57 "Net-(U202-Pad4)")
  (net 58 "/left/D+")
  (net 59 "/left/USART3_TX")
  (net 60 "/left/USART2_RX")
  (net 61 "/left/+3V3")
  (net 62 "/left/VBUS")
  (net 63 "Net-(J215-PadB5)")
  (net 64 "/right/GND")
  (net 65 "/right/+3V3")
  (net 66 "/left/SPI2_CIPO")
  (net 67 "Net-(U301-Pad9)")
  (net 68 "Net-(U301-Pad8)")
  (net 69 "Net-(D301-Pad3)")
  (net 70 "Net-(D301-Pad4)")
  (net 71 "Net-(D301-Pad1)")
  (net 72 "/right/SPI2_~{CS}")
  (net 73 "/right/SPI2_COPI")
  (net 74 "/right/SPI2_SCK")
  (net 75 "/right/SPI2_CIPO")
  (net 76 "/right/SD_DET")
  (net 77 "/right/NRST")
  (net 78 "Net-(J301-Pad1)")
  (net 79 "Net-(J301-Pad8)")
  (net 80 "/right/SWCLK")
  (net 81 "/right/SWDIO")
  (net 82 "Net-(J302-Pad6)")
  (net 83 "Net-(J302-Pad7)")
  (net 84 "Net-(J302-Pad8)")
  (net 85 "Net-(J309-PadA5)")
  (net 86 "/right/VBUS")
  (net 87 "/right/BOOT0")
  (net 88 "/right/USART4_RX")
  (net 89 "/right/USART4_TX")
  (net 90 "/right/D+")
  (net 91 "/right/D-")
  (net 92 "/right/USART3_TX")
  (net 93 "/right/USART2_RX")
  (net 94 "/right/P59")
  (net 95 "/right/P58")
  (net 96 "Net-(U301-Pad57)")
  (net 97 "/right/P56")
  (net 98 "/right/P55")
  (net 99 "Net-(U301-Pad2)")
  (net 100 "Net-(U301-Pad53)")
  (net 101 "/right/P43")
  (net 102 "/right/P42")
  (net 103 "Net-(U301-Pad41)")
  (net 104 "Net-(U301-Pad40)")
  (net 105 "Net-(U301-Pad39)")
  (net 106 "/right/P35")
  (net 107 "/right/P34")
  (net 108 "/right/P33")
  (net 109 "/right/P30")
  (net 110 "/right/P28")
  (net 111 "/right/P27")
  (net 112 "/right/P26")
  (net 113 "/right/P25")
  (net 114 "/right/P23")
  (net 115 "/right/P22")
  (net 116 "/right/P21")
  (net 117 "/right/P20")
  (net 118 "/right/P17")
  (net 119 "/right/P16")
  (net 120 "/right/P15")
  (net 121 "/right/P14")
  (net 122 "Net-(U301-Pad38)")
  (net 123 "Net-(U301-Pad37)")
  (net 124 "Net-(U301-Pad3)")
  (net 125 "Net-(U301-Pad4)")
  (net 126 "Net-(J309-PadA8)")
  (net 127 "Net-(U302-Pad4)")
  (net 128 "Net-(J309-PadB5)")
  (net 129 "Net-(J309-PadB8)")
  (net 130 "Net-(U301-Pad36)")
  (net 131 "/right/LED_R")
  (net 132 "/right/LED_G")
  (net 133 "/right/LED_B")
  (net 134 "/left/SPI2_COPI")
  (footprint "Connector_USB:USB_C_Receptacle_Palconn_UTC16-G" (layer "F.Cu")
    (at 194.1 54.3 180)
    (descr "http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf")
    (tags "USB C Type-C Receptacle USB2.0")
    (property "Reference" "J215" (at 0 -5.2 -90) (layer "F.SilkS"))
    (property "Value" "USB_C_Receptacle_USB2.0" (at 0 6.24 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "PCB Edge" (at 0 3.43 0) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 1.18 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.89 -1.45) (size 0.6 0.6) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 2.89 -1.45) (size 0.6 0.6) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "A1" smd rect (at -3.2 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "A4" smd rect (at -2.4 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/left/VBUS") (pinfunction "VBUS")
    )
    (pad "A5" smd rect (at -1.25 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(J215-PadA5)") (pinfunction "CC1")
    )
    (pad "A6" smd rect (at -0.25 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/left/D+") (pinfunction "D+")
    )
    (pad "A7" smd rect (at 0.25 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/left/D-") (pinfunction "D-")
    )
    (pad "A8" smd rect (at 1.25 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J215-PadA8)") (pinfunction "SBU1")
    )
    (pad "A9" smd rect (at 2.4 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/left/VBUS") (pinfunction "VBUS")
    )
    (pad "A12" smd rect (at 3.2 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "B1" smd rect (at 3.2 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "B4" smd rect (at 2.4 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/left/VBUS") (pinfunction "VBUS")
    )
    (pad "B5" smd rect (at 1.75 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(J215-PadB5)") (pinfunction "CC2")
    )
    (pad "B6" smd rect (at 0.75 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/left/D+") (pinfunction "D+")
    )
    (pad "B7" smd rect (at -0.75 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/left/D-") (pinfunction "D-")
    )
    (pad "B8" smd rect (at -1.75 -2.51) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J215-PadB8)") (pinfunction "SBU2")
    )
    (pad "B9" smd rect (at -2.4 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/left/VBUS") (pinfunction "VBUS")
    )
    (pad "B12" smd rect (at -3.2 -2.51 180) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "S1" thru_hole oval (at -4.32 -1.93 270) (size 2 0.9) (drill oval 1.7 0.6) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at -4.32 2.24 270) (size 1.7 0.9) (drill oval 1.4 0.6) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at 4.32 -1.93 270) (size 2 0.9) (drill oval 1.7 0.6) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at 4.32 2.24 270) (size 1.7 0.9) (drill oval 1.4 0.6) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "SHIELD")
    )
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Palconn_UTC16-G.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0805_2012Metric_Castellated" (layer "F.Cu")
    (at 183.7 55.4 90)
    (descr "Fuse SMD 0805 (2012 Metric), castellated end terminal, IPC_7351. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "fuse castellated")
    (property "Reference" "TH201" (at -2.525 1.3 90) (layer "F.SilkS"))
    (property "Value" "Thermistor_PTC" (at 0 1.6 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9625 0 90) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(C217-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9625 0 90) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 62 "/left/VBUS")
    )
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 180.85 55.4 -90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Reference" "U202" (at 2.9 -0.15 180) (layer "F.SilkS"))
    (property "Value" "TLV75533PDBV" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C217-Pad1)") (pinfunction "IN")
    )
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "3" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C217-Pad1)") (pinfunction "EN")
    )
    (pad "4" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(U202-Pad4)") (pinfunction "NC")
    )
    (pad "5" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/left/+3V3") (pinfunction "OUT")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 175.9 55.3 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C218" (at -0.1 1.8 90) (layer "F.SilkS"))
    (property "Value" "100µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C217-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 59.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C215" (at 0.19 2.6 0) (layer "F.SilkS"))
    (property "Value" "100µF" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 178 55.3 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C217" (at 2.9 1.2 180) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C217-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 57.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C216" (at 0.11 3.57 0) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_RGB_5050-6" (layer "F.Cu")
    (at 163.8 73.6 180)
    (descr "http://cdn.sparkfun.com/datasheets/Components/LED/5060BRG4.pdf")
    (tags "RGB LED 5050-6")
    (property "Reference" "D201" (at 0 -3.5 180) (layer "F.SilkS"))
    (property "Value" "APA102" (at 0 3.3 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4 -1.7 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/left/APA_DI") (pinfunction "DI")
    )
    (pad "2" smd rect (at -2.4 0 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/left/APA_CI") (pinfunction "CI")
    )
    (pad "3" smd rect (at -2.4 1.7 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "4" smd rect (at 2.4 1.7 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/left/+3V3") (pinfunction "VCC")
    )
    (pad "5" smd rect (at 2.4 0 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D201-Pad5)") (pinfunction "CO")
    )
    (pad "6" smd rect (at 2.4 -1.7 270) (size 1.1 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D201-Pad6)") (pinfunction "DO")
    )
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_RGB_5050-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 198.4 68.15)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J210" (at -0.63 -1.98 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 21 "/left/SWCLK") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 173.537087 67.2 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C211" (at 3.250631 -1.907129 180) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/left/P25")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 173.501634 107.133163)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R305" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "5" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "/right/LED_B")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(D301-Pad3)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left" (layer "F.Cu")
    (at 172.069712 84.518533 90)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (property "Reference" "J216" (at 0.175 -7.51 180) (layer "F.SilkS"))
    (property "Value" "Conn_01x04_Male" (at 0 6.14 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.655 -3.81 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/left/GND") (pinfunction "Pin_1")
    )
    (pad "2" smd rect (at 1.655 -1.27 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/left/USART3_TX") (pinfunction "Pin_2")
    )
    (pad "3" smd rect (at -1.655 1.27 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/left/USART2_RX") (pinfunction "Pin_3")
    )
    (pad "4" smd rect (at 1.655 3.81 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/left/+3V3") (pinfunction "Pin_4")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 173.499038 105.089713)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R304" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "5" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "/right/LED_G")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(D301-Pad4)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 189.19 74.85 -45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C214" (at 1.845549 -2.708219 0) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 185.972858 104.567571 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Reference" "J307" (at 2.132429 0.872858 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x03_Male" (at 0 7.41 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "/right/BOOT0") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/right/+3V3") (pinfunction "Pin_3")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "waad:R_pads" (layer "F.Cu")
    (at 152.68 127.07 180)
    (property "Reference" "J305" (at -0.5 -31 0) (layer "F.SilkS") hide)
    (property "Value" "cap_pads" (at -0.25 -26 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd custom (at 45.5 -1.5) (size 1.524 1.524) (layers "F.Cu")
      (net 112 "/right/P26") (pinfunction "Pin_1") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 7.842879 7.862396)
            (xy 7.86647 7.815828)
            (xy 7.899576 7.698563)
            (xy 7.939173 7.523634)
            (xy 7.982233 7.304077)
            (xy 8.013142 7.128881)
            (xy 8.264762 5.731274)
            (xy 8.556322 4.277424)
            (xy 8.883958 2.783541)
            (xy 9.243809 1.265839)
            (xy 9.632012 -0.259473)
            (xy 10.044703 -1.776182)
            (xy 10.478019 -3.268077)
            (xy 10.537854 -3.466592)
            (xy 10.619607 -3.742268)
            (xy 10.690162 -3.99118)
            (xy 10.746547 -4.201909)
            (xy 10.785791 -4.363034)
            (xy 10.804922 -4.463138)
            (xy 10.804453 -4.491147)
            (xy 10.755884 -4.516049)
            (xy 10.640988 -4.565129)
            (xy 10.472816 -4.633111)
            (xy 10.26442 -4.714716)
            (xy 10.030246 -4.804144)
            (xy 9.874181 -4.862471)
            (xy 9.649823 -4.945478)
            (xy 9.361643 -5.051542)
            (xy 9.014115 -5.17904)
            (xy 8.611711 -5.326349)
            (xy 8.158903 -5.491847)
            (xy 7.660163 -5.673909)
            (xy 7.119965 -5.870914)
            (xy 6.54278 -6.081239)
            (xy 5.933081 -6.30326)
            (xy 5.29534 -6.535354)
            (xy 4.63403 -6.775898)
            (xy 3.953623 -7.02327)
            (xy 3.258592 -7.275847)
            (xy 2.553409 -7.532005)
            (xy 1.842546 -7.790121)
            (xy 1.130476 -8.048574)
            (xy 0.421672 -8.305738)
            (xy -0.279395 -8.559993)
            (xy -0.968252 -8.809714)
            (xy -1.640426 -9.053279)
            (xy -2.291445 -9.289065)
            (xy -2.916837 -9.515448)
            (xy -3.512128 -9.730806)
            (xy -4.072848 -9.933516)
            (xy -4.594523 -10.121955)
            (xy -5.07268 -10.2945)
            (xy -5.502848 -10.449528)
            (xy -5.880555 -10.585416)
            (xy -6.201326 -10.700541)
            (xy -6.460691 -10.79328)
            (xy -6.654177 -10.86201)
            (xy -6.777311 -10.905108)
            (xy -6.825621 -10.920951)
            (xy -6.826032 -10.921)
            (xy -6.829517 -10.879344)
            (xy -6.832905 -10.757085)
            (xy -6.83618 -10.558289)
            (xy -6.839325 -10.28702)
            (xy -6.842322 -9.947341)
            (xy -6.845154 -9.543317)
            (xy -6.847805 -9.079013)
            (xy -6.850256 -8.558492)
            (xy -6.852492 -7.98582)
            (xy -6.854495 -7.36506)
            (xy -6.856247 -6.700278)
            (xy -6.857733 -5.995536)
            (xy -6.858934 -5.254901)
            (xy -6.859833 -4.482435)
            (xy -6.860414 -3.682203)
            (xy -6.860659 -2.85827)
            (xy -6.860666 -2.689084)
            (xy -6.860666 5.542831)
            (xy -6.723083 5.566885)
            (xy -6.65977 5.577312)
            (xy -6.517774 5.600262)
            (xy -6.302029 5.634946)
            (xy -6.017465 5.680579)
            (xy -5.669016 5.736372)
            (xy -5.261613 5.80154)
            (xy -4.800187 5.875295)
            (xy -4.289672 5.956851)
            (xy -3.735 6.04542)
            (xy -3.141101 6.140215)
            (xy -2.512909 6.24045)
            (xy -1.855355 6.345337)
            (xy -1.173372 6.45409)
            (xy -0.471891 6.565921)
            (xy 0.244156 6.680044)
            (xy 0.969836 6.795671)
            (xy 1.700217 6.912016)
            (xy 2.430368 7.028292)
            (xy 3.155357 7.143712)
            (xy 3.87025 7.257488)
            (xy 4.562045 7.36755)
            (xy 5.075053 7.448811)
            (xy 5.564214 7.52563)
            (xy 6.023034 7.597029)
            (xy 6.445018 7.662027)
            (xy 6.823671 7.719645)
            (xy 7.152498 7.768904)
            (xy 7.425003 7.808823)
            (xy 7.634692 7.838422)
            (xy 7.775071 7.856724)
            (xy 7.839643 7.862746)
            (xy 7.842879 7.862396)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "2" smd custom (at 40 11.5) (size 1.524 1.524) (layers "F.Cu")
      (net 111 "/right/P27") (pinfunction "Pin_2") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 5.502759 7.995657)
            (xy 5.542558 7.884932)
            (xy 5.602782 7.714647)
            (xy 5.679827 7.495037)
            (xy 5.770093 7.236338)
            (xy 5.869976 6.948786)
            (xy 5.885149 6.905)
            (xy 6.433125 5.359607)
            (xy 6.984542 3.879869)
            (xy 7.547354 2.446895)
            (xy 8.129517 1.041792)
            (xy 8.738984 -0.354329)
            (xy 9.38371 -1.760361)
            (xy 10.071648 -3.195195)
            (xy 10.514927 -4.090698)
            (xy 10.641247 -4.343941)
            (xy 10.753871 -4.571393)
            (xy 10.847561 -4.762337)
            (xy 10.917078 -4.906057)
            (xy 10.957184 -4.991835)
            (xy 10.965 -5.011448)
            (xy 10.923236 -5.013273)
            (xy 10.80022 -5.015058)
            (xy 10.599366 -5.016795)
            (xy 10.324089 -5.018478)
            (xy 9.977804 -5.020101)
            (xy 9.563926 -5.021658)
            (xy 9.085868 -5.023143)
            (xy 8.547047 -5.024548)
            (xy 7.950875 -5.025868)
            (xy 7.300768 -5.027097)
            (xy 6.60014 -5.028228)
            (xy 5.852406 -5.029254)
            (xy 5.060981 -5.03017)
            (xy 4.229279 -5.03097)
            (xy 3.360715 -5.031646)
            (xy 2.458704 -5.032192)
            (xy 1.526659 -5.032603)
            (xy 0.567996 -5.032872)
            (xy -0.413871 -5.032993)
            (xy -0.697833 -5.033)
            (xy -12.360666 -5.033)
            (xy -12.359892 -1.720416)
            (xy -12.359117 1.592167)
            (xy -8.094809 3.135043)
            (xy -7.472826 3.360099)
            (xy -6.841787 3.588462)
            (xy -6.21018 3.81706)
            (xy -5.58649 4.042818)
            (xy -4.979206 4.262665)
            (xy -4.396815 4.473526)
            (xy -3.847805 4.67233)
            (xy -3.340662 4.856002)
            (xy -2.883874 5.02147)
            (xy -2.485929 5.165661)
            (xy -2.155314 5.285501)
            (xy -2.031333 5.330461)
            (xy -1.18188 5.638441)
            (xy -0.369209 5.93287)
            (xy 0.40368 6.212667)
            (xy 1.133788 6.476753)
            (xy 1.818117 6.724048)
            (xy 2.453667 6.953473)
            (xy 3.037439 7.163949)
            (xy 3.566435 7.354396)
            (xy 4.037655 7.523734)
            (xy 4.4481 7.670885)
            (xy 4.794772 7.794768)
            (xy 5.074671 7.894305)
            (xy 5.284799 7.968416)
            (xy 5.422155 8.01602)
            (xy 5.483743 8.03604)
            (xy 5.486984 8.036585)
            (xy 5.502759 7.995657)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "3" smd custom (at 28.5 -5.5) (size 1.524 1.524) (layers "F.Cu")
      (net 114 "/right/P23") (pinfunction "Pin_3") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 7.946187 6.366258)
            (xy 8.000967 6.173415)
            (xy 8.072083 5.918495)
            (xy 8.157834 5.607849)
            (xy 8.256522 5.247828)
            (xy 8.366445 4.844784)
            (xy 8.485905 4.405067)
            (xy 8.613201 3.935029)
            (xy 8.746633 3.441022)
            (xy 8.884501 2.929396)
            (xy 9.025106 2.406502)
            (xy 9.166747 1.878692)
            (xy 9.307724 1.352317)
            (xy 9.446338 0.833728)
            (xy 9.580889 0.329276)
            (xy 9.709676 -0.154687)
            (xy 9.831 -0.61181)
            (xy 9.94316 -1.035742)
            (xy 10.044457 -1.420133)
            (xy 10.133192 -1.758629)
            (xy 10.207663 -2.044882)
            (xy 10.26617 -2.272538)
            (xy 10.307015 -2.435248)
            (xy 10.328497 -2.526659)
            (xy 10.331298 -2.544813)
            (xy 10.291447 -2.559773)
            (xy 10.176611 -2.601898)
            (xy 9.991409 -2.669512)
            (xy 9.740459 -2.76094)
            (xy 9.428381 -2.874508)
            (xy 9.059793 -3.00854)
            (xy 8.639313 -3.161361)
            (xy 8.17156 -3.331296)
            (xy 7.661154 -3.516669)
            (xy 7.112711 -3.715806)
            (xy 6.530852 -3.927032)
            (xy 5.920195 -4.148671)
            (xy 5.285358 -4.379048)
            (xy 4.630961 -4.616488)
            (xy 3.961621 -4.859316)
            (xy 3.281958 -5.105856)
            (xy 2.59659 -5.354435)
            (xy 1.910136 -5.603375)
            (xy 1.227214 -5.851003)
            (xy 0.552444 -6.095643)
            (xy -0.109557 -6.33562)
            (xy -0.75417 -6.569259)
            (xy -1.376775 -6.794885)
            (xy -1.972754 -7.010822)
            (xy -2.537489 -7.215396)
            (xy -3.066361 -7.406931)
            (xy -3.554751 -7.583753)
            (xy -3.99804 -7.744185)
            (xy -4.391611 -7.886553)
            (xy -4.730844 -8.009182)
            (xy -5.01112 -8.110397)
            (xy -5.227821 -8.188522)
            (xy -5.376329 -8.241882)
            (xy -5.39191 -8.247458)
            (xy -5.547619 -8.301401)
            (xy -5.642784 -8.327113)
            (xy -5.695955 -8.326567)
            (xy -5.725684 -8.301736)
            (xy -5.735905 -8.284036)
            (xy -5.758909 -8.223205)
            (xy -5.802317 -8.093163)
            (xy -5.862444 -7.905868)
            (xy -5.935606 -7.673277)
            (xy -6.018118 -7.407346)
            (xy -6.106295 -7.120034)
            (xy -6.196452 -6.823297)
            (xy -6.284905 -6.529092)
            (xy -6.367969 -6.249376)
            (xy -6.441959 -5.996107)
            (xy -6.456306 -5.946333)
            (xy -6.633846 -5.314568)
            (xy -6.821503 -4.621114)
            (xy -7.013801 -3.887501)
            (xy -7.205264 -3.135258)
            (xy -7.390415 -2.385914)
            (xy -7.56378 -1.661)
            (xy -7.719882 -0.982045)
            (xy -7.726871 -0.95087)
            (xy -7.823672 -0.511495)
            (xy -7.921197 -0.055619)
            (xy -8.018047 0.409209)
            (xy -8.112822 0.875439)
            (xy -8.204123 1.335524)
            (xy -8.290552 1.781913)
            (xy -8.370707 2.207059)
            (xy -8.443191 2.603413)
            (xy -8.506604 2.963426)
            (xy -8.559547 3.279549)
            (xy -8.60062 3.544234)
            (xy -8.628424 3.749931)
            (xy -8.64156 3.889092)
            (xy -8.638628 3.954168)
            (xy -8.636653 3.957131)
            (xy -8.628142 3.963083)
            (xy -8.612597 3.969663)
            (xy -8.585512 3.977615)
            (xy -8.542384 3.987685)
            (xy -8.478706 4.000615)
            (xy -8.389975 4.017151)
            (xy -8.271685 4.038037)
            (xy -8.119331 4.064018)
            (xy -7.928408 4.095839)
            (xy -7.694412 4.134243)
            (xy -7.412837 4.179975)
            (xy -7.079179 4.233781)
            (xy -6.688933 4.296403)
            (xy -6.237594 4.368587)
            (xy -5.720656 4.451078)
            (xy -5.133615 4.54462)
            (xy -4.471967 4.649956)
            (xy -3.731205 4.767833)
            (xy -3.731166 4.767839)
            (xy -3.304963 4.83558)
            (xy -2.83163 4.910683)
            (xy -2.317004 4.992229)
            (xy -1.76692 5.079298)
            (xy -1.187213 5.170974)
            (xy -0.58372 5.266336)
            (xy 0.037723 5.364467)
            (xy 0.671282 5.464446)
            (xy 1.31112 5.565357)
            (xy 1.951402 5.66628)
            (xy 2.586291 5.766297)
            (xy 3.209953 5.864488)
            (xy 3.816552 5.959935)
            (xy 4.400251 6.05172)
            (xy 4.955215 6.138923)
            (xy 5.475609 6.220627)
            (xy 5.955596 6.295912)
            (xy 6.389342 6.363859)
            (xy 6.771009 6.423551)
            (xy 7.094764 6.474068)
            (xy 7.354769 6.514491)
            (xy 7.545189 6.543903)
            (xy 7.660189 6.561384)
            (xy 7.684033 6.564868)
            (xy 7.880899 6.592682)
            (xy 7.946187 6.366258)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "4" smd custom (at 23.5 9) (size 1.524 1.524) (layers "F.Cu")
      (net 110 "/right/P28") (pinfunction "Pin_4") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 5.4468 11.466359)
            (xy 5.455438 11.462425)
            (xy 5.458064 11.460048)
            (xy 5.474199 11.415027)
            (xy 5.510004 11.296532)
            (xy 5.563147 11.112844)
            (xy 5.631297 10.872246)
            (xy 5.712121 10.583021)
            (xy 5.803288 10.253453)
            (xy 5.902466 9.891823)
            (xy 5.987084 9.581038)
            (xy 6.063733 9.298255)
            (xy 6.15937 8.944796)
            (xy 6.272458 8.526374)
            (xy 6.401458 8.048703)
            (xy 6.544833 7.517497)
            (xy 6.701044 6.938468)
            (xy 6.868552 6.31733)
            (xy 7.04582 5.659797)
            (xy 7.23131 4.971583)
            (xy 7.423483 4.258399)
            (xy 7.620801 3.525961)
            (xy 7.821726 2.779982)
            (xy 8.024719 2.026174)
            (xy 8.228243 1.270253)
            (xy 8.43076 0.51793)
            (xy 8.63073 -0.225081)
            (xy 8.826617 -0.953066)
            (xy 9.016881 -1.660311)
            (xy 9.199985 -2.341104)
            (xy 9.37439 -2.98973)
            (xy 9.538558 -3.600476)
            (xy 9.690952 -4.16763)
            (xy 9.830032 -4.685476)
            (xy 9.95426 -5.148303)
            (xy 10.062099 -5.550396)
            (xy 10.152011 -5.886042)
            (xy 10.222456 -6.149527)
            (xy 10.258349 -6.284166)
            (xy 10.338288 -6.583776)
            (xy 10.411816 -6.857822)
            (xy 10.475945 -7.095288)
            (xy 10.527686 -7.285157)
            (xy 10.564051 -7.416414)
            (xy 10.582051 -7.478043)
            (xy 10.582776 -7.480083)
            (xy 10.570467 -7.486774)
            (xy 10.526146 -7.492912)
            (xy 10.446745 -7.498516)
            (xy 10.329194 -7.503609)
            (xy 10.170424 -7.50821)
            (xy 9.967367 -7.51234)
            (xy 9.716954 -7.516021)
            (xy 9.416115 -7.519272)
            (xy 9.061781 -7.522115)
            (xy 8.650885 -7.524571)
            (xy 8.180355 -7.52666)
            (xy 7.647124 -7.528402)
            (xy 7.048123 -7.529819)
            (xy 6.380282 -7.530932)
            (xy 5.640533 -7.531761)
            (xy 4.825806 -7.532327)
            (xy 3.933033 -7.532651)
            (xy 2.959145 -7.532753)
            (xy 2.798613 -7.53275)
            (xy -5.005833 -7.532501)
            (xy -5.393951 -6.781333)
            (xy -5.846005 -5.887269)
            (xy -6.312374 -4.928646)
            (xy -6.785309 -3.922647)
            (xy -7.25706 -2.886456)
            (xy -7.719879 -1.837254)
            (xy -8.166015 -0.792224)
            (xy -8.58772 0.231451)
            (xy -8.825626 0.827834)
            (xy -9.011742 1.305346)
            (xy -9.196934 1.789453)
            (xy -9.378929 2.273589)
            (xy -9.555453 2.751183)
            (xy -9.724234 3.215668)
            (xy -9.882999 3.660475)
            (xy -10.029474 4.079034)
            (xy -10.161388 4.464778)
            (xy -10.276468 4.811138)
            (xy -10.372439 5.111545)
            (xy -10.44703 5.35943)
            (xy -10.497968 5.548225)
            (xy -10.52298 5.671362)
            (xy -10.519792 5.722271)
            (xy -10.519304 5.722577)
            (xy -10.466343 5.74433)
            (xy -10.337288 5.793415)
            (xy -10.135722 5.868532)
            (xy -9.86523 5.968381)
            (xy -9.529396 6.091664)
            (xy -9.131803 6.237081)
            (xy -8.676037 6.403332)
            (xy -8.165681 6.589118)
            (xy -7.604319 6.79314)
            (xy -6.995536 7.014098)
            (xy -6.342916 7.250693)
            (xy -5.650042 7.501624)
            (xy -4.920499 7.765594)
            (xy -4.157872 8.041302)
            (xy -3.365743 8.32745)
            (xy -2.547698 8.622737)
            (xy -1.707321 8.925864)
            (xy -0.848195 9.235531)
            (xy 0.026095 9.55044)
            (xy 0.911965 9.869291)
            (xy 1.725167 10.161783)
            (xy 2.351267 10.386884)
            (xy 2.902513 10.585)
            (xy 3.383716 10.757802)
            (xy 3.79969 10.906966)
            (xy 4.155248 11.034165)
            (xy 4.455202 11.141074)
            (xy 4.704367 11.229365)
            (xy 4.907554 11.300714)
            (xy 5.069578 11.356793)
            (xy 5.19525 11.399277)
            (xy 5.289384 11.429841)
            (xy 5.356793 11.450156)
            (xy 5.40229 11.461899)
            (xy 5.430688 11.466742)
            (xy 5.4468 11.466359)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "5" smd custom (at 10 -11.5) (size 1.524 1.524) (layers "F.Cu")
      (net 116 "/right/P21") (pinfunction "Pin_5") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 9.871282 6.977783)
            (xy 10.122084 6.977582)
            (xy 11.191 6.976667)
            (xy 11.191 3.258306)
            (xy 11.190637 2.630209)
            (xy 11.189585 1.972459)
            (xy 11.187903 1.297657)
            (xy 11.185647 0.618401)
            (xy 11.182876 -0.052708)
            (xy 11.179647 -0.703071)
            (xy 11.176017 -1.320089)
            (xy 11.172045 -1.891161)
            (xy 11.167788 -2.403689)
            (xy 11.163303 -2.845072)
            (xy 11.162967 -2.874245)
            (xy 11.134934 -5.288436)
            (xy 1.796717 -6.840916)
            (xy 0.918678 -6.986907)
            (xy 0.062327 -7.129322)
            (xy -0.768556 -7.267532)
            (xy -1.57019 -7.400907)
            (xy -2.338797 -7.528818)
            (xy -3.070596 -7.650635)
            (xy -3.761807 -7.765727)
            (xy -4.408651 -7.873466)
            (xy -5.007348 -7.97322)
            (xy -5.554118 -8.064361)
            (xy -6.045182 -8.146258)
            (xy -6.476759 -8.218282)
            (xy -6.845069 -8.279803)
            (xy -7.146334 -8.330191)
            (xy -7.376772 -8.368816)
            (xy -7.532605 -8.395048)
            (xy -7.610052 -8.408258)
            (xy -7.618008 -8.409702)
            (xy -7.69654 -8.388268)
            (xy -7.733338 -8.334087)
            (xy -7.746562 -8.292715)
            (xy -7.774413 -8.196195)
            (xy -7.817336 -8.042875)
            (xy -7.875777 -7.831104)
            (xy -7.950181 -7.559229)
            (xy -8.040995 -7.225599)
            (xy -8.148663 -6.828563)
            (xy -8.273632 -6.366468)
            (xy -8.416348 -5.837663)
            (xy -8.577255 -5.240496)
            (xy -8.7568 -4.573315)
            (xy -8.955429 -3.834469)
            (xy -9.173587 -3.022306)
            (xy -9.41172 -2.135174)
            (xy -9.670273 -1.171422)
            (xy -9.949693 -0.129397)
            (xy -10.250425 0.992552)
            (xy -10.294183 1.155834)
            (xy -10.462988 1.786319)
            (xy -10.624316 2.390025)
            (xy -10.776873 2.962048)
            (xy -10.919363 3.497486)
            (xy -11.050492 3.991437)
            (xy -11.168965 4.438999)
            (xy -11.273486 4.835269)
            (xy -11.362761 5.175344)
            (xy -11.435494 5.454323)
            (xy -11.490391 5.667303)
            (xy -11.526156 5.809382)
            (xy -11.541495 5.875658)
            (xy -11.542 5.879531)
            (xy -11.53367 5.891516)
            (xy -11.502788 5.903514)
            (xy -11.440518 5.916745)
            (xy -11.338023 5.932431)
            (xy -11.186468 5.951792)
            (xy -10.977016 5.97605)
            (xy -10.700829 6.006426)
            (xy -10.356666 6.043333)
            (xy -8.612102 6.219678)
            (xy -6.835413 6.381011)
            (xy -5.051314 6.525404)
            (xy -3.284522 6.650926)
            (xy -1.559753 6.755649)
            (xy -0.577666 6.806617)
            (xy -0.071134 6.830702)
            (xy 0.410108 6.85253)
            (xy 0.872435 6.872201)
            (xy 1.322218 6.889818)
            (xy 1.765833 6.905483)
            (xy 2.209651 6.919297)
            (xy 2.660046 6.931362)
            (xy 3.123392 6.94178)
            (xy 3.606062 6.950653)
            (xy 4.11443 6.958083)
            (xy 4.654868 6.964172)
            (xy 5.233751 6.96902)
            (xy 5.857451 6.972731)
            (xy 6.532342 6.975406)
            (xy 7.264797 6.977147)
            (xy 8.06119 6.978055)
            (xy 8.927894 6.978234)
            (xy 9.871282 6.977783)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "6" smd custom (at 6.5 6.5) (size 1.524 1.524) (layers "F.Cu")
      (net 107 "/right/P34") (pinfunction "Pin_6") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 7.691 -10.033)
            (xy -5.93707 -10.033)
            (xy -5.980392 -9.87425)
            (xy -6.0545 -9.602033)
            (xy -6.145631 -9.266192)
            (xy -6.252617 -8.871064)
            (xy -6.374297 -8.420984)
            (xy -6.509505 -7.920289)
            (xy -6.657077 -7.373317)
            (xy -6.815848 -6.784402)
            (xy -6.984655 -6.157882)
            (xy -7.162333 -5.498093)
            (xy -7.347719 -4.809372)
            (xy -7.539646 -4.096055)
            (xy -7.736952 -3.362479)
            (xy -7.938472 -2.612979)
            (xy -8.143042 -1.851894)
            (xy -8.349497 -1.083559)
            (xy -8.556674 -0.31231)
            (xy -8.763407 0.457516)
            (xy -8.968533 1.221581)
            (xy -9.170887 1.975551)
            (xy -9.369305 2.715088)
            (xy -9.562623 3.435856)
            (xy -9.749676 4.133519)
            (xy -9.929301 4.803739)
            (xy -10.100333 5.44218)
            (xy -10.261607 6.044507)
            (xy -10.411959 6.606382)
            (xy -10.550226 7.123468)
            (xy -10.675242 7.59143)
            (xy -10.785843 8.005931)
            (xy -10.880866 8.362635)
            (xy -10.959146 8.657204)
            (xy -11.019518 8.885303)
            (xy -11.060819 9.042595)
            (xy -11.081884 9.124743)
            (xy -11.08445 9.136328)
            (xy -11.042017 9.144458)
            (xy -10.919823 9.16583)
            (xy -10.721629 9.199815)
            (xy -10.451196 9.245782)
            (xy -10.112285 9.3031)
            (xy -9.708657 9.371139)
            (xy -9.244074 9.44927)
            (xy -8.722296 9.536861)
            (xy -8.147085 9.633282)
            (xy -7.522201 9.737903)
            (xy -6.851407 9.850093)
            (xy -6.138462 9.969223)
            (xy -5.387128 10.094661)
            (xy -4.601167 10.225778)
            (xy -3.784339 10.361943)
            (xy -2.940405 10.502526)
            (xy -2.073127 10.646897)
            (xy -1.806334 10.691288)
            (xy -0.931218 10.836889)
            (xy -0.077478 10.978947)
            (xy 0.75107 11.116827)
            (xy 1.550607 11.249894)
            (xy 2.317319 11.37751)
            (xy 3.047388 11.499042)
            (xy 3.736997 11.613852)
            (xy 4.38233 11.721307)
            (xy 4.97957 11.820769)
            (xy 5.524901 11.911604)
            (xy 6.014505 11.993175)
            (xy 6.444567 12.064847)
            (xy 6.811268 12.125985)
            (xy 7.110794 12.175952)
            (xy 7.339326 12.214114)
            (xy 7.493048 12.239834)
            (xy 7.568145 12.252477)
            (xy 7.574584 12.253591)
            (xy 7.691 12.27455)
            (xy 7.691 -10.033)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "7" smd custom (at -11.5 -11.5) (size 1.524 1.524) (layers "F.Cu")
      (net 108 "/right/P33") (pinfunction "Pin_7") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -9.38825 6.957217)
            (xy -9.21492 6.949388)
            (xy -8.973211 6.939506)
            (xy -8.679371 6.928182)
            (xy -8.349645 6.916025)
            (xy -8.00028 6.903646)
            (xy -7.647523 6.891654)
            (xy -7.599666 6.89007)
            (xy -5.893102 6.822374)
            (xy -4.123604 6.730388)
            (xy -2.308901 6.615559)
            (xy -0.466719 6.479335)
            (xy 1.385214 6.323164)
            (xy 3.229173 6.148492)
            (xy 5.047429 5.956768)
            (xy 6.822256 5.74944)
            (xy 7.6615 5.643778)
            (xy 8.184591 5.575829)
            (xy 8.6277 5.517239)
            (xy 8.994925 5.467415)
            (xy 9.290364 5.425761)
            (xy 9.518114 5.391684)
            (xy 9.682274 5.364588)
            (xy 9.786941 5.34388)
            (xy 9.836213 5.328965)
            (xy 9.837774 5.328073)
            (xy 9.838047 5.283121)
            (xy 9.827875 5.157239)
            (xy 9.807627 4.953471)
            (xy 9.777675 4.67486)
            (xy 9.73839 4.324451)
            (xy 9.690143 3.905285)
            (xy 9.633304 3.420406)
            (xy 9.568244 2.872859)
            (xy 9.495334 2.265685)
            (xy 9.414944 1.60193)
            (xy 9.327447 0.884635)
            (xy 9.233211 0.116844)
            (xy 9.132609 -0.698398)
            (xy 9.02601 -1.55805)
            (xy 8.913787 -2.459066)
            (xy 8.796309 -3.398405)
            (xy 8.673947 -4.373023)
            (xy 8.547073 -5.379876)
            (xy 8.416056 -6.41592)
            (xy 8.281268 -7.478114)
            (xy 8.192122 -8.178666)
            (xy 8.145404 -8.546682)
            (xy 8.102224 -8.889293)
            (xy 8.06373 -9.19721)
            (xy 8.031069 -9.461146)
            (xy 8.005389 -9.671813)
            (xy 7.987835 -9.819924)
            (xy 7.979556 -9.896189)
            (xy 7.979052 -9.90375)
            (xy 7.970203 -9.931365)
            (xy 7.937784 -9.945895)
            (xy 7.872884 -9.945787)
            (xy 7.766595 -9.929489)
            (xy 7.610009 -9.895448)
            (xy 7.394215 -9.842112)
            (xy 7.110305 -9.767928)
            (xy 6.941834 -9.723018)
            (xy 6.827666 -9.692659)
            (xy 6.63588 -9.641909)
            (xy 6.370743 -9.571892)
            (xy 6.036525 -9.48373)
            (xy 5.637495 -9.378547)
            (xy 5.17792 -9.257465)
            (xy 4.662071 -9.121607)
            (xy 4.094216 -8.972097)
            (xy 3.478623 -8.810056)
            (xy 2.819562 -8.636608)
            (xy 2.121301 -8.452876)
            (xy 1.38811 -8.259982)
            (xy 0.624256 -8.05905)
            (xy -0.165991 -7.851202)
            (xy -0.978362 -7.637562)
            (xy -1.808588 -7.419252)
            (xy -2.652401 -7.197394)
            (xy -3.505532 -6.973113)
            (xy -4.363712 -6.74753)
            (xy -5.222672 -6.521769)
            (xy -6.078144 -6.296953)
            (xy -6.925858 -6.074204)
            (xy -7.761546 -5.854645)
            (xy -8.580938 -5.639399)
            (xy -9.379767 -5.42959)
            (xy -9.726916 -5.338424)
            (xy -9.885666 -5.296736)
            (xy -9.885666 6.981768)
            (xy -9.38825 6.957217)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "8" smd custom (at -9.5 7) (size 1.524 1.524) (layers "F.Cu")
      (net 106 "/right/P35") (pinfunction "Pin_8") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -7.802485 12.703263)
            (xy -7.681357 12.676748)
            (xy -7.492474 12.631993)
            (xy -7.24287 12.570761)
            (xy -6.939576 12.494816)
            (xy -6.589625 12.405922)
            (xy -6.200051 12.305844)
            (xy -5.777885 12.196345)
            (xy -5.330161 12.079189)
            (xy -5.234742 12.054092)
            (xy -4.230624 11.789719)
            (xy -3.234784 11.527442)
            (xy -2.250542 11.268139)
            (xy -1.281218 11.012687)
            (xy -0.330133 10.761964)
            (xy 0.599391 10.516849)
            (xy 1.504034 10.278218)
            (xy 2.380474 10.046949)
            (xy 3.225392 9.82392)
            (xy 4.035466 9.610009)
            (xy 4.807376 9.406093)
            (xy 5.5378 9.213051)
            (xy 6.223418 9.031759)
            (xy 6.860908 8.863095)
            (xy 7.446951 8.707938)
            (xy 7.978225 8.567164)
            (xy 8.451409 8.441652)
            (xy 8.863182 8.33228)
            (xy 9.210224 8.239924)
            (xy 9.489214 8.165463)
            (xy 9.696831 8.109774)
            (xy 9.829753 8.073735)
            (xy 9.884661 8.058224)
            (xy 9.88599 8.057701)
            (xy 9.88236 8.014954)
            (xy 9.868764 7.892965)
            (xy 9.845796 7.696501)
            (xy 9.814049 7.430326)
            (xy 9.774118 7.099206)
            (xy 9.726594 6.707905)
            (xy 9.672071 6.261188)
            (xy 9.611142 5.763821)
            (xy 9.544401 5.220569)
            (xy 9.472441 4.636196)
            (xy 9.395854 4.015467)
            (xy 9.315235 3.363148)
            (xy 9.231177 2.684003)
            (xy 9.144272 1.982799)
            (xy 9.055113 1.264298)
            (xy 8.964295 0.533268)
            (xy 8.872411 -0.205528)
            (xy 8.780053 -0.947324)
            (xy 8.687814 -1.687355)
            (xy 8.596289 -2.420857)
            (xy 8.50607 -3.143063)
            (xy 8.417751 -3.84921)
            (xy 8.331924 -4.534532)
            (xy 8.249183 -5.194264)
            (xy 8.170122 -5.823641)
            (xy 8.095332 -6.417899)
            (xy 8.025409 -6.972271)
            (xy 7.960944 -7.481993)
            (xy 7.902532 -7.9423)
            (xy 7.850764 -8.348427)
            (xy 7.806236 -8.695609)
            (xy 7.769539 -8.979081)
            (xy 7.741267 -9.194077)
            (xy 7.722013 -9.335834)
            (xy 7.713141 -9.395416)
            (xy 7.689164 -9.533)
            (xy -7.885666 -9.533)
            (xy -7.885666 1.577002)
            (xy -7.885528 2.576764)
            (xy -7.885119 3.548939)
            (xy -7.884451 4.490274)
            (xy -7.883534 5.397513)
            (xy -7.882379 6.267402)
            (xy -7.880998 7.096688)
            (xy -7.879399 7.882115)
            (xy -7.877596 8.620429)
            (xy -7.875597 9.308376)
            (xy -7.873415 9.942702)
            (xy -7.871059 10.520152)
            (xy -7.868541 11.037472)
            (xy -7.865872 11.491408)
            (xy -7.863061 11.878704)
            (xy -7.86012 12.196107)
            (xy -7.85706 12.440363)
            (xy -7.853891 12.608217)
            (xy -7.850624 12.696414)
            (xy -7.848825 12.709773)
            (xy -7.802485 12.703263)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "9" smd custom (at -27.5 -7.5) (size 1.524 1.524) (layers "F.Cu")
      (net 101 "/right/P43") (pinfunction "Pin_9") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -4.676666 9.132986)
            (xy -3.860926 9.010269)
            (xy -2.978982 8.870822)
            (xy -2.047009 8.717482)
            (xy -1.081179 8.553082)
            (xy -0.097664 8.380459)
            (xy 0.887363 8.202447)
            (xy 1.857728 8.021882)
            (xy 2.79726 7.8416)
            (xy 3.622215 7.678079)
            (xy 4.049235 7.59124)
            (xy 4.499889 7.498247)
            (xy 4.966477 7.400786)
            (xy 5.441298 7.300547)
            (xy 5.91665 7.199216)
            (xy 6.384832 7.098482)
            (xy 6.838143 7.000031)
            (xy 7.268881 6.905553)
            (xy 7.669345 6.816735)
            (xy 8.031835 6.735263)
            (xy 8.348648 6.662827)
            (xy 8.612084 6.601114)
            (xy 8.814441 6.551811)
            (xy 8.948018 6.516607)
            (xy 9.001251 6.499251)
            (xy 9.018853 6.479594)
            (xy 9.020839 6.437035)
            (xy 9.004203 6.362596)
            (xy 8.965936 6.247299)
            (xy 8.903031 6.082165)
            (xy 8.812481 5.858218)
            (xy 8.691279 5.566478)
            (xy 8.678867 5.536834)
            (xy 8.204883 4.373414)
            (xy 7.776981 3.253904)
            (xy 7.387553 2.156747)
            (xy 7.028991 1.060386)
            (xy 6.693687 -0.056734)
            (xy 6.646893 -0.2205)
            (xy 6.552164 -0.561118)
            (xy 6.450312 -0.93972)
            (xy 6.345284 -1.340595)
            (xy 6.241024 -1.748032)
            (xy 6.141478 -2.146319)
            (xy 6.050591 -2.519747)
            (xy 5.97231 -2.852603)
            (xy 5.910579 -3.129176)
            (xy 5.882892 -3.262753)
            (xy 5.808493 -3.638006)
            (xy 6.255683 -4.067086)
            (xy 6.668452 -4.484644)
            (xy 7.017125 -4.887365)
            (xy 7.315388 -5.293859)
            (xy 7.576926 -5.722736)
            (xy 7.809747 -6.180459)
            (xy 8.091827 -6.868142)
            (xy 8.29348 -7.55844)
            (xy 8.416639 -8.261844)
            (xy 8.463239 -8.988842)
            (xy 8.444692 -9.624539)
            (xy 8.430476 -9.8363)
            (xy 8.418507 -10.021824)
            (xy 8.409959 -10.162378)
            (xy 8.406008 -10.239224)
            (xy 8.405906 -10.242916)
            (xy 8.389673 -10.303945)
            (xy 8.372584 -10.313404)
            (xy 8.328389 -10.30235)
            (xy 8.207359 -10.270998)
            (xy 8.014517 -10.220668)
            (xy 7.754887 -10.152681)
            (xy 7.433493 -10.068359)
            (xy 7.055359 -9.969023)
            (xy 6.62551 -9.855992)
            (xy 6.148968 -9.730589)
            (xy 5.630759 -9.594134)
            (xy 5.075905 -9.447949)
            (xy 4.489432 -9.293353)
            (xy 3.876363 -9.131669)
            (xy 3.387834 -9.002775)
            (xy 2.683857 -8.817022)
            (xy 1.953434 -8.624321)
            (xy 1.206513 -8.427297)
            (xy 0.45304 -8.228572)
            (xy -0.297037 -8.030769)
            (xy -1.033771 -7.836509)
            (xy -1.747215 -7.648417)
            (xy -2.427421 -7.469114)
            (xy -3.064443 -7.301223)
            (xy -3.648333 -7.147368)
            (xy -4.169143 -7.01017)
            (xy -4.570833 -6.904388)
            (xy -5.059179 -6.775743)
            (xy -5.52319 -6.653371)
            (xy -5.956436 -6.538977)
            (xy -6.352489 -6.434266)
            (xy -6.704918 -6.340941)
            (xy -7.007295 -6.260705)
            (xy -7.25319 -6.195264)
            (xy -7.436175 -6.146321)
            (xy -7.549819 -6.115581)
            (xy -7.587702 -6.104787)
            (xy -7.587991 -6.084181)
            (xy -7.583084 -6.024432)
            (xy -7.572611 -5.922537)
            (xy -7.556202 -5.775495)
            (xy -7.533487 -5.580302)
            (xy -7.504098 -5.333957)
            (xy -7.467664 -5.033456)
            (xy -7.423816 -4.675798)
            (xy -7.372185 -4.257981)
            (xy -7.3124 -3.777001)
            (xy -7.244093 -3.229856)
            (xy -7.166893 -2.613544)
            (xy -7.080432 -1.925063)
            (xy -6.984339 -1.16141)
            (xy -6.878245 -0.319583)
            (xy -6.769597 0.5415)
            (xy -6.643217 1.542528)
            (xy -6.52698 2.462942)
            (xy -6.42045 3.306131)
            (xy -6.32319 4.075486)
            (xy -6.234764 4.774396)
            (xy -6.154738 5.40625)
            (xy -6.082675 5.974438)
            (xy -6.018138 6.482349)
            (xy -5.960694 6.933374)
            (xy -5.909904 7.330901)
            (xy -5.865334 7.67832)
            (xy -5.826548 7.97902)
            (xy -5.79311 8.236391)
            (xy -5.764584 8.453823)
            (xy -5.740534 8.634705)
            (xy -5.720525 8.782427)
            (xy -5.70412 8.900378)
            (xy -5.690883 8.991948)
            (xy -5.68038 9.060526)
            (xy -5.672173 9.109501)
            (xy -5.665827 9.142264)
            (xy -5.661191 9.161232)
            (xy -5.629166 9.271963)
            (xy -4.676666 9.132986)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "10" smd custom (at -25.5 9) (size 1.524 1.524) (layers "F.Cu")
      (net 98 "/right/P55") (pinfunction "Pin_10") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -5.520849 9.905552)
            (xy -5.391799 9.873004)
            (xy -5.191119 9.821491)
            (xy -4.923628 9.752283)
            (xy -4.594146 9.666649)
            (xy -4.207493 9.56586)
            (xy -3.768489 9.451185)
            (xy -3.281953 9.323894)
            (xy -2.752705 9.185257)
            (xy -2.185564 9.036543)
            (xy -1.58535 8.879022)
            (xy -0.956884 8.713964)
            (xy -0.304984 8.542638)
            (xy 0.36553 8.366315)
            (xy 1.049839 8.186263)
            (xy 1.743121 8.003753)
            (xy 2.440559 7.820055)
            (xy 3.137332 7.636438)
            (xy 3.82862 7.454172)
            (xy 4.509604 7.274526)
            (xy 5.175464 7.098771)
            (xy 5.821381 6.928176)
            (xy 6.442534 6.76401)
            (xy 7.034105 6.607545)
            (xy 7.591273 6.460048)
            (xy 8.109219 6.322791)
            (xy 8.583123 6.197042)
            (xy 9.008166 6.084072)
            (xy 9.379528 5.98515)
            (xy 9.692389 5.901546)
            (xy 9.941929 5.834529)
            (xy 10.123329 5.78537)
            (xy 10.23177 5.755339)
            (xy 10.262989 5.745789)
            (xy 10.262858 5.693738)
            (xy 10.234871 5.578447)
            (xy 10.184223 5.414625)
            (xy 10.116109 5.216982)
            (xy 10.035725 5.000228)
            (xy 9.948265 4.779071)
            (xy 9.858924 4.568221)
            (xy 9.805557 4.450596)
            (xy 9.451981 3.794546)
            (xy 9.026798 3.18176)
            (xy 8.533236 2.615899)
            (xy 7.974526 2.100628)
            (xy 7.353895 1.639612)
            (xy 7.292834 1.599422)
            (xy 7.121538 1.483459)
            (xy 6.973914 1.375356)
            (xy 6.866408 1.287688)
            (xy 6.816803 1.235447)
            (xy 6.799301 1.157384)
            (xy 6.791003 1.003148)
            (xy 6.79135 0.780668)
            (xy 6.799784 0.497872)
            (xy 6.815746 0.162689)
            (xy 6.838677 -0.216953)
            (xy 6.868019 -0.633124)
            (xy 6.903213 -1.077896)
            (xy 6.943702 -1.543341)
            (xy 6.988925 -2.021528)
            (xy 7.038325 -2.504531)
            (xy 7.091343 -2.984419)
            (xy 7.146743 -3.447833)
            (xy 7.210248 -3.930928)
            (xy 7.285058 -4.455038)
            (xy 7.367837 -4.999414)
            (xy 7.455245 -5.543308)
            (xy 7.543946 -6.065972)
            (xy 7.630602 -6.546657)
            (xy 7.711876 -6.964616)
            (xy 7.714593 -6.977904)
            (xy 7.755184 -7.17723)
            (xy 7.788748 -7.344227)
            (xy 7.812056 -7.462673)
            (xy 7.821881 -7.516345)
            (xy 7.822 -7.517654)
            (xy 7.780361 -7.519237)
            (xy 7.658223 -7.520774)
            (xy 7.459751 -7.522258)
            (xy 7.189114 -7.523681)
            (xy 6.850478 -7.525034)
            (xy 6.448009 -7.52631)
            (xy 5.985876 -7.527499)
            (xy 5.468244 -7.528595)
            (xy 4.899281 -7.529589)
            (xy 4.283154 -7.530472)
            (xy 3.624029 -7.531236)
            (xy 2.926074 -7.531874)
            (xy 2.193455 -7.532378)
            (xy 1.430339 -7.532738)
            (xy 0.640894 -7.532947)
            (xy -0.009666 -7.533)
            (xy -0.968791 -7.53296)
            (xy -1.8468 -7.53282)
            (xy -2.647244 -7.532548)
            (xy -3.373673 -7.532113)
            (xy -4.02964 -7.531484)
            (xy -4.618693 -7.530629)
            (xy -5.144385 -7.529516)
            (xy -5.610265 -7.528115)
            (xy -6.019886 -7.526393)
            (xy -6.376797 -7.52432)
            (xy -6.684549 -7.521864)
            (xy -6.946693 -7.518994)
            (xy -7.166781 -7.515678)
            (xy -7.348362 -7.511885)
            (xy -7.494988 -7.507583)
            (xy -7.610209 -7.502741)
            (xy -7.697576 -7.497328)
            (xy -7.76064 -7.491312)
            (xy -7.802952 -7.484662)
            (xy -7.828063 -7.477346)
            (xy -7.839522 -7.469333)
            (xy -7.841333 -7.463732)
            (xy -7.836146 -7.417181)
            (xy -7.820989 -7.291476)
            (xy -7.796472 -7.091471)
            (xy -7.763202 -6.822015)
            (xy -7.721788 -6.48796)
            (xy -7.672839 -6.094157)
            (xy -7.616964 -5.645457)
            (xy -7.554769 -5.14671)
            (xy -7.486865 -4.602769)
            (xy -7.41386 -4.018483)
            (xy -7.336361 -3.398704)
            (xy -7.254978 -2.748283)
            (xy -7.170318 -2.072071)
            (xy -7.082991 -1.374919)
            (xy -6.993605 -0.661678)
            (xy -6.902769 0.062801)
            (xy -6.81109 0.793667)
            (xy -6.719177 1.526069)
            (xy -6.627639 2.255157)
            (xy -6.537085 2.976077)
            (xy -6.448122 3.683981)
            (xy -6.361359 4.374017)
            (xy -6.277404 5.041334)
            (xy -6.196867 5.68108)
            (xy -6.120356 6.288405)
            (xy -6.048478 6.858458)
            (xy -5.981843 7.386388)
            (xy -5.921059 7.867344)
            (xy -5.866734 8.296474)
            (xy -5.819477 8.668928)
            (xy -5.779896 8.979855)
            (xy -5.748601 9.224404)
            (xy -5.731365 9.358)
            (xy -5.700667 9.587399)
            (xy -5.676068 9.745376)
            (xy -5.653987 9.844622)
            (xy -5.630846 9.897829)
            (xy -5.603064 9.917685)
            (xy -5.57345 9.917866)
            (xy -5.520849 9.905552)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "11" smd custom (at -42 -5) (size 1.524 1.524) (layers "F.Cu")
      (net 97 "/right/P56") (pinfunction "Pin_11") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -4.876323 8.841692)
            (xy -4.73834 8.817674)
            (xy -4.530693 8.77376)
            (xy -4.25929 8.711512)
            (xy -3.930037 8.632495)
            (xy -3.54884 8.538273)
            (xy -3.121605 8.430409)
            (xy -2.654239 8.310468)
            (xy -2.152648 8.180014)
            (xy -1.622739 8.04061)
            (xy -1.070417 7.89382)
            (xy -0.50159 7.741209)
            (xy 0.077837 7.58434)
            (xy 0.661957 7.424778)
            (xy 1.244864 7.264085)
            (xy 1.820651 7.103827)
            (xy 2.383412 6.945567)
            (xy 2.927241 6.790869)
            (xy 3.446231 6.641297)
            (xy 3.934476 6.498415)
            (xy 4.05375 6.46312)
            (xy 4.995667 6.183704)
            (xy 4.995667 -2.277148)
            (xy 4.995511 -3.116892)
            (xy 4.995052 -3.933769)
            (xy 4.994305 -4.723774)
            (xy 4.993286 -5.482901)
            (xy 4.992009 -6.207143)
            (xy 4.99049 -6.892496)
            (xy 4.988744 -7.534952)
            (xy 4.986785 -8.130506)
            (xy 4.984628 -8.675152)
            (xy 4.98229 -9.164884)
            (xy 4.979784 -9.595696)
            (xy 4.977126 -9.963582)
            (xy 4.974331 -10.264536)
            (xy 4.971413 -10.494552)
            (xy 4.968389 -10.649625)
            (xy 4.965272 -10.725747)
            (xy 4.963917 -10.733211)
            (xy 4.916122 -10.721464)
            (xy 4.797487 -10.690776)
            (xy 4.61898 -10.644028)
            (xy 4.391566 -10.584103)
            (xy 4.126211 -10.513883)
            (xy 3.833882 -10.436248)
            (xy 3.8315 -10.435615)
            (xy 3.486456 -10.343895)
            (xy 3.091991 -10.239163)
            (xy 2.654442 -10.123095)
            (xy 2.180148 -9.997364)
            (xy 1.675446 -9.863647)
            (xy 1.146675 -9.723619)
            (xy 0.600172 -9.578954)
            (xy 0.042275 -9.431329)
            (xy -0.520677 -9.282418)
            (xy -1.082347 -9.133896)
            (xy -1.636396 -8.987438)
            (xy -2.176487 -8.84472)
            (xy -2.696282 -8.707417)
            (xy -3.189443 -8.577205)
            (xy -3.649631 -8.455757)
            (xy -4.070509 -8.34475)
            (xy -4.445739 -8.245858)
            (xy -4.768983 -8.160757)
            (xy -5.033902 -8.091122)
            (xy -5.23416 -8.038628)
            (xy -5.363417 -8.00495)
            (xy -5.408642 -7.993373)
            (xy -5.674118 -7.927347)
            (xy -5.641476 -7.54409)
            (xy -5.61877 -7.180459)
            (xy -5.608898 -6.791218)
            (xy -5.611275 -6.396178)
            (xy -5.625315 -6.015146)
            (xy -5.650433 -5.667932)
            (xy -5.686044 -5.374345)
            (xy -5.709405 -5.245197)
            (xy -5.898052 -4.523029)
            (xy -6.152842 -3.820141)
            (xy -6.467298 -3.150311)
            (xy -6.834947 -2.527312)
            (xy -7.249313 -1.964919)
            (xy -7.253985 -1.959267)
            (xy -7.374807 -1.821167)
            (xy -7.534547 -1.649453)
            (xy -7.710285 -1.468343)
            (xy -7.843857 -1.336002)
            (xy -8.218971 -0.972171)
            (xy -8.063717 -0.298835)
            (xy -7.778749 0.86471)
            (xy -7.454292 2.060444)
            (xy -7.100666 3.252089)
            (xy -6.72819 4.403365)
            (xy -6.716289 4.4385)
            (xy -6.572582 4.854694)
            (xy -6.419288 5.285117)
            (xy -6.259419 5.722303)
            (xy -6.095988 6.158787)
            (xy -5.932008 6.587102)
            (xy -5.77049 6.999781)
            (xy -5.614448 7.389357)
            (xy -5.466893 7.748365)
            (xy -5.330838 8.069337)
            (xy -5.209296 8.344808)
            (xy -5.105278 8.567311)
            (xy -5.021798 8.72938)
            (xy -4.961867 8.823547)
            (xy -4.938737 8.844248)
            (xy -4.876323 8.841692)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "12" smd custom (at -40.5 11) (size 1.524 1.524) (layers "F.Cu")
      (net 95 "/right/P58") (pinfunction "Pin_12") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -4.173721 7.611281)
            (xy -4.120162 7.597693)
            (xy -3.989692 7.563835)
            (xy -3.787274 7.511011)
            (xy -3.51787 7.440524)
            (xy -3.186441 7.353675)
            (xy -2.797949 7.251769)
            (xy -2.357356 7.136106)
            (xy -1.869624 7.00799)
            (xy -1.339716 6.868725)
            (xy -0.772592 6.719611)
            (xy -0.173216 6.561952)
            (xy 0.453451 6.397051)
            (xy 1.102447 6.22621)
            (xy 1.204 6.199472)
            (xy 6.4745 4.811736)
            (xy 6.485251 -0.360632)
            (xy 6.496003 -5.533)
            (xy -6.70907 -5.533)
            (xy -6.750658 -5.37425)
            (xy -6.792723 -5.195423)
            (xy -6.844665 -4.945224)
            (xy -6.904337 -4.636085)
            (xy -6.969592 -4.280442)
            (xy -7.038284 -3.890729)
            (xy -7.108267 -3.479382)
            (xy -7.177395 -3.058836)
            (xy -7.24352 -2.641525)
            (xy -7.304497 -2.239885)
            (xy -7.35818 -1.866349)
            (xy -7.366272 -1.807666)
            (xy -7.415555 -1.427243)
            (xy -7.465579 -1.00324)
            (xy -7.515256 -0.548032)
            (xy -7.563502 -0.073993)
            (xy -7.60923 0.406502)
            (xy -7.651355 0.881079)
            (xy -7.68879 1.337364)
            (xy -7.72045 1.762982)
            (xy -7.745249 2.14556)
            (xy -7.762101 2.472721)
            (xy -7.769921 2.732093)
            (xy -7.77034 2.797087)
            (xy -7.767092 2.935951)
            (xy -7.748669 3.018702)
            (xy -7.701347 3.073885)
            (xy -7.611397 3.130043)
            (xy -7.60977 3.130971)
            (xy -7.459085 3.225878)
            (xy -7.263793 3.361722)
            (xy -7.04326 3.523981)
            (xy -6.816853 3.698132)
            (xy -6.603939 3.869654)
            (xy -6.451303 3.999651)
            (xy -6.051869 4.394091)
            (xy -5.6659 4.856405)
            (xy -5.304059 5.369849)
            (xy -4.977009 5.917676)
            (xy -4.695413 6.483141)
            (xy -4.469934 7.049498)
            (xy -4.426877 7.178928)
            (xy -4.36293 7.375897)
            (xy -4.316395 7.505094)
            (xy -4.279604 7.579616)
            (xy -4.244889 7.612557)
            (xy -4.204581 7.617013)
            (xy -4.173721 7.611281)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "13" smd custom (at -31 30.5) (size 1.524 1.524) (layers "F.Cu")
      (net 120 "/right/P15") (pinfunction "Pin_13") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 6.174334 -6.014333)
            (xy -6.398666 -6.014333)
            (xy -6.398666 6.516334)
            (xy 6.174334 6.516334)
            (xy 6.174334 -6.014333)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "14" smd custom (at -42.5 30) (size 1.524 1.524) (layers "F.Cu")
      (net 121 "/right/P14") (pinfunction "Pin_14") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 4.495667 -6.514333)
            (xy -4.902333 -6.514333)
            (xy -4.902333 6.016334)
            (xy 4.495667 6.016334)
            (xy 4.495667 -6.514333)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "15" smd custom (at 4.5 -21) (size 1.524 1.524) (layers "F.Cu")
      (net 115 "/right/P22") (pinfunction "Pin_15") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -13.019779 1.915135)
            (xy -12.023606 1.914874)
            (xy -11.011634 1.914426)
            (xy -9.987307 1.913792)
            (xy -8.954069 1.912978)
            (xy -7.915363 1.911985)
            (xy -6.874631 1.910819)
            (xy -5.835319 1.909483)
            (xy -4.800868 1.90798)
            (xy -3.774723 1.906314)
            (xy -2.760326 1.904488)
            (xy -1.761122 1.902507)
            (xy -0.780553 1.900373)
            (xy 0.177937 1.89809)
            (xy 1.110904 1.895663)
            (xy 2.014906 1.893094)
            (xy 2.886499 1.890387)
            (xy 3.722239 1.887546)
            (xy 4.518683 1.884575)
            (xy 5.272388 1.881476)
            (xy 5.97991 1.878254)
            (xy 6.637806 1.874912)
            (xy 7.242632 1.871454)
            (xy 7.790946 1.867884)
            (xy 8.279303 1.864204)
            (xy 8.70426 1.860419)
            (xy 9.062375 1.856533)
            (xy 9.350203 1.852548)
            (xy 9.564301 1.848469)
            (xy 9.701226 1.844298)
            (xy 9.712667 1.843775)
            (xy 11.849738 1.730611)
            (xy 13.917325 1.601227)
            (xy 15.929297 1.454248)
            (xy 17.899524 1.288303)
            (xy 19.841877 1.102018)
            (xy 21.770224 0.894023)
            (xy 23.698437 0.662943)
            (xy 25.640385 0.407406)
            (xy 27.609937 0.12604)
            (xy 28.635667 -0.02879)
            (xy 31.213306 -0.443109)
            (xy 33.749083 -0.88848)
            (xy 36.257462 -1.36806)
            (xy 38.752908 -1.885007)
            (xy 41.249885 -2.442478)
            (xy 43.762858 -3.043631)
            (xy 46.306292 -3.691622)
            (xy 48.894651 -4.38961)
            (xy 49.897584 -4.6699)
            (xy 51.495667 -5.120715)
            (xy 51.495667 -7.208691)
            (xy 51.494867 -7.695006)
            (xy 51.492525 -8.125416)
            (xy 51.488725 -8.495516)
            (xy 51.483551 -8.800907)
            (xy 51.477088 -9.037184)
            (xy 51.469421 -9.199948)
            (xy 51.460635 -9.284794)
            (xy 51.455533 -9.296666)
            (xy 51.405663 -9.285138)
            (xy 51.285741 -9.252658)
            (xy 51.106877 -9.202379)
            (xy 50.88018 -9.137455)
            (xy 50.61676 -9.061042)
            (xy 50.344283 -8.98117)
            (xy 46.688523 -7.948207)
            (xy 43.016864 -6.998265)
            (xy 39.329019 -6.131296)
            (xy 35.624699 -5.347253)
            (xy 31.903618 -4.646091)
            (xy 28.165487 -4.027762)
            (xy 24.410019 -3.49222)
            (xy 20.636926 -3.039417)
            (xy 16.845919 -2.669308)
            (xy 13.036712 -2.381846)
            (xy 9.209017 -2.176983)
            (xy 8.146334 -2.134872)
            (xy 7.828535 -2.125227)
            (xy 7.434258 -2.116571)
            (xy 6.971686 -2.108905)
            (xy 6.449003 -2.102228)
            (xy 5.874391 -2.09654)
            (xy 5.256034 -2.091843)
            (xy 4.602114 -2.088135)
            (xy 3.920815 -2.085418)
            (xy 3.220319 -2.083691)
            (xy 2.50881 -2.082953)
            (xy 1.794471 -2.083207)
            (xy 1.085485 -2.08445)
            (xy 0.390034 -2.086685)
            (xy -0.283697 -2.08991)
            (xy -0.927526 -2.094126)
            (xy -1.53327 -2.099332)
            (xy -2.092746 -2.10553)
            (xy -2.597771 -2.11272)
            (xy -3.040162 -2.1209)
            (xy -3.411735 -2.130072)
            (xy -3.558833 -2.1347)
            (xy -5.172401 -2.196363)
            (xy -6.737157 -2.269532)
            (xy -8.272321 -2.355547)
            (xy -9.79711 -2.455747)
            (xy -11.330744 -2.571471)
            (xy -12.892442 -2.704058)
            (xy -14.501422 -2.854847)
            (xy -15.856666 -2.991678)
            (xy -16.260629 -3.034633)
            (xy -16.587936 -3.072078)
            (xy -16.846299 -3.105613)
            (xy -17.04343 -3.13684)
            (xy -17.187041 -3.167357)
            (xy -17.284844 -3.198767)
            (xy -17.34455 -3.23267)
            (xy -17.373871 -3.270666)
            (xy -17.380666 -3.307989)
            (xy -17.409731 -3.363656)
            (xy -17.433583 -3.370648)
            (xy -17.472852 -3.372658)
            (xy -17.503975 -3.381909)
            (xy -17.525776 -3.404812)
            (xy -17.537075 -3.447776)
            (xy -17.536697 -3.517212)
            (xy -17.523463 -3.619531)
            (xy -17.496197 -3.761141)
            (xy -17.453721 -3.948455)
            (xy -17.394857 -4.187881)
            (xy -17.318428 -4.48583)
            (xy -17.223257 -4.848712)
            (xy -17.108166 -5.282938)
            (xy -17.024705 -5.596757)
            (xy -16.877946 -6.149104)
            (xy -16.751963 -6.625193)
            (xy -16.645408 -7.030493)
            (xy -16.556934 -7.370472)
            (xy -16.485196 -7.650597)
            (xy -16.428846 -7.876337)
            (xy -16.386538 -8.05316)
            (xy -16.356924 -8.186534)
            (xy -16.338658 -8.281926)
            (xy -16.330394 -8.344805)
            (xy -16.330784 -8.38064)
            (xy -16.335993 -8.393104)
            (xy -16.355455 -8.399755)
            (xy -16.406304 -8.411266)
            (xy -16.490165 -8.427899)
            (xy -16.608661 -8.449917)
            (xy -16.763416 -8.477582)
            (xy -16.956054 -8.511157)
            (xy -17.188198 -8.550904)
            (xy -17.461473 -8.597088)
            (xy -17.777501 -8.649969)
            (xy -18.137908 -8.709811)
            (xy -18.544316 -8.776876)
            (xy -18.99835 -8.851427)
            (xy -19.501633 -8.933727)
            (xy -20.05579 -9.024038)
            (xy -20.662443 -9.122623)
            (xy -21.323216 -9.229745)
            (xy -22.039735 -9.345666)
            (xy -22.813621 -9.47065)
            (xy -23.646499 -9.604958)
            (xy -24.539994 -9.748853)
            (xy -25.495728 -9.902598)
            (xy -26.515325 -10.066456)
            (xy -27.600409 -10.240689)
            (xy -28.752605 -10.42556)
            (xy -29.973535 -10.621332)
            (xy -31.264824 -10.828267)
            (xy -32.628095 -11.046628)
            (xy -34.064973 -11.276678)
            (xy -35.57708 -11.518679)
            (xy -37.166041 -11.772894)
            (xy -38.83348 -12.039585)
            (xy -40.58102 -12.319016)
            (xy -42.410285 -12.611449)
            (xy -42.717166 -12.660502)
            (xy -43.352586 -12.762125)
            (xy -43.965676 -12.860287)
            (xy -44.551138 -12.954132)
            (xy -45.103673 -13.042807)
            (xy -45.617983 -13.125459)
            (xy -46.08877 -13.201233)
            (xy -46.510735 -13.269275)
            (xy -46.87858 -13.328732)
            (xy -47.187006 -13.378748)
            (xy -47.430715 -13.418471)
            (xy -47.604409 -13.447046)
            (xy -47.702789 -13.46362)
            (xy -47.723083 -13.467357)
            (xy -47.818333 -13.489279)
            (xy -47.818333 -11.773973)
            (xy -47.817995 -11.40219)
            (xy -47.817031 -11.058126)
            (xy -47.815513 -10.750684)
            (xy -47.813517 -10.488768)
            (xy -47.811114 -10.281282)
            (xy -47.80838 -10.137129)
            (xy -47.805387 -10.065213)
            (xy -47.804146 -10.058666)
            (xy -47.760918 -10.046948)
            (xy -47.650882 -10.014606)
            (xy -47.488168 -9.965861)
            (xy -47.286908 -9.904936)
            (xy -47.158563 -9.865827)
            (xy -46.079213 -9.5422)
            (xy -44.93082 -9.209095)
            (xy -43.727961 -8.870306)
            (xy -42.485214 -8.529625)
            (xy -41.217157 -8.190846)
            (xy -39.938366 -7.857761)
            (xy -38.663419 -7.534164)
            (xy -37.406893 -7.223847)
            (xy -36.183366 -6.930603)
            (xy -35.007415 -6.658226)
            (xy -33.893617 -6.410509)
            (xy -33.806 -6.391516)
            (xy -32.979381 -6.21557)
            (xy -32.105086 -6.034792)
            (xy -31.195794 -5.851555)
            (xy -30.264181 -5.668238)
            (xy -29.322927 -5.487215)
            (xy -28.384709 -5.310862)
            (xy -27.462205 -5.141556)
            (xy -26.568093 -4.981671)
            (xy -25.715052 -4.833585)
            (xy -24.915759 -4.699673)
            (xy -24.182892 -4.58231)
            (xy -24.005833 -4.554959)
            (xy -23.639878 -4.497133)
            (xy -23.349471 -4.445953)
            (xy -23.126089 -4.398039)
            (xy -22.961208 -4.350012)
            (xy -22.846305 -4.298494)
            (xy -22.772856 -4.240103)
            (xy -22.73234 -4.171461)
            (xy -22.716232 -4.089188)
            (xy -22.714666 -4.043006)
            (xy -22.726662 -3.961198)
            (xy -22.761707 -3.803478)
            (xy -22.818384 -3.574988)
            (xy -22.89528 -3.280871)
            (xy -22.990978 -2.926269)
            (xy -23.104064 -2.516325)
            (xy -23.233122 -2.056182)
            (xy -23.376738 -1.550983)
            (xy -23.533496 -1.00587)
            (xy -23.70198 -0.425986)
            (xy -23.834186 0.025244)
            (xy -23.944544 0.401624)
            (xy -24.047152 0.753533)
            (xy -24.139594 1.072543)
            (xy -24.219456 1.350229)
            (xy -24.284322 1.578164)
            (xy -24.331777 1.747922)
            (xy -24.359405 1.851076)
            (xy -24.365666 1.879492)
            (xy -24.323907 1.883497)
            (xy -24.200925 1.887244)
            (xy -24.000164 1.890738)
            (xy -23.725066 1.893982)
            (xy -23.379076 1.89698)
            (xy -22.965636 1.899736)
            (xy -22.48819 1.902253)
            (xy -21.950182 1.904534)
            (xy -21.355055 1.906584)
            (xy -20.706252 1.908406)
            (xy -20.007217 1.910003)
            (xy -19.261393 1.91138)
            (xy -18.472223 1.912539)
            (xy -17.643152 1.913485)
            (xy -16.777621 1.91422)
            (xy -15.879075 1.914749)
            (xy -14.950957 1.915076)
            (xy -13.996711 1.915203)
            (xy -13.019779 1.915135)
          )
          (width 0.01) (fill yes))
      )
    )
    (pad "16" smd custom (at -19.5 32.5) (size 1.524 1.524) (layers "F.Cu")
      (net 119 "/right/P16") (pinfunction "Pin_16") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 4.678 -4.014333)
            (xy -3.3738 -4.014333)
            (xy -4.239344 -4.014141)
            (xy -5.072986 -4.013578)
            (xy -5.871128 -4.01266)
            (xy -6.630171 -4.011403)
            (xy -7.346515 -4.009824)
            (xy -8.016564 -4.00794)
            (xy -8.636718 -4.005768)
            (xy -9.203378 -4.003323)
            (xy -9.712946 -4.000623)
            (xy -10.161822 -3.997684)
            (xy -10.54641 -3.994522)
            (xy -10.863109 -3.991155)
            (xy -11.108322 -3.9876)
            (xy -11.278449 -3.983872)
            (xy -11.369892 -3.979988)
            (xy -11.385383 -3.977337)
            (xy -11.34847 -3.948562)
            (xy -11.247254 -3.870688)
            (xy -11.084726 -3.746)
            (xy -10.863873 -3.576786)
            (xy -10.587686 -3.365329)
            (xy -10.259153 -3.113915)
            (xy -9.881264 -2.82483)
            (xy -9.457007 -2.500359)
            (xy -8.989372 -2.142788)
            (xy -8.481348 -1.754403)
            (xy -7.935924 -1.337487)
            (xy -7.356089 -0.894328)
            (xy -6.744833 -0.427211)
            (xy -6.105144 0.061579)
            (xy -5.440012 0.569757)
            (xy -4.752425 1.095037)
            (xy -4.045374 1.635133)
            (xy -3.598166 1.976714)
            (xy -2.877287 2.52733)
            (xy -2.172264 3.065869)
            (xy -1.486203 3.589958)
            (xy -0.822209 4.097223)
            (xy -0.183387 4.585291)
            (xy 0.427158 5.051789)
            (xy 1.00632 5.494344)
            (xy 1.550995 5.910582)
            (xy 2.058077 6.298131)
            (xy 2.524461 6.654617)
            (xy 2.947043 6.977667)
            (xy 3.322718 7.264908)
            (xy 3.648379 7.513966)
            (xy 3.920922 7.722469)
            (xy 4.137243 7.888043)
            (xy 4.294235 8.008315)
            (xy 4.388794 8.080912)
            (xy 4.413417 8.099933)
            (xy 4.678 8.306096)
            (xy 4.678 -4.014333)
          )
          (width 0.01) (fill yes))
      )
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 155.2 97.8 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C311" (at -3.676955 -8.34386 135 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/right/P30")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 149.125 92.15 45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R202" (at -0.141421 -1.767767 45) (layer "F.SilkS"))
    (property "Value" "1k" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 45 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 45 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 45 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 45) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/left/P43")
    )
    (pad "2" smd roundrect (at 0.937501 0 45) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/left/P43")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 187.9 77.05)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J201" (at 2.9 0.95 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 14 "/left/SPI2_~{CS}") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 183.7 61.725 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R201" (at 1.235 -2.49 180) (layer "F.SilkS"))
    (property "Value" "1k" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/left/P14")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/left/P14")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 170.7 69.15)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J204" (at -2.92 -0.19 0) (layer "F.SilkS"))
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 15 "/left/SPI2_SCK") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 176.079002 65.509152 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C213" (at 4.036274 0.714284 135) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 158 95 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C303" (at -3.747666 -10.111627 135 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "/right/P20")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169.948957 106.809359)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C309" (at -0.149467 1.851876 180 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/right/P59")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 185.856499 68.090052 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J206" (at 1.72 4.01 180) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 66 "/left/SPI2_CIPO") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 185.8513 64.022873 -45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C205" (at -3.446561 2.537401 -45) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 191.1625 58.6 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R203" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "5k1" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J215-PadB5)")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 119.2625 148.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C315" (at -0.1 2.6375 90) (layer "F.SilkS"))
    (property "Value" "100µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 159.402913 93.602913 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C310" (at -6.444694 -11.030866 135 unlocked) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 171.9375 64.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C208" (at 3.959798 0 0) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/left/P20")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 184.437087 65.437087 -45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C207" (at -3.538485 1.661701 135) (layer "F.SilkS"))
    (property "Value" "10nF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 194.25 67.3)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J209" (at -0.45 -1.8 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 20 "/left/SWDIO") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 115.1 144.3 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C318" (at -0.5 4.6 -90) (layer "F.SilkS"))
    (property "Value" "100µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C317-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "waad:R_borders" (layer "F.Cu")
    (at 148.68 125.95 180)
    (property "Reference" "REF**" (at -0.25 -32.675 180 unlocked) (layer "F.SilkS"))
    (property "Value" "R_borders" (at 0 -26.975 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REF}" (at -0.5 -29.7 180 unlocked) (layer "F.Fab"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 144.711846 108.488154 135)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Reference" "J308" (at -2.941564 2.98138 135) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x04_Male" (at 0 9.949999 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 3.81 45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 2.54 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "/right/USART4_TX") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 5.079999 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "/right/USART4_RX") (pinfunction "Pin_3")
    )
    (pad "4" thru_hole oval (at 0 7.62 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/right/+3V3") (pinfunction "Pin_4")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 185.722913 80.032913 -45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C202" (at 3.920323 -0.148492 135) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -45 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/left/P55")
    )
    (pad "2" smd roundrect (at 0.937501 0 315) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 187.312528 66.397028 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J202" (at 2.14 3.51 180) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 134 "/left/SPI2_COPI") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 196.8 58.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R204" (at 0.8 1.7 0) (layer "F.SilkS"))
    (property "Value" "5k1" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J215-PadA5)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:LQFP-64_10x10mm_P0.5mm" (layer "F.Cu")
    (at 180.25 73.5 -135)
    (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Reference" "U201" (at -7.954951 -6.116474 0) (layer "F.SilkS"))
    (property "Value" "STM32F072R8Tx" (at 0 7.4 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.675 -3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VBAT")
    )
    (pad "2" smd roundrect (at -5.675 -3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "PC13")
    )
    (pad "3" smd roundrect (at -5.675 -2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/left/SD_DET") (pinfunction "PC14")
    )
    (pad "4" smd roundrect (at -5.675 -2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U201-Pad4)") (pinfunction "PC15")
    )
    (pad "5" smd roundrect (at -5.675 -1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(U201-Pad5)") (pinfunction "PF0")
    )
    (pad "6" smd roundrect (at -5.675 -1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(U201-Pad6)") (pinfunction "PF1")
    )
    (pad "7" smd roundrect (at -5.675 -0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/left/NRST") (pinfunction "NRST")
    )
    (pad "8" smd roundrect (at -5.675 -0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(U201-Pad8)") (pinfunction "PC0")
    )
    (pad "9" smd roundrect (at -5.675 0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U201-Pad9)") (pinfunction "PC1")
    )
    (pad "10" smd roundrect (at -5.675 0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/left/SPI2_CIPO") (pinfunction "PC2")
    )
    (pad "11" smd roundrect (at -5.675 1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "/left/SPI2_COPI") (pinfunction "PC3")
    )
    (pad "12" smd roundrect (at -5.675 1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND") (pinfunction "VSSA")
    )
    (pad "13" smd roundrect (at -5.675 2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VDDA")
    )
    (pad "14" smd roundrect (at -5.675 2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/left/P14") (pinfunction "PA0")
    )
    (pad "15" smd roundrect (at -5.675 3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/left/P15") (pinfunction "PA1")
    )
    (pad "16" smd roundrect (at -5.675 3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/left/P16") (pinfunction "PA2")
    )
    (pad "17" smd roundrect (at -3.749999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/left/P17") (pinfunction "PA3")
    )
    (pad "18" smd roundrect (at -3.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND") (pinfunction "VSS")
    )
    (pad "19" smd roundrect (at -2.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VDD")
    )
    (pad "20" smd roundrect (at -2.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/left/P20") (pinfunction "PA4")
    )
    (pad "21" smd roundrect (at -1.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/left/P21") (pinfunction "PA5")
    )
    (pad "22" smd roundrect (at -1.249999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/left/P22") (pinfunction "PA6")
    )
    (pad "23" smd roundrect (at -0.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/left/P23") (pinfunction "PA7")
    )
    (pad "24" smd roundrect (at -0.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/left/USART3_TX") (pinfunction "PC4")
    )
    (pad "25" smd roundrect (at 0.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/left/P25") (pinfunction "PC5")
    )
    (pad "26" smd roundrect (at 0.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/left/P26") (pinfunction "PB0")
    )
    (pad "27" smd roundrect (at 1.249999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/left/P27") (pinfunction "PB1")
    )
    (pad "28" smd roundrect (at 1.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/left/P28") (pinfunction "PB2")
    )
    (pad "29" smd roundrect (at 2.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/left/SPI2_SCK") (pinfunction "PB10")
    )
    (pad "30" smd roundrect (at 2.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/left/P30") (pinfunction "PB11")
    )
    (pad "31" smd roundrect (at 3.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND") (pinfunction "VSS")
    )
    (pad "32" smd roundrect (at 3.749999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VDD")
    )
    (pad "33" smd roundrect (at 5.675 3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/left/P33") (pinfunction "PB12")
    )
    (pad "34" smd roundrect (at 5.675 3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/left/P34") (pinfunction "PB13")
    )
    (pad "35" smd roundrect (at 5.675 2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/left/P35") (pinfunction "PB14")
    )
    (pad "36" smd roundrect (at 5.675 2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U201-Pad36)") (pinfunction "PB15")
    )
    (pad "37" smd roundrect (at 5.675 1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/left/APA_DI") (pinfunction "PC6")
    )
    (pad "38" smd roundrect (at 5.675 1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/left/APA_CI") (pinfunction "PC7")
    )
    (pad "39" smd roundrect (at 5.675 0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/left/USART3_TX") (pinfunction "PC8")
    )
    (pad "40" smd roundrect (at 5.675 0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U201-Pad40)") (pinfunction "PC9")
    )
    (pad "41" smd roundrect (at 5.675 -0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U201-Pad41)") (pinfunction "PA8")
    )
    (pad "42" smd roundrect (at 5.675 -0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/left/P42") (pinfunction "PA9")
    )
    (pad "43" smd roundrect (at 5.675 -1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/left/P43") (pinfunction "PA10")
    )
    (pad "44" smd roundrect (at 5.675 -1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/left/D-") (pinfunction "PA11")
    )
    (pad "45" smd roundrect (at 5.675 -2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/left/D+") (pinfunction "PA12")
    )
    (pad "46" smd roundrect (at 5.675 -2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/left/SWDIO") (pinfunction "PA13")
    )
    (pad "47" smd roundrect (at 5.675 -3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND") (pinfunction "VSS")
    )
    (pad "48" smd roundrect (at 5.675 -3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VDDIO2")
    )
    (pad "49" smd roundrect (at 3.749999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/left/SWCLK") (pinfunction "PA14")
    )
    (pad "50" smd roundrect (at 3.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/left/USART2_RX") (pinfunction "PA15")
    )
    (pad "51" smd roundrect (at 2.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/left/USART4_TX") (pinfunction "PC10")
    )
    (pad "52" smd roundrect (at 2.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/left/USART4_RX") (pinfunction "PC11")
    )
    (pad "53" smd roundrect (at 1.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/left/SWCLK") (pinfunction "PC12")
    )
    (pad "54" smd roundrect (at 1.249999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U201-Pad54)") (pinfunction "PD2")
    )
    (pad "55" smd roundrect (at 0.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/left/P55") (pinfunction "PB3")
    )
    (pad "56" smd roundrect (at 0.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/left/P56") (pinfunction "PB4")
    )
    (pad "57" smd roundrect (at -0.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U201-Pad57)") (pinfunction "PB5")
    )
    (pad "58" smd roundrect (at -0.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/left/P58") (pinfunction "PB6")
    )
    (pad "59" smd roundrect (at -1.249999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/left/P59") (pinfunction "PB7")
    )
    (pad "60" smd roundrect (at -1.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/left/BOOT0") (pinfunction "BOOT0")
    )
    (pad "61" smd roundrect (at -2.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U201-Pad61)") (pinfunction "PB8")
    )
    (pad "62" smd roundrect (at -2.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/left/SPI2_~{CS}") (pinfunction "PB9")
    )
    (pad "63" smd roundrect (at -3.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND") (pinfunction "VSS")
    )
    (pad "64" smd roundrect (at -3.749999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3") (pinfunction "VDD")
    )
    (model "${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 160.858524 92.175854 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C301" (at -2.94554 0.507229 135 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/right/P17")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 176.9 81.1 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C203" (at -3.358757 1.308148 0) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_CK_RS282G05A3" (layer "F.Cu")
    (at 185.304094 108.899435 180)
    (descr "https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf")
    (tags "SPST button tactile switch")
    (property "Reference" "SW301" (at -7.43 0.12 0) (layer "F.SilkS") hide)
    (property "Value" "SW_Push" (at 0 3 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 -2.6 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.9 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "1")
    )
    (pad "2" smd rect (at 3.9 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/right/NRST") (pinfunction "2")
    )
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 174.25 79.5 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C204" (at 1.088944 3.959798 -135) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/left/P42")
    )
    (pad "2" smd roundrect (at 0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 117.1625 148.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C316" (at -0.1 3.6375 90) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo_12mm_SilkScreen" (layer "F.Cu")
    (at 121 97.6)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (property "Reference" "REF**" (at 0 -8.89 0) (layer "F.SilkS") hide)
    (property "Value" "KiCad-Logo_12mm_SilkScreen" (at 1.27 8.89 0) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 156.9 108.5 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C307" (at 2.870854 1.951615 180 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "/right/P42")
    )
    (pad "2" smd roundrect (at 0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 177.9 63.9 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C210" (at 4.012247 -0.141421 135) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/left/P17")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 191.1 105.2)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J304" (at 2.94 -0.14 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 80 "/right/SWCLK") (pinfunction "Pin_1")
    )
  )
  (footprint "Package_QFP:LQFP-64_10x10mm_P0.5mm" (layer "F.Cu")
    (at 162.7 102.3 -135)
    (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Reference" "U301" (at 0.219203 -9.340881 0) (layer "F.SilkS") hide)
    (property "Value" "STM32F072R8Tx" (at 0 7.4 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.675 -3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VBAT")
    )
    (pad "2" smd roundrect (at -5.675 -3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(U301-Pad2)") (pinfunction "PC13")
    )
    (pad "3" smd roundrect (at -5.675 -2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U301-Pad3)") (pinfunction "PC14")
    )
    (pad "4" smd roundrect (at -5.675 -2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(U301-Pad4)") (pinfunction "PC15")
    )
    (pad "5" smd roundrect (at -5.675 -1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "/right/LED_G") (pinfunction "PF0")
    )
    (pad "6" smd roundrect (at -5.675 -1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/right/LED_R") (pinfunction "PF1")
    )
    (pad "7" smd roundrect (at -5.675 -0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/right/NRST") (pinfunction "NRST")
    )
    (pad "8" smd roundrect (at -5.675 -0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(U301-Pad8)") (pinfunction "PC0")
    )
    (pad "9" smd roundrect (at -5.675 0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(U301-Pad9)") (pinfunction "PC1")
    )
    (pad "10" smd roundrect (at -5.675 0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/right/SPI2_CIPO") (pinfunction "PC2")
    )
    (pad "11" smd roundrect (at -5.675 1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/right/SPI2_COPI") (pinfunction "PC3")
    )
    (pad "12" smd roundrect (at -5.675 1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND") (pinfunction "VSSA")
    )
    (pad "13" smd roundrect (at -5.675 2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VDDA")
    )
    (pad "14" smd roundrect (at -5.675 2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "/right/P14") (pinfunction "PA0")
    )
    (pad "15" smd roundrect (at -5.675 3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/right/P15") (pinfunction "PA1")
    )
    (pad "16" smd roundrect (at -5.675 3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "/right/P16") (pinfunction "PA2")
    )
    (pad "17" smd roundrect (at -3.749999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/right/P17") (pinfunction "PA3")
    )
    (pad "18" smd roundrect (at -3.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND") (pinfunction "VSS")
    )
    (pad "19" smd roundrect (at -2.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VDD")
    )
    (pad "20" smd roundrect (at -2.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "/right/P20") (pinfunction "PA4")
    )
    (pad "21" smd roundrect (at -1.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "/right/P21") (pinfunction "PA5")
    )
    (pad "22" smd roundrect (at -1.249999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "/right/P22") (pinfunction "PA6")
    )
    (pad "23" smd roundrect (at -0.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "/right/P23") (pinfunction "PA7")
    )
    (pad "24" smd roundrect (at -0.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/right/USART3_TX") (pinfunction "PC4")
    )
    (pad "25" smd roundrect (at 0.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/right/P25") (pinfunction "PC5")
    )
    (pad "26" smd roundrect (at 0.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/right/P26") (pinfunction "PB0")
    )
    (pad "27" smd roundrect (at 1.249999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/right/P27") (pinfunction "PB1")
    )
    (pad "28" smd roundrect (at 1.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/right/P28") (pinfunction "PB2")
    )
    (pad "29" smd roundrect (at 2.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/right/SPI2_SCK") (pinfunction "PB10")
    )
    (pad "30" smd roundrect (at 2.75 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/right/P30") (pinfunction "PB11")
    )
    (pad "31" smd roundrect (at 3.25 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND") (pinfunction "VSS")
    )
    (pad "32" smd roundrect (at 3.749999 5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VDD")
    )
    (pad "33" smd roundrect (at 5.675 3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/right/P33") (pinfunction "PB12")
    )
    (pad "34" smd roundrect (at 5.675 3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "/right/P34") (pinfunction "PB13")
    )
    (pad "35" smd roundrect (at 5.675 2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/right/P35") (pinfunction "PB14")
    )
    (pad "36" smd roundrect (at 5.675 2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(U301-Pad36)") (pinfunction "PB15")
    )
    (pad "37" smd roundrect (at 5.675 1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(U301-Pad37)") (pinfunction "PC6")
    )
    (pad "38" smd roundrect (at 5.675 1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(U301-Pad38)") (pinfunction "PC7")
    )
    (pad "39" smd roundrect (at 5.675 0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(U301-Pad39)") (pinfunction "PC8")
    )
    (pad "40" smd roundrect (at 5.675 0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(U301-Pad40)") (pinfunction "PC9")
    )
    (pad "41" smd roundrect (at 5.675 -0.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(U301-Pad41)") (pinfunction "PA8")
    )
    (pad "42" smd roundrect (at 5.675 -0.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "/right/P42") (pinfunction "PA9")
    )
    (pad "43" smd roundrect (at 5.675 -1.249999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "/right/P43") (pinfunction "PA10")
    )
    (pad "44" smd roundrect (at 5.675 -1.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/right/D-") (pinfunction "PA11")
    )
    (pad "45" smd roundrect (at 5.675 -2.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/right/D+") (pinfunction "PA12")
    )
    (pad "46" smd roundrect (at 5.675 -2.75 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/right/SWDIO") (pinfunction "PA13")
    )
    (pad "47" smd roundrect (at 5.675 -3.25 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND") (pinfunction "VSS")
    )
    (pad "48" smd roundrect (at 5.675 -3.749999 225) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VDDIO2")
    )
    (pad "49" smd roundrect (at 3.749999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/right/SWCLK") (pinfunction "PA14")
    )
    (pad "50" smd roundrect (at 3.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "/right/USART2_RX") (pinfunction "PA15")
    )
    (pad "51" smd roundrect (at 2.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/right/USART4_TX") (pinfunction "PC10")
    )
    (pad "52" smd roundrect (at 2.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/right/USART4_RX") (pinfunction "PC11")
    )
    (pad "53" smd roundrect (at 1.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(U301-Pad53)") (pinfunction "PC12")
    )
    (pad "54" smd roundrect (at 1.249999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "/right/LED_B") (pinfunction "PD2")
    )
    (pad "55" smd roundrect (at 0.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/right/P55") (pinfunction "PB3")
    )
    (pad "56" smd roundrect (at 0.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "/right/P56") (pinfunction "PB4")
    )
    (pad "57" smd roundrect (at -0.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U301-Pad57)") (pinfunction "PB5")
    )
    (pad "58" smd roundrect (at -0.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "/right/P58") (pinfunction "PB6")
    )
    (pad "59" smd roundrect (at -1.249999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/right/P59") (pinfunction "PB7")
    )
    (pad "60" smd roundrect (at -1.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/right/BOOT0") (pinfunction "BOOT0")
    )
    (pad "61" smd roundrect (at -2.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/right/SD_DET") (pinfunction "PB8")
    )
    (pad "62" smd roundrect (at -2.75 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/right/SPI2_~{CS}") (pinfunction "PB9")
    )
    (pad "63" smd roundrect (at -3.25 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND") (pinfunction "VSS")
    )
    (pad "64" smd roundrect (at -3.749999 -5.675 225) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3") (pinfunction "VDD")
    )
    (model "${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 170.7 86.7 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C201" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 188.45 70.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J203" (at 2.65 0.45 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 61 "/left/+3V3") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 112.2 143)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R301" (at 5.2 0.7 180 unlocked) (layer "F.SilkS"))
    (property "Value" "5k1" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(J309-PadB5)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 189 105.2)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J303" (at 1.91 1.88 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 81 "/right/SWDIO") (pinfunction "Pin_1")
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 114.2625 148 -90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Reference" "U302" (at -2 -3.2375 180 unlocked) (layer "F.SilkS"))
    (property "Value" "TLV75533PDBV" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C317-Pad1)") (pinfunction "IN")
    )
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "3" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C317-Pad1)") (pinfunction "EN")
    )
    (pad "4" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(U302-Pad4)") (pinfunction "NC")
    )
    (pad "5" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/right/+3V3") (pinfunction "OUT")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_APFA3010_3x1.5mm_Horizontal" (layer "F.Cu")
    (at 177.05 104.17 -25)
    (descr "LED RGB, APFA3010, http://www.kingbrightusa.com/images/catalog/SPEC/APFA3010LSEEZGKQBKC.pdf")
    (tags "LED RGB APFA3010 KINGBRIGHT 3x1.5mm")
    (property "Reference" "D301" (at 0 1.8 155) (layer "F.SilkS") hide)
    (property "Value" "LED_RABG" (at 0 3 155) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -25 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -25 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -25 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 155) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 335) (size 1 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(D301-Pad1)") (pinfunction "RK")
    )
    (pad "2" smd rect (at 1.5 0 335) (size 1 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/right/+3V3") (pinfunction "A")
    )
    (pad "3" smd rect (at 0.4 0.45 335) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(D301-Pad3)") (pinfunction "BK")
    )
    (pad "4" smd rect (at -0.4 0.45 335) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(D301-Pad4)") (pinfunction "GK")
    )
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_Kingbright_APFA3010_3x1.5mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 173.500224 103.004626)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R303" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "50" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/right/LED_R")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(D301-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_Palconn_UTC16-G" (layer "F.Cu")
    (at 105.08 145.64)
    (descr "http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf")
    (tags "USB C Type-C Receptacle USB2.0")
    (property "Reference" "J309" (at 0.82 1.76 180 unlocked) (layer "F.SilkS"))
    (property "Value" "USB_C_Receptacle_USB2.0" (at 0 6.24 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "PCB Edge" (at 0 3.43 0) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 1.18 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 180) (size 0.6 0.6) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 180) (size 0.6 0.6) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "A1" smd rect (at -3.2 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "A4" smd rect (at -2.4 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/right/VBUS") (pinfunction "VBUS")
    )
    (pad "A5" smd rect (at -1.25 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(J309-PadA5)") (pinfunction "CC1")
    )
    (pad "A6" smd rect (at -0.25 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/right/D+") (pinfunction "D+")
    )
    (pad "A7" smd rect (at 0.25 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/right/D-") (pinfunction "D-")
    )
    (pad "A8" smd rect (at 1.25 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J309-PadA8)") (pinfunction "SBU1")
    )
    (pad "A9" smd rect (at 2.4 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/right/VBUS") (pinfunction "VBUS")
    )
    (pad "A12" smd rect (at 3.2 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "B1" smd rect (at 3.2 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "B4" smd rect (at 2.4 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/right/VBUS") (pinfunction "VBUS")
    )
    (pad "B5" smd rect (at 1.75 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "Net-(J309-PadB5)") (pinfunction "CC2")
    )
    (pad "B6" smd rect (at 0.75 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/right/D+") (pinfunction "D+")
    )
    (pad "B7" smd rect (at -0.75 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/right/D-") (pinfunction "D-")
    )
    (pad "B8" smd rect (at -1.75 -2.51 180) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(J309-PadB8)") (pinfunction "SBU2")
    )
    (pad "B9" smd rect (at -2.4 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/right/VBUS") (pinfunction "VBUS")
    )
    (pad "B12" smd rect (at -3.2 -2.51) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "S1" thru_hole oval (at -4.32 -1.93 90) (size 2 0.9) (drill oval 1.7 0.6) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at -4.32 2.24 90) (size 1.7 0.9) (drill oval 1.4 0.6) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at 4.32 -1.93 90) (size 2 0.9) (drill oval 1.7 0.6) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "S1" thru_hole oval (at 4.32 2.24 90) (size 1.7 0.9) (drill oval 1.4 0.6) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Palconn_UTC16-G.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 159.402913 93.602913 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C313" (at -3.828399 -11.045008 135 unlocked) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 156.6 96.4 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C305" (at -3.747666 -9.263099 135 unlocked) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/right/P25")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 153.2 99.8 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C312" (at 0 -1.65 135 unlocked) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 135) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 171.645923 73.241489 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C212" (at 3.27704 0.507287 45) (layer "F.SilkS"))
    (property "Value" "1µF" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 189.75 69)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J205" (at 2.85 0 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 8 "/left/GND") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 112.1625 145)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C317" (at 5.3375 -0.2 180 unlocked) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C317-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 106.7925 141.19)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R302" (at 3.1075 0.41 180 unlocked) (layer "F.SilkS"))
    (property "Value" "5k1" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(J309-PadA5)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169.700529 72.264549 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C209" (at -0.243259 1.629936 45) (layer "F.SilkS"))
    (property "Value" "10µF" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/left/+3V3")
    )
    (pad "2" smd roundrect (at 0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 170.7 102.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C314" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (property "Value" "1µF" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0805_2012Metric_Castellated" (layer "F.Cu")
    (at 111.3625 148 -90)
    (descr "Fuse SMD 0805 (2012 Metric), castellated end terminal, IPC_7351. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "fuse castellated")
    (property "Reference" "TH301" (at -0.1 -1.1375 90) (layer "F.SilkS"))
    (property "Value" "Thermistor_PTC" (at 0 1.6 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9625 0 270) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(C317-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9625 0 270) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 86 "/right/VBUS")
    )
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 188.05 68.5 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Reference" "J207" (at 1.6 2.05 180) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01_Male" (at 0 1.55 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 19 "/left/SD_DET") (pinfunction "Pin_1")
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 172.75 78 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C206" (at 1.096016 3.259762 45) (layer "F.SilkS"))
    (property "Value" "C_Small" (at 0 1.65 45) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -135 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/left/P35")
    )
    (pad "2" smd roundrect (at 0.937501 0 225) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/left/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (at 186.9 51.9 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Reference" "J212" (at 1.9 -0.7 -90) (layer "B.SilkS") hide)
    (property "Value" "Conn_01x02_Male" (at 0 -4.87 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 -1.27 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "/left/VBUS") (pinfunction "Pin_2")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Card:microSD_HC_Molex_104031-0811" (layer "B.Cu")
    (at 172.9 100.6 180)
    (descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
    (tags "microSD SD molex")
    (property "Reference" "J301" (at -6.92 8.2 180 unlocked) (layer "B.SilkS"))
    (property "Value" "Micro_SD_Card_Det" (at 0 -7.39 180) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -3.105 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "Net-(J301-Pad1)") (pinfunction "DAT2")
    )
    (pad "2" smd rect (at -2.005 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "/right/SPI2_~{CS}") (pinfunction "DAT3/CD")
    )
    (pad "3" smd rect (at -0.905 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "/right/SPI2_COPI") (pinfunction "CMD")
    )
    (pad "4" smd rect (at 0.195 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "/right/+3V3") (pinfunction "VDD")
    )
    (pad "5" smd rect (at 1.295 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "/right/SPI2_SCK") (pinfunction "CLK")
    )
    (pad "6" smd rect (at 2.395 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "VSS")
    )
    (pad "7" smd rect (at 3.495 5.45 180) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/right/SPI2_CIPO") (pinfunction "DAT0")
    )
    (pad "8" smd rect (at 4.545 5.45 180) (size 0.75 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(J301-Pad8)") (pinfunction "DAT1")
    )
    (pad "9" smd rect (at -5.74 -0.7 180) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "DET_B")
    )
    (pad "10" smd rect (at -5.74 -4.4 180) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "/right/SD_DET") (pinfunction "DET_A")
    )
    (pad "11" smd rect (at -5.565 5.325 180) (size 1.55 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "11" smd rect (at -2.24 -5.375 180) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "11" smd rect (at 3.73 -5.375 180) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (pad "11" smd rect (at 5.755 5.1 180) (size 1.17 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "SHIELD")
    )
    (model "${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Molex_104031-0811.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 148.1 96.9 135)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Reference" "J214" (at -0.070711 2.899138 -45) (layer "B.SilkS"))
    (property "Value" "Conn_01x04_Male" (at 0 -9.949999 -45) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 135 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 -3.81 -135) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 -2.54 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "/left/USART4_TX") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 -5.079999 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "/left/USART4_RX") (pinfunction "Pin_3")
    )
    (pad "4" thru_hole oval (at 0 -7.62 135) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/left/+3V3") (pinfunction "Pin_4")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left" (layer "B.Cu")
    (at 196.1 107.9)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (property "Reference" "J310" (at 0 6.14 180 unlocked) (layer "B.SilkS"))
    (property "Value" "Conn_01x04_Male" (at 0 -6.14 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.655 3.81) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "Pin_1")
    )
    (pad "2" smd rect (at 1.655 1.27) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "/right/USART3_TX") (pinfunction "Pin_2")
    )
    (pad "3" smd rect (at -1.655 -1.27) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "/right/USART2_RX") (pinfunction "Pin_3")
    )
    (pad "4" smd rect (at 1.655 -3.81) (size 2.51 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "/right/+3V3") (pinfunction "Pin_4")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 164.672189 99.205151 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C306" (at 3.984849 0.062189 90) (layer "B.SilkS"))
    (property "Value" "1µF" (at 0 -1.65 90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 161.2 112.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C302" (at -3.81 0.02 180 unlocked) (layer "B.SilkS"))
    (property "Value" "10µF" (at 0 -1.65 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "B.Cu")
    (at 186.4 98.4)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Reference" "J302" (at 0.1 -4.5 180 unlocked) (layer "B.SilkS"))
    (property "Value" "Conn_ARM_JTAG_SWD_10" (at 0 -4.235 180) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "/right/+3V3") (pinfunction "VTref")
    )
    (pad "2" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/right/SWDIO") (pinfunction "SWDIO/TMS")
    )
    (pad "3" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "4" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "/right/SWCLK") (pinfunction "SWDCLK/TCK")
    )
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "GND")
    )
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "Net-(J302-Pad6)") (pinfunction "SWO/TDO")
    )
    (pad "7" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "Net-(J302-Pad7)") (pinfunction "KEY")
    )
    (pad "8" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(J302-Pad8)") (pinfunction "NC/TDI")
    )
    (pad "9" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/right/GND") (pinfunction "GNDDetect")
    )
    (pad "10" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "/right/NRST") (pinfunction "~RESET~")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "B.Cu")
    (at 194 53.9)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Reference" "J208" (at 3.6 4.7 0) (layer "B.SilkS") hide)
    (property "Value" "Conn_ARM_JTAG_SWD_10" (at 0 -4.235 180) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "/left/+3V3") (pinfunction "VTref")
    )
    (pad "2" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/left/SWDIO") (pinfunction "SWDIO/TMS")
    )
    (pad "3" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "4" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/left/SWCLK") (pinfunction "SWDCLK/TCK")
    )
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/left/GND") (pinfunction "GND")
    )
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "Net-(J208-Pad6)") (pinfunction "SWO/TDO")
    )
    (pad "7" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(J208-Pad7)") (pinfunction "KEY")
    )
    (pad "8" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(J208-Pad8)") (pinfunction "NC/TDI")
    )
    (pad "9" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/left/GND") (pinfunction "GNDDetect")
    )
    (pad "10" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/left/NRST") (pinfunction "~RESET~")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 164.66708 95.756683 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C308" (at -0.153317 -1.67708 90) (layer "B.SilkS"))
    (property "Value" "10nF" (at 0 -1.65 90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 183.2 51.9 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Reference" "J213" (at 0.58 -9.92 0) (layer "B.SilkS") hide)
    (property "Value" "Conn_01x03_Male" (at 0 -7.41 -90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 -2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/left/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "/left/BOOT0") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/left/+3V3") (pinfunction "Pin_3")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 161.2 110.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C304" (at -3.77 -0.16 180 unlocked) (layer "B.SilkS"))
    (property "Value" "1µF" (at 0 -1.65 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/right/+3V3")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/right/GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (at 101.1 140.9 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Reference" "J306" (at -1.6 -0.4 180 unlocked) (layer "F.SilkS"))
    (property "Value" "Conn_01x02_Male" (at 0 -4.87 -90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 -1.27 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/right/GND") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 86 "/right/VBUS") (pinfunction "Pin_2")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "waad:L_borders" (layer "B.Cu")
    (at 149.88 73.26 180)
    (property "Reference" "J211" (at 0.5 40.5 0) (layer "B.SilkS") hide)
    (property "Value" "cap_pads" (at 0.5 34 0) (layer "B.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
  )
  (footprint "Button_Switch_SMD:SW_SPST_CK_RS282G05A3" (layer "B.Cu")
    (at 180.1 55.4 180)
    (descr "https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf")
    (tags "SPST button tactile switch")
    (property "Reference" "SW201" (at 6.1 1.6 0) (layer "B.SilkS") hide)
    (property "Value" "SW_Push" (at 0 -3 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 2.6 0) (layer "B.Fab"))
    (pad "1" smd rect (at -3.9 0 180) (size 1.5 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/left/GND") (pinfunction "1")
    )
    (pad "2" smd rect (at 3.9 0 180) (size 1.5 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/left/NRST") (pinfunction "2")
    )
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo_12mm_SilkScreen" (layer "B.Cu")
    (at 118.1 129.9)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (property "Reference" "REF**" (at 0 8.89 0) (layer "B.SilkS") hide)
    (property "Value" "KiCad-Logo_12mm_SilkScreen" (at 1.27 -8.89 0) (layer "B.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
  )
  (gr_line (start 159.88 89.72) (end 157.984953 91.614953)
    (layer "Edge.Cuts"))
  (gr_arc (start 140.407924 110.24785) (mid 140.284497 110.329094) (end 140.139999 110.359999)
    (layer "Edge.Cuts"))
  (gr_arc (start 141.4602 108.139808) (mid 141.990096 108.1501) (end 141.98 108.679999)
    (layer "Edge.Cuts"))
  (gr_line (start 100 150) (end 100 110.36)
    (layer "Edge.Cuts"))
  (gr_arc (start 158.51 92.149999) (mid 157.982465 92.142535) (end 157.984953 91.614953)
    (layer "Edge.Cuts"))
  (gr_line (start 99.998604 57.295318) (end 100 109.6)
    (layer "Edge.Cuts"))
  (gr_line (start 200 50) (end 150 50)
    (layer "Edge.Cuts"))
  (gr_line (start 111.4 109.6) (end 140 109.6)
    (layer "Edge.Cuts"))
  (gr_arc (start 200.001396 142.704682) (mid 175.265398 148.166566) (end 150 150)
    (layer "Edge.Cuts"))
  (gr_arc (start 99.998604 57.295318) (mid 124.734602 51.833434) (end 150 50)
    (layer "Edge.Cuts"))
  (gr_line (start 140 109.6) (end 141.4602 108.139808)
    (layer "Edge.Cuts"))
  (gr_line (start 145.6 104) (end 153.9 95.7)
    (layer "Edge.Cuts"))
  (gr_line (start 108.4 109.6) (end 100 109.6)
    (layer "Edge.Cuts"))
  (gr_line (start 200 90.36) (end 160.3 90.36)
    (layer "Edge.Cuts"))
  (gr_arc (start 153.9 95.7) (mid 154.429896 95.710292) (end 154.4198 96.240191)
    (layer "Edge.Cuts"))
  (gr_line (start 200.001396 142.704682) (end 200 90.36)
    (layer "Edge.Cuts"))
  (gr_arc (start 159.882239 89.722162) (mid 160.013691 89.631805) (end 160.17 89.6)
    (layer "Edge.Cuts"))
  (gr_line (start 200 50) (end 200 89.6)
    (layer "Edge.Cuts"))
  (gr_line (start 100 150) (end 150 150)
    (layer "Edge.Cuts"))
  (gr_line (start 141.98 108.68) (end 140.41 110.25)
    (layer "Edge.Cuts"))
  (gr_line (start 140.41 110.25) (end 140.407924 110.24785)
    (layer "Edge.Cuts"))
  (gr_line (start 154.4198 96.240191) (end 146.125047 104.535046)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.4 109.6) (mid 109.9 108.1) (end 111.4 109.6)
    (layer "Edge.Cuts"))
  (gr_line (start 159.882239 89.722162) (end 159.88 89.72)
    (layer "Edge.Cuts"))
  (gr_arc (start 146.125047 104.535046) (mid 145.597512 104.527582) (end 145.6 104)
    (layer "Edge.Cuts"))
  (gr_line (start 100 110.36) (end 140.14 110.36)
    (layer "Edge.Cuts"))
  (gr_line (start 160.3 90.36) (end 158.51 92.149999)
    (layer "Edge.Cuts"))
  (gr_line (start 200 89.6) (end 160.17 89.6)
    (layer "Edge.Cuts"))
  (gr_text "GND" (at 191 111.8 180) (layer "B.SilkS"))
  (gr_text "3.3V" (at 152.5 105.3 135) (layer "B.SilkS"))
  (gr_text "USART4_TX" (at 150.3 110.2 135) (layer "B.SilkS"))
  (gr_text "3.3V" (at 181 107.7 270) (layer "B.SilkS"))
  (gr_text "GND" (at 101.4 138.5 180) (layer "B.SilkS"))
  (gr_text "USART3_TX" (at 189.9 109.9 180) (layer "B.SilkS"))
  (gr_text "SWD" (at 193.84 58.61 0) (layer "B.SilkS"))
  (gr_text "10" (at 120.69 81.37 0) (layer "B.SilkS"))
  (gr_text "3" (at 177.12 69.29 0) (layer "B.SilkS"))
  (gr_text "GND" (at 146.9 110.7 135) (layer "B.SilkS"))
  (gr_text "6" (at 154.84 75.33 0) (layer "B.SilkS"))
  (gr_text "boot" (at 173.03 51.54 0) (layer "B.SilkS"))
  (gr_text "2" (at 184.59 84.86 0) (layer "B.SilkS"))
  (gr_text "NRST" (at 197.833333 95.45 180) (layer "B.SilkS"))
  (gr_text "GND" (at 147.17 95.49 315) (layer "B.SilkS"))
  (gr_text "https://gitlab.com/evils/waad" (at 132.4 143.6 180) (layer "B.SilkS"))
  (gr_text "SWDIO" (at 197.404762 101.25 180) (layer "B.SilkS"))
  (gr_text "3.3V" (at 192.9 104.2 180) (layer "B.SilkS"))
  (gr_text "SWD" (at 186.4 92.1 180) (layer "B.SilkS"))
  (gr_text "vbus" (at 186.849999 57.1705 0) (layer "B.SilkS"))
  (gr_text "14" (at 103.92 105.93 0) (layer "B.SilkS"))
  (gr_text "7" (at 135.57 63.82 0) (layer "B.SilkS"))
  (gr_text "13" (at 116.56 106.3 0) (layer "B.SilkS"))
  (gr_text "9" (at 117.29 68.89 0) (layer "B.SilkS"))
  (gr_text "4" (at 174.72 82.22 0) (layer "B.SilkS"))
  (gr_text "1" (at 190.26 73.48 0) (layer "B.SilkS"))
  (gr_text "GND" (at 192.695238 99.8375 180) (layer "B.SilkS"))
  (gr_text "NC" (at 198.690476 98.35 180) (layer "B.SilkS"))
  (gr_text "16" (at 129.02 106.41 0) (layer "B.SilkS"))
  (gr_text "3.3V" (at 140.84 101.41 315) (layer "B.SilkS"))
  (gr_text "USART4\nTX RX" (at 143.22 97.53 45) (layer "B.SilkS"))
  (gr_text "maybe half a stenographic keyboard?" (at 145.1 140.1 180) (layer "B.SilkS"))
  (gr_text "Vbus\n(3.6-5.5v)" (at 103.3 137.8 180) (layer "B.SilkS"))
  (gr_text "11" (at 105.33 71.72 0) (layer "B.SilkS"))
  (gr_text "NC" (at 193.195238 96.9125 180) (layer "B.SilkS"))
  (gr_text "5" (at 155.05 61.97 0) (layer "B.SilkS"))
  (gr_text "12" (at 108.37 82.73 0) (layer "B.SilkS"))
  (gr_text "RESET" (at 180.14 59.48 0) (layer "B.SilkS"))
  (gr_text "GND" (at 192.695238 95.45 180) (layer "B.SilkS"))
  (gr_text "USART2_RX" (at 189.8 108.2 180) (layer "B.SilkS"))
  (gr_text "GND" (at 192.695238 98.375 180) (layer "B.SilkS"))
  (gr_text "GND" (at 185.8 106.8 180) (layer "B.SilkS"))
  (gr_text "3.3V" (at 192.6 101.3 180) (layer "B.SilkS"))
  (gr_text "boot" (at 183.3 107.7 270) (layer "B.SilkS"))
  (gr_text "USART4_RX" (at 152.1 108.5 135) (layer "B.SilkS"))
  (gr_text "SWCLK" (at 197.261905 99.8 180) (layer "B.SilkS"))
  (gr_text "NC" (at 198.690476 96.9 180) (layer "B.SilkS"))
  (gr_text "8" (at 136.2 76.45 0) (layer "B.SilkS"))
  (gr_text "RESET" (at 177.1 109.3 180) (layer "F.SilkS"))
  (gr_text "GND" (at 165.39 86.78 0) (layer "F.SilkS"))
  (gr_text "9" (at 182.33 132.15 180) (layer "F.SilkS"))
  (gr_text "3" (at 122.67 130.71 180) (layer "F.SilkS"))
  (gr_text "2" (at 115.36 116.58 180) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 189.06 106.36 180) (layer "F.SilkS"))
  (gr_text "sd_det" (at 190.68 67.42 0) (layer "F.SilkS"))
  (gr_text "11" (at 194.01 128.96 180) (layer "F.SilkS"))
  (gr_text "1" (at 111.21 127.02 180) (layer "F.SilkS"))
  (gr_text "boot" (at 183.66 106.42 180) (layer "F.SilkS"))
  (gr_text "8" (at 164.06 123.06 180) (layer "F.SilkS"))
  (gr_text "5" (at 145.01 137.92 180) (layer "F.SilkS"))
  (gr_text "3.3V" (at 190.76 70.58 0) (layer "F.SilkS"))
  (gr_text "USART4" (at 149.7 108.2 225) (layer "F.SilkS"))
  (gr_text "GND" (at 191.99 69.03 0) (layer "F.SilkS"))
  (gr_text "R" (at 172.6 101.4 180) (layer "F.SilkS"))
  (gr_text "B" (at 175.71 107.26 180) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 197.38 69.73 0) (layer "F.SilkS"))
  (gr_text "spi2_cipo" (at 189.78 65.07 45) (layer "F.SilkS"))
  (gr_text "4" (at 125.34 120.7 180) (layer "F.SilkS"))
  (gr_text "7" (at 164.46 136.21 180) (layer "F.SilkS"))
  (gr_text "https://gitlab.com/evils/waad" (at 144.2 58.6 0) (layer "F.SilkS"))
  (gr_text "RX  TX" (at 148.8 107.2 225) (layer "F.SilkS"))
  (gr_text "3.3V" (at 179.33 84.35 0) (layer "F.SilkS"))
  (gr_text "10" (at 179.62 119.17 180) (layer "F.SilkS"))
  (gr_text "supposedly a stenographic keyboard" (at 151.8 63.1 0) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 194 105.1 180) (layer "F.SilkS"))
  (gr_text "status" (at 176.96 106.08 155) (layer "F.SilkS"))
  (gr_text "spi2_~{cs}" (at 191.54 77.35 0) (layer "F.SilkS"))
  (gr_text "15" (at 128.62 147.36 180) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 192.26 65.77 0) (layer "F.SilkS"))
  (gr_text "12" (at 193.52 117.59 180) (layer "F.SilkS"))
  (gr_text "copi" (at 191.28 62.14 45) (layer "F.SilkS"))
  (gr_text "G" (at 171.38 105.1 180) (layer "F.SilkS"))
  (gr_text "USART2_RX" (at 178.33 87.09 0) (layer "F.SilkS"))
  (gr_text "16" (at 171.41 94.08 180) (layer "F.SilkS"))
  (gr_text "14" (at 195.84 94.86 180) (layer "F.SilkS"))
  (gr_text "USART3_TX" (at 165.68 82.22 0) (layer "F.SilkS"))
  (gr_text "6" (at 145.14 125.11 180) (layer "F.SilkS"))
  (gr_text "13" (at 183.69 94.6 180) (layer "F.SilkS"))
  (zone (net 8) (net_name "/left/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer)
      (hatch_thickness 0.2) (hatch_gap 2) (hatch_orientation 45)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 200 89.6)
        (xy 160 89.6)
        (xy 140 109.6)
        (xy 100 109.6)
        (xy 100 49.9)
        (xy 200 49.9)
      )
    )
  )
  (zone (net 8) (net_name "/left/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.49 76.37)
        (xy 160.14 76.37)
        (xy 160.17 70.82)
        (xy 167.47 70.82)
      )
    )
  )
  (zone (net 64) (net_name "/right/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.2) (thermal_bridge_width 0.3)
      (hatch_thickness 0.2) (hatch_gap 0.4) (hatch_orientation 137.5)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 200 150)
        (xy 100 150)
        (xy 100 110.3)
        (xy 140.3 110.3)
        (xy 160.3 90.3)
        (xy 200 90.3)
      )
    )
  )
  (zone (net 8) (net_name "/left/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.71 73.47)
        (xy 180.26 81.92)
        (xy 171.78 73.57)
        (xy 180.26 65.06)
      )
    )
  )
  (zone (net 8) (net_name "/left/GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer)
      (hatch_thickness 0.2) (hatch_gap 0.4) (hatch_orientation 137.5)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 154.7 94.7)
        (xy 139.7 110)
        (xy 123 97.2)
        (xy 100.1 97.2)
        (xy 100.1 90.4)
        (xy 159 90.4)
      )
    )
  )
  (zone (net 36) (net_name "/left/P21") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.5 63.9)
        (xy 183.3 69.9)
        (xy 182.5 72.8)
        (xy 181.5 76.3)
        (xy 165.4 70.5)
        (xy 167.8 61.2)
      )
    )
  )
  (zone (net 35) (net_name "/left/P56") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.9 77.2)
        (xy 200.1 83.4)
        (xy 200.1 89.7)
        (xy 176.3 89.7)
        (xy 178.2 85.9)
        (xy 179.7 82.41)
        (xy 180.6 80.07)
        (xy 181.4 77.8)
        (xy 181.7 77)
        (xy 181.8 76.8)
      )
    )
  )
  (zone (net 37) (net_name "/left/P59") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.4 76.7)
        (xy 181.2 77.3)
        (xy 180.9 78.12)
        (xy 180.2 80.1)
        (xy 178.5 84.4)
        (xy 176.6 88.4)
        (xy 176 89.6)
        (xy 160.2 89.6)
        (xy 165.3 70.9)
      )
    )
  )
  (zone (net 64) (net_name "/right/GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.2) (thermal_bridge_width 0.3)
      (hatch_thickness 0.2) (hatch_gap 2) (hatch_orientation 45)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 200 150)
        (xy 100 150)
        (xy 100 110.3)
        (xy 140.3 110.3)
        (xy 160.3 90.3)
        (xy 200 90.3)
      )
    )
  )
  (zone (net 50) (net_name "/left/P33") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.7 109.6)
        (xy 100 109.6)
        (xy 100.01 97.5)
        (xy 109.7 97.5)
      )
    )
  )
  (zone (net 44) (net_name "/left/P30") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.7 90.1)
        (xy 113.8 90.1)
        (xy 114 89.3)
        (xy 114.42 86.88)
        (xy 114.82 83.57)
        (xy 114.93 81.19)
        (xy 113.26 79.94)
        (xy 112.04 78.31)
        (xy 111.36 76.64)
        (xy 127.46 72.4)
      )
    )
  )
  (zone (net 48) (net_name "/left/P43") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.85 109.7)
        (xy 123.1 109.7)
        (xy 123.1 97.7)
      )
    )
  )
  (zone (net 34) (net_name "/left/P58") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.9 66.4)
        (xy 199.9 83.01)
        (xy 181.8 76.5)
        (xy 184 68.4)
        (xy 184.8 64)
      )
    )
  )
  (zone (net 39) (net_name "/left/P16") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.7 67.3)
        (xy 127.7 72)
        (xy 125.8 56.5)
        (xy 136.13 55.32)
        (xy 145.7 54.9)
      )
    )
  )
  (zone (net 8) (net_name "/left/GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201 62.7)
        (xy 197 61.6)
        (xy 186.3 58.85)
        (xy 179.8 57.6)
        (xy 174.2 56.6)
        (xy 176.2 49.4)
        (xy 201 49.6)
      )
    )
  )
  (zone (net 49) (net_name "/left/P34") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.695 97.4875)
        (xy 122.7 109.6)
        (xy 110 109.6)
        (xy 110 97.5125)
      )
    )
  )
  (zone (net 47) (net_name "/left/P28") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.6 78.2)
        (xy 112.2 79.2)
        (xy 112.8 80)
        (xy 113.6 80.7)
        (xy 114.2 81.12)
        (xy 114.6 81.4)
        (xy 114.5 83.1)
        (xy 114.3 85.4)
        (xy 114.1 86.8)
        (xy 113.8 88.4)
        (xy 113.5 90.1)
        (xy 100.1 90.1)
        (xy 100.1 79.6)
        (xy 111 76.7)
      )
    )
  )
  (zone (net 45) (net_name "/left/P14") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.6 50.4)
        (xy 173.75 56.8)
        (xy 180.65 58)
        (xy 185.8 59.05)
        (xy 193.35 60.975)
        (xy 200.05 62.8)
        (xy 199.9 66.1)
        (xy 196.5 65.5)
        (xy 192.4 64.9)
        (xy 187.4 64.1)
        (xy 180 62.9)
        (xy 175.6 62.2)
        (xy 170.3 61.3)
        (xy 167.9 60.9)
        (xy 169.3 55.7)
        (xy 163.95 55.2)
        (xy 158.4 54.8)
        (xy 151.1 54.6)
        (xy 145.82 54.6)
        (xy 140.4 54.8)
        (xy 136.2 55.1)
        (xy 130.14 55.7)
        (xy 125.5 56.3)
        (xy 119.2 57.3)
        (xy 114.48 58.2)
        (xy 110.35 59.1)
        (xy 105.2 60.4)
        (xy 101.4 61.5)
        (xy 100.1 61.9)
        (xy 100 50)
      )
    )
  )
  (zone (net 33) (net_name "/left/P26") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.9 70.8)
        (xy 160.4 87.47)
        (xy 159.7 90.1)
        (xy 146 90.1)
        (xy 146.1 67.6)
      )
    )
  )
  (zone (net 46) (net_name "/left/P27") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.7 60.51)
        (xy 111.1 61.45)
        (xy 111.7 63)
        (xy 112.2 64.51)
        (xy 112.8 66.44)
        (xy 113.3 68.4)
        (xy 113.5 69.4)
        (xy 112.8 70.1)
        (xy 112.1 71)
        (xy 111.5 72.2)
        (xy 111 73.6)
        (xy 110.9 74.5)
        (xy 110.9 75.4)
        (xy 111 76.4)
        (xy 100.1 79.2)
        (xy 100.1 62.2)
        (xy 104.74 60.9)
        (xy 110.3 59.5)
      )
    )
  )
  (zone (net 40) (net_name "/left/P23") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.7 90.1)
        (xy 130 90.1)
        (xy 127.8 72.3)
        (xy 145.7 67.6)
      )
    )
  )
  (zone (net 38) (net_name "/left/P15") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.06 55.3)
        (xy 168.9 56)
        (xy 165 70.4)
        (xy 146 67.3)
        (xy 146 54.9)
        (xy 154.9 55)
      )
    )
  )
  (zone (net 41) (net_name "/left/P22") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.4 72.1)
        (xy 111.3 76.3)
        (xy 111.2 75.3)
        (xy 111.2 74.2)
        (xy 111.5 72.9)
        (xy 112.1 71.6)
        (xy 112.9 70.5)
        (xy 113.9 69.5)
        (xy 113.1 66.21)
        (xy 112.1 63.1)
        (xy 110.6 59.4)
        (xy 114.7 58.5)
        (xy 120.3 57.4)
        (xy 125.5 56.6)
      )
    )
  )
)
