(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power "GND")
    (2 "In2.Cu" power "PWR")
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.2) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.0175))
      (layer "dielectric 2" (type "core") (thickness 1.065) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.0175))
      (layer "dielectric 3" (type "prepreg") (thickness 0.2) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 152.4 101.6)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/JLCPCB/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/3V3")
  (net 3 "/NRESET")
  (net 4 "/TSG4CAP")
  (net 5 "/TSG1CAP")
  (net 6 "/TSG7CAP")
  (net 7 "/5V")
  (net 8 "/Supply/VIN")
  (net 9 "Net-(C21-Pad1)")
  (net 10 "Net-(C22-Pad1)")
  (net 11 "/Supply/VBAT+")
  (net 12 "Net-(C26-Pad1)")
  (net 13 "Net-(C29-Pad1)")
  (net 14 "Net-(C28-Pad1)")
  (net 15 "Net-(D1-Pad2)")
  (net 16 "Net-(D2-Pad2)")
  (net 17 "Net-(D3-Pad2)")
  (net 18 "Net-(D4-Pad2)")
  (net 19 "/Supply/NSTDBY")
  (net 20 "Net-(D5-Pad2)")
  (net 21 "/NCHRG")
  (net 22 "/SCL")
  (net 23 "/SDA")
  (net 24 "Net-(P1-Pad3)")
  (net 25 "Net-(P1-Pad2)")
  (net 26 "/SWO")
  (net 27 "/SWCLK")
  (net 28 "/SWDIO")
  (net 29 "/DACOUT")
  (net 30 "/Supply/VUSB")
  (net 31 "/TSG1LEFT")
  (net 32 "/4.096V")
  (net 33 "Net-(P8-Pad1)")
  (net 34 "/DACOUTB")
  (net 35 "GNDA")
  (net 36 "Net-(C30-Pad2)")
  (net 37 "Net-(C30-Pad1)")
  (net 38 "/-5V")
  (net 39 "Net-(C31-Pad1)")
  (net 40 "/Supply/VCHRG")
  (net 41 "Net-(R6-Pad2)")
  (net 42 "Net-(R9-Pad1)")
  (net 43 "Net-(R10-Pad1)")
  (net 44 "Net-(R11-Pad2)")
  (net 45 "/TSG4MEM")
  (net 46 "/TSG1DOWN")
  (net 47 "/TSG7SET")
  (net 48 "/TSG7UP")
  (net 49 "/TSG7RIGHT")
  (net 50 "/TSG1ON")
  (net 51 "Net-(D6-Pad2)")
  (net 52 "/VBAT")
  (net 53 "Net-(D7-Pad2)")
  (net 54 "Net-(D8-Pad2)")
  (net 55 "Net-(RL1-Pad9)")
  (net 56 "/5VFILT")
  (net 57 "/OUTON")
  (net 58 "/OUTOFF")
  (net 59 "/VOUT")
  (net 60 "/ATTON")
  (net 61 "/ATTOFF")
  (net 62 "Net-(P1-Pad1)")
  (net 63 "/Supply/6V")
  (net 64 "/USBRX")
  (net 65 "/USBTX")
  (net 66 "Net-(P4-Pad3)")
  (net 67 "Net-(P4-Pad2)")
  (net 68 "Net-(P4-Pad1)")
  (net 69 "Net-(P5-Pad1)")
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -35.052 0.646 -90)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C29" (at 3.556 0 90) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C29-Pad1)")
    )
    (pad "2" smd rect (at 0.9 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X125" (layer "F.Cu")
    (at -38.1635 4.2655)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C31" (at -3.0425 0.381 0) (layer "F.SilkS"))
    (property "Value" "4.7µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(C31-Pad1)")
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x127.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at 42.1005 -3.81)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R3" (at 0 -1.651 0) (layer "F.SilkS"))
    (property "Value" "4.7K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/SDA")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -4.064 -12.5095)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C6" (at -0.762 1.7145 0) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -30.734 22.7965 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R11" (at -2.3495 0 90) (layer "F.SilkS"))
    (property "Value" "47K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Supply/6V")
    )
    (pad "2" smd rect (at 1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -35.052 -3.164 -90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R14" (at -2.3605 0 180) (layer "F.SilkS"))
    (property "Value" "0E" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 270) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 1 0 270) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C29-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbols:KiCad-Logo2_6mm_SilkScreen" locked (layer "F.Cu")
    (at 35.3 -27.9)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (property "Reference" "REF***" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Value" "KiCad-Logo2_6mm_SilkScreen" (at 0.75 0 0) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -12.903 -28.5085 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C5" (at 3.109 0 0) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -13.42775 14.331171 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C11" (at -2.54 0 180) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -0.1245 19.479671 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C16" (at 3.109 0 90) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -6.9215 -6.35)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R1" (at 0 1.651 0) (layer "F.SilkS"))
    (property "Value" "33K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/Supply/VBAT+")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/VBAT")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at 9.0805 22.385671 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R6" (at 2.3495 0 180) (layer "F.SilkS"))
    (property "Value" "99K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DACOUTB")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R6-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -44.45 -5.45338 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R15" (at -2.413 -0.0385 180) (layer "F.SilkS"))
    (property "Value" "3.9K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D4-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:L0805" (layer "F.Cu")
    (at -17.22628 23.592171 180)
    (descr "RESISTOR")
    (tags "RESISTOR")
    (property "Reference" "L1" (at -0.03175 -2.286 180) (layer "F.SilkS"))
    (property "Value" "FB0805" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA")
    )
    (pad "2" smd rect (at 0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LEDs:LED_0805" (layer "F.Cu")
    (at -44.45 -9.92378 -90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (property "Reference" "D4" (at -2.54 0 180) (layer "F.SilkS"))
    (property "Value" "LED0805-G" (at 0 1.75 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/Supply/NSTDBY") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D4-Pad2)") (pinfunction "A")
    )
    (model "LEDs.3dshapes/LED_0805.wrl"
      (offset (xyz -0.199999997 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors:USB_Mini-B" (layer "F.Cu")
    (at -34.925 -28.0035 -90)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (property "Reference" "P8" (at 0.5715 -4.826 90) (layer "F.SilkS"))
    (property "Value" "USB_B" (at -0.5 0 180) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "" np_thru_hole circle (at 0.8509 -2.19964 270) (size 0.89916 0.89916) (drill 0.89916) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0.8509 2.19964 270) (size 0.89916 0.89916) (drill 0.89916) (layers "*.Cu" "*.Mask"))
    (pad "1" smd rect (at 3.44932 -1.6002 270) (size 2.30124 0.50038) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(P8-Pad1)") (pinfunction "VBUS")
    )
    (pad "2" smd rect (at 3.44932 -0.8001 270) (size 2.30124 0.50038) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "D-")
    )
    (pad "3" smd rect (at 3.44932 0 270) (size 2.30124 0.50038) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "D+")
    )
    (pad "4" smd rect (at 3.44932 0.8001 270) (size 2.30124 0.50038) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "ID")
    )
    (pad "5" smd rect (at 3.44932 1.6002 270) (size 2.30124 0.50038) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "6" smd rect (at -2.14884 -4.45008 270) (size 2.49936 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "shield")
    )
    (pad "6" smd rect (at -2.14884 4.45008 270) (size 2.49936 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "shield")
    )
    (pad "6" smd rect (at 3.35026 -4.45008 270) (size 2.49936 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "shield")
    )
    (pad "6" smd rect (at 3.35026 4.45008 270) (size 2.49936 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "shield")
    )
    (model "${KISYS3DMOD}/Connectors.3dshapes/USBmini_SMD.wrl"
      (offset (xyz -5.1 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm_PowerPAD" (layer "F.Cu")
    (at -43.434 -18.8595 180)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "U6" (at 0 -3.6195 0) (layer "F.SilkS"))
    (property "Value" "TP4056" (at 0 3.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "TEMP")
    )
    (pad "2" smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(R10-Pad1)") (pinfunction "PROG")
    )
    (pad "3" smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "4" smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/Supply/VUSB") (pinfunction "VCC")
    )
    (pad "5" smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Supply/VCHRG") (pinfunction "BAT")
    )
    (pad "6" smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/Supply/NSTDBY") (pinfunction "~STDBY")
    )
    (pad "7" smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/NCHRG") (pinfunction "~CHRG")
    )
    (pad "8" smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/Supply/VUSB") (pinfunction "CE")
    )
    (pad "9" smd rect (at 0 0 180) (size 2.4 3.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (model "Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at 33.528 12.56475 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D8" (at -3.3655 0 90) (layer "F.SilkS"))
    (property "Value" "1N4148WS" (at 0 -1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(D8-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relais_SMD:EE2-xTNUH" (layer "F.Cu")
    (at 36.1315 22.1615 90)
    (property "Reference" "RL2" (at -8.3 0 0) (layer "F.SilkS"))
    (property "Value" "EE2-3TNUH" (at 0 -0.4064 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd rect (at -6.35 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "3" smd rect (at -1.27 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at 1.27 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at 3.81 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 6.35 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "7" smd rect (at 6.35 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(D8-Pad2)")
    )
    (pad "8" smd rect (at 3.81 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(RL1-Pad9)")
    )
    (pad "9" smd rect (at 1.27 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/VOUT")
    )
    (pad "10" smd rect (at -1.27 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "12" smd rect (at -6.35 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(D7-Pad2)")
    )
    (model "${KISYS3DMOD}/Relays_SMD/EE2-xNUH.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Buttons_Switches_THT:SK12D07G8" (layer "F.Cu")
    (at -37.1475 29.718 180)
    (property "Reference" "SW1" (at -6.6167 0 0) (layer "F.SilkS"))
    (property "Value" "SK12D07-G8" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2 0 180) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "/Supply/VIN") (pinfunction "A")
    )
    (pad "2" thru_hole circle (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "/Supply/VBAT+") (pinfunction "B")
    )
    (pad "3" thru_hole circle (at 2 0 180) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (pinfunction "C")
    )
    (pad "Case" thru_hole circle (at -4.1 0 180) (size 2 2) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Case")
    )
    (pad "Case" thru_hole circle (at 4.1 0 180) (size 2 2) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Case")
    )
    (model "E:/Repository_local/KiCad/3Dmodels/Buttons_Switches_ThroughHole.3dshapes/SS12D07.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -40.8432 20.1168 -90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C22" (at -2.4765 -0.0635 180) (layer "F.SilkS"))
    (property "Value" "2.7N" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C22-Pad1)") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_TO_SOT_SMD:SOT89-3_Housing" (layer "F.Cu")
    (at -31.369 1.5985 180)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (property "Reference" "U8" (at 0 -3.4815 0) (layer "F.SilkS"))
    (property "Value" "HT7850" (at 0.45 3.25 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.50114 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND/ADJ")
    )
    (pad "2" smd rect (at 0 -1.09982 180) (size 1.99898 2.99974) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0 0.762 180) (size 1.00076 1.00076) (layers "F.Cu")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "3" smd rect (at 1.50114 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C29-Pad1)") (pinfunction "VO")
    )
    (model "${KISYS3DMOD}/Housings_TO_SOT.3dshapes/SOT89-3_Housing.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -17.0815 -16.1925 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C9" (at 3.109 0 0) (layer "F.SilkS"))
    (property "Value" "15N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/TSG1CAP") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X125" (layer "F.Cu")
    (at 43.2435 16.764 -90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C10" (at -2.413 0 180) (layer "F.SilkS"))
    (property "Value" "10µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "2" smd rect (at 0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x127.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at 14.605 27.051 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D1" (at -3.175 0 0) (layer "F.SilkS"))
    (property "Value" "1N4148WS" (at 0 -1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D1-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors_JST:JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled" locked (layer "F.Cu")
    (at -45.1485 8.255)
    (descr "http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (property "Reference" "P10" (at -1.5 -6 0) (layer "F.SilkS"))
    (property "Value" "JSTPHMHS-2" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "" smd rect locked (at -3.4 2.775) (size 1.6 3.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at 3.4 2.775) (size 1.6 3.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "1" smd rect locked (at -1 -2.775) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/Supply/VBAT+") (pinfunction "P1")
    )
    (pad "2" smd rect locked (at 1 -2.775) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "P2")
    )
    (model "${KISYS3DMOD}/Conn_JST.3dshapes/JST-XH-S2B-XH-SM4-TB-No-Support.stp"
      (offset (xyz 0 4 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X125" (layer "F.Cu")
    (at -45.212 -22.86)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C24" (at -2.4765 0 90) (layer "F.SilkS"))
    (property "Value" "10µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Supply/VCHRG")
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x127.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -39.497 15.3035 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C21" (at -0.4318 1.6891 180) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C21-Pad1)") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -30.607 17.8435 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C25" (at -2.413 0 -90) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Supply/6V")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -2.1465 23.646671 -90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C18" (at 0.7075 -1.7909 90) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at 16.512593 -27.051 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C4" (at 3.109 0 90) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/NRESET") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -30.607 20.3835 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C23" (at -2.413 0 -90) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Supply/6V")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -32.026 -13.7519 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C26" (at -2.9955 0.0635 180) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -1.727 -15.6815)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C8" (at -0.94 1.648 0) (layer "F.SilkS"))
    (property "Value" "15N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/TSG7CAP") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors_JST:JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled" (layer "F.Cu")
    (at 35.2 -18.3 90)
    (descr "http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (property "Reference" "P3" (at 3.2385 -4.2545 -90) (layer "F.SilkS"))
    (property "Value" "JSTPHMHS-2" (at 0 6 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "" smd rect (at -3.4 2.775 90) (size 1.6 3.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "" smd rect (at 3.4 2.775 90) (size 1.6 3.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "1" smd rect (at -1 -2.775 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (pinfunction "P1")
    )
    (pad "2" smd rect (at 1 -2.775 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/VOUT") (pinfunction "P2")
    )
    (model "${KISYS3DMOD}/Conn_JST.3dshapes/JST-XH-S2B-XH-SM4-TB-No-Support.stp"
      (offset (xyz 0 4 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Inductors_SMD:L0805" (layer "F.Cu")
    (at -1.27 26.924 180)
    (descr "RESISTOR")
    (tags "RESISTOR")
    (property "Reference" "L5" (at 0 1.7145 180) (layer "F.SilkS"))
    (property "Value" "FB0805" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_TO_SOT_SMD:SC-70-5" (layer "F.Cu")
    (at -5.0165 23.630671 180)
    (descr "SC70-5 SOT323-5")
    (property "Reference" "U4" (at 0 -2.3 0) (layer "F.SilkS"))
    (property "Value" "OPA333AIDCKR" (at 0 2.3 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.6604 1.016 180) (size 0.4064 0.6604) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/DACOUT") (pinfunction "+")
    )
    (pad "2" smd rect (at 0 1.016 180) (size 0.4064 0.6604) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (pinfunction "V-")
    )
    (pad "3" smd rect (at 0.6604 1.016 180) (size 0.4064 0.6604) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DACOUTB") (pinfunction "-")
    )
    (pad "4" smd rect (at 0.6604 -1.016 180) (size 0.4064 0.6604) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DACOUTB")
    )
    (pad "5" smd rect (at -0.6604 -1.016 180) (size 0.4064 0.6604) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (pinfunction "V+")
    )
    (model "${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.85 0.7 0.5))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -34.7781 -8.2909 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R13" (at 0.4318 -1.5748 -90) (layer "F.SilkS"))
    (property "Value" "0E" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C28-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at 29.21 27.051 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D7" (at -3.175 0 0) (layer "F.SilkS"))
    (property "Value" "1N4148WS" (at 0 -1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(D7-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LEDs:LED_0805" (layer "F.Cu")
    (at -42.0116 -9.97458 -90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (property "Reference" "D5" (at -2.54 0 180) (layer "F.SilkS"))
    (property "Value" "LED0805-Y" (at 0 1.75 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/NCHRG") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D5-Pad2)") (pinfunction "A")
    )
    (model "LEDs.3dshapes/LED_0805.wrl"
      (offset (xyz -0.199999997 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -42.0116 -5.50418 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R16" (at -2.413 -0.0385 180) (layer "F.SilkS"))
    (property "Value" "3.9K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D5-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -2.4255 -23.368 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C3" (at 3.109 0 90) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -35.6345 -11.4659 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C28" (at -0.381 1.7145 0) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C28-Pad1)")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -42.1132 -0.7112)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C32" (at -3.0988 -0.0508 0) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/-5V") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:L0805" (layer "F.Cu")
    (at -42.164 1.9304 180)
    (descr "RESISTOR")
    (tags "RESISTOR")
    (property "Reference" "L4" (at -2.3876 0 0) (layer "F.SilkS"))
    (property "Value" "FB0805" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(C31-Pad1)")
    )
    (pad "2" smd rect (at 0.89916 0 180) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/-5V")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC6332X65" (layer "F.Cu")
    (at -34.9885 -20.7645)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (property "Reference" "R8" (at 4.801 0.0253 90) (layer "F.SilkS"))
    (property "Value" "0.2E" (at 0 3.1 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -3.1 0) (size 1 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/Supply/VUSB")
    )
    (pad "2" smd rect (at 3.1 0) (size 1 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(P8-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512_6332Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at -23.2664 -16.7132)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D6" (at 0 1.75 180) (layer "F.SilkS"))
    (property "Value" "BAT54WS" (at 0 -1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/NCHRG") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(D6-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at 38.862 -6.5405 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C13" (at 0.6985 1.651 0) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESCAXE80P160X320X70-8" (layer "F.Cu")
    (at -14.4145 -11.684 -90)
    (descr "Resistor,Chip Array,0.80mm pitch;8 pin,1.60mm L X 3.20mm W X 0.70mm H")
    (property "Reference" "RN2" (at 2.4384 0 0) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (clearance 0.1524)
    (attr smd)
    (pad "1" smd rect (at -0.9 -1.2 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/TSG1DOWN") (pinfunction "R1.1")
    )
    (pad "2" smd rect (at -0.9 -0.4 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/TSG1LEFT") (pinfunction "R2.1")
    )
    (pad "3" smd rect (at -0.9 0.4 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/TSG1ON") (pinfunction "R3.1")
    )
    (pad "4" smd rect (at -0.9 1.2 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/TSG4MEM") (pinfunction "R4.1")
    )
    (pad "5" smd rect (at 0.9 1.2 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(P5-Pad1)") (pinfunction "R4.2")
    )
    (pad "6" smd rect (at 0.9 0.4 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(P4-Pad3)") (pinfunction "R3.2")
    )
    (pad "7" smd rect (at 0.9 -0.4 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(P4-Pad2)") (pinfunction "R2.2")
    )
    (pad "8" smd rect (at 0.9 -1.2 270) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(P4-Pad1)") (pinfunction "R1.2")
    )
    (model "E:/Repository_local/KiCad/packages3d/Resistors_SMD.3dshapes/RESCAVE80P160X160X60-4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23" (layer "F.Cu")
    (at 27.110645 7.740645 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q1" (at -2.6035 0.0025 180) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.15 -0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/ATTON") (pinfunction "G")
    )
    (pad "2" smd rect (at -1.15 0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S")
    )
    (pad "3" smd rect (at 1.15 0 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D1-Pad2)") (pinfunction "D")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm" (layer "F.Cu")
    (at -35.306 18.2245 90)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (property "Reference" "U5" (at -0.7747 2.3368 90) (layer "F.SilkS"))
    (property "Value" "TPS61085" (at 0 2.55 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (clearance 0.1524)
    (attr smd)
    (pad "1" smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(R9-Pad1)") (pinfunction "COMP")
    )
    (pad "2" smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R11-Pad2)") (pinfunction "FB")
    )
    (pad "3" smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Supply/VIN") (pinfunction "EN")
    )
    (pad "4" smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "5" smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D3-Pad2)") (pinfunction "SW")
    )
    (pad "6" smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Supply/VIN") (pinfunction "IN")
    )
    (pad "7" smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Supply/VIN") (pinfunction "FREQ")
    )
    (pad "8" smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C21-Pad1)") (pinfunction "SS")
    )
    (model "${KISYS3DMOD}/Housings_SSOP_TSSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at -38.117 0.8285 90)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Reference" "U9" (at -0.77 -2.3905 90) (layer "F.SilkS"))
    (property "Value" "LM2776" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(C31-Pad1)") (pinfunction "Vout")
    )
    (pad "2" smd rect (at -1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd")
    )
    (pad "3" smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C29-Pad1)") (pinfunction "Vin")
    )
    (pad "4" smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C29-Pad1)") (pinfunction "EN")
    )
    (pad "5" smd rect (at 1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C30-Pad1)") (pinfunction "C1+")
    )
    (pad "6" smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(C30-Pad2)") (pinfunction "C1-")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors_Samtec:SAMTEC-FTSH-107-01-X-DV" (layer "F.Cu")
    (at 22.481593 -23.5585 90)
    (descr "translated Allegro footprint")
    (property "Reference" "P2" (at 0 5.1 90) (layer "F.SilkS"))
    (property "Value" "MA07-2S-1.27" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "1" (at -5 1 90) (layer "F.SilkS"))
    (fp_text user "1" (at -5 1 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -3.175 0 90) (size 0.7 0.7) (drill 0.7) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 3.175 0 90) (size 0.7 0.7) (drill 0.7) (layers "*.Cu" "*.Mask"))
    (pad "1" smd rect (at -3.81 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste"))
    (pad "2" smd rect (at -3.81 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste"))
    (pad "3" smd rect (at -2.54 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 2 "/3V3") (pinfunction "T_VCC")
    )
    (pad "4" smd rect (at -2.54 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 28 "/SWDIO") (pinfunction "T_JMTS/T_SWDIO")
    )
    (pad "5" smd rect (at -1.27 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "6" smd rect (at -1.27 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 27 "/SWCLK") (pinfunction "T_JCLK/T_SWCLK")
    )
    (pad "7" smd rect (at 0 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "8" smd rect (at 0 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 26 "/SWO") (pinfunction "T_JTDO/T_SWO")
    )
    (pad "9" smd rect (at 1.27 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (pinfunction "T_JCLK")
    )
    (pad "10" smd rect (at 1.27 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (pinfunction "T_JTDI")
    )
    (pad "11" smd rect (at 2.54 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 1 "GND") (pinfunction "GNDdet")
    )
    (pad "12" smd rect (at 2.54 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 3 "/NRESET") (pinfunction "T_NRST")
    )
    (pad "13" smd rect (at 3.81 2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 64 "/USBRX") (pinfunction "T_VCP_RX")
    )
    (pad "14" smd rect (at 3.81 -2.032 90) (size 0.74 2.79) (layers "F.Cu" "F.Paste")
      (net 65 "/USBTX") (pinfunction "T_VCP_TX")
    )
    (model "${KISYS3DMOD}/Conn_Samtec.3dshapes/FTSH-107-01-L-DV-TR.stp"
      (offset (xyz 0 0 0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -31.9405 -2.7305 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C27" (at -2.4765 0 -90) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC3216X125" (layer "F.Cu")
    (at -36.5252 24.2824 180)
    (descr "Capacitor,non-polarized,Chip;3.20mm L X 1.60mm W X 1.25mm H")
    (property "Reference" "C19" (at 0.0508 -1.9304 0) (layer "F.SilkS"))
    (property "Value" "10µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.5 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Supply/VIN")
    )
    (pad "2" smd rect (at 1.5 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC3216x190.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:L0805" (layer "F.Cu")
    (at -27.686 3.556 90)
    (descr "RESISTOR")
    (tags "RESISTOR")
    (property "Reference" "L3" (at 2.2225 0 -90) (layer "F.SilkS"))
    (property "Value" "FB0805" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.89916 0 90) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Supply/6V")
    )
    (pad "2" smd rect (at 0.89916 0 90) (size 0.79756 1.59766) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at 15.494 14.2875 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D2" (at -3.2385 0 0) (layer "F.SilkS"))
    (property "Value" "1N4148WS" (at 0 -1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0 270) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D2-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at -46 28)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH1" (at 0 -3.35 0) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.9) (clearance 1.9)
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X125" (layer "F.Cu")
    (at 28.702 14.7295 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C15" (at -2.5425 0.0635 0) (layer "F.SilkS"))
    (property "Value" "10µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x127.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at 5.9055 21.369671 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R7" (at 0 1.7145 0) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R6-Pad2)")
    )
    (pad "2" smd rect (at 1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 35.1155 -2.032)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC1" (at 0 3.4925 0) (layer "F.SilkS"))
    (property "Value" "24C01" (at 0 3.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A0")
    )
    (pad "2" smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A1")
    )
    (pad "3" smd rect (at -2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A2")
    )
    (pad "4" smd rect (at -2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "5" smd rect (at 2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/SDA") (pinfunction "SDA")
    )
    (pad "6" smd rect (at 2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/SCL") (pinfunction "SCL")
    )
    (pad "7" smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "WP")
    )
    (pad "8" smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -48.133 -9.652 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R17" (at -2.413 -0.0385 180) (layer "F.SilkS"))
    (property "Value" "0E" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/Supply/VBAT+")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Supply/VCHRG")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23" (layer "F.Cu")
    (at 32.131 7.747 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q4" (at -2.54 0.0025 180) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.15 -0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/OUTOFF") (pinfunction "G")
    )
    (pad "2" smd rect (at -1.15 0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S")
    )
    (pad "3" smd rect (at 1.15 0 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(D8-Pad2)") (pinfunction "D")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -1.727 -18.92)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C2" (at -0.3175 -1.5875 0) (layer "F.SilkS"))
    (property "Value" "15N" (at 0.381 0.254 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/TSG4CAP") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X95" (layer "F.Cu")
    (at -38.1635 -2.5925 180)
    (descr "Capacitor,non-polarized,Chip;2.00mm L X 1.25mm W X 1.35mm H")
    (property "Reference" "C30" (at 0 1.5985 0) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C30-Pad1)")
    )
    (pad "2" smd rect (at 0.9 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(C30-Pad2)")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at -10.31625 14.328671 -90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Reference" "U2" (at 2.606 0 180) (layer "F.SilkS"))
    (property "Value" "LM4132AMF-4.1" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (pinfunction "Gnd")
    )
    (pad "3" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (pinfunction "EN")
    )
    (pad "4" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (pinfunction "Vin")
    )
    (pad "5" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/4.096V") (pinfunction "Vref")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SOD-323" (layer "F.Cu")
    (at -31.115 15.3035 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Reference" "D3" (at -2.5654 1.7399 180) (layer "F.SilkS"))
    (property "Value" "PMEG2010A" (at 0 -1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.35 0 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Supply/6V") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.35 0 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D3-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.STEP"
      (offset (xyz 0 -0.65 0))
      (scale (xyz 1.1 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:CDRH6D28" (layer "F.Cu")
    (at -33.6428 9.8425 90)
    (property "Reference" "L2" (at -0.381 -4.953 90) (layer "F.SilkS"))
    (property "Value" "3.3µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd rect (at 0 -2.35 90) (size 7.3 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Supply/VIN")
    )
    (pad "2" smd rect (at 0 2.35 90) (size 7.3 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D3-Pad2)")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_SMD_CDRH127.STEP"
      (offset (xyz -3.5 3.5 0))
      (scale (xyz 0.6 0.5 0.6))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Housings_SSOP:SOP65P490X110-8N-8µMax" (layer "F.Cu")
    (at -4.693 19.139671)
    (property "Reference" "U3" (at 0.205 -2.362 0) (layer "F.SilkS"))
    (property "Value" "MAX5217GUA+" (at 0 2.45 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (clearance 0.1524)
    (attr through_hole)
    (pad "1" smd rect (at -2.165 -0.975) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/4.096V") (pinfunction "REF")
    )
    (pad "2" smd rect (at -2.165 -0.325) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "ADDR")
    )
    (pad "3" smd rect (at -2.165 0.325) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/SCL") (pinfunction "SCL")
    )
    (pad "4" smd rect (at -2.165 0.975) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/SDA") (pinfunction "SDA")
    )
    (pad "5" smd rect (at 2.165 0.975) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (pinfunction "~AUX")
    )
    (pad "6" smd rect (at 2.165 0.325) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/DACOUT") (pinfunction "OUT")
    )
    (pad "7" smd rect (at 2.165 -0.325) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/5VFILT") (pinfunction "VDD")
    )
    (pad "8" smd rect (at 2.165 -0.975) (size 1.42 0.47) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (pinfunction "GND")
    )
    (model "${KISYS3DMOD}/Housings_SSOP_TSSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -2.667 -6.35)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R18" (at 0 1.651 0) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/VBAT")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 46 28)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH2" (at 0 -3.35 0) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.9) (clearance 1.9)
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -37.1475 -17.399)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R10" (at -0.5715 1.7145 0) (layer "F.SilkS"))
    (property "Value" "1.8K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(R10-Pad1)")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESCAXE80P160X320X70-8" (layer "F.Cu")
    (at 3.0355 -16.888)
    (descr "Resistor,Chip Array,0.80mm pitch;8 pin,1.60mm L X 3.20mm W X 0.70mm H")
    (property "Reference" "RN1" (at 0 -3.1115 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.9 -1.2) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/TSG7RIGHT") (pinfunction "R1.1")
    )
    (pad "2" smd rect (at -0.9 -0.4) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/TSG7SET") (pinfunction "R2.1")
    )
    (pad "3" smd rect (at -0.9 0.4) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/TSG7UP") (pinfunction "R3.1")
    )
    (pad "4" smd rect (at -0.9 1.2) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "R4.1")
    )
    (pad "5" smd rect (at 0.9 1.2) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "R4.2")
    )
    (pad "6" smd rect (at 0.9 0.4) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(P1-Pad3)") (pinfunction "R3.2")
    )
    (pad "7" smd rect (at 0.9 -0.4) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(P1-Pad2)") (pinfunction "R2.2")
    )
    (pad "8" smd rect (at 0.9 -1.2) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(P1-Pad1)") (pinfunction "R1.2")
    )
    (model "E:/Repository_local/KiCad/packages3d/Resistors_SMD.3dshapes/RESCAVE80P160X160X60-4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 46 -28)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH3" (at 0 -3.35 0) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.9) (clearance 1.9)
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -30.734 25.146)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R12" (at -0.6604 1.6764 0) (layer "F.SilkS"))
    (property "Value" "12K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R11-Pad2)")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23" (layer "F.Cu")
    (at 36.7055 7.747 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q3" (at -2.54 0.066 180) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.15 -0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/OUTON") (pinfunction "G")
    )
    (pad "2" smd rect (at -1.15 0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S")
    )
    (pad "3" smd rect (at 1.15 0 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(D7-Pad2)") (pinfunction "D")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Relais_SMD:EE2-xTNUH" (layer "F.Cu")
    (at 21.7805 22.098 90)
    (property "Reference" "RL1" (at -8.3 0 0) (layer "F.SilkS"))
    (property "Value" "EE2-3TNUH" (at 0 -0.4064 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd rect (at -6.35 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "3" smd rect (at -1.27 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at 1.27 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (pad "5" smd rect (at 3.81 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 6.35 4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3")
    )
    (pad "7" smd rect (at 6.35 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D2-Pad2)")
    )
    (pad "8" smd rect (at 3.81 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R6-Pad2)")
    )
    (pad "9" smd rect (at 1.27 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(RL1-Pad9)")
    )
    (pad "10" smd rect (at -1.27 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DACOUTB")
    )
    (pad "12" smd rect (at -6.35 -4 90) (size 1 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D1-Pad2)")
    )
    (model "${KISYS3DMOD}/Relays_SMD/EE2-xNUH.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23" (layer "F.Cu")
    (at 16.256 7.747 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q2" (at -2.682 -0.015 0) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.15 -0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/ATTOFF") (pinfunction "G")
    )
    (pad "2" smd rect (at -1.15 0.95 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S")
    )
    (pad "3" smd rect (at 1.15 0 270) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D2-Pad2)") (pinfunction "D")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -12.903 -25.905 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C1" (at 3.109 0 0) (layer "F.SilkS"))
    (property "Value" "4.7µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -8.4074 25.621671 -90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R5" (at -2.4765 0.0381 180) (layer "F.SilkS"))
    (property "Value" "4.7K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 270) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DACOUTB")
    )
    (pad "2" smd rect (at 1 0 270) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/-5V")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -17.0815 -18.796 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C7" (at 3.109 0 0) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at 41.0845 2.22 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C12" (at -2.4155 1.397 180) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm" (layer "F.Cu")
    (at -9.2075 -19.05)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (property "Reference" "U1" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "STM32L151C8Tx" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.35 -2.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VLCD")
    )
    (pad "2" smd rect (at -4.35 -2.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(D6-Pad2)") (pinfunction "PC13")
    )
    (pad "3" smd rect (at -4.35 -1.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PC14")
    )
    (pad "4" smd rect (at -4.35 -1.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PC15")
    )
    (pad "5" smd rect (at -4.35 -0.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PH0")
    )
    (pad "6" smd rect (at -4.35 -0.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PH1")
    )
    (pad "7" smd rect (at -4.35 0.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/NRESET") (pinfunction "NRST")
    )
    (pad "8" smd rect (at -4.35 0.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSSA")
    )
    (pad "9" smd rect (at -4.35 1.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "VDDA")
    )
    (pad "10" smd rect (at -4.35 1.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/TSG1CAP") (pinfunction "PA0")
    )
    (pad "11" smd rect (at -4.35 2.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/TSG1ON") (pinfunction "PA1")
    )
    (pad "12" smd rect (at -4.35 2.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/TSG1LEFT") (pinfunction "PA2")
    )
    (pad "13" smd rect (at -2.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/TSG1DOWN") (pinfunction "PA3")
    )
    (pad "14" smd rect (at -2.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA4")
    )
    (pad "15" smd rect (at -1.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/VBAT") (pinfunction "PA5")
    )
    (pad "16" smd rect (at -1.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA6")
    )
    (pad "17" smd rect (at -0.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA7")
    )
    (pad "18" smd rect (at -0.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/ATTOFF") (pinfunction "PB0")
    )
    (pad "19" smd rect (at 0.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/ATTON") (pinfunction "PB1")
    )
    (pad "20" smd rect (at 0.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/OUTOFF") (pinfunction "PB2")
    )
    (pad "21" smd rect (at 1.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/OUTON") (pinfunction "PB10")
    )
    (pad "22" smd rect (at 1.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PB11")
    )
    (pad "23" smd rect (at 2.25 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS")
    )
    (pad "24" smd rect (at 2.75 4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "VDD")
    )
    (pad "25" smd rect (at 4.35 2.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/TSG7CAP") (pinfunction "PB12")
    )
    (pad "26" smd rect (at 4.35 2.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/TSG7UP") (pinfunction "PB13")
    )
    (pad "27" smd rect (at 4.35 1.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/TSG7SET") (pinfunction "PB14")
    )
    (pad "28" smd rect (at 4.35 1.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/TSG7RIGHT") (pinfunction "PB15")
    )
    (pad "29" smd rect (at 4.35 0.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/TSG4CAP") (pinfunction "PA8")
    )
    (pad "30" smd rect (at 4.35 0.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/TSG4MEM") (pinfunction "PA9")
    )
    (pad "31" smd rect (at 4.35 -0.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/USBRX") (pinfunction "PA10")
    )
    (pad "32" smd rect (at 4.35 -0.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA11")
    )
    (pad "33" smd rect (at 4.35 -1.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA12")
    )
    (pad "34" smd rect (at 4.35 -1.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SWDIO") (pinfunction "PA13")
    )
    (pad "35" smd rect (at 4.35 -2.25) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS")
    )
    (pad "36" smd rect (at 4.35 -2.75) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "VDD")
    )
    (pad "37" smd rect (at 2.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SWCLK") (pinfunction "PA14")
    )
    (pad "38" smd rect (at 2.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PA15")
    )
    (pad "39" smd rect (at 1.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SWO") (pinfunction "PB3")
    )
    (pad "40" smd rect (at 1.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PB4")
    )
    (pad "41" smd rect (at 0.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PB5")
    )
    (pad "42" smd rect (at 0.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/USBTX") (pinfunction "PB6")
    )
    (pad "43" smd rect (at -0.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/SDA") (pinfunction "PB7")
    )
    (pad "44" smd rect (at -0.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "BOOT0")
    )
    (pad "45" smd rect (at -1.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/SCL") (pinfunction "PB8")
    )
    (pad "46" smd rect (at -1.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PB9")
    )
    (pad "47" smd rect (at -2.25 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS")
    )
    (pad "48" smd rect (at -2.75 -4.35 90) (size 1.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/3V3") (pinfunction "VDD")
    )
    (model "Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at -38.354 20.1836 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R9" (at 2.5052 -0.0508 180) (layer "F.SilkS"))
    (property "Value" "12K" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(R9-Pad1)")
    )
    (pad "2" smd rect (at 1 0 90) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C22-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:CAPC2012X60" (layer "F.Cu")
    (at -6.88725 14.458171 90)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.70mm H")
    (property "Reference" "C14" (at 2.855 -0.03175 180) (layer "F.SilkS"))
    (property "Value" "1µ" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/4.096V") (zone_connect 1)
    )
    (pad "2" smd rect (at 0.95 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "GNDA") (zone_connect 1)
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_SMD:RESC2012X60" (layer "F.Cu")
    (at 42.1005 -1.3335)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "R2" (at 1.0795 1.7145 0) (layer "F.SilkS"))
    (property "Value" "4.7K" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/5V")
    )
    (pad "2" smd rect (at 1 0) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/SCL")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/RESC2012x60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at -46 -28)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH4" (at 0 -3.35 0) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.9) (clearance 1.9)
    )
  )
  (footprint "Housings_TO_SOT_SMD:SOT89-3_Housing" (layer "F.Cu")
    (at -31.15648 -9.61424 180)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (property "Reference" "U7" (at -3.048 -0.0635 -90) (layer "F.SilkS"))
    (property "Value" "HT7833" (at 0.45 3.25 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -1.50114 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND/ADJ")
    )
    (pad "2" smd rect (at 0 -1.09982 180) (size 1.99898 2.99974) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0 0.762 180) (size 1.00076 1.00076) (layers "F.Cu")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "2" smd rect (at 0 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C26-Pad1)")
    )
    (pad "3" smd rect (at 1.50114 1.85166 180) (size 1.00076 1.50114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C28-Pad1)") (pinfunction "VO")
    )
    (model "${KISYS3DMOD}/Housings_TO_SOT.3dshapes/SOT89-3_Housing.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm" (layer "B.Cu")
    (at 10.16 -5.08 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Reference" "P1" (at 0 6.14 0) (layer "B.SilkS"))
    (property "Value" "FE04-1" (at 0 -6.14 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 3.81 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(P1-Pad1)") (pinfunction "P1")
    )
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(P1-Pad2)") (pinfunction "P2")
    )
    (pad "3" thru_hole oval (at 0 -1.27 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(P1-Pad3)") (pinfunction "P3")
    )
    (pad "4" thru_hole oval (at 0 -3.81 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P4")
    )
    (model "${KISYS3DMOD}/Socket_Headers.3dshapes/Socket_Strip_Straight_1x04.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Opto-Devices:OLED_0.96_TYP1_PCB" locked (layer "B.Cu")
    (at 33.4645 0 90)
    (property "Reference" "MOD1" (at -10.9855 -14.9 -90) (layer "B.SilkS"))
    (property "Value" "OLED128X64YB0.96" (at 0.05 -11.95 -90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "VDD" (at -1.25 9.05 180 unlocked) (layer "B.Fab"))
    (fp_text user "visible area" (at 0.3 1.75 -90) (layer "B.Fab"))
    (fp_text user "SCK" (at 1.25 9.05 180 unlocked) (layer "B.Fab"))
    (fp_text user "SDA" (at 3.85 9.05 180 unlocked) (layer "B.Fab"))
    (fp_text user "GND" (at -3.9 9.05 180 unlocked) (layer "B.Fab"))
    (pad "" np_thru_hole circle locked (at -10.35 -11.6 90) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.4) (clearance 1.4)
    )
    (pad "" np_thru_hole circle locked (at -10.35 11.6 90) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.4) (clearance 1.4)
    )
    (pad "" np_thru_hole circle locked (at 10.35 -11.6 90) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.4) (clearance 1.4)
    )
    (pad "" np_thru_hole circle locked (at 10.35 11.6 90) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.4) (clearance 1.4)
    )
    (pad "1" thru_hole circle locked (at -3.81 12.0015 90) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "2" thru_hole circle locked (at -1.27 12.0015 90) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "/5V") (pinfunction "VCC")
    )
    (pad "3" thru_hole circle locked (at 1.27 12.0015 90) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "/SCL") (pinfunction "SCK")
    )
    (pad "4" thru_hole circle locked (at 3.81 12.0015 90) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "/SDA") (pinfunction "SDA")
    )
    (model "C:/Users/offic/Downloads/096_oled_display.STEP"
      (offset (xyz 0 0 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (layer "B.Cu")
    (at -20.32 -7.62 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Reference" "P5" (at 0 3.6 0) (layer "B.SilkS"))
    (property "Value" "FE02-1" (at 0 -3.6 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole roundrect (at 0 1.27 180) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(P5-Pad1)") (pinfunction "P1")
    )
    (pad "2" thru_hole circle (at 0 -1.27 180) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P2")
    )
    (model "${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.step"
      (offset (xyz 0 1.27 0))
      (scale (xyz 1 1 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm" (layer "B.Cu")
    (at 10.16 10.16 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Reference" "P4" (at 0 6.14 0) (layer "B.SilkS"))
    (property "Value" "FE04-1" (at 0 -6.14 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 3.81 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(P4-Pad1)") (pinfunction "P1")
    )
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(P4-Pad2)") (pinfunction "P2")
    )
    (pad "3" thru_hole oval (at 0 -1.27 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(P4-Pad3)") (pinfunction "P3")
    )
    (pad "4" thru_hole oval (at 0 -3.81 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P4")
    )
    (model "${KISYS3DMOD}/Socket_Headers.3dshapes/Socket_Strip_Straight_1x04.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start -46 32) (end 46 32)
    (layer "Edge.Cuts"))
  (gr_line (start -46 -32) (end 46 -32)
    (layer "Edge.Cuts"))
  (gr_arc (start 50 28) (mid 48.828427 30.828427) (end 46 32)
    (layer "Edge.Cuts"))
  (gr_arc (start -50 -28) (mid -48.828427 -30.828427) (end -46 -32)
    (layer "Edge.Cuts"))
  (gr_line (start 50 28) (end 50 -28)
    (layer "Edge.Cuts"))
  (gr_arc (start 46 -32) (mid 48.828427 -30.828427) (end 50 -28)
    (layer "Edge.Cuts"))
  (gr_arc (start -46 32) (mid -48.828427 30.828427) (end -50 28)
    (layer "Edge.Cuts"))
  (gr_line (start -50 -28) (end -50 28)
    (layer "Edge.Cuts"))
  (gr_text "CHRG" (at -45.974 -11.684 90) (layer "F.SilkS"))
  (gr_text "STDBY" (at -40.132 -11.938 90) (layer "F.SilkS"))
  (gr_text "WorldInOne M.Straub (C) 2020" (at -17.7165 30.226 0) (layer "F.SilkS"))
  (gr_text "PVS V1.0" (at -8.89 1.826 0) (layer "F.SilkS"))
  (gr_text "Precision Voltage Source" (at -8.89 4.826 0) (layer "F.SilkS"))
  (zone (net 33) (net_name "Net-(P8-Pad1)") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -32.8676 -22.6568)
        (xy -31.242 -22.6568)
        (xy -31.242 -18.9992)
        (xy -33.7312 -18.9992)
        (xy -33.7312 -25.908)
        (xy -32.8676 -25.908)
      )
    )
  )
  (zone (net 8) (net_name "/Supply/VIN") (layer "F.Cu") (name "VBAT+") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -34.7726 24.139525)
        (xy -35.2044 24.130002)
        (xy -35.2044 20.113627)
        (xy -35.8648 20.1168)
        (xy -35.8648 10.72515)
        (xy -36.83 10.7315)
        (xy -36.83 6.4135)
        (xy -34.7218 6.442075)
      )
    )
  )
  (zone (net 30) (net_name "/Supply/VUSB") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -37.8968 -20.2184)
        (xy -41.6052 -20.2184)
        (xy -41.6052 -21.336)
        (xy -37.8968 -21.336)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (name "GNDA") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -16.764 24.557371)
        (xy -17.7292 24.557371)
        (xy -17.7292 22.626971)
        (xy -16.764 22.626971)
      )
    )
  )
  (zone (net 17) (net_name "Net-(D3-Pad2)") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -31.3944 15.9512)
        (xy -34.4932 15.9512)
        (xy -34.4932 14.5796)
        (xy -32.6136 14.5796)
        (xy -32.639 9.779)
        (xy -31.3944 9.7536)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -14.3 -18.031)
        (xy -15.3795 -18.031)
        (xy -15.3795 -18.6025)
        (xy -14.3 -18.6025)
      )
    )
  )
  (zone (net 63) (net_name "/Supply/6V") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -28.9052 21.2852)
        (xy -30.48 21.2852)
        (xy -30.48 14.5796)
        (xy -29.6926 14.5796)
        (xy -27.8892 14.5796)
        (xy -27.8892 16.1036)
        (xy -28.9052 16.1036)
      )
    )
  )
  (zone (net 63) (net_name "/Supply/6V") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -26.797 3.8735)
        (xy -26.797 6.4643)
        (xy -28.575 6.4643)
        (xy -28.575 3.8735)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.652 -24.1935)
        (xy -10.287 -24.1935)
        (xy -10.287 -24.7015)
        (xy -9.652 -24.7015)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (name "VBAT+") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -32.7152 13.50645)
        (xy -34.596986 13.49375)
        (xy -34.596986 6.19125)
        (xy -32.7152 6.20395)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F.Cu" "In1.Cu" "B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 50.038 32.004)
        (xy -50.038 32.004)
        (xy -50.038 -32.004)
        (xy 50.038 -32.004)
      )
    )
  )
  (zone (net 35) (net_name "GNDA") (layers "F.Cu" "In1.Cu" "B.Cu") (name "GNDA") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 5.6515 25.646551)
        (xy -17.11963 25.66145)
        (xy -17.037065 11.4057)
        (xy 5.607065 11.454301)
      )
    )
  )
  (zone (net 2) (net_name "/3V3") (layer "In2.Cu") (name "GND") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 41.0845 27.432)
        (xy 5.715 27.432)
        (xy 5.588 -5.2705)
        (xy -50.038 -5.334)
        (xy -50.038 -32.004)
        (xy 41.2115 -32.004)
      )
    )
  )
  (zone (net 7) (net_name "/5V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -49.911 -5.000505)
        (xy 5.334 -4.953)
        (xy 5.334 27.813)
        (xy 41.402 27.686)
        (xy 41.402 -32.004)
        (xy 49.9745 -32.004)
        (xy 50.038 32.004)
        (xy -50.038 32.004)
        (xy -50.038 -5.079357)
        (xy -50.038 -5.08)
      )
    )
  )
  (zone (net 56) (net_name "/5VFILT") (layer "In2.Cu") (name "5VFILT") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 0.66675 25.370171)
        (xy -12.60475 25.370171)
        (xy -12.7 14.956171)
        (xy 0.508 14.956171)
      )
    )
  )
)
