(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad2)")
  (net 2 "Net-(R1-Pad1)")
  (net 3 "Net-(R2-Pad1)")
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 111.506 80.814)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R2" (at 0 -1.17 0) (layer "F.SilkS"))
    (property "Value" "R_Small" (at 0 1.17 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/dom/Downloads/test/test.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(R2-Pad1)")
    )
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(R1-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 111.506 82.804)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R1" (at 0 -1.17 0) (layer "F.SilkS"))
    (property "Value" "R_Small" (at 0 1.17 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/dom/Downloads/test/test.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(R1-Pad1)")
    )
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(R1-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 114.416 80.814)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R3" (at 0 -1.17 0) (layer "F.SilkS"))
    (property "Value" "R_Small" (at 0 1.17 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/dom/Downloads/test/test.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(R2-Pad1)")
    )
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(R1-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 73.8378 65.3288) (end 165.5064 114.554)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 3) (net_name "Net-(R2-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.126 76.7334)
        (xy 118.6434 88.9254)
        (xy 105.5878 89.1794)
        (xy 105.8672 76.8858)
      )
    )
  )
)
