(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6383)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.0127))
      (layer "F.Cu" (type "copper") (thickness 0.034798))
      (layer "dielectric 1" (type "core") (thickness 0.23622) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.034798))
      (layer "dielectric 2" (type "prepreg") (thickness 0.9906) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.034798))
      (layer "dielectric 3" (type "core") (thickness 0.24892) (material "FR4") (epsilon_r 4.1) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.034798))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.0127))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(P1-Pad1)")
  (net 3 "Net-(C32-Pad1)")
  (net 4 "/+Vout_WFG")
  (net 5 "Net-(R38-Pad1)")
  (net 6 "Net-(R37-Pad2)")
  (net 7 "Net-(R20-Pad2)")
  (net 8 "Net-(R42-Pad1)")
  (net 9 "Net-(C30-Pad1)")
  (net 10 "Net-(C32-Pad2)")
  (net 11 "Net-(C35-Pad2)")
  (net 12 "/+20V")
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(R35-Pad1)")
  (net 15 "Net-(R38-Pad2)")
  (net 16 "Net-(R47-Pad2)")
  (net 17 "Net-(R47-Pad1)")
  (net 18 "Net-(R49-Pad1)")
  (net 19 "Net-(R52-Pad1)")
  (net 20 "Net-(U13-Pad11)")
  (net 21 "Net-(U13-Pad9)")
  (net 22 "Net-(U13-Pad8)")
  (net 23 "Net-(R20-Pad3)")
  (footprint "My_SMD:TP-50" (layer "F.Cu")
    (at 19.304 65.786 180)
    (property "Reference" "TP2" (at 0.254 -1.27 0) (layer "F.SilkS"))
    (property "Value" "Test_Point" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd circle (at 0 0 180) (size 1.27 1.27) (layers "F.Cu" "F.Mask")
      (net 4 "/+Vout_WFG") (pinfunction "TP")
    )
  )
  (footprint "My_SMD:TP-50" (layer "F.Cu")
    (at 21.59 48.514)
    (property "Reference" "TP11" (at 0.0508 1.4732 0) (layer "F.SilkS"))
    (property "Value" "Test_Point" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" smd circle (at 0 0) (size 1.27 1.27) (layers "F.Cu" "F.Mask")
      (net 4 "/+Vout_WFG") (pinfunction "TP")
    )
  )
  (footprint "SamacSys_Parts:DIP794W56P254L2013H533Q16N" (layer "F.Cu")
    (at 47.7139 11.962 180)
    (descr "XR2206CP-F_a")
    (tags "Integrated Circuit")
    (property "Reference" "U13" (at -0.381 -11.938 180) (layer "F.SilkS"))
    (property "Value" "XR2206CP-F" (at 0 0 180) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "Parity Functions 10V-26V 0.01Hz-1MHz temp 0C to 70C" (at 47.7139 11.962 0) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (property "Height" "5.33" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer_Name" "EXAR" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer_Part_Number" "XR2206CP-F" (at 0 0 0) (layer "F.Fab") hide)
    (property "RS Part Number" "6866027P" (at 0 0 0) (layer "F.Fab") hide)
    (property "RS Price/Stock" "http://uk.rs-online.com/web/p/products/6866027P" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -0.381 -11.938 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.97 -8.89 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 14 "Net-(R35-Pad1)") (pinfunction "AMSI")
    )
    (pad "2" thru_hole circle (at -3.97 -6.35 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(R37-Pad2)") (pinfunction "STO")
    )
    (pad "3" thru_hole circle (at -3.97 -3.81 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(R1-Pad2)") (pinfunction "MO")
    )
    (pad "4" thru_hole circle (at -3.97 -1.27 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 4 "/+Vout_WFG") (pinfunction "VCC")
    )
    (pad "5" thru_hole circle (at -3.97 1.27 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C32-Pad1)") (pinfunction "TC1")
    )
    (pad "6" thru_hole circle (at -3.97 3.81 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C32-Pad2)") (pinfunction "TC2")
    )
    (pad "7" thru_hole circle (at -3.97 6.35 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 19 "Net-(R52-Pad1)") (pinfunction "TR1")
    )
    (pad "8" thru_hole circle (at -3.97 8.89 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 22 "Net-(U13-Pad8)") (pinfunction "TR2")
    )
    (pad "9" thru_hole circle (at 3.97 8.89 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U13-Pad9)") (pinfunction "FSKI")
    )
    (pad "10" thru_hole circle (at 3.97 6.35 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C35-Pad2)") (pinfunction "BIAS")
    )
    (pad "11" thru_hole circle (at 3.97 3.81 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U13-Pad11)") (pinfunction "SYNCO")
    )
    (pad "12" thru_hole circle (at 3.97 1.27 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 18 "Net-(R49-Pad1)") (pinfunction "GND")
    )
    (pad "13" thru_hole circle (at 3.97 -1.27 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(R47-Pad1)") (pinfunction "WAVEA1")
    )
    (pad "14" thru_hole circle (at 3.97 -3.81 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(R47-Pad2)") (pinfunction "WAVEA2")
    )
    (pad "15" thru_hole circle (at 3.97 -6.35 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(R38-Pad1)") (pinfunction "SYMA1")
    )
    (pad "16" thru_hole circle (at 3.97 -8.89 180) (size 1.16 1.16) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(R38-Pad2)") (pinfunction "SYMA2")
    )
    (model "C:/Users/Art Grigoryev/OneDrive/Designs/Hardware design/KiCad Libraries/Import/SamacSys_Parts.3dshapes/XR2206CP-F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SamacSys_Parts:Y006910K0000J0L" (layer "F.Cu")
    (at 34.535369 11.1506 90)
    (descr "Y006910K0000J0L-1")
    (tags "Variable Resistor")
    (property "Reference" "R20" (at 7.9248 0.1524 180) (layer "F.SilkS"))
    (property "Value" "10K" (at 2.525 0.32 90) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "10 kOhms 0.25W, 1/4W PC Pins Through Hole Trimmer Potentiometer Metal Foil 21 Turn Top Adjustment" (at 34.535369 11.1506 0) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Vishay Foil Resistors (Division of Vishay Precision Group)" (at 0 0 0) (layer "F.Fab") hide)
    (property "Part_Number" "804-1000-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price" "26.57" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price_Break_Quantity" "1" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 4 "/+Vout_WFG")
    )
    (pad "2" thru_hole circle (at 5.08 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 7 "Net-(R20-Pad2)")
    )
    (pad "3" thru_hole circle (at 2.54 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R20-Pad3)")
    )
    (model "C:/Users/Art Grigoryev/OneDrive/Designs/Hardware design/KiCad Libraries/Import/SamacSys_Parts.3dshapes/Y006910K0000J0L.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SamacSys_Parts:Y006910K0000J0L" (layer "F.Cu")
    (at 34.535369 21.8186 90)
    (descr "Y006910K0000J0L-1")
    (tags "Variable Resistor")
    (property "Reference" "R42" (at 7.8486 0.1524 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 2.525 0.32 -90) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "10 kOhms 0.25W, 1/4W PC Pins Through Hole Trimmer Potentiometer Metal Foil 21 Turn Top Adjustment" (at 34.535369 21.8186 0) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Vishay Foil Resistors (Division of Vishay Precision Group)" (at 0 0 0) (layer "F.Fab") hide)
    (property "Part_Number" "804-1000-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price" "26.57" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price_Break_Quantity" "1" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(R42-Pad1)")
    )
    (pad "2" thru_hole circle (at 5.08 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C30-Pad1)")
    )
    (pad "3" thru_hole circle (at 2.54 0 90) (size 1.493 1.493) (drill 0.96) (layers "*.Cu" "*.Mask")
      (net 1 "GND")
    )
    (model "C:/Users/Art Grigoryev/OneDrive/Designs/Hardware design/KiCad Libraries/Import/SamacSys_Parts.3dshapes/Y006910K0000J0L.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Conn:Molex_1724480004" (layer "F.Cu")
    (at 9.906 55.88 -90)
    (property "Reference" "P1" (at -5.842 1.524 180) (layer "F.SilkS"))
    (property "Value" "1724480004" (at 0 -2.9 90) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "Connector Header Through Hole, Right Angle 4 position 0.165\" (4.20mm)" (at 9.906 55.88 0) (layer "F.Fab") hide)
    (property "Distributor" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Molex" (at 0 0 0) (layer "F.Fab") hide)
    (property "Part_Number" "WM16295-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price" "0.9" (at 0 0 0) (layer "F.Fab") hide)
    (property "Price_Break_Quantity" "1" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" np_thru_hole circle (at 0 7.2898 270) (size 2.999999 2.999999) (drill 2.999999) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.0865 0 270) (size 3.159999 3.159999) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(P1-Pad1)") (pinfunction "P1")
    )
    (pad "2" thru_hole circle (at -2.1045 0 270) (size 3.16 3.16) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P2")
    )
    (pad "3" thru_hole circle (at 2.0955 -5.5118 270) (size 3.159999 3.159999) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 12 "/+20V") (pinfunction "P3")
    )
    (pad "4" thru_hole circle (at -2.1045 -5.5118 270) (size 3.159999 3.159999) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P4")
    )
    (model "${KISYS3DMOD}/connectors/Molex/1724480004.stp"
      (offset (xyz 0 -13.843 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_line (start 82.55 76.2) (end 82.55 0)
    (layer "Edge.Cuts"))
  (gr_line (start 0 76.2) (end 82.55 76.2)
    (layer "Edge.Cuts"))
  (gr_line (start 82.55 0) (end 0 0)
    (layer "Edge.Cuts"))
  (gr_line (start 0 0) (end 0 76.2)
    (layer "Edge.Cuts"))
  (gr_text "OFF" (at 2.794 48.006 270) (layer "F.SilkS"))
  (gr_text "BandWdth" (at 39.37 19.304 90) (layer "F.SilkS"))
  (gr_text "JAMX Module Rev 1.0" (at 66.04 60.96 90) (layer "F.SilkS"))
  (gr_text "GND\n" (at 11.43 62.23 270) (layer "F.SilkS"))
  (gr_text "GND\n" (at 9.144 62.23 270) (layer "F.SilkS"))
  (gr_text "Freq" (at 39.624 8.89 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 76.2)
        (xy 0 76.2)
        (xy 0 0)
        (xy 82.55 0)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 76.2)
        (xy 0 76.2)
        (xy 0 0)
        (xy 82.55 0)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 76.2)
        (xy 0 76.2)
        (xy 0 0)
        (xy 82.55 0)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 76.2)
        (xy 0 76.2)
        (xy 0 0)
        (xy 82.55 0)
      )
    )
  )
)
