(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (property "REVISION" "69")
  (net 0 "")
  (net 1 "Net-(R1-Pad1)")
  (footprint "Generic:Fiducial_rotondo" locked (layer "F.Cu")
    (at 99.822 118.364)
    (descr "Fiducial, Modern, Copper Top, Passermarke,")
    (tags "Fiducial, Modern, Copper Top, Passermarke,")
    (property "Reference" "REF**" (at 0 -2.25 0) (layer "F.SilkS") hide)
    (property "Value" "Fiducial_Modern_CopperTop" (at 0 2.5 0) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (zone_connect 0)
    (attr smd)
    (pad "~" smd circle locked (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1) (clearance 1) (zone_connect 0)
    )
  )
  (footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P30.48mm" (layer "F.Cu")
    (at 131.572 102.87)
    (descr "Resistor, Axial_Power series, Box, pin pitch=30.48mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 30.48mm 4W length 20mm width 6.4mm height 6.4mm")
    (property "Reference" "R1" (at 15.24 -4.32 0) (layer "F.SilkS"))
    (property "Value" "R" (at 15.24 4.32 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/michele/Documenti/pcb/kicad/TestPcb/test/test.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 15.24 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(R1-Pad1)")
    )
    (pad "2" thru_hole oval (at 30.48 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(R1-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P30.48mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Generic:Fiducial_quadro" locked (layer "F.Cu")
    (at 193.294 83.566)
    (descr "Fiducial, Classical, Big, Copper Top, Typ 2, Passermarke,")
    (tags "Fiducial, Classical, Big, Copper Top, Typ 2, Passermarke,")
    (property "Reference" "REF**" (at 0 -2.75 0) (layer "F.SilkS") hide)
    (property "Value" "Fiducial_Modern_CopperTop" (at 0 2.75 0) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (zone_connect 0)
    (attr smd)
    (pad "~" smd rect locked (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1) (clearance 1) (zone_connect 0)
    )
  )
  (gr_rect (start 92.202 77.216) (end 200.66 125.984)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "TEST ${REVISION}" (at 147.066 116.586 0) (layer "F.Cu"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.1378 106.0958)
        (xy 181.0004 106.0958)
        (xy 181.0004 93.1672)
        (xy 188.1378 93.1672)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 200.152 125.476)
        (xy 92.71 125.476)
        (xy 92.71 77.724)
        (xy 200.152 77.724)
      )
    )
  )
)
