(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "A")
  (net 2 "B")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 125 75)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Reference" "J2" (at 0 -2.33 0) (layer "F.SilkS"))
    (property "Value" "Conn_01x01" (at 0 2.33 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/alex/kicad-shorted-zone-test/kicad-shorted-zone-test/kicad-shorted-zone-test.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "B") (pinfunction "Pin_1")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 133 75)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Reference" "J1" (at 0 -2.33 0) (layer "F.SilkS"))
    (property "Value" "Conn_01x01" (at 0 2.33 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/alex/kicad-shorted-zone-test/kicad-shorted-zone-test/kicad-shorted-zone-test.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "A") (pinfunction "Pin_1")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 120 70) (end 140 80)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 2) (net_name "B") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 80)
        (xy 120 80)
        (xy 120 70)
        (xy 140 70)
      )
    )
  )
  (zone (net 1) (net_name "A") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.57933 78.081171)
        (xy 121.57933 78.081171)
        (xy 121.57933 72.081171)
        (xy 137.57933 72.081171)
      )
    )
  )
)
