(kicad_pcb
	(version 20241228)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "I2C soil moisture sensor")
		(date "2020-09-29")
		(rev "2.7.9")
		(company "Catnip electronics")
		(comment 1 "albertas@technarium.lt")
	)
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 86 13)
		(grid_origin 96.3 30.2)
		(pcbplotparams
			(layerselection 0x55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "mfgset/")
		)
	)
	(net 0 "")
	(net 1 "Net-(C1-Pad1)")
	(net 2 "GND")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "VCC")
	(net 5 "/SENSE_LOW")
	(net 6 "/SENSOR_TRACK")
	(net 7 "/THERMISTOR")
	(net 8 "/RESET")
	(net 9 "/EXCITATION")
	(net 10 "Net-(D3-Pad1)")
	(net 11 "/SCK/SCL")
	(net 12 "/MOSI/SDA")
	(net 13 "/MISO/SENSE_HIGH")
	(net 14 "Net-(IC1-Pad11)")
	(net 15 "Net-(IC1-Pad12)")
	(footprint "Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 91.25 26 90)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "X1"
			(at 0 -3.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "16MHz"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0.65 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(C1-Pad1)")
		)
		(pad "2" smd rect
			(at 1.1 0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
		)
		(pad "3" smd rect
			(at 1.1 -0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(C2-Pad1)")
		)
		(pad "4" smd rect
			(at -1.1 -0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d/CRY_SMD3225.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(layer "F.Cu")
		(at 95.804 40.842)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "D2"
			(at 0 1.458 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT54"
			(at -1.296 -2.858 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/SENSOR_TRACK")
		)
		(pad "2" smd rect
			(at -0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/MISO/SENSE_HIGH")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(layer "F.Cu")
		(at 93.01 40.842)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "D1"
			(at 0 1.458 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT54"
			(at 1.11 -2.858 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/SENSE_LOW")
		)
		(pad "2" smd rect
			(at -0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/SENSOR_TRACK")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 91.25 28.9 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3.75 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "33p"
			(at 2.35 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(C1-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 91.05 23.1)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -0.25 -1.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "33pp"
			(at -2.75 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 94.90234 22.577514)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -1.80234 0.022486 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 95.8 38.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -5.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 1.85 -0.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/MISO/SENSE_HIGH")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 91.2 30.4 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 3.7 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 1.8 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/RESET")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 91.2 32 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 3.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.2 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/RESET")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 97.328 33.984)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.528 0.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k 0.1%"
			(at 4.272 -0.084 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(IC1-Pad11)")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/THERMISTOR")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 90 40.95)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.3 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at -2.2 -0.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/SENSOR_TRACK")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/EXCITATION")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 92.764533 35.762 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 4.564533 0.062 180)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 2.01 -0.038 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/SENSE_LOW")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(IC1-Pad11)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 92.76272 37.312)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -4.61 -0.012 0)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at -2.01 0.06 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/SENSE_LOW")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 95.804 37.3 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 5.604 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at -1.996 0.14 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/MISO/SENSE_HIGH")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "w_logo:Logo_silk_OSHW_6x6mm"
		(layer "F.Cu")
		(at 95.2 57.2)
		(descr "Open Hardware Logo, 6x6mm")
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0 0.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 97.1 28)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC1"
			(at 0.7 -5.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "ATTINY441-SSU"
			(at 0 5.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(C1-Pad1)")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/RESET")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/EXCITATION")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/SENSE_LOW")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/MOSI/SDA")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/MISO/SENSE_HIGH")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/SCK/SCL")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/THERMISTOR")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(IC1-Pad11)")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(IC1-Pad12)")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D3-Pad1)")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 92.8 38.8 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 4.65 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 1.75 0.15 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/SENSE_LOW")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 95.804 35.762)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -5.504 -0.062 0)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at -0.204 -1.062 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/MISO/SENSE_HIGH")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(IC1-Pad11)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 98.8 35.844001)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "TH1"
			(at 1.3 -1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "NCP18XH103F03RB"
			(at 8.3 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/THERMISTOR")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "chirp_logo:ziogas"
		(layer "B.Cu")
		(at 95.95 82.8 -90)
		(property "Reference" "G***"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(embedded_fonts no)
	)
	(footprint "Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm"
		(layer "B.Cu")
		(at 91.7 14.799451 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "P2"
			(at 0.17 -10 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "CONN_01X04"
			(at 0 -10.01 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
		)
		(pad "2" smd oval
			(at 0 -2.54 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/MOSI/SDA")
		)
		(pad "3" smd oval
			(at 0 -5.08 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/SCK/SCL")
		)
		(pad "4" smd oval
			(at 0 -7.62 270)
			(size 2.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint "programming_header:Pin_Header_Straight_2x03"
		(layer "B.Cu")
		(at 98.3 27.2 180)
		(descr "Through hole pin header")
		(tags "pin header")
		(property "Reference" "P1"
			(at 0 3.81 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "CONN_02X03"
			(at 0.25 -3 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at -2.54 -1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/MISO/SENSE_HIGH")
		)
		(pad "2" smd circle
			(at -2.54 1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "VCC")
		)
		(pad "3" smd circle
			(at 0 -1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/SCK/SCL")
		)
		(pad "4" smd circle
			(at 0 1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/MOSI/SDA")
		)
		(pad "5" smd circle
			(at 2.54 -1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "/RESET")
		)
		(pad "6" smd circle
			(at 2.54 1.27 180)
			(size 1.7272 1.7272)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 99.2 19.9)
		(end 104.3 25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.3 40.2)
		(end 104.3 25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.3 42.2)
		(end 86.3 41.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.3 45.2)
		(end 85.3 100.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.3 43.2)
		(end 105.3 45.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.2 16.4)
		(end 99.2 19.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.2 13.2)
		(end 91.4 13.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.4 16.4)
		(end 91.4 19.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.3 40.2)
		(end 104.3 41.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.3 41.2)
		(end 103.3 42.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.4 19.9)
		(end 86.3 25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.3 113.2)
		(end 85.3 100.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.3 113.2)
		(end 105.3 100.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.3 42.2)
		(end 87.3 43.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.3 42.2)
		(end 103.3 43.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 91.4 16.4)
		(mid 89.8 14.8)
		(end 91.4 13.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.3 100.2)
		(end 105.3 45.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.3 45.2)
		(end 87.3 43.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.3 41.2)
		(end 86.3 40.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.2 13.2)
		(mid 100.8 14.8)
		(end 99.2 16.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.3 40.2)
		(end 86.3 25)
		(layer "Edge.Cuts")
	)
	(gr_text "temp\nsensor"
		(at 100.2 40.3 0)
		(layer "F.SilkS")
	)
	(gr_text "Soil moisture \nsensor v2.7.9"
		(at 95.7 51.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Catnip Electronics\nhttp://wemakethings.net/chirp\nmic@wemakethings.net"
		(at 94 76.5 270)
		(layer "B.SilkS")
	)
	(gr_text "GND\n\nSDA\n\nSCL\n\nVCC"
		(at 95.5 17.5 90)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 86.3 13.2) (xy 104.3 13.2)
		)
		(height -11)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "18.0000 mm"
			(at 95.3 1.05 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 86 13) (xy 86 46.8)
		)
		(height 5.1)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "33.8000 mm"
			(at 79.75 29.9 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 104.3 113.2) (xy 104.3 13.2)
		)
		(height 4.25)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.175)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "100.0000 mm"
			(at 107.675 63.2 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 104.3 100.2) (xy 86.3 100.2)
		)
		(height -13)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.175)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "18.0000 mm"
			(at 95.3 112.325 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 100.8 14.8) (xy 104.3 25)
		)
		(height -4.2)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.5 mm"
			(at 110.6 10.8 0)
			(layer "Cmts.User")
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 87.8 13.2) (xy 102.8 13.2) (xy 102.8 43.2) (xy 87.8 43.2)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 87.8 13.2) (xy 102.8 13.2) (xy 102.8 43.2) (xy 87.8 43.2)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 102.8 99.1) (xy 95.3 109.6) (xy 87.8 99.1) (xy 87.8 13.2) (xy 102.8 13.2)
			)
		)
		(polygon
			(pts
				(xy 94.9 40.7) (xy 94.886251 45.1) (xy 93.163539 45.1) (xy 90.799103 42.400705) (xy 90.8 40.8) (xy 88.3 40.8)
				(xy 88.3 45.2) (xy 90.4 47.2) (xy 90.4 99.3) (xy 93.495238 102.8) (xy 97.214677 102.8) (xy 100.1 99.2)
				(xy 100.2 46.2) (xy 98.1 46.2) (xy 98.1 40.7)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 102.8 43.2) (xy 87.8 43.2) (xy 87.8 13.2) (xy 102.8 13.2)
			)
		)
	)
	(embedded_fonts no)
)
