(kicad_pcb (version 20201002) (generator pcbnew)
  (general
    (thickness 0.6)
  )
  (paper "A4" portrait)
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (grid_origin 118.35 87.8)
    (pcbplotparams
      (layerselection 0x0020000_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/")
    )
  )
  (net 0 "")
  (module "Library:QFN-20_EPthermal_4x4_Pitch0.5mm" (layer "F.Cu") (tedit 5A577FBB)
    (at 111.85 167.8)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference "U1" (at 3.1212 2.10262) (layer "F.SilkS"))
    (fp_text value "DRV8662" (at -0.95 1.55) (layer "F.Fab"))
    (pad "" smd rect (at 0.7 -0.45 180) (size 1.15 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "" smd rect (at 0.45 0 270) (size 2.5 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "" smd rect (at -0.7 -0.45 180) (size 1.15 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "" smd rect (at -0.7 0.45 180) (size 1.15 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "" smd rect (at 0.7 0.45 180) (size 1.15 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "" smd rect (at -0.45 0 270) (size 2.5 0.5) (layers "F.Paste")
      (solder_paste_margin -0.001) (solder_paste_margin_ratio -0.00001))
    (pad "1" smd oval (at -2 -1 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd oval (at -2 -0.5 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd oval (at -2 0 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd oval (at -2 0.5 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd oval (at -2 1 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd oval (at -1 2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "7" smd oval (at -0.5 2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "8" smd oval (at 0 2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "9" smd oval (at 0.5 2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "10" smd oval (at 1 2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd oval (at 2 1 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "12" smd oval (at 2 0.5 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "13" smd oval (at 2 0 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "14" smd oval (at 2 -0.5 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "15" smd oval (at 2 -1 90) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "16" smd oval (at 1 -2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "17" smd oval (at 0.5 -2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "18" smd oval (at 0 -2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "19" smd oval (at -0.5 -2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "20" smd oval (at -1 -2) (size 0.28 0.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "21" smd rect (at 0 0) (size 2.69 2.69) (layers "F.Cu" "F.Mask")
      (solder_paste_margin -0.1) (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0.9 -0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0 0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0.9 0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at -0.9 -0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0 -0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" smd rect (at 0 0) (size 2.69 2.69) (layers "B.Cu")
      (solder_paste_margin -0.1) (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at -0.9 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at 0.9 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
    (pad "21" thru_hole circle (at -0.9 0.9) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (solder_paste_margin_ratio -0.5))
  )
)
