(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal "Top")
    (31 "B.Cu" signal "Bottom")
    (35 "F.Paste" user)
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
    (50 "User.1" user "Mechanical.1")
    (51 "User.2" user "Mechanical.2")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.5) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010e8_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Manufacture/Gerber/JLCPCB/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C10-Pad1)")
  (net 3 "Net-(D8-Pad2)")
  (net 4 "Net-(FH1-Pad1)")
  (net 5 "Net-(Q1-Pad2)")
  (net 6 "Net-(Q1-Pad1)")
  (net 7 "Net-(R13-Pad1)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "/170V")
  (net 10 "/UIN")
  (net 11 "Net-(Q2-Pad3)")
  (net 12 "/HVON")
  (net 13 "/U170V")
  (net 14 "/CASETEMP")
  (net 15 "Net-(R7-Pad1)")
  (net 16 "Net-(P2-Pad2)")
  (net 17 "Net-(C2-Pad2)")
  (net 18 "/5V")
  (net 19 "Net-(U1-Pad1)")
  (net 20 "/UB")
  (net 21 "Net-(L3-Pad1)")
  (net 22 "Net-(R3-Pad2)")
  (net 23 "Net-(R11-Pad1)")
  (net 24 "Net-(C11-Pad2)")
  (net 25 "Net-(P1-Pad1)")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 114.8865 97.79 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R4" (at 0 1.3335 0 unlocked) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/U170V")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R2-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at 101.5 77)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH4" (at 3.2115 -0.038 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 5 5) (drill 2.7) (layers "*.Mask")
      (solder_mask_margin 1.2) (clearance 1.2)
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 119.53225 95.1215)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R1" (at -1.61275 1.3985 0 unlocked) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(Q2-Pad3)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/UIN")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_95" (layer "F.Cu")
    (at 119.3195 105.2195 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C1" (at 2.8605 0 90 unlocked) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 1.82 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "1206" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "25V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 20 "/UB")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1206_3216.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_Elec_8x10.2" (layer "F.Cu")
    (at 108.5215 80.518 90)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 8.0x10.2mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Reference" "C15" (at -5.08 2.794 0 unlocked) (layer "F.SilkS"))
    (property "Value" "3.3µ" (at 0 5.2 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Case" "830x1050" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "400V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CPS" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.6 0 90) (size 4.5 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952)
      (net 9 "/170V")
    )
    (pad "2" smd roundrect (at 3.6 0 90) (size 4.5 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_Radial_SMD/C_Elec_8x10.2.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "WIO_Mech:PJ-051A" (layer "F.Cu")
    (at 150 77.851 -90)
    (property "Reference" "X1" (at 2.413 -6.985 90 unlocked) (layer "F.SilkS"))
    (property "Value" "PJ-051A" (at 1.778 -2.921 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Current" "2.5A" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manuf" "CUI" (at 0 0 0) (layer "F.Fab") hide)
    (property "ManufCode" "PJ-047A" (at 0 0 0) (layer "F.Fab") hide)
    (property "OrderNo" "CP-047A-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Supplier" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole oval (at 6.3 3.3 270) (size 3 1.8) (drill oval 2 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(FH1-Pad1)") (pinfunction "1")
    )
    (pad "2" thru_hole oval (at 6.3 -5.3 270) (size 3 1.8) (drill oval 2 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (thermal_bridge_width 1.016)
    )
    (pad "3" thru_hole oval (at 6.3 -0.1 270) (size 3 1.8) (drill oval 2 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "3") (thermal_bridge_width 1.016)
    )
    (pad "CASE" thru_hole oval (at -1 -6.2 270) (size 4 2) (drill oval 2.3 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "CASE1") (thermal_bridge_width 1.016)
    )
    (pad "CASE" thru_hole oval (at -1 3.7 270) (size 4 2) (drill oval 2.3 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "CASE1") (thermal_bridge_width 1.016)
    )
    (model "${KISYS3DMOD}/WIO_packages3d/PJ-051.step"
      (offset (xyz -4 1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 -180 -90))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 110.363 97.79 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R2" (at 0 -1.65 0 unlocked) (layer "F.SilkS"))
    (property "Value" "470K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R2-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/170V")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 113.03 111.618 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R11" (at 0 1.524 90 unlocked) (layer "F.SilkS"))
    (property "Value" "52.3K" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R11-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/5V")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x03_P2.54mm_Horizontal" locked (layer "F.Cu")
    (at 132.5 111 180)
    (descr "Through hole angled socket strip, 2x03, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x03 2.54mm double row")
    (property "Reference" "P1" (at 1.944 2.542 90 unlocked) (layer "F.SilkS"))
    (property "Value" "FE03-2W" (at -5.65 7.85 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -8.315 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(P1-Pad1)") (pinfunction "P1")
    )
    (pad "2" thru_hole oval locked (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/CASETEMP") (pinfunction "P2")
    )
    (pad "3" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/U170V") (pinfunction "P3")
    )
    (pad "4" thru_hole oval locked (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/HVON") (pinfunction "P4")
    )
    (pad "5" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/5V") (pinfunction "P5")
    )
    (pad "6" thru_hole oval locked (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "P6")
    )
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x03_P2.54mm_Horizontal.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_95" (layer "F.Cu")
    (at 126.111 106.8345 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C12" (at -3.4565 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "16V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 18 "/5V")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1206_3216.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 113.03 115.316 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R3" (at 2.634 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C11-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at 101.5 123)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH1" (at 0 -3.35 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 5 5) (drill 2.7) (layers "*.Mask")
      (solder_mask_margin 1.2) (clearance 1.2)
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23" (layer "F.Cu")
    (at 119.768 98.2345 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q2" (at -1.7075 -2.3495 0 unlocked) (layer "F.SilkS"))
    (property "Value" "BSS138" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -1.15 -0.95 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(P2-Pad2)") (pinfunction "G")
    )
    (pad "2" smd rect (at -1.15 0.95 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S")
    )
    (pad "3" smd rect (at 1.15 0 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(Q2-Pad3)") (pinfunction "D")
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 114.808 107.6325 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R12" (at 0.0155 1.5875 90 unlocked) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R11-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval" (layer "F.Cu")
    (at 130.556 97.7265 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Reference" "U1" (at 3.2385 -2.9845 0) (layer "F.SilkS"))
    (property "Value" "LM335Z" (at 1.27 2.794 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 0) (size 0.89916 1.50114) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-Pad1)") (pinfunction "Adj")
    )
    (pad "2" thru_hole oval (at 1.27 0) (size 0.89916 1.50114) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(R7-Pad1)") (pinfunction "+")
    )
    (pad "3" thru_hole oval (at 2.54 0) (size 0.89916 1.50114) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "-")
    )
    (model "E:/Github_Repositories/packages3d/Package_TO_SOT_THT.3dshapes/TO-92_Inline.step"
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 117.2845 113.4745 -90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "U2" (at 4.7295 0.0635 0 unlocked) (layer "F.SilkS"))
    (property "Value" "AOZ1015AI" (at 0 3.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PGND")
    )
    (pad "2" smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/UB") (pinfunction "VIN")
    )
    (pad "3" smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "AGND")
    )
    (pad "4" smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(R11-Pad1)") (pinfunction "FB")
    )
    (pad "5" smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(R3-Pad2)") (pinfunction "COMP")
    )
    (pad "6" smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/UB") (pinfunction "EN")
    )
    (pad "7" smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(L3-Pad1)") (pinfunction "LX")
    )
    (pad "8" smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(L3-Pad1)") (pinfunction "LX")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 104.6695 97.8535 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C17" (at -0.042 2.667 0 unlocked) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 2.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "1812" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "250V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.125 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 9 "/170V")
    )
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.125 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1812_4532.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric" (layer "F.Cu")
    (at 127.0635 91.059 -90)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R10" (at 3.4925 -2.032 90) (layer "F.SilkS"))
    (property "Value" "0.05E" (at 0 2.28 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "1206" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.25 0 270) (size 1.35 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 5 "Net-(Q1-Pad2)")
    )
    (pad "2" smd roundrect (at 2.25 0 270) (size 1.35 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010_5025Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SMA_Standard" (layer "F.Cu")
    (at 115.189 79.756 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (property "Reference" "D8" (at -4.6355 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "ES1G" (at 0 4.3 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/170V") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D8-Pad2)") (pinfunction "A") (zone_connect 2) (thermal_bridge_width 0.4064)
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA_Standard.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 116.2685 93.726 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R16" (at 0 -1.4605 90 unlocked) (layer "F.SilkS"))
    (property "Value" "8.2K" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C2-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_60" (layer "F.Cu")
    (at 123.24525 95.1215 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C10" (at -2.86575 -0.446 0 unlocked) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C10-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_60" (layer "F.Cu")
    (at 110.617 115.301 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C11" (at -2.649 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "2.7N" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C11-Pad2)")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at 135.5 123)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH2" (at 0 -3.35 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 5 5) (drill 2.7) (layers "*.Mask")
      (solder_mask_margin 1.2) (clearance 1.2)
    )
  )
  (footprint "Diodes_SMD:SMB_Standard" (layer "F.Cu")
    (at 101.6 84.08416 90)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (property "Reference" "D10" (at -3.16484 2.921 0) (layer "F.SilkS"))
    (property "Value" "SMBJ5388B" (at 0.0635 3.302 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "A" (at 4.3815 -0.0635 90) (layer "F.Fab"))
    (fp_text user "K" (at -4.3815 -0.0635 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.14884 0 90) (size 2.49936 2.30124) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/170V") (pinfunction "K")
    )
    (pad "2" smd rect (at 2.14884 0 90) (size 2.49936 2.30124) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB_Standard.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 136.002 114.2365)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R8" (at 0 1.651 0 unlocked) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/CASETEMP")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:Inductor_0630" (layer "F.Cu")
    (at 124.2695 113.538 90)
    (property "Reference" "L3" (at -4.793 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "10µ" (at -0.0635 4.2545 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0630" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "L" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "1" smd rect (at -2.8 0 90) (size 1.9 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(L3-Pad1)") (pinfunction "1")
    )
    (pad "2" smd rect (at 2.8 0 90) (size 1.9 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/5V") (pinfunction "2")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_SMD_CDRH127.STEP"
      (offset (xyz 2.9972 2.921 0.254))
      (scale (xyz 0.5 0.3 0.5))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_95" (layer "F.Cu")
    (at 123.2535 106.771 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C13" (at -3.393 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "16V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 18 "/5V")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1206_3216.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 107.681 91.5035 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R13" (at 0 1.524 0 unlocked) (layer "F.SilkS"))
    (property "Value" "470K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R13-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/170V")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_Tantalum_SMD:Tantalum_Case-D_EIA-7343-31_Reflow" (layer "F.Cu")
    (at 133.9215 91.313 180)
    (descr "Tantalum capacitor, Case D, EIA 7343-31, 7.3x4.3x2.8mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (property "Reference" "C7" (at 2.413 -3.429 0 unlocked) (layer "F.SilkS"))
    (property "Value" "100µ" (at 0 3.9 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "7343" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "16V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CT" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -3.175 0 180) (size 2.55 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN")
    )
    (pad "2" smd rect (at 3.175 0 180) (size 2.55 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_SMD:SMA_Standard" (layer "F.Cu")
    (at 150.114 90.551)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (property "Reference" "D7" (at -0.0635 -2.6035 0 unlocked) (layer "F.SilkS"))
    (property "Value" "SS34" (at 0 4.3 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A") (thermal_bridge_width 0.4064)
    )
    (model "${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA_Standard.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965" locked (layer "F.Cu")
    (at 141.5 77)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Reference" "MH3" (at -3.324 -3.2765 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "Mounting_Hole" (at 0 3.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "" np_thru_hole circle locked (at 0 0) (size 5 5) (drill 2.7) (layers "*.Mask")
      (solder_mask_margin 1.2) (clearance 1.2)
    )
  )
  (footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 121.4755 90.805)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "U3" (at -0.127 -3.683 0 unlocked) (layer "F.SilkS"))
    (property "Value" "MAX1771" (at 0 3.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Q1-Pad1)") (pinfunction "EXT")
    )
    (pad "2" smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN") (pinfunction "VCC")
    )
    (pad "3" smd rect (at -2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(C2-Pad2)") (pinfunction "FB")
    )
    (pad "4" smd rect (at -2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(Q2-Pad3)") (pinfunction "SHDN")
    )
    (pad "5" smd rect (at 2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C10-Pad1)") (pinfunction "REF")
    )
    (pad "6" smd rect (at 2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "AGND")
    )
    (pad "7" smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND")
    )
    (pad "8" smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Q1-Pad2)") (pinfunction "CS")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 112.0775 91.5035 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R15" (at 0 1.4605 0 unlocked) (layer "F.SilkS"))
    (property "Value" "470K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C2-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R13-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal" (layer "F.Cu")
    (at 103.251 112.2045 -90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Reference" "P3" (at -4.826 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "JSTPHMHS-2" (at 0 5.8 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 1.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/170V") (pinfunction "P1")
    )
    (pad "2" smd roundrect (at 1 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "P2")
    )
    (pad "MP" smd roundrect (at -3.35 2.9 270) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333))
    (pad "MP" smd roundrect (at 3.35 2.9 270) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB.STEP"
      (offset (xyz -7.9 12.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 123.19 98.2495 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R6" (at 0 -1.65 -90 unlocked) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(P2-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_95" (layer "F.Cu")
    (at 119.3195 108.1405 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C9" (at 2.797 0 90 unlocked) (layer "F.SilkS"))
    (property "Value" "22µ" (at 0 1.82 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "1206" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "25V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 20 "/UB")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1206_3216.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_95" (layer "F.Cu")
    (at 110.0455 94.0435)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C2" (at 0 1.7145 0) (layer "F.SilkS"))
    (property "Value" "100P" (at 0 1.82 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Case" "1206" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "250V" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 9 "/170V")
    )
    (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 17 "Net-(C2-Pad2)")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/C_1206_3216.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:INDC2012X110" (layer "F.Cu")
    (at 118.9195 102.5525 180)
    (descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
    (property "Reference" "L1" (at -0.016 1.5875 0 unlocked) (layer "F.SilkS"))
    (property "Value" "FB0805" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "1" smd rect (at -1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN")
    )
    (pad "2" smd rect (at 1 0 180) (size 0.95 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/UB")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 131.587 102.6795 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R9" (at 0 1.524 0 unlocked) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/5V")
    )
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R7-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_60" (layer "F.Cu")
    (at 116.1415 89.296 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C8" (at -1.128 -1.4605 90 unlocked) (layer "F.SilkS"))
    (property "Value" "100N" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "Dielectric" "X7R" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "CK" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/UIN")
    )
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012X60.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 135.255 96.647)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Reference" "P2" (at -2.159 2.54 90 unlocked) (layer "F.SilkS"))
    (property "Value" "MA03-1" (at 0 7.41 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 2.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/5V") (pinfunction "P1")
    )
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(P2-Pad2)") (pinfunction "P2")
    )
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/HVON") (pinfunction "P3")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132.1585 114.2365)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R7" (at 0 1.651 0 unlocked) (layer "F.SilkS"))
    (property "Value" "15K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R7-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/CASETEMP")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductors_SMD:CDRH127" (layer "F.Cu")
    (at 132.08 81.7245 180)
    (property "Reference" "L2" (at -6.858 1.397 90 unlocked) (layer "F.SilkS"))
    (property "Value" "100µ" (at 0 0 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Case" "CDRH127" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "L" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "1" smd rect (at 0 -4.95 180) (size 5.4 2.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN") (pinfunction "1")
    )
    (pad "2" smd rect (at 0 4.95 180) (size 5.4 2.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D8-Pad2)") (pinfunction "2")
    )
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_SMD_CDRH127.STEP"
      (offset (xyz -6 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo2_5mm_SilkScreen" locked (layer "F.Cu")
    (at 118.0465 122.7455)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (property "Reference" "REF**" (at 0 -5.08 0) (layer "F.SilkS") hide)
    (property "Value" "KiCad-Logo2_5mm_SilkScreen" (at 0 5.08 0) (layer "F.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
  )
  (footprint "Housings_TO_SOT_SMD:TO-252" (layer "F.Cu")
    (at 121.412 82.167 90)
    (property "Reference" "Q1" (at 6.983 -4.953 0 unlocked) (layer "F.SilkS"))
    (property "Value" "FQD18N20" (at 0 0 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "OrderNo" "497-13749-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Supplier" "Digikey" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (pad "" smd rect (at 1.5625 -1.7375 270) (size 2.457 2.457) (layers "F.Paste"))
    (pad "" smd rect (at 1.5625 1.7375 270) (size 2.457 2.457) (layers "F.Paste"))
    (pad "" smd rect (at 5.0375 -1.7375 270) (size 2.457 2.457) (layers "F.Paste"))
    (pad "" smd rect (at 5.0375 1.7375 270) (size 2.457 2.457) (layers "F.Paste"))
    (pad "1" smd rect (at -3.6 -2.3 270) (size 2.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Q1-Pad1)") (pinfunction "G")
    )
    (pad "2" smd rect (at -3.6 2.3 270) (size 2.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Q1-Pad2)") (pinfunction "S")
    )
    (pad "3" smd rect (at 3.3 0 270) (size 6.95 6.95) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(D8-Pad2)") (pinfunction "D") (clearance 0.508)
    )
    (model "${KISYS3DMOD}/Housings_TO_SOT.3dshapes/TO-252-2.step"
      (offset (xyz 1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 114.8865 100.0125)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R5" (at 2.398 0 90 unlocked) (layer "F.SilkS"))
    (property "Value" "3.9K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Case" "0805" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "Tolerance" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "R" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND")
    )
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/U170V")
    )
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse_Holders_and_Fuses:Littelfuse_Nano2_1808_Fuse_Holder_SMD" (layer "F.Cu")
    (at 141.986 87.386 -90)
    (property "Reference" "FH1" (at -6.487 -0.0635 0 unlocked) (layer "F.SilkS"))
    (property "Value" "FH1808" (at 0 -0.4064 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Case" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "P_or_V" "_" (at 0 0 0) (layer "F.Fab") hide)
    (property "WIO_Prefix" "_" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "E:/Projects_local/001.YANC/Hardware/001.04.010.1020_compact/001.04.010.1020.kicad_sch")
    (attr through_hole)
    (pad "1" smd rect (at -3.185 0 270) (size 4.24 3.81) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(FH1-Pad1)")
    )
    (pad "2" smd rect (at 3.185 0 270) (size 4.24 3.81) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/UIN")
    )
    (model "E:/Repository_local/KiCad/3Dmodels/Fuse_Holders_and_Fuses.3dshapes/Littelfuse_OMNI-BLOK.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 158 93) (end 158 74.5)
    (layer "Edge.Cuts"))
  (gr_line (start 157 73.5) (end 99 73.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 157 73.5) (mid 157.707107 73.792893) (end 158 74.5)
    (layer "Edge.Cuts"))
  (gr_line (start 140 94) (end 157 94)
    (layer "Edge.Cuts"))
  (gr_arc (start 139 95) (mid 139.292893 94.292893) (end 140 94)
    (layer "Edge.Cuts"))
  (gr_line (start 138 126.5) (end 99 126.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 99 126.5) (mid 98.292893 126.207107) (end 98 125.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 139 125.5) (mid 138.707107 126.207107) (end 138 126.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 98 74.5) (mid 98.292893 73.792893) (end 99 73.5)
    (layer "Edge.Cuts"))
  (gr_line (start 139 125.5) (end 139 95)
    (layer "Edge.Cuts"))
  (gr_line (start 98 74.5) (end 98 125.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 158 93) (mid 157.707107 93.707107) (end 157 94)
    (layer "Edge.Cuts"))
  (gr_text "YANC PS" (at 108.0135 103.1875 0) (layer "F.SilkS"))
  (gr_text "1" (at 137.541 96.647 0) (layer "F.SilkS"))
  (gr_text "M" (at 137.541 101.727 0) (layer "F.SilkS"))
  (gr_text "WorldInOne M.Straub (C) 2020" (at 99.695 97.8535 270) (layer "F.SilkS"))
  (gr_text "V7.0" (at 107.95 105.156 0) (layer "F.SilkS"))
  (gr_text "750mA" (at 145.6055 88.7095 90) (layer "F.SilkS"))
  (gr_text "X reference" (at 150 64.1985 0) (layer "User.1"))
  (gr_text "Y reference" (at 167 99.75 0) (layer "User.1"))
  (dimension (type orthogonal) (layer "User.1")
    (pts (xy 101.5 123) (xy 163 100))
    (height 60)
    (orientation 1)
    (gr_text "23.0 mm" (at 161.5 111.5 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1524) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1")
    (pts (xy 101.5 77) (xy 135.5 123))
    (height 53.5)
    (orientation 0)
    (gr_text "34.0 mm" (at 118.5 130.5 0) (layer "User.1"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1524) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1")
    (pts (xy 101.5 77) (xy 161.5 100))
    (height 60)
    (orientation 1)
    (gr_text "23.0 mm" (at 161.5 88.5 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1524) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5))
  )
  (dimension (type orthogonal) (layer "User.1")
    (pts (xy 135.5 123) (xy 150 129.5))
    (height 7.5)
    (orientation 0)
    (gr_text "14.5 mm" (at 142.75 130.5 0) (layer "User.1"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1524) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1")
    (pts (xy 141.5 77) (xy 150 65.25))
    (height -8.5)
    (orientation 0)
    (gr_text "8.5 mm" (at 145.75 68.5 0) (layer "User.1"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1524) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 21) (net_name "Net-(L3-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 126.365 117.602)
        (xy 117.2845 117.602)
        (xy 117.2845 115.062)
        (xy 126.365 115.062)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D8-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 134.6835 78.105)
        (xy 122.4915 78.105)
        (xy 122.4915 79.5655)
        (xy 119.9515 79.5655)
        (xy 119.937989 79.254902)
        (xy 114.098719 79.197457)
        (xy 114.11223 75.507555)
        (xy 134.6835 75.438)
      )
    )
  )
  (zone (net 5) (net_name "Net-(Q1-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 124.333 88.3285)
        (xy 128.055671 88.3285)
        (xy 128.067585 89.3445)
        (xy 123.063 89.3445)
        (xy 123.063 85.598)
        (xy 124.333 85.598)
      )
    )
  )
  (zone (net 4) (net_name "Net-(FH1-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 146.7 85.651)
        (xy 141.7955 85.6615)
        (xy 141.7955 82.677)
        (xy 146.7 82.651)
      )
    )
  )
  (zone (net 9) (net_name "/170V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 116.332003 83.185)
        (xy 109.7915 83.185)
        (xy 109.7915 86.5505)
        (xy 102.9335 86.5505)
        (xy 102.9335 87.63)
        (xy 100.2665 87.63)
        (xy 100.2665 84.836)
        (xy 107.2515 84.836)
        (xy 107.2515 80.3275)
        (xy 116.332003 80.3275)
      )
    )
  )
  (zone (net 20) (net_name "/UB") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 118.5545 111.727)
        (xy 117.2845 111.727)
        (xy 117.2845 101.672221)
        (xy 118.5545 101.672221)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.649 99.288422)
        (xy 108.0135 99.288422)
        (xy 108.0135 90.000999)
        (xy 112.649 90.000999)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.9195 82.8675)
        (xy 116.6495 82.8675)
        (xy 116.6495 79.9465)
        (xy 117.9195 79.9465)
      )
    )
  )
  (zone (net 6) (net_name "Net-(Q1-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 119.761 89.3445)
        (xy 117.856 89.3445)
        (xy 117.856 88.3285)
        (xy 118.491 88.3285)
        (xy 118.491 85.471)
        (xy 119.761 85.471)
      )
    )
  )
  (zone (net 10) (net_name "/UIN") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 137.668 88.3285)
        (xy 144.0815 88.265)
        (xy 144.0815 92.837)
        (xy 133.2865 92.9005)
        (xy 133.2865 88.3285)
        (xy 129.2225 88.265)
        (xy 129.286 85.0265)
        (xy 137.668 85.0265)
      )
    )
  )
  (zone (net 18) (net_name "/5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 127.381 112.0445)
        (xy 122.047 112.0445)
        (xy 122.047 107.282)
        (xy 127.381 107.282)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 157.2 126.5)
        (xy 98 126.5)
        (xy 98 73.5)
        (xy 158 73.5)
      )
    )
  )
)
