(kicad_pcb (version 20210722) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Lora - RS485 bridge")
    (date "2019-11-05")
    (rev "1.1")
    (company "Albertas Mickenas")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 85 143)
    (grid_origin 85 143)
    (pcbplotparams
      (layerselection 0x00010f8_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "manufacturing/gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(Q7-Pad1)")
  (net 3 "+3V3")
  (net 4 "/VOUT")
  (net 5 "/SWD_IO")
  (net 6 "/SWD_CLK")
  (net 7 "/~{MCU_RST}")
  (net 8 "/RX")
  (net 9 "/TX")
  (net 10 "/D+")
  (net 11 "/D-")
  (net 12 "/I2C_SCL")
  (net 13 "/I2C_SDA")
  (net 14 "+BATT")
  (net 15 "VBUS")
  (net 16 "/VIN")
  (net 17 "/A")
  (net 18 "/B")
  (net 19 "Net-(J9-Pad4)")
  (net 20 "/~{RS485_RE}")
  (net 21 "/~{I2C_ENABLE}")
  (net 22 "/RS485_DE")
  (net 23 "Net-(SW1-Pad2)")
  (net 24 "Net-(U4-Pad4)")
  (net 25 "/ANTENNA")
  (net 26 "/BATT_MON")
  (net 27 "/VOUT_1")
  (net 28 "Net-(Q1-Pad1)")
  (net 29 "Net-(J5-Pad4)")
  (net 30 "Net-(J5-Pad5)")
  (net 31 "Net-(D6-Pad2)")
  (net 32 "Net-(D7-Pad2)")
  (net 33 "Net-(D8-Pad2)")
  (net 34 "/LED1")
  (net 35 "/LED2")
  (net 36 "/LED3")
  (net 37 "Net-(Q2-Pad1)")
  (net 38 "Net-(J5-Pad1)")
  (net 39 "/RS485_ENABLE")
  (net 40 "Net-(D5-Pad1)")
  (net 41 "Net-(D2-Pad1)")
  (net 42 "Net-(U5-Pad34)")
  (net 43 "Net-(U5-Pad21)")
  (net 44 "/A1")
  (net 45 "/RF")
  (net 46 "/MOSI")
  (net 47 "/SS")
  (net 48 "/SCK")
  (net 49 "/MISO")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 89.4 119.6 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R1" (at 0 2.4 90) (layer "F.SilkS"))
    (fp_text value "1k" (at -1.3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/~{MCU_RST}"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "F.Cu")
    (tedit 5CA1CA7F)
    (at 138 117 -90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "SW1" (at -0.1 0 90) (layer "F.SilkS"))
    (fp_text value "SW_Test" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.1 -2.3 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 3.975 -2.25 270) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1"))
    (pad "1" smd rect locked (at -3.975 -2.25 270) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1"))
    (pad "2" smd rect locked (at -3.975 2.25 270) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(SW1-Pad2)") (pinfunction "2"))
    (pad "2" smd rect locked (at 3.975 2.25 270) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(SW1-Pad2)") (pinfunction "2"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 110 126.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C6" (at 2.3 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 91 119.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -2.9 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 1.3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/~{MCU_RST}"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "miceuz-lib:TC2030-MCP-NL" (layer "F.Cu")
    (tedit 5A0DBC9A)
    (at 92 134.8 180)
    (property "DNP" "DNP")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J5" (at 1.1 -2.4) (layer "F.SilkS") hide)
    (fp_text value "SWD" (at 0 0) (layer "F.SilkS") hide)
    (pad "" np_thru_hole circle locked (at 5.08 1.016 180) (size 0.889 0.889) (drill 0.889) (layers *.Cu))
    (pad "" np_thru_hole circle locked (at 5.08 -1.016 180) (size 0.889 0.889) (drill 0.889) (layers *.Cu))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 0.889 0.889) (drill 0.889) (layers *.Cu))
    (pad "1" smd circle locked (at 1.27 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 38 "Net-(J5-Pad1)") (pinfunction "Pin_1"))
    (pad "2" smd circle locked (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 5 "/SWD_IO") (pinfunction "Pin_2"))
    (pad "3" smd circle locked (at 2.54 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 6 "/SWD_CLK") (pinfunction "Pin_3"))
    (pad "4" smd circle locked (at 2.54 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 29 "Net-(J5-Pad4)") (pinfunction "Pin_4"))
    (pad "5" smd circle locked (at 3.81 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 30 "Net-(J5-Pad5)") (pinfunction "Pin_5"))
    (pad "6" smd circle locked (at 3.81 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_6"))
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 145 115)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 88 115)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 109.2 129.1 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C14" (at 0.4 -1.3 90) (layer "F.SilkS"))
    (fp_text value "1u" (at -1.3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 112 116 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D7" (at 2.3 0 90) (layer "F.SilkS"))
    (fp_text value "LED" (at -1.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D7-Pad2)") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 121.201034 116 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D8" (at 2.3 0 90) (layer "F.SilkS"))
    (fp_text value "LED" (at -1.5 0.001034 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D8-Pad2)") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 114.800136 116.074626 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R13" (at -2.7 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.274626 -0.000136 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/LED1"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D6-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 110.332885 116 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R14" (at -2.7 0.025 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.3 -0.032885 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/LED2"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D7-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 119.555585 116 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R15" (at -2.7 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.2 0.044415 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/LED3"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D8-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 116.463828 116 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D6" (at 2.3 0 90) (layer "F.SilkS"))
    (fp_text value "LED" (at -1.5 -0.036172 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D6-Pad2)") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "miceuz-lib:catnip" (layer "F.Cu")
    (tedit 0)
    (at 124.7 116.1)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 126.1 133.9125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Comment" "Generic X5R capacitor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "C12" (at 5.6 0 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 0.0125 0.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 129.58 130.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Manufacturer" "TDK")
    (property "PartNo" "C1608X5R1C475K080AE")
    (property "Sheet file" "voltage-regulation.kicad_sch")
    (property "Sheet name" "voltage-regulation")
    (attr smd)
    (fp_text reference "C11" (at 0.124 -4.8) (layer "F.SilkS"))
    (fp_text value "4.7u" (at 1.52 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5F776153)
    (at 121.9 126.6 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Manufacturer" "ON SEMICONDUCTOR")
    (property "PartNo" "NTR4003NT1G")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "Q2" (at -1.5 -1.4 180) (layer "F.SilkS"))
    (fp_text value "NTR4003" (at 1.1 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1 0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(Q2-Pad1)") (pinfunction "G"))
    (pad "2" smd rect locked (at 1 -0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S"))
    (pad "3" smd rect locked (at -1 0 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(Q1-Pad1)") (pinfunction "D"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 108.5 135.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "R7" (at 0 -2.7) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 0.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/VOUT"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/I2C_SCL"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 117.9 126.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "R8" (at 2.2 0) (layer "F.SilkS"))
    (fp_text value "1M" (at -1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(Q1-Pad1)"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+BATT"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-2.54mm_4pol" locked (layer "F.Cu")
    (tedit 59FF0755)
    (at 107.26 139.6)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J3" (at 3.84 -1.8) (layer "F.SilkS"))
    (fp_text value "i2c" (at 3.81 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -1.5) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "/VOUT") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "/I2C_SCL") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 "/I2C_SDA") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4"))
    (model "${KIPRJMOD}/pxc_1725737_05_MPT-0-5-10-2-54_3D.stp"
      (offset (xyz -1.5 -3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
    (model "${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO_SOT_Packages_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F775D19)
    (at 129.98 128.05)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Manufacturer" "ON SEMICONDUCTOR")
    (property "PartNo" "NCP718ASN330T1G")
    (property "Sheet file" "voltage-regulation.kicad_sch")
    (property "Sheet name" "voltage-regulation")
    (attr smd)
    (fp_text reference "U4" (at -2.38 -0.05 270) (layer "F.SilkS"))
    (fp_text value "NCP718" (at -1.28 0.05 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+BATT") (pinfunction "Vin"))
    (pad "2" smd rect locked (at 1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "3" smd rect locked (at 1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+BATT") (pinfunction "~SHDN"))
    (pad "4" smd rect locked (at -1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U4-Pad4)") (pinfunction "NC"))
    (pad "5" smd rect locked (at -1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "Vout"))
    (model "${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 104.7 134.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Comment" "Generic 5% resistor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "R9" (at -2.4 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/RS485_DE"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5F776133)
    (at 117.9 128.6 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Comment" "Exact as specified")
    (property "Distributor" "1894738")
    (property "Manufacturer" "NXP")
    (property "PartNo" "NX2301P,215 ")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.5 180) (layer "F.SilkS"))
    (fp_text value "NX2301P" (at 1.1 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1 0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(Q1-Pad1)") (pinfunction "G"))
    (pad "2" smd rect locked (at 1 -0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+BATT") (pinfunction "S"))
    (pad "3" smd rect locked (at -1 0 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/VOUT_1") (pinfunction "D"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 121.8 124.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "R16" (at 2.7 0) (layer "F.SilkS"))
    (fp_text value "1M" (at -1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/RS485_ENABLE"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "miceuz-lib:SC89" (layer "F.Cu")
    (tedit 5F775AEB)
    (at 111 135.2 90)
    (property "Manufacturer" "ON SEMICONDUCTOR")
    (property "PartNo" " NZL5V6AXV3T1G")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "D9" (at 0 1.6 90) (layer "F.SilkS"))
    (fp_text value "5V6" (at -1.7 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0.57 0.5 180) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/I2C_SDA") (pinfunction "A1"))
    (pad "2" smd rect locked (at 0.57 -0.5 180) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/I2C_SCL") (pinfunction "A2"))
    (pad "3" smd rect locked (at -0.57 0 180) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "common"))
    (model "/home/miceuz/Xaltura/zive/electronics/3d/User Library-FDY102PZ.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5F775FA9)
    (at 103.6 141 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Comment" "Exact as specified")
    (property "Distributor" "1894738")
    (property "Manufacturer" "NXP")
    (property "PartNo" "NX2301P,215 ")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "Q7" (at -2.4 0 270) (layer "F.SilkS"))
    (fp_text value "NX2301P" (at 1.1 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1 0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(Q7-Pad1)") (pinfunction "G"))
    (pad "2" smd rect locked (at 1 -0.95 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "S"))
    (pad "3" smd rect locked (at -1 0 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/VOUT") (pinfunction "D"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 132.98 129.85 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Manufacturer" "TDK")
    (property "PartNo" "C1608X5R1C475K080AE")
    (property "Sheet file" "voltage-regulation.kicad_sch")
    (property "Sheet name" "voltage-regulation")
    (attr smd)
    (fp_text reference "C7" (at -0.55 -1.32 90) (layer "F.SilkS"))
    (fp_text value "4.7u" (at 1.55 -0.02 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+BATT"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 126.1 130.9125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Comment" "Generic 5% resistor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "R3" (at 4.8 0 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/~{RS485_RE}"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 103.699999 138.499999 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "R4" (at 2.3 0) (layer "F.SilkS"))
    (fp_text value "1M" (at -1.300001 -0.000001) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/~{I2C_ENABLE}"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-2.54mm_2pol" locked (layer "F.Cu")
    (tedit 5EBC122F)
    (at 127.58 139.6)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J1" (at 1.32 -1.9) (layer "F.SilkS"))
    (fp_text value "battery" (at 1.52 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.52 -1.5) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 16 "/VIN") (pinfunction "Pin_2"))
    (model "${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 133.389762 126.85 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Manufacturer" "TDK")
    (property "PartNo" "C1608X5R1C475K080AE")
    (property "Sheet file" "voltage-regulation.kicad_sch")
    (property "Sheet name" "voltage-regulation")
    (attr smd)
    (fp_text reference "C16" (at -0.25 1.22 90) (layer "F.SilkS"))
    (fp_text value "4.7u" (at 1.55 0.010238 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+BATT"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5F775CBA)
    (at 122.6 132.4 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Distributor" "2542747")
    (property "Manufacturer" "TEXAS INSTRUMENTS")
    (property "PartNo" "SN65HVD72DR")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "U1" (at 3.1 0 270) (layer "F.SilkS"))
    (fp_text value "SN65HVD72" (at 2.8 0 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.905 2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/RX") (pinfunction "RO"))
    (pad "2" smd roundrect locked (at -0.635 2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/~{RS485_RE}") (pinfunction "~RE~"))
    (pad "3" smd roundrect locked (at 0.635 2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/RS485_DE") (pinfunction "DE"))
    (pad "4" smd roundrect locked (at 1.905 2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/TX") (pinfunction "DI"))
    (pad "5" smd roundrect locked (at 1.905 -2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "6" smd roundrect locked (at 0.635 -2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/A") (pinfunction "A"))
    (pad "7" smd roundrect locked (at -0.635 -2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/B") (pinfunction "B"))
    (pad "8" smd roundrect locked (at -1.905 -2.475 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VCC"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 108.5 133.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "R6" (at 0 -2.6) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/VOUT"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/I2C_SDA"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 88 139.9)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-2.54mm_4pol" locked (layer "F.Cu")
    (tedit 59FF0755)
    (at 117.42 139.6)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J4" (at 3.98 -1.8) (layer "F.SilkS"))
    (fp_text value "rs485" (at 3.78 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.68 -1.5) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 27 "/VOUT_1") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 17 "/A") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 18 "/B") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4"))
    (model "${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-2.54mm_4pol.wrl"
      (offset (xyz 3.809999943 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "F.Cu")
    (tedit 5CA1CA7F)
    (at 88.3 126.1 90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "SW2" (at 0 0.1 90) (layer "F.SilkS"))
    (fp_text value "SW_Reset" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1"))
    (pad "1" smd rect locked (at 3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1"))
    (pad "2" smd rect locked (at 3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/~{MCU_RST}") (pinfunction "2"))
    (pad "2" smd rect locked (at -3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/~{MCU_RST}") (pinfunction "2"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 124.5 124.9 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "rs485-interface.kicad_sch")
    (property "Sheet name" "RS485-interface")
    (attr smd)
    (fp_text reference "R10" (at -2.6 0.1 90) (layer "F.SilkS"))
    (fp_text value "150" (at 1.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(Q2-Pad1)"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/RS485_ENABLE"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 116.3 133.09 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C13" (at -0.01 -2.2 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 1.29 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/BATT_MON"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 117.8 133.1 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R12" (at 0 2.6 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -1.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/BATT_MON"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 118.2 135.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R11" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "20k" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/VOUT_1"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/BATT_MON"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 132.6 133.7 -90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Manufacturer" "Littlefuse")
    (property "PartNo" "SMF11A")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "D5" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "SMF11A" (at 0 1.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.9 0.5 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(D5-Pad1)") (pinfunction "A1"))
    (pad "2" smd rect locked (at 1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A2"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 145 139.9)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H2" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7)
    (at 135.08 133.7 -90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Manufacturer" "Diodes Inc")
    (property "PartNo" "1N4148W-7-F")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "D3" (at -3.1 0 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0 1.18 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.9 0.48 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.65 0 270) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+BATT") (pinfunction "K"))
    (pad "2" smd rect locked (at 1.65 0 270) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connectors_USB:USB_Micro-B_Vertical_Molex-105133-0001" (layer "F.Cu")
    (tedit 5E73B4E8)
    (at 137.3 140.225)
    (descr "Molex Vertical Micro USB Typ-B (http://www.molex.com/pdm_docs/sd/1051330001_sd.pdf)")
    (tags "Micro-USB SMD Typ-B Vertical")
    (property "Manufacturer" "MOLEX")
    (property "PartNo" "1051330011")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J9" (at 5 -0.025) (layer "F.SilkS"))
    (fp_text value "USB micro" (at -0.025 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.375) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.3 -0.825) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "VBUS"))
    (pad "2" smd rect locked (at -0.65 -0.825) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/D-") (pinfunction "D-"))
    (pad "3" smd rect locked (at 0 -0.825) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/D+") (pinfunction "D+"))
    (pad "4" smd rect locked (at 0.65 -0.825) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J9-Pad4)") (pinfunction "ID"))
    (pad "5" smd rect locked (at 1.3 -0.825) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "6" thru_hole oval locked (at 0 1.075) (size 2.2 1.1) (drill oval 1.6 0.5) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "Shield"))
    (pad "6" thru_hole oval locked (at -2.8 -1.075) (size 1.8 1.1) (drill oval 1.2 0.5) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "Shield"))
    (pad "6" thru_hole oval locked (at 2.8 -1.075) (size 1.8 1.1) (drill oval 1.2 0.5) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "Shield"))
    (model "${KIPRJMOD}/3d/1051330011.stp"
      (offset (xyz 0 0 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "miceuz-lib:SC89" (layer "F.Cu")
    (tedit 5F775AEB)
    (at 135.15 137.1)
    (property "Manufacturer" "ON SEMICONDUCTOR")
    (property "PartNo" " NZL5V6AXV3T1G")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D1" (at 0 3.85 180) (layer "F.SilkS"))
    (fp_text value "5V6" (at 0.1 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0.57 0.5 90) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "A1"))
    (pad "2" smd rect locked (at 0.57 -0.5 90) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "A2"))
    (pad "3" smd rect locked (at -0.57 0 90) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "common"))
    (model "/home/miceuz/Xaltura/zive/electronics/3d/User Library-FDY102PZ.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "miceuz-lib:SC89" (layer "F.Cu")
    (tedit 5F775AEB)
    (at 137.15 137.076584 -90)
    (property "Manufacturer" "ON SEMICONDUCTOR")
    (property "PartNo" " NZL5V6AXV3T1G")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D4" (at 3.45 0.023416 90) (layer "F.SilkS"))
    (fp_text value "5V6" (at 0.723416 0.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.1 0.1) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0.57 0.5) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/D-") (pinfunction "A1"))
    (pad "2" smd rect locked (at 0.57 -0.5) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/D+") (pinfunction "A2"))
    (pad "3" smd rect locked (at -0.57 0) (size 0.5 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "common"))
    (model "/home/miceuz/Xaltura/zive/electronics/3d/User Library-FDY102PZ.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5F776113)
    (at 138.143138 132.855373)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Comment" "Exact as specified")
    (property "Distributor" "1894738")
    (property "Manufacturer" "NXP")
    (property "PartNo" "NX2301P,215 ")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "Q3" (at 2.25 -0.62 90) (layer "F.SilkS"))
    (fp_text value "NX2301P" (at -1.08 0.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "G"))
    (pad "2" smd rect locked (at 1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(D2-Pad1)") (pinfunction "S"))
    (pad "3" smd rect locked (at -1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(D5-Pad1)") (pinfunction "D"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5F7760E5)
    (at 136.88 129.15)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Comment" "Exact as specified")
    (property "Distributor" "1894738")
    (property "Manufacturer" "NXP")
    (property "PartNo" "NX2301P,215 ")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "Q4" (at 0.12 -2.15) (layer "F.SilkS"))
    (fp_text value "NX2301P" (at -0.98 0.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 0.1 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 1.1 1.05 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "G"))
    (pad "2" smd rect locked (at 1.1 -0.85 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(D2-Pad1)") (pinfunction "S"))
    (pad "3" smd rect locked (at -0.9 0.1 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+BATT") (pinfunction "D"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 140.68 132.85 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1M" (at -1.35 -0.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D2-Pad1)"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "VBUS"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 140.2 127.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "R24" (at 0 1.4) (layer "F.SilkS"))
    (fp_text value "1M" (at -1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "VBUS"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 103.7 136.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "i2c-interface.kicad_sch")
    (property "Sheet name" "I2C-interface")
    (attr smd)
    (fp_text reference "R5" (at 2.300001 0.000001) (layer "F.SilkS"))
    (fp_text value "150" (at -1.4 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Q7-Pad1)"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/~{I2C_ENABLE}"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 130.2 133.7 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Manufacturer" "TECHFUSE")
    (property "PartNo" "nSMD075-13.2V")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "TH1" (at 0 -1.6 90) (layer "F.SilkS"))
    (fp_text value "Thermistor_PTC" (at 0 -1.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 90) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 16 "/VIN"))
    (pad "2" smd roundrect locked (at 1.4 0 90) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 40 "Net-(D5-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 87.2 132)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R25" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SWD_CLK"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tedit 58641739)
    (at 140.88 129.65 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Manufacturer" "ON SEMI")
    (property "PartNo" "MM3Z7V5ST1G")
    (property "Sheet file" "battery-protection.kicad_sch")
    (property "Sheet name" "battery-protection")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.4 90) (layer "F.SilkS"))
    (fp_text value "7.6V" (at -0.05 1.12 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 -1.18 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(D2-Pad1)") (pinfunction "K"))
    (pad "2" smd rect locked (at 1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "VBUS") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducials:Fiducial_1mm_Dia_2mm_Outer" (layer "F.Cu")
    (tedit 59FE003E)
    (at 144.1 119.1)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "FID1" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "~" smd circle locked (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducials:Fiducial_1mm_Dia_2mm_Outer" (layer "F.Cu")
    (tedit 61045879)
    (at 86.3 141.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "FID2" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "~" smd circle locked (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5))
  )
  (footprint "miceuz-lib:SMA_6.35_EdgeMount" locked (layer "F.Cu")
    (tedit 5E21D115)
    (at 97 140.9 -90)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Comment" "Can be replaced with compatible footprint connector specified up to 3GHz, VSWR < 1.2")
    (property "Manufacturer" "RF Solutions")
    (property "PartNo" "CON-SMA-EDGE-S")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J2" (at 0 4.7 90) (layer "F.SilkS"))
    (fp_text value "ANT" (at 0.2 0.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0.15 0) (size 1.27 3.7) (layers "F.Cu" "F.Mask")
      (net 25 "/ANTENNA") (pinfunction "Pin_1"))
    (pad "2" smd rect locked (at 0 2.825) (size 1.35 4.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_2"))
    (pad "2" smd rect locked (at 0 -2.825) (size 1.35 4.2) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_2"))
    (pad "2" smd rect locked (at 0 -2.825) (size 1.35 4.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_2"))
    (pad "2" smd rect locked (at 0 2.825) (size 1.35 4.2) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_2"))
    (model "${KIPRJMOD}/SMA-J-P-H-ST-EM1.STP--3DModel-STEP-66336.STEP"
      (offset (xyz 4 0 0.55))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (footprint "miceuz-lib:RAK4260-footprint_w_solder_paste" (layer "F.Cu")
    (tedit 5F69EDF3)
    (at 100 125.3 90)
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U5" (at 8.2 6.7 180) (layer "F.SilkS"))
    (fp_text value "RAK4260" (at 0 -0.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 -0.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -7.5 -4.22 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "2" smd roundrect locked (at -7.5 -3.02 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/RF") (pinfunction "RFC"))
    (pad "3" smd roundrect locked (at -7.5 -1.82 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "4" smd roundrect locked (at -7.5 -0.62 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/~{I2C_ENABLE}") (pinfunction "PA27"))
    (pad "5" smd roundrect locked (at -7.5 0.58 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/A1") (pinfunction "PA06"))
    (pad "6" smd roundrect locked (at -7.5 1.78 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/BATT_MON") (pinfunction "PA07"))
    (pad "7" smd roundrect locked (at -7.5 2.98 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/~{RS485_RE}") (pinfunction "PA08"))
    (pad "8" smd roundrect locked (at -7.5 4.18 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/RS485_DE") (pinfunction "PA09"))
    (pad "9" smd roundrect locked (at -7.5 5.38 90) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/LED3") (pinfunction "PB22"))
    (pad "10" smd roundrect locked (at -4.2 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "11" smd roundrect locked (at -3 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VCC3V3"))
    (pad "12" smd roundrect locked (at -1.8 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VCC3V3"))
    (pad "13" smd roundrect locked (at -0.6 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/I2C_SCL") (pinfunction "PA17_SCL"))
    (pad "14" smd roundrect locked (at 0.6 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/I2C_SDA") (pinfunction "PA16_SDA"))
    (pad "15" smd roundrect locked (at 1.8 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/RS485_ENABLE") (pinfunction "PA15"))
    (pad "16" smd roundrect locked (at 3 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(SW1-Pad2)") (pinfunction "PA14"))
    (pad "17" smd roundrect locked (at 4.2 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "18" smd roundrect locked (at 5.4 7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "19" smd roundrect locked (at 7.5 4.25 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/LED1") (pinfunction "PA18_UART3_RX"))
    (pad "20" smd roundrect locked (at 7.5 3.05 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/LED2") (pinfunction "PA19_UART3_TX"))
    (pad "21" smd roundrect locked (at 7.5 1.85 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(U5-Pad21)") (pinfunction "NC"))
    (pad "22" smd roundrect locked (at 7.5 0.65 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/MISO") (pinfunction "PA23_MOSI"))
    (pad "23" smd roundrect locked (at 7.5 -0.55 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/SS") (pinfunction "PA22_SS"))
    (pad "24" smd roundrect locked (at 7.5 -1.75 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/SCK") (pinfunction "PB23_SCK"))
    (pad "25" smd roundrect locked (at 7.5 -2.95 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/MOSI") (pinfunction "PB02_MISO"))
    (pad "26" smd roundrect locked (at 7.5 -4.15 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/D+") (pinfunction "PA25_USB_P"))
    (pad "27" smd roundrect locked (at 7.5 -5.35 270) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/D-") (pinfunction "PA24_USB_N"))
    (pad "28" smd roundrect locked (at 4.06 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "29" smd roundrect locked (at 2.86 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/~{MCU_RST}") (pinfunction "RST"))
    (pad "30" smd roundrect locked (at 1.66 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SWD_CLK") (pinfunction "PA30_SWDCLK"))
    (pad "31" smd roundrect locked (at 0.46 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SWD_IO") (pinfunction "PA31_SWDIO"))
    (pad "32" smd roundrect locked (at -0.74 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/TX") (pinfunction "PA04_UART1_TX"))
    (pad "33" smd roundrect locked (at -1.94 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/RX") (pinfunction "PA05_UART1_RX"))
    (pad "34" smd roundrect locked (at -3.14 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(U5-Pad34)") (pinfunction "NC"))
    (pad "35" smd roundrect locked (at -4.34 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "36" smd roundrect locked (at -5.54 -7.5 180) (size 0.95 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "37" smd rect locked (at -5.85 6.48 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (solder_paste_margin -0.1))
    (pad "37" smd rect locked (at -6.61 -5.71 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (solder_paste_margin -0.1))
    (pad "37" smd rect locked (at 6.6 5.85 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (solder_paste_margin -0.1))
    (pad "37" smd rect locked (at 5.83 -6.47 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (solder_paste_margin -0.1))
    (model "${KIPRJMOD}/3d/RAK4260.STEP"
      (offset (xyz -8.72 -11.4 -16.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 97.1 136.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C2" (at -2.2 0.1 90) (layer "F.SilkS"))
    (fp_text value "47p" (at -1.4 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/RF"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/ANTENNA"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm" (layer "F.Cu")
    (tedit 59650532)
    (at 103.98 114.8 -90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheet file" "/home/miceuz/Xaltura/LoRaNode/LoRaNode.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J6" (at 0 -2.33 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x05_Female" (at -1.8 5.28 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/A1") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/MISO") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/SS") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/SCK") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/MOSI") (pinfunction "Pin_5"))
    (model "${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbols:OSHW-Logo2_9.8x8mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 89.8 125.9)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo2_9.8x8mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Symbols:ESD-Logo_6.6x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 130.8 115.9)
    (descr "Electrostatic discharge Logo")
    (tags "Logo ESD")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "ESD-Logo_6.6x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Symbols:CE-Logo_8.5x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 122.6 116)
    (descr "CE marking")
    (tags "Logo CE certification")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "CE-Logo_8.5x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (gr_line (start 148 112) (end 85 112) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 85 143) (end 148 143) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 148 143) (end 148 112) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 85 112) (end 85 143) (layer "Edge.Cuts") (width 0.05))
  (gr_text "MISO" (at 101.4 116 270) (layer "B.SilkS"))
  (gr_text "Current:\n0.1A max" (at 111.1 132.3 180) (layer "B.SilkS"))
  (gr_text "Current:\n0.5A max" (at 121.4 132.3 180) (layer "B.SilkS"))
  (gr_text "VIN\n4-12V" (at 128.9 132.3 180) (layer "B.SilkS"))
  (gr_text "B" (at 122.5 138.2 90) (layer "B.SilkS"))
  (gr_text "A" (at 119.9 138.2 90) (layer "B.SilkS"))
  (gr_text "VIN" (at 130.2 138.2 90) (layer "B.SilkS"))
  (gr_text "GND" (at 125.1 138.2 90) (layer "B.SilkS"))
  (gr_text "GND" (at 127.6 138.2 90) (layer "B.SilkS"))
  (gr_text "Catnip electronics\nMindaugo 25\n03011 Vilnius\nLithuania\ninfo@catnip.lt" (at 146.4 121.6 180) (layer "B.SilkS"))
  (gr_text "A1" (at 103.8 116 270) (layer "B.SilkS"))
  (gr_text "SS" (at 98.8 116.1 270) (layer "B.SilkS"))
  (gr_text "SCK" (at 96.2 116.1 270) (layer "B.SilkS"))
  (gr_text "MOSI" (at 93.8 116 270) (layer "B.SilkS"))
  (gr_text "https://github.com/miceuz/LoRaNode\nhttps://www.tindie.com/stores/miceuz/" (at 94.7 123.9 180) (layer "B.SilkS"))
  (gr_text "RoHS\ncompliant" (at 134.7 114.4 180) (layer "B.SilkS"))
  (gr_text "RST" (at 88.3 130.3) (layer "F.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 99.7 129.9) (layer "F.SilkS"))
  (gr_text "BATT" (at 121 113.3) (layer "F.SilkS"))
  (gr_text "SENS" (at 116.5 113.3) (layer "F.SilkS"))
  (gr_text "LoRa-RS485/I2C node v2.0\n2020-05-13\n" (at 146.4 127.4 90) (layer "F.SilkS"))
  (gr_text "WAN" (at 112 113.3) (layer "F.SilkS"))
  (gr_text "CATNIP\nELECTRONICS\n" (at 127.3 116.3) (layer "F.SilkS"))
  (gr_text "TEST" (at 137.9 122.8) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 148 112) (xy 148 143))
    (height -12.5)
    (gr_text "31.0 mm" (at 159.35 127.5 90) (layer "Cmts.User"))
    (format (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 148 143) (xy 85 143))
    (height -13.8)
    (gr_text "63.0 mm" (at 116.5 155.65) (layer "Cmts.User"))
    (format (units 2) (units_format 1) (precision 1))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 143)
        (xy 85 143)
        (xy 85 112)
        (xy 148 112)
      )
    )
  )
  (zone (net 3) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.5 131.1)
        (xy 128.8 132)
        (xy 128.8 133.5)
        (xy 127 133.5)
        (xy 127 130.1)
        (xy 129.5 130.1)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 143)
        (xy 85 143)
        (xy 85 112)
        (xy 148 112)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.8 143.2)
        (xy 95 143.1)
        (xy 95.1 130.8)
        (xy 98.9 130.8)
      )
    )
  )
  (zone (net 3) (net_name "+3V3") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 143)
        (xy 85 143)
        (xy 85 112)
        (xy 148 112)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 112)
        (xy 85 112)
        (xy 85 143)
        (xy 148 143)
      )
    )
  )
  (zone (net 14) (net_name "+BATT") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.7 131.6)
        (xy 135 131.6)
        (xy 135 129.7)
        (xy 115.1 129.7)
        (xy 115 125.2)
        (xy 136.7 125.2)
      )
    )
  )
)
