(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 80 30)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D10-Pad1)")
  (net 4 "Net-(D10-Pad2)")
  (net 5 "Net-(D11-Pad1)")
  (net 6 "Net-(D11-Pad2)")
  (net 7 "Net-(D12-Pad1)")
  (net 8 "Net-(D12-Pad2)")
  (net 9 "Net-(D13-Pad1)")
  (net 10 "Net-(D13-Pad2)")
  (net 11 "Net-(D14-Pad1)")
  (net 12 "Net-(D14-Pad2)")
  (net 13 "Net-(D15-Pad1)")
  (net 14 "Net-(D15-Pad2)")
  (net 15 "Net-(D16-Pad1)")
  (net 16 "Net-(D16-Pad2)")
  (net 17 "+12V")
  (net 18 "GND")
  (net 19 "Net-(J11-Pad2)")
  (net 20 "Net-(J12-Pad2)")
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 58.7756 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D9" (at 0 2 0) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 82.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R6" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D14-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 77.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J6" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D13-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 83.7692 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D14" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D14-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D14-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 52.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J1" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 17 "+12V") (pinfunction "Pin_1")
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 91.2368 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D8" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D16-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D16-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 73.7616 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D12" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D12-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D12-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 71.2216 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D4" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D12-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D12-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 87.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J8" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D15-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 92.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R8" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D16-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 78.74 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D13" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D13-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D13-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 66.2432 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D3" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D11-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D11-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 62.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R2" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D10-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 92.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J9" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D16-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 67.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J4" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D11-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 72.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J5" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D12-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 67.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R3" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D11-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 86.2076 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D7" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D15-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D15-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 72.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R4" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D12-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 62.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J3" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D10-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 81.2292 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D6" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D14-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D14-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 63.8048 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D10" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D10-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D10-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 76.2 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D5" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D13-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D13-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 56.2356 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D1" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (at 111 80.54 -90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Reference" "J13" (at -5.54 -2.8 90) (layer "F.SilkS") hide)
    (property "Value" "DB9_Female_MountingHoles" (at -5.54 18.61 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -5.54 14.025 90) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -18.04 1.42 270) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 18 "GND") (pinfunction "PAD")
    )
    (pad "0" thru_hole circle (at 6.96 1.42 270) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 18 "GND") (pinfunction "PAD")
    )
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J12-Pad2)") (pinfunction "1")
    )
    (pad "2" thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D15-Pad2)") (pinfunction "2")
    )
    (pad "3" thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D13-Pad2)") (pinfunction "3")
    )
    (pad "4" thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D11-Pad2)") (pinfunction "4")
    )
    (pad "5" thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-Pad1)") (pinfunction "5")
    )
    (pad "6" thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D16-Pad2)") (pinfunction "6")
    )
    (pad "7" thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D14-Pad2)") (pinfunction "7")
    )
    (pad "8" thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D12-Pad2)") (pinfunction "8")
    )
    (pad "9" thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D10-Pad2)") (pinfunction "9")
    )
    (model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d/db_9f.wrl"
      (offset (xyz -5.5 -8.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 87.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R7" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D15-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 88.7476 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D15" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D15-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D15-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 93.7768 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D16" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D16-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D16-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 105.5 96.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Reference" "J12" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x03" (at 0 7.41 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -1.27 -0.635 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+12V") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J12-Pad2)") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "GND") (pinfunction "Pin_3")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 132.588 68.7832 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D11" (at 0 2.5 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D11-Pad1)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D11-Pad2)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 105.5 53.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Reference" "J11" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x03" (at 0 7.41 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+12V") (pinfunction "Pin_1")
    )
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)") (pinfunction "Pin_2")
    )
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "GND") (pinfunction "Pin_3")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 77.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R5" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D13-Pad1)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 82.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J7" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D14-Pad2)") (pinfunction "Pin_1")
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 127.9144 61.2648 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Reference" "D2" (at 0 2 180) (layer "F.SilkS") hide)
    (property "Value" "LED" (at 0 1.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D10-Pad2)") (pinfunction "K")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D10-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 97.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J10" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 18 "GND") (pinfunction "Pin_1")
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 124.6 57.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Reference" "R1" (at 0 -1.65 0) (layer "F.SilkS") hide)
    (property "Value" "4k7" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-Pad2)")
    )
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J11-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_Drill1.5mm" (layer "F.Cu")
    (at 137.5 57.5)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "J2" (at 0 -3.81 0) (layer "F.SilkS") hide)
    (property "Value" "Conn_01x01" (at 0 3.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "E:/Mes documents/KiCad_v6_new_format/moas_ii_adapter_tht/moas_ii_adapter.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-Pad1)") (pinfunction "Pin_1")
    )
  )
  (gr_line (start 149 50) (end 149 100)
    (layer "Edge.Cuts"))
  (gr_arc (start 105 100) (mid 101.464466 98.535534) (end 100 95)
    (layer "Edge.Cuts"))
  (gr_line (start 149 100) (end 105 100)
    (layer "Edge.Cuts"))
  (gr_line (start 105 50) (end 149 50)
    (layer "Edge.Cuts"))
  (gr_arc (start 100 55) (mid 101.464466 51.464466) (end 105 50)
    (layer "Edge.Cuts"))
  (gr_line (start 100 55) (end 100 95)
    (layer "Edge.Cuts"))
  (gr_text "12V" (at 120.75 97.75 0) (layer "F.SilkS"))
  (gr_text "GND" (at 120.75 95.25 0) (layer "F.SilkS"))
  (gr_text "V 1.0\n(C) F6FVY" (at 106.5 93 0) (layer "F.SilkS"))
  (gr_text "1" (at 125.5 64.5 90) (layer "F.SilkS"))
  (gr_text "2" (at 125.5 69.5 90) (layer "F.SilkS"))
  (gr_text "MOAS II DB9\nadapter THT" (at 106.5 57 0) (layer "F.SilkS"))
  (gr_text "MOAS sinks to GND" (at 120.75 54.75 0) (layer "F.SilkS"))
  (gr_text "MOAS sources 12V" (at 120.75 52.25 0) (layer "F.SilkS"))
  (gr_text "0" (at 125.5 59.5 90) (layer "F.SilkS"))
  (gr_text "5" (at 125.5 84.5 90) (layer "F.SilkS"))
  (gr_text "3" (at 125.5 74.5 90) (layer "F.SilkS"))
  (gr_text "on pin 1 DB9" (at 124 96.5 0) (layer "F.SilkS"))
  (gr_text "4" (at 125.5 79.5 90) (layer "F.SilkS"))
  (gr_text "6" (at 125.5 89.5 90) (layer "F.SilkS"))
  (gr_text "7" (at 125.5 94.5 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149 50) (xy 149 100))
    (height -7)
    (gr_text "50 mm" (at 154.2 75 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 0))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149 50) (xy 100 50))
    (height 6)
    (gr_text "49 mm" (at 124.5 42.2 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 0))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 18) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 102)
        (xy 98 102)
        (xy 98 48)
        (xy 140 48)
      )
    )
  )
  (zone (net 18) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.5 100.75)
        (xy 99 101)
        (xy 99 49)
        (xy 150 49)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 100)
        (xy 140 100)
        (xy 140 50)
        (xy 150 50)
      )
    )
  )
)
