(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab true)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "Net-(C101-Pad2)")
  (net 2 "Net-(C102-Pad1)")
  (net 3 "Net-(C103-Pad1)")
  (net 4 "Net-(C104-Pad2)")
  (net 5 "Net-(C104-Pad1)")
  (net 6 "Net-(C105-Pad2)")
  (net 7 "Net-(C105-Pad1)")
  (net 8 "Net-(C107-Pad1)")
  (net 9 "Net-(C109-Pad2)")
  (net 10 "Net-(C110-Pad2)")
  (net 11 "Net-(D101-Pad1)")
  (net 12 "/START#")
  (net 13 "/RUN#")
  (net 14 "Net-(P101-PadA9)")
  (net 15 "Net-(P101-PadA10)")
  (net 16 "/Circuit/FLD2")
  (net 17 "Net-(P101-PadA13)")
  (net 18 "Net-(P101-PadA14)")
  (net 19 "Net-(P101-PadA16)")
  (net 20 "Net-(P101-PadA18)")
  (net 21 "Net-(P101-PadA19)")
  (net 22 "Net-(P101-PadA26)")
  (net 23 "Net-(P101-PadA27)")
  (net 24 "Net-(P101-PadA28)")
  (net 25 "Net-(P101-PadA29)")
  (net 26 "Net-(P101-PadA30)")
  (net 27 "Net-(P101-PadB7)")
  (net 28 "Net-(P101-PadB8)")
  (net 29 "/Circuit/HDOT0")
  (net 30 "/Circuit/HDOT1")
  (net 31 "/Circuit/HDOT2")
  (net 32 "/Circuit/POS0")
  (net 33 "/Circuit/POS1")
  (net 34 "Net-(P101-PadB11)")
  (net 35 "Net-(P101-PadB12)")
  (net 36 "Net-(P101-PadB16)")
  (net 37 "Net-(P101-PadB17)")
  (net 38 "Net-(P101-PadB18)")
  (net 39 "Net-(P101-PadB19)")
  (net 40 "Net-(P101-PadB27)")
  (net 41 "Net-(P101-PadB28)")
  (net 42 "Net-(P101-PadB31)")
  (net 43 "Net-(P101-PadC5)")
  (net 44 "Net-(P101-PadC6)")
  (net 45 "Net-(P101-PadC9)")
  (net 46 "POR#")
  (net 47 "POR")
  (net 48 "VCC")
  (net 49 "Net-(P101-PadC10)")
  (net 50 "Net-(P101-PadC13)")
  (net 51 "/Circuit/POS2")
  (net 52 "/Circuit/DESCENDER0")
  (net 53 "Net-(P101-PadC14)")
  (net 54 "/Circuit/DESCENDER1")
  (net 55 "/Circuit/LINE0")
  (net 56 "/Circuit/LINE1")
  (net 57 "/Circuit/LINE2")
  (net 58 "/Circuit/LASTDOT")
  (net 59 "/Circuit/FLDREQ0")
  (net 60 "/Circuit/FLDREQ1")
  (net 61 "/Circuit/FLDREQ2")
  (net 62 "Net-(P101-PadC16)")
  (net 63 "Net-(P101-PadC17)")
  (net 64 "Net-(P101-PadC18)")
  (net 65 "Net-(P101-PadC26)")
  (net 66 "Net-(P101-PadC29)")
  (net 67 "/ZSEL")
  (net 68 "Net-(P101-PadC31)")
  (net 69 "RUN")
  (net 70 "/FLD3")
  (net 71 "/Circuit/POSREQ0")
  (net 72 "/Circuit/POSREQ1")
  (net 73 "/Circuit/FLDREQ3")
  (net 74 "/Circuit/FINISHREQ")
  (net 75 "/Circuit/POSREQ2")
  (net 76 "Net-(R114-Pad1)")
  (net 77 "Net-(R115-Pad1)")
  (net 78 "Net-(R119-Pad1)")
  (net 79 "/Circuit/FLD0")
  (net 80 "/Circuit/FLD1")
  (net 81 "/Circuit/CHAR0")
  (net 82 "/Circuit/CHAR1")
  (net 83 "/Circuit/CHAR2")
  (net 84 "/Circuit/CHAR3")
  (net 85 "/Circuit/CHAR4")
  (net 86 "/Circuit/CHAR5")
  (net 87 "/Circuit/FLD_BOTTOM")
  (net 88 "/Circuit/CHAR6")
  (net 89 "Net-(R134-Pad2)")
  (net 90 "Net-(R142-Pad2)")
  (net 91 "GND")
  (net 92 "+15V")
  (net 93 "-15V")
  (net 94 "DOTCLK")
  (net 95 "Net-(U102-Pad15)")
  (net 96 "Net-(U102-Pad14)")
  (net 97 "/Circuit/~{LASTDOT}")
  (net 98 "Net-(U103-Pad15)")
  (net 99 "Net-(U103-Pad11)")
  (net 100 "REQCLK")
  (net 101 "Net-(U104-Pad15)")
  (net 102 "Net-(U104-Pad11)")
  (net 103 "/Circuit/NEXTPOSREQ")
  (net 104 "/Circuit/NEXTFLDREQ")
  (net 105 "/Circuit/INTERLINE_BLANK#")
  (net 106 "/Circuit/STARTCMD")
  (net 107 "Net-(U106-Pad2)")
  (net 108 "Net-(U107-Pad12)")
  (net 109 "/Circuit/~{LASTPOSREQ}")
  (net 110 "/Circuit/~{LASTLINE}")
  (net 111 "Net-(U108-Pad10)")
  (net 112 "Net-(U108-Pad9)")
  (net 113 "Net-(U109-Pad1)")
  (net 114 "Net-(U111-Pad15)")
  (net 115 "/Circuit/READY")
  (net 116 "Net-(U114-Pad9)")
  (net 117 "DONE")
  (net 118 "/Circuit/FINISH#")
  (net 119 "Net-(U115-Pad13)")
  (net 120 "/Circuit/LATCHBUS")
  (net 121 "Net-(U115-Pad10)")
  (net 122 "Net-(U115-Pad7)")
  (net 123 "/CHAR7")
  (net 124 "Net-(U118-Pad12)")
  (net 125 "Net-(U118-Pad8)")
  (net 126 "Net-(U118-Pad6)")
  (net 127 "/CHAR5")
  (net 128 "/CHAR2")
  (net 129 "/CHAR6")
  (net 130 "/CHAR3")
  (net 131 "/CHAR0")
  (net 132 "Net-(R109-Pad2)")
  (net 133 "/CHAR4")
  (net 134 "/CHAR1")
  (net 135 "/POS0")
  (net 136 "/FLD2")
  (net 137 "/INTEN#")
  (net 138 "/V-")
  (net 139 "/V+")
  (net 140 "/POS1")
  (net 141 "/FLD0")
  (net 142 "/POS2")
  (net 143 "/FLD1")
  (net 144 "/Circuit/FLD3")
  (net 145 "/Circuit/PIX_BLANK#")
  (net 146 "/Circuit/INTEN")
  (net 147 "/H-")
  (net 148 "/H+")
  (net 149 "Net-(U120-Pad15)")
  (net 150 "Net-(U120-Pad11)")
  (net 151 "Net-(U121-Pad26)")
  (net 152 "Net-(U121-Pad22)")
  (net 153 "/Circuit/CHAR7")
  (net 154 "Net-(U121-Pad20)")
  (net 155 "Net-(U121-Pad21)")
  (net 156 "Net-(U121-Pad19)")
  (net 157 "Net-(U121-Pad17)")
  (net 158 "Net-(U121-Pad12)")
  (net 159 "Net-(U121-Pad1)")
  (net 160 "Net-(R111-Pad2)")
  (net 161 "Net-(R112-Pad1)")
  (net 162 "Net-(R113-Pad1)")
  (net 163 "Net-(R116-Pad1)")
  (net 164 "Net-(R117-Pad1)")
  (net 165 "Net-(R118-Pad1)")
  (net 166 "Net-(R120-Pad2)")
  (net 167 "Net-(R122-Pad1)")
  (net 168 "Net-(R123-Pad1)")
  (net 169 "Net-(R124-Pad2)")
  (net 170 "Net-(R125-Pad2)")
  (net 171 "Net-(R127-Pad1)")
  (net 172 "Net-(R128-Pad1)")
  (net 173 "Net-(R129-Pad1)")
  (net 174 "Net-(R139-Pad2)")
  (net 175 "Net-(R140-Pad2)")
  (net 176 "Net-(R150-Pad2)")
  (net 177 "Net-(R155-Pad2)")
  (net 178 "Net-(R156-Pad2)")
  (net 179 "Net-(R157-Pad2)")
  (net 180 "Net-(R158-Pad1)")
  (net 181 "Net-(R159-Pad2)")
  (net 182 "Net-(R160-Pad1)")
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 60 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD112" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 142 81.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD120" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 227.5 54.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R157" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C109-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 179 "Net-(R157-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 205 109)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R108" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 131 "/CHAR0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 205 70 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD114" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 133.1 98.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD113" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 233.5 115 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "RT103" (at 0 -1.82 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "250mA" (at 0 1.82 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "507-1799-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 42 "Net-(P101-PadB31)")
    )
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 93 "-15V")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132 88 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R113" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 162 "Net-(R113-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 72 "/Circuit/POSREQ1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 69.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD118" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 222 44.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R144" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "274k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:311-2836-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 171 "Net-(R127-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 169 78.6)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U103" (at -4 -6.1 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC161" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:MC74HC161ADR2GOSCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~MR")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "CK")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P0")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P1")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P2")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P3")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "ENP")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~Pe")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "ENT")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(U103-Pad11)") (pinfunction "Q3")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/Circuit/LINE2") (pinfunction "Q2")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/Circuit/LINE1") (pinfunction "Q1")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/Circuit/LINE0") (pinfunction "Q0")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(U103-Pad15)") (pinfunction "Tc")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 233.5 59 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R158" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 180 "Net-(R158-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 179 "Net-(R157-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (at 210 67)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Reference" "D101" (at -5.25 0 0 unlocked) (layer "F.SilkS"))
    (property "Value" "LL4448" (at 0 1.75 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 -2 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 0) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D101-Pad1)") (pinfunction "K")
    )
    (pad "2" smd rect (at 1.75 0) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C107-Pad1)") (pinfunction "A")
    )
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 43.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD115" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "os2_footprints:DIN41612_B_3x32_Horizontal" (layer "F.Cu")
    (at 244.699993 40.629992 -90)
    (descr "DIN 41612 connector, type B, horizontal, 32 pins wide, 2 rows, full configuration")
    (tags "DIN 41512 IEC 60603 B")
    (property "Reference" "P101" (at -4.435 2.54 0 unlocked) (layer "F.SilkS"))
    (property "Value" "DIN41612_M_3x32_OS2" (at 39.38 -3.712 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (zone_connect 1)
    (attr through_hole)
    (fp_text user "Board edge" (at 39.37 -7.3 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 39.37 -2.54 90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -5.08 -2.54 270) (size 2.8 2.8) (drill 2.8) (layers "*.Cu" "*.Mask")
      (zone_connect 1)
    )
    (pad "" np_thru_hole circle (at 83.82 -2.54 270) (size 2.8 2.8) (drill 2.8) (layers "*.Cu" "*.Mask")
      (zone_connect 1)
    )
    (pad "A1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 148 "/H+") (pinfunction "TS+") (zone_connect 1)
    )
    (pad "A3" thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 147 "/H-") (pinfunction "TS-") (zone_connect 1)
    )
    (pad "A4" thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A5" thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/START#") (pinfunction "SS0") (zone_connect 1)
    )
    (pad "A6" thru_hole circle (at 12.7 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/RUN#") (pinfunction "SS1") (zone_connect 1)
    )
    (pad "A7" thru_hole circle (at 15.24 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A8" thru_hole circle (at 17.78 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A9" thru_hole circle (at 20.32 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(P101-PadA9)") (pinfunction "SS2") (zone_connect 1)
    )
    (pad "A10" thru_hole circle (at 22.86 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(P101-PadA10)") (pinfunction "SS3") (zone_connect 1)
    )
    (pad "A11" thru_hole circle (at 25.4 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A12" thru_hole circle (at 27.94 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A13" thru_hole circle (at 30.48 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(P101-PadA13)") (pinfunction "SS4") (zone_connect 1)
    )
    (pad "A14" thru_hole circle (at 33.02 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(P101-PadA14)") (pinfunction "SS5") (zone_connect 1)
    )
    (pad "A15" thru_hole circle (at 35.56 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A16" thru_hole circle (at 38.1 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(P101-PadA16)") (pinfunction "SA2") (zone_connect 1)
    )
    (pad "A17" thru_hole circle (at 40.64 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "A18" thru_hole circle (at 43.18 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(P101-PadA18)") (pinfunction "SA7") (zone_connect 1)
    )
    (pad "A19" thru_hole circle (at 45.72 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(P101-PadA19)") (pinfunction "SA9") (zone_connect 1)
    )
    (pad "A20" thru_hole circle (at 48.26 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "/ZSEL") (pinfunction "SA11") (zone_connect 1)
    )
    (pad "A21" thru_hole circle (at 50.8 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 136 "/FLD2") (pinfunction "SA14") (zone_connect 1)
    )
    (pad "A22" thru_hole circle (at 53.34 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 134 "/CHAR1") (pinfunction "CHAR1") (zone_connect 1)
    )
    (pad "A23" thru_hole circle (at 55.88 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 133 "/CHAR4") (pinfunction "CHAR4") (zone_connect 1)
    )
    (pad "A24" thru_hole circle (at 58.42 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 123 "/CHAR7") (pinfunction "CHINT") (zone_connect 1)
    )
    (pad "A25" thru_hole circle (at 60.96 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 142 "/POS2") (pinfunction "POS2") (zone_connect 1)
    )
    (pad "A26" thru_hole circle (at 63.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(P101-PadA26)") (pinfunction "nc") (zone_connect 1)
    )
    (pad "A27" thru_hole circle (at 66.04 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(P101-PadA27)") (pinfunction "nc") (zone_connect 1)
    )
    (pad "A28" thru_hole circle (at 68.58 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(P101-PadA28)") (pinfunction "+12V") (zone_connect 1)
    )
    (pad "A29" thru_hole circle (at 71.12 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(P101-PadA29)") (pinfunction "+12V") (zone_connect 1)
    )
    (pad "A30" thru_hole circle (at 73.66 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 26 "Net-(P101-PadA30)") (pinfunction "+5V") (zone_connect 1)
    )
    (pad "A31" thru_hole circle (at 76.2 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 26 "Net-(P101-PadA30)") (pinfunction "+5V") (zone_connect 1)
    )
    (pad "A32" thru_hole circle (at 78.74 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B1" thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B2" thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B3" thru_hole circle (at 5.08 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B4" thru_hole circle (at 7.62 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B5" thru_hole circle (at 10.16 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B6" thru_hole circle (at 12.7 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B7" thru_hole circle (at 15.24 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(P101-PadB7)") (pinfunction "IN2+") (zone_connect 1)
    )
    (pad "B8" thru_hole circle (at 17.78 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(P101-PadB8)") (pinfunction "IN2-") (zone_connect 1)
    )
    (pad "B9" thru_hole circle (at 20.32 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B10" thru_hole circle (at 22.86 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B11" thru_hole circle (at 25.4 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(P101-PadB11)") (pinfunction "IN4+") (zone_connect 1)
    )
    (pad "B12" thru_hole circle (at 27.94 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(P101-PadB12)") (pinfunction "IN4-") (zone_connect 1)
    )
    (pad "B13" thru_hole circle (at 30.48 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B14" thru_hole circle (at 33.02 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B15" thru_hole circle (at 35.56 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B16" thru_hole circle (at 38.1 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 36 "Net-(P101-PadB16)") (pinfunction "SA1") (zone_connect 1)
    )
    (pad "B17" thru_hole circle (at 40.64 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 37 "Net-(P101-PadB17)") (pinfunction "SA4") (zone_connect 1)
    )
    (pad "B18" thru_hole circle (at 43.18 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 38 "Net-(P101-PadB18)") (pinfunction "SA6") (zone_connect 1)
    )
    (pad "B19" thru_hole circle (at 45.72 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 39 "Net-(P101-PadB19)") (pinfunction "SA8") (zone_connect 1)
    )
    (pad "B20" thru_hole circle (at 48.26 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B21" thru_hole circle (at 50.8 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 143 "/FLD1") (pinfunction "SA13") (zone_connect 1)
    )
    (pad "B22" thru_hole circle (at 53.34 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 131 "/CHAR0") (pinfunction "CHAR0") (zone_connect 1)
    )
    (pad "B23" thru_hole circle (at 55.88 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 130 "/CHAR3") (pinfunction "CHAR3") (zone_connect 1)
    )
    (pad "B24" thru_hole circle (at 58.42 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 129 "/CHAR6") (pinfunction "CHAR6") (zone_connect 1)
    )
    (pad "B25" thru_hole circle (at 60.96 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 140 "/POS1") (pinfunction "POS1") (zone_connect 1)
    )
    (pad "B26" thru_hole circle (at 63.5 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B27" thru_hole circle (at 66.04 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 40 "Net-(P101-PadB27)") (pinfunction "nc") (zone_connect 1)
    )
    (pad "B28" thru_hole circle (at 68.58 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 41 "Net-(P101-PadB28)") (pinfunction "+15V") (zone_connect 1)
    )
    (pad "B29" thru_hole circle (at 71.12 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B30" thru_hole circle (at 73.66 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "B31" thru_hole circle (at 76.2 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 42 "Net-(P101-PadB31)") (pinfunction "-15V") (zone_connect 1)
    )
    (pad "B32" thru_hole circle (at 78.74 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C1" thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C2" thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 139 "/V+") (pinfunction "SIG+") (zone_connect 1)
    )
    (pad "C3" thru_hole circle (at 5.08 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 138 "/V-") (pinfunction "SIG-") (zone_connect 1)
    )
    (pad "C4" thru_hole circle (at 7.62 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C5" thru_hole circle (at 10.16 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 43 "Net-(P101-PadC5)") (pinfunction "IN1+") (zone_connect 1)
    )
    (pad "C6" thru_hole circle (at 12.7 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 44 "Net-(P101-PadC6)") (pinfunction "IN1-") (zone_connect 1)
    )
    (pad "C7" thru_hole circle (at 15.24 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C8" thru_hole circle (at 17.78 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C9" thru_hole circle (at 20.32 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 45 "Net-(P101-PadC9)") (pinfunction "IN3+") (zone_connect 1)
    )
    (pad "C10" thru_hole circle (at 22.86 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 49 "Net-(P101-PadC10)") (pinfunction "IN3-") (zone_connect 1)
    )
    (pad "C11" thru_hole circle (at 25.4 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C12" thru_hole circle (at 27.94 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C13" thru_hole circle (at 30.48 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 50 "Net-(P101-PadC13)") (pinfunction "IN5+") (zone_connect 1)
    )
    (pad "C14" thru_hole circle (at 33.02 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 53 "Net-(P101-PadC14)") (pinfunction "IN5-") (zone_connect 1)
    )
    (pad "C15" thru_hole circle (at 35.56 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C16" thru_hole circle (at 38.1 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 62 "Net-(P101-PadC16)") (pinfunction "SA0") (zone_connect 1)
    )
    (pad "C17" thru_hole circle (at 40.64 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 63 "Net-(P101-PadC17)") (pinfunction "SA3") (zone_connect 1)
    )
    (pad "C18" thru_hole circle (at 43.18 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 64 "Net-(P101-PadC18)") (pinfunction "SA5") (zone_connect 1)
    )
    (pad "C19" thru_hole circle (at 45.72 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C20" thru_hole circle (at 48.26 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 137 "/INTEN#") (pinfunction "SA10") (zone_connect 1)
    )
    (pad "C21" thru_hole circle (at 50.8 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 141 "/FLD0") (pinfunction "SA12") (zone_connect 1)
    )
    (pad "C22" thru_hole circle (at 53.34 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 70 "/FLD3") (pinfunction "SA15") (zone_connect 1)
    )
    (pad "C23" thru_hole circle (at 55.88 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 128 "/CHAR2") (pinfunction "CHAR2") (zone_connect 1)
    )
    (pad "C24" thru_hole circle (at 58.42 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 127 "/CHAR5") (pinfunction "CHAR5") (zone_connect 1)
    )
    (pad "C25" thru_hole circle (at 60.96 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 135 "/POS0") (pinfunction "POS0") (zone_connect 1)
    )
    (pad "C26" thru_hole circle (at 63.5 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 65 "Net-(P101-PadC26)") (pinfunction "FIELD") (zone_connect 1)
    )
    (pad "C27" thru_hole circle (at 66.04 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C28" thru_hole circle (at 68.58 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C29" thru_hole circle (at 71.12 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(P101-PadC29)") (pinfunction "nc") (zone_connect 1)
    )
    (pad "C30" thru_hole circle (at 73.66 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (pad "C31" thru_hole circle (at 76.2 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 68 "Net-(P101-PadC31)") (pinfunction "nc") (zone_connect 1)
    )
    (pad "C32" thru_hole circle (at 78.74 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (zone_layer_connections)
      (net 91 "GND") (pinfunction "GND") (zone_connect 1)
    )
    (model "${KIPRJMOD}/../../libraries/3d/86093967113755elf.stp"
      (offset (xyz -7.5 12.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 95 35)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Reference" "H101" (at -0.065 4.37 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "HOLE" (at 0 4.2 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (zone_connect 2)
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0.3 0 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 81.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD108" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 52 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R134" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 89 "Net-(R134-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 187 63.2)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U108" (at -4 -5.95 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC109" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-7923-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~R")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(U106-Pad2)") (pinfunction "J")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(U106-Pad2)") (pinfunction "~K")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "DOTCLK") (pinfunction "C")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "Q")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "POR") (pinfunction "~Q")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(U108-Pad9)") (pinfunction "~Q")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(U108-Pad10)") (pinfunction "Q")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "C")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/START#") (pinfunction "~K")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/START#") (pinfunction "J")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~R")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 194 73)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R120" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k96" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:2019-RK73H2ATTD1961FCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "Net-(C103-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 166 "Net-(R120-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 227.5 59)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U110" (at -8.7 -4.2 0 unlocked) (layer "F.SilkS"))
    (property "Value" "NE5532" (at 0 3.4 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:296-52672-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C109-Pad2)")
    )
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C104-Pad2)") (pinfunction "-")
    )
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "+")
    )
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "-15V") (pinfunction "V-")
    )
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "+")
    )
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(R157-Pad2)") (pinfunction "-")
    )
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(R158-Pad1)")
    )
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "+15V") (pinfunction "V+")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 230 50.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R162" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k5" (at 0 1.82 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF1206JT1K50CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 180 "Net-(R158-Pad1)")
    )
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 148 "/H+")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 44.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R142" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 90 "Net-(R142-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (at 215 94)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U111" (at -4.25 -8 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC245" (at 0 7.35 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-3784-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "A->B")
    )
    (pad "2" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/Circuit/POSREQ0") (pinfunction "A0")
    )
    (pad "3" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/Circuit/POSREQ1") (pinfunction "A1")
    )
    (pad "4" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/Circuit/POSREQ2") (pinfunction "A2")
    )
    (pad "5" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "A3")
    )
    (pad "6" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/Circuit/FLDREQ0") (pinfunction "A4")
    )
    (pad "7" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/Circuit/FLDREQ1") (pinfunction "A5")
    )
    (pad "8" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/Circuit/FLDREQ2") (pinfunction "A6")
    )
    (pad "9" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/Circuit/FLDREQ3") (pinfunction "A7")
    )
    (pad "10" smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "11" smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/FLD3") (pinfunction "B7")
    )
    (pad "12" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "/FLD2") (pinfunction "B6")
    )
    (pad "13" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "/FLD1") (pinfunction "B5")
    )
    (pad "14" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "/FLD0") (pinfunction "B4")
    )
    (pad "15" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(U111-Pad15)") (pinfunction "B3")
    )
    (pad "16" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "/POS2") (pinfunction "B2")
    )
    (pad "17" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "/POS1") (pinfunction "B1")
    )
    (pad "18" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "/POS0") (pinfunction "B0")
    )
    (pad "19" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "CE")
    )
    (pad "20" smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 65.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C108" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "100p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-15000-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C107-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C104-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 95 125)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Reference" "H102" (at -0.065 -4.35 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "HOLE" (at 0 4.2 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (zone_connect 2)
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0.3 0 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "Pin_1") (zone_connect 2)
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 58 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R140" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "9k76" (at 0 1.65 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT9K76CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 175 "Net-(R140-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 62.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C104" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "100p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-15000-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C104-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C104-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 235 52 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R164" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k5" (at 0 1.82 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF1206JT1K50CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 182 "Net-(R160-Pad1)")
    )
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 138 "/V-")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 151 105)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U115" (at -4 -6.25 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC109" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-7923-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~R")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/Circuit/NEXTPOSREQ") (pinfunction "J")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/Circuit/NEXTPOSREQ") (pinfunction "~K")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "C")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/Circuit/LATCHBUS") (pinfunction "Q")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(U115-Pad7)") (pinfunction "~Q")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/Circuit/FINISH#") (pinfunction "~Q")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(U115-Pad10)") (pinfunction "Q")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/Circuit/LATCHBUS") (pinfunction "C")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(U115-Pad13)") (pinfunction "~K")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(U115-Pad13)") (pinfunction "J")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~R")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 152 94)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R116" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 163 "Net-(R116-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 60 "/Circuit/FLDREQ1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 98.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD110" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 169 105)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U104" (at -4 -6.25 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC161" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:MC74HC161ADR2GOSCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~MR")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "CK")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P0")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P1")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P2")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P3")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/Circuit/NEXTPOSREQ") (pinfunction "ENP")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~Pe")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "ENT")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(U104-Pad11)") (pinfunction "Q3")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/Circuit/POSREQ2") (pinfunction "Q2")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/Circuit/POSREQ1") (pinfunction "Q1")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/Circuit/POSREQ0") (pinfunction "Q0")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(U104-Pad15)") (pinfunction "Tc")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 55 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R125" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k96" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:2019-RK73H2ATTD1961FCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 170 "Net-(R125-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (at 232 83.5)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Reference" "RV102" (at -7 -0.3 0) (layer "F.SilkS"))
    (property "Value" "20k" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Adjustment" "VPOS" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 0) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.8 -1) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "+15V") (pinfunction "1")
    )
    (pad "2" smd rect (at 1.45 0) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "Net-(R150-Pad2)") (pinfunction "2")
    )
    (pad "3" smd rect (at -1.8 1) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "-15V") (pinfunction "3")
    )
    (model "${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 187 75.8)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U106" (at -3.75 -5.55 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC14" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:74HC14DCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C101-Pad2)")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(U106-Pad2)")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Circuit/HDOT2")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/Circuit/LASTDOT")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "/Circuit/~{LASTDOT}")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/Circuit/STARTCMD")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/START#")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(R120-Pad2)")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C102-Pad1)")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/Circuit/INTERLINE_BLANK#")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C103-Pad1)")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 151 111.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD117" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 42.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD107" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 205 113)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R106" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 128 "/CHAR2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R130" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 57 "/Circuit/LINE2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 221 37 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R127" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "274k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:311-2836-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 171 "Net-(R127-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 29 "/Circuit/HDOT0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 169 117.6)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U119" (at -4 -5.35 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC03" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:296-14826-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/RUN#")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "/Circuit/INTEN")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "/INTEN#")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/ZSEL")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U118-Pad12)")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/ZSEL")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/Circuit/STARTCMD")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "DONE")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 115 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R104" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 133 "/CHAR4")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 56.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R139" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "9k76" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT9K76CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 174 "Net-(R139-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132 86 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R112" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 161 "Net-(R112-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 71 "/Circuit/POSREQ0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 217.5 40.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R146" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "274k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:311-2836-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 31 "/Circuit/HDOT2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 223.9 70.3 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD126" (at 0 -1.68 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "-15V")
    )
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 222 58 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C109" (at 0 -1.68 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "330p" (at 0 1.68 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-1130-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C109-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 187 87.8)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U107" (at -3.75 -5.55 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC10" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:296-14828-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U102-Pad14)")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/Circuit/HDOT0")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/Circuit/LINE0")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/Circuit/LINE1")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/Circuit/LINE2")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/Circuit/~{LASTLINE}")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/Circuit/~{LASTPOSREQ}")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/Circuit/POSREQ2")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/Circuit/POSREQ1")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/Circuit/POSREQ0")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(U107-Pad12)")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Circuit/HDOT2")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 151 98.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD111" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 222.5 66)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C110" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "330p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-1130-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C110-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 233.5 56)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD124" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "+15V")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 152 86)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R119" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 78 "Net-(R119-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "/Circuit/FINISHREQ")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 205 76)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U113" (at -4 -5.75 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC86" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-6441-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/Circuit/FLD1")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D101-Pad1)")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Circuit/FLD2")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C105-Pad1)")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/Circuit/FLD_BOTTOM")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Circuit/FLD2")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "/Circuit/FLD3")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "Net-(R111-Pad2)")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/Circuit/LASTDOT")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 180 74 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R109" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "Net-(C101-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 132 "Net-(R109-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (at 215 112)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U117" (at -4.5 -7.75 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HCT273" (at 0 7.35 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-2844-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~Mr")
    )
    (pad "2" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/Circuit/CHAR0") (pinfunction "Q0")
    )
    (pad "3" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/CHAR0") (pinfunction "D0")
    )
    (pad "4" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "/CHAR1") (pinfunction "D1")
    )
    (pad "5" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/Circuit/CHAR1") (pinfunction "Q1")
    )
    (pad "6" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/Circuit/CHAR2") (pinfunction "Q2")
    )
    (pad "7" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "/CHAR2") (pinfunction "D2")
    )
    (pad "8" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "/CHAR3") (pinfunction "D3")
    )
    (pad "9" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "/Circuit/CHAR3") (pinfunction "Q3")
    )
    (pad "10" smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "11" smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/Circuit/LATCHBUS") (pinfunction "Cp")
    )
    (pad "12" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/Circuit/CHAR4") (pinfunction "Q4")
    )
    (pad "13" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "/CHAR4") (pinfunction "D4")
    )
    (pad "14" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "/CHAR5") (pinfunction "D5")
    )
    (pad "15" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/Circuit/CHAR5") (pinfunction "Q5")
    )
    (pad "16" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/Circuit/CHAR6") (pinfunction "Q6")
    )
    (pad "17" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "/CHAR6") (pinfunction "D6")
    )
    (pad "18" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "/CHAR7") (pinfunction "D7")
    )
    (pad "19" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "/Circuit/CHAR7") (pinfunction "Q7")
    )
    (pad "20" smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 187 50)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U102" (at -4 -6.25 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC161" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:MC74HC161ADR2GOSCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~MR")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "DOTCLK") (pinfunction "CK")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P0")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P1")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P2")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P3")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "ENP")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "/Circuit/~{LASTDOT}") (pinfunction "~Pe")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "ENT")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Circuit/HDOT2") (pinfunction "Q3")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Circuit/HDOT1") (pinfunction "Q2")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/Circuit/HDOT0") (pinfunction "Q1")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U102-Pad14)") (pinfunction "Q0")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(U102-Pad15)") (pinfunction "Tc")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 214.5 40.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R133" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 33 "/Circuit/POS1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 133 105)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U114" (at -4 -6.25 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC109" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-7923-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~R")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(U109-Pad1)") (pinfunction "J")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/Circuit/FINISH#") (pinfunction "~K")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "C")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "Q")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "DONE") (pinfunction "~Q")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(U114-Pad9)") (pinfunction "~Q")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "/Circuit/READY") (pinfunction "Q")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "~S")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "C")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~K")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/Circuit/NEXTPOSREQ") (pinfunction "J")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~R")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 234 75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R151" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 176 "Net-(R150-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 96 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD105" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132 92 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R114" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 76 "Net-(R114-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 75 "/Circuit/POSREQ2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 142 117 180)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Reference" "CD101" (at 1.75 -5.25 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "470µ" (at 1.75 5.25 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:493-1743-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.75 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "VCC")
    )
    (pad "2" thru_hole circle (at 3.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (at 228.5 64.1 180)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Reference" "RV105" (at 10.7 -0.5 90) (layer "F.SilkS"))
    (property "Value" "500" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Adjustment" "VGAIN" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 0) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.8 -1 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C110-Pad2)") (pinfunction "1")
    )
    (pad "2" smd rect (at 1.45 0 180) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C110-Pad2)") (pinfunction "2")
    )
    (pad "3" smd rect (at -1.8 1 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "Net-(R156-Pad2)") (pinfunction "3")
    )
    (model "${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (at 219 70 -90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Reference" "RV103" (at 4 4.2 0) (layer "F.SilkS"))
    (property "Value" "1k" (at 0 2.5 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Adjustment" "VSEP" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 -90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.8 -1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "Net-(R123-Pad1)") (pinfunction "1")
    )
    (pad "2" smd rect (at 1.45 0 270) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "Net-(R123-Pad1)") (pinfunction "2")
    )
    (pad "3" smd rect (at -1.8 1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C105-Pad2)") (pinfunction "3")
    )
    (model "${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (at 228 39 -90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Reference" "RV101" (at -5.4 3.2 180) (layer "F.SilkS"))
    (property "Value" "20k" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Adjustment" "HPOS" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.8 -1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "+15V") (pinfunction "1")
    )
    (pad "2" smd rect (at 1.45 0 270) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(R142-Pad2)") (pinfunction "2")
    )
    (pad "3" smd rect (at -1.8 1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "-15V") (pinfunction "3")
    )
    (model "${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 235 107.75 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "RT101" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "250mA" (at 0 1.82 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "507-1799-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 41 "Net-(P101-PadB28)")
    )
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 92 "+15V")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 180 72)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C101" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "100p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-15000-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C101-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 233.5 118 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "RT102" (at 0 -1.82 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "250mA" (at 0 1.82 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "507-1799-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 26 "Net-(P101-PadA30)")
    )
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 48 "VCC")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 217.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R137" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 87 "/Circuit/FLD_BOTTOM")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 104 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD103" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 205 46.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD106" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 72 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD121" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 68.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C105" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "100p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-15000-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C105-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C105-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 220.5 40.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R132" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "274k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:311-2836-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 30 "/Circuit/HDOT1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 205 53)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U120" (at -4 -6.2 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC237" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:74HC237DCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "/Circuit/FLD0") (pinfunction "A0")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/Circuit/FLD1") (pinfunction "A1")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Circuit/FLD2") (pinfunction "A2")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "~LE")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "~E1")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "E2")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C104-Pad1)") (pinfunction "Y7")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 175 "Net-(R140-Pad2)") (pinfunction "Y6")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "Net-(R139-Pad2)") (pinfunction "Y5")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(U120-Pad11)") (pinfunction "Y4")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 170 "Net-(R125-Pad2)") (pinfunction "Y3")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(R134-Pad2)") (pinfunction "Y2")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 169 "Net-(R124-Pad2)") (pinfunction "Y1")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(U120-Pad15)") (pinfunction "Y0")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 223.5 40.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R143" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 90 "Net-(R142-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 109 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R101" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 123 "/CHAR7")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 205 115)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R105" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 130 "/CHAR3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 221.5 61 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD127" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "-15V")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_LCC:PLCC-32_THT-Socket" (layer "F.Cu")
    (at 188.2 103)
    (descr "PLCC, 32 pins, through hole, http://www.assmann-wsw.com/fileadmin/datasheets/ASS_0981_CO.pdf")
    (tags "plcc leaded")
    (property "Reference" "U121" (at -8.45 17.4 0 unlocked) (layer "F.SilkS"))
    (property "Value" "27C512" (at -1.27 16.38 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:AT27C512R-45JU-ND, DK:AE11106-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -1.27 5.08 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 159 "Net-(U121-Pad1)") (pinfunction "NC")
    )
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "A15")
    )
    (pad "3" thru_hole circle (at -2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "/Circuit/CHAR6") (pinfunction "A12")
    )
    (pad "4" thru_hole circle (at -5.08 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "/Circuit/CHAR1") (pinfunction "A7")
    )
    (pad "5" thru_hole circle (at -7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "/Circuit/CHAR0") (pinfunction "A6")
    )
    (pad "6" thru_hole circle (at -5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "/Circuit/LINE2") (pinfunction "A5")
    )
    (pad "7" thru_hole circle (at -7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "/Circuit/LINE1") (pinfunction "A4")
    )
    (pad "8" thru_hole circle (at -5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "/Circuit/LINE0") (pinfunction "A3")
    )
    (pad "9" thru_hole circle (at -7.62 5.08) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/Circuit/HDOT2") (pinfunction "A2")
    )
    (pad "10" thru_hole circle (at -5.08 5.08) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/Circuit/HDOT1") (pinfunction "A1")
    )
    (pad "11" thru_hole circle (at -7.62 7.62) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "/Circuit/HDOT0") (pinfunction "A0")
    )
    (pad "12" thru_hole circle (at -5.08 7.62) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 158 "Net-(U121-Pad12)") (pinfunction "NC")
    )
    (pad "13" thru_hole circle (at -7.62 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "/Circuit/DESCENDER0") (pinfunction "O0")
    )
    (pad "14" thru_hole circle (at -5.08 12.7) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "/Circuit/DESCENDER1") (pinfunction "O1")
    )
    (pad "15" thru_hole circle (at -5.08 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 146 "/Circuit/INTEN") (pinfunction "O2")
    )
    (pad "16" thru_hole circle (at -2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "17" thru_hole circle (at -2.54 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 157 "Net-(U121-Pad17)") (pinfunction "NC")
    )
    (pad "18" thru_hole circle (at 0 12.7) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 145 "/Circuit/PIX_BLANK#") (pinfunction "O3")
    )
    (pad "19" thru_hole circle (at 0 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 156 "Net-(U121-Pad19)") (pinfunction "O4")
    )
    (pad "20" thru_hole circle (at 2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 154 "Net-(U121-Pad20)") (pinfunction "O5")
    )
    (pad "21" thru_hole circle (at 5.08 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 155 "Net-(U121-Pad21)") (pinfunction "O6")
    )
    (pad "22" thru_hole circle (at 2.54 10.16) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 152 "Net-(U121-Pad22)") (pinfunction "O7")
    )
    (pad "23" thru_hole circle (at 5.08 7.62) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "~CE")
    )
    (pad "24" thru_hole circle (at 2.54 7.62) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "/Circuit/CHAR4") (pinfunction "A10")
    )
    (pad "25" thru_hole circle (at 5.08 5.08) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "~OE~/VPP")
    )
    (pad "26" thru_hole circle (at 2.54 5.08) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 151 "Net-(U121-Pad26)") (pinfunction "NC")
    )
    (pad "27" thru_hole circle (at 5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "/Circuit/CHAR5") (pinfunction "A11")
    )
    (pad "28" thru_hole circle (at 2.54 2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "/Circuit/CHAR3") (pinfunction "A9")
    )
    (pad "29" thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "/Circuit/CHAR2") (pinfunction "A8")
    )
    (pad "30" thru_hole circle (at 2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 153 "/Circuit/CHAR7") (pinfunction "A13")
    )
    (pad "31" thru_hole circle (at 2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "A14")
    )
    (pad "32" thru_hole circle (at 0 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_THT-Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 53.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R135" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 89 "Net-(R134-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 235.5 64.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R160" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 182 "Net-(R160-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 181 "Net-(R159-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (at 215 83 180)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Reference" "CD102" (at 0 -2.35 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "10µ" (at 0 2.35 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DB:CAP_TANT_10U_16V_B" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 85.2 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD119" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 152 88)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R118" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 165 "Net-(R118-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 73 "/Circuit/FLDREQ3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 59.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R141" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "9k76" (at 0 1.65 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT9K76CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 175 "Net-(R140-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 47.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R148" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 51 "/Circuit/POS2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 50.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R124" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 169 "Net-(R124-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 222.5 63.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R156" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 178 "Net-(R156-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 113 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R103" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 127 "/CHAR5")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 235 67.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD123" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "+15V")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 169 111.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD116" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 86 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD104" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 49 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R149" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 51 "/Circuit/POS2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 219 44.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R145" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "274k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:311-2836-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 31 "/Circuit/HDOT2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 187 56.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "CD109" (at 0 -1.68 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1µ" (at 0 1.68 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-6470-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (at 232 43 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Reference" "CD125" (at 1 -3.75 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "47µ" (at 1 3.75 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:493-1817-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND")
    )
    (pad "2" thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "-15V")
    )
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 219.5 58 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R155" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 177 "Net-(R155-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 231 75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R138" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 54 "/Circuit/DESCENDER1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 227.5 50.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R161" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k5" (at 0 1.82 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF1206JT1K50CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 9 "Net-(C109-Pad2)")
    )
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 147 "/H-")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 215 71.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C106" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "100p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-15000-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C105-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C105-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 229 69.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U112" (at 5.8 2.7 0 unlocked) (layer "F.SilkS"))
    (property "Value" "NE5532" (at 0 3.4 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:296-52672-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C110-Pad2)")
    )
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C105-Pad2)") (pinfunction "-")
    )
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "+")
    )
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "-15V") (pinfunction "V-")
    )
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "+")
    )
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(R159-Pad2)") (pinfunction "-")
    )
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(R160-Pad1)")
    )
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "+15V") (pinfunction "V+")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 219 75 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R136" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "680k" (at 0 1.65 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805JT680KCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 87 "/Circuit/FLD_BOTTOM")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 152 92)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R117" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 164 "Net-(R117-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 61 "/Circuit/FLDREQ2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 194 76)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R111" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k96" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:2019-RK73H2ATTD1961FCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "Net-(C102-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 160 "Net-(R111-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 180 76)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R110" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 132 "Net-(R109-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 205 111)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R107" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 134 "/CHAR1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 169 66)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U109" (at -4 -5.5 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC02" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-2031-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(U109-Pad1)")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(U108-Pad10)")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/Circuit/LASTDOT")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(U107-Pad12)")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Circuit/HDOT1")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/Circuit/~{LASTLINE}")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "/Circuit/~{LASTDOT}")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/Circuit/NEXTPOSREQ")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/Circuit/~{LASTPOSREQ}")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/Circuit/~{LASTLINE}")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/Circuit/NEXTFLDREQ")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (at 235 37 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Reference" "CD122" (at 1 -3.75 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "47µ" (at 1 3.75 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:493-1817-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "+15V")
    )
    (pad "2" thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 215 37 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R128" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 172 "Net-(R128-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 32 "/Circuit/POS0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 207.75 63.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R121" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "680k" (at 0 1.65 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805JT680KCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(D101-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(C107-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 222 75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R152" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 167 "Net-(R122-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132 94 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R115" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 77 "Net-(R115-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 59 "/Circuit/FLDREQ0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 220.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R122" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 167 "Net-(R122-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 55 "/Circuit/LINE0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (at 223.5 53 -90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Reference" "RV104" (at -4.8 3.9 180) (layer "F.SilkS"))
    (property "Value" "500" (at 0 2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Adjustment" "HGAIN" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.8 -1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C109-Pad2)") (pinfunction "1")
    )
    (pad "2" smd rect (at 1.45 0 270) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C109-Pad2)") (pinfunction "2")
    )
    (pad "3" smd rect (at -1.8 1 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "Net-(R155-Pad2)") (pinfunction "3")
    )
    (model "${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 169 91.8)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U105" (at -4 -6.05 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC161" (at 0 5.9 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:MC74HC161ADR2GOSCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "POR#") (pinfunction "~MR")
    )
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "REQCLK") (pinfunction "CK")
    )
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P0")
    )
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P1")
    )
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P2")
    )
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "P3")
    )
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "ENP")
    )
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~Pe")
    )
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/Circuit/NEXTFLDREQ") (pinfunction "ENT")
    )
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/Circuit/FLDREQ3") (pinfunction "Q3")
    )
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/Circuit/FLDREQ2") (pinfunction "Q2")
    )
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/Circuit/FLDREQ1") (pinfunction "Q1")
    )
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/Circuit/FLDREQ0") (pinfunction "Q0")
    )
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/Circuit/FINISHREQ") (pinfunction "Tc")
    )
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 229.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R129" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 173 "Net-(R129-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 52 "/Circuit/DESCENDER0")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (at 142 90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U116" (at -4.25 -7.75 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HCT273" (at 0 7.35 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1727-2844-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "RUN") (pinfunction "~Mr")
    )
    (pad "2" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/Circuit/POS0") (pinfunction "Q0")
    )
    (pad "3" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "Net-(R112-Pad1)") (pinfunction "D0")
    )
    (pad "4" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(R113-Pad1)") (pinfunction "D1")
    )
    (pad "5" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Circuit/POS1") (pinfunction "Q1")
    )
    (pad "6" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/Circuit/POS2") (pinfunction "Q2")
    )
    (pad "7" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R114-Pad1)") (pinfunction "D2")
    )
    (pad "8" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R115-Pad1)") (pinfunction "D3")
    )
    (pad "9" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "/Circuit/FLD0") (pinfunction "Q3")
    )
    (pad "10" smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "11" smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/Circuit/LATCHBUS") (pinfunction "Cp")
    )
    (pad "12" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/Circuit/FLD1") (pinfunction "Q4")
    )
    (pad "13" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "Net-(R116-Pad1)") (pinfunction "D4")
    )
    (pad "14" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(R117-Pad1)") (pinfunction "D5")
    )
    (pad "15" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Circuit/FLD2") (pinfunction "Q5")
    )
    (pad "16" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "/Circuit/FLD3") (pinfunction "Q6")
    )
    (pad "17" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(R118-Pad1)") (pinfunction "D6")
    )
    (pad "18" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R119-Pad1)") (pinfunction "D7")
    )
    (pad "19" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(U115-Pad13)") (pinfunction "Q7")
    )
    (pad "20" smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Oscillator:Oscillator_SeikoEpson_SG-8002DC" (layer "F.Cu")
    (at 165 47)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (property "Reference" "U101" (at 0 -4.5 0 unlocked) (layer "F.SilkS"))
    (property "Value" "2MHz" (at 3.81 11.46 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:SER4343-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 3.865 3.66 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "VCC") (pinfunction "OE")
    )
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "DOTCLK") (pinfunction "OUT")
    )
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "VCC") (pinfunction "Vcc")
    )
    (model "${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SeikoEpson_SG-8002DC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 194 78)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C102" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "47p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-1156-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C102-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 233 64.5 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R159" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "5k9" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT5K90CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(C110-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 181 "Net-(R159-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 228 75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R154" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 173 "Net-(R129-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 61 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R126" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k96" (at 0 1.65 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:2019-RK73H2ATTD1961FCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(C104-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 151 117.6)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U118" (at -4 -5.35 0 unlocked) (layer "F.SilkS"))
    (property "Value" "'HC10" (at 0 5.28 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:296-14828-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "/Circuit/PIX_BLANK#")
    )
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/Circuit/INTERLINE_BLANK#")
    )
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(U118-Pad6)")
    )
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND") (pinfunction "GND")
    )
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(U118-Pad8)")
    )
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC")
    )
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U118-Pad12)")
    )
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "/Circuit/READY")
    )
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "VCC") (pinfunction "VCC")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 232.5 52 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R163" (at 0 -1.82 90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k5" (at 0 1.82 90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF1206JT1K50CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 10 "Net-(C110-Pad2)")
    )
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 139 "/V+")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 216 44.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R147" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C104-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 172 "Net-(R128-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 211 64)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C107" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "330p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:399-1130-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C107-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C104-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 232.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R150" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "39k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT39K0CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 176 "Net-(R150-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 226.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R131" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 57 "/Circuit/LINE2")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 194 71)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Reference" "C103" (at 0 -1.68 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "47p" (at 0 1.68 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:1276-1156-1-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C103-Pad1)")
    )
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 223.5 79 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R153" (at 0 -1.65 -90 unlocked) (layer "F.SilkS") hide)
    (property "Value" "205k" (at 0 1.65 -90 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RR12P205KDCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C105-Pad2)")
    )
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 56 "/Circuit/LINE1")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 211 70 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R123" (at 0 -1.65 180 unlocked) (layer "F.SilkS") hide)
    (property "Value" "1k96" (at 0 1.65 180 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:2019-RK73H2ATTD1961FCT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetname "Circuit")
    (sheetfile "circuit.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 168 "Net-(R123-Pad1)")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(C105-Pad1)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 225 111 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Reference" "R102" (at 0 -1.65 0 unlocked) (layer "F.SilkS") hide)
    (property "Value" "2k37" (at 0 1.65 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "BOM" "DK:RMCF0805FT2K37CT-ND" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "/home/alex/electronics/projects/os2/pcbs/gfx/gfx.kicad_sch")
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "VCC")
    )
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 129 "/CHAR6")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 90 30) (end 250 30)
    (layer "Edge.Cuts"))
  (gr_line (start 250 30) (end 250 130)
    (layer "Edge.Cuts"))
  (gr_line (start 90 130) (end 90 120)
    (layer "Edge.Cuts"))
  (gr_line (start 250 130) (end 90 130)
    (layer "Edge.Cuts"))
  (gr_line (start 90 30) (end 90 120)
    (layer "Edge.Cuts"))
  (gr_text "13" (at 237.715 71.11 0) (layer "B.SilkS"))
  (gr_text "C" (at 239.62 121.91 0) (layer "B.SilkS"))
  (gr_text "32" (at 237.715 119.37 0) (layer "B.SilkS"))
  (gr_text "4" (at 237.715 48.25 0) (layer "B.SilkS"))
  (gr_text "11" (at 237.715 66.03 0) (layer "B.SilkS"))
  (gr_text "25" (at 237.715 101.59 0) (layer "B.SilkS"))
  (gr_text "17" (at 237.715 81.27 0) (layer "B.SilkS"))
  (gr_text "29" (at 237.715 111.75 0) (layer "B.SilkS"))
  (gr_text "15" (at 237.715 76.19 0) (layer "B.SilkS"))
  (gr_text "B" (at 242.16 121.91 0) (layer "B.SilkS"))
  (gr_text "7" (at 237.715 55.87 0) (layer "B.SilkS"))
  (gr_text "6" (at 237.715 53.33 0) (layer "B.SilkS"))
  (gr_text "A" (at 244.7 38.09 0) (layer "B.SilkS"))
  (gr_text "8" (at 237.715 58.41 0) (layer "B.SilkS"))
  (gr_text "B" (at 242.16 38.09 0) (layer "B.SilkS"))
  (gr_text "14" (at 237.715 73.65 0) (layer "B.SilkS"))
  (gr_text "C" (at 239.62 38.09 0) (layer "B.SilkS"))
  (gr_text "24" (at 237.715 99.05 0) (layer "B.SilkS"))
  (gr_text "12" (at 237.715 68.57 0) (layer "B.SilkS"))
  (gr_text "1" (at 237.715 40.63 0) (layer "B.SilkS"))
  (gr_text "10" (at 237.715 63.49 0) (layer "B.SilkS"))
  (gr_text "31" (at 237.715 116.83 0) (layer "B.SilkS"))
  (gr_text "30" (at 237.715 114.29 0) (layer "B.SilkS"))
  (gr_text "23" (at 237.715 96.51 0) (layer "B.SilkS"))
  (gr_text "18" (at 237.715 83.81 0) (layer "B.SilkS"))
  (gr_text "9" (at 237.715 60.95 0) (layer "B.SilkS"))
  (gr_text "3" (at 237.715 45.71 0) (layer "B.SilkS"))
  (gr_text "16" (at 237.715 78.73 0) (layer "B.SilkS"))
  (gr_text "21" (at 237.715 91.43 0) (layer "B.SilkS"))
  (gr_text "28" (at 237.715 109.21 0) (layer "B.SilkS"))
  (gr_text "A" (at 244.7 121.91 0) (layer "B.SilkS"))
  (gr_text "19" (at 237.715 86.35 0) (layer "B.SilkS"))
  (gr_text "2" (at 237.715 43.17 0) (layer "B.SilkS"))
  (gr_text "27" (at 237.715 106.67 0) (layer "B.SilkS"))
  (gr_text "26" (at 237.715 104.13 0) (layer "B.SilkS"))
  (gr_text "22" (at 237.715 93.97 0) (layer "B.SilkS"))
  (gr_text "5" (at 237.715 50.79 0) (layer "B.SilkS"))
  (gr_text "20" (at 237.715 88.89 0) (layer "B.SilkS"))
  (gr_text "21" (at 237.715 91.43 0) (layer "F.SilkS"))
  (gr_text "30" (at 237.715 114.29 0) (layer "F.SilkS"))
  (gr_text "VPOS" (at 225 84.6 0) (layer "F.SilkS"))
  (gr_text "VGAIN" (at 219 64.2 90) (layer "F.SilkS"))
  (gr_text "25" (at 237.715 101.59 0) (layer "F.SilkS"))
  (gr_text "19" (at 237.715 86.35 0) (layer "F.SilkS"))
  (gr_text "11" (at 237.715 66.03 0) (layer "F.SilkS"))
  (gr_text "17" (at 237.715 81.27 0) (layer "F.SilkS"))
  (gr_text "28" (at 237.715 109.21 0) (layer "F.SilkS"))
  (gr_text "B" (at 242.16 38.09 0) (layer "F.SilkS"))
  (gr_text "+" (at 218.25 83 0) (layer "F.SilkS"))
  (gr_text "A" (at 244.7 121.91 0) (layer "F.SilkS"))
  (gr_text "20" (at 237.715 88.89 0) (layer "F.SilkS"))
  (gr_text "HGAIN" (at 219.6 49.4 0) (layer "F.SilkS"))
  (gr_text "A" (at 244.7 38.1 0) (layer "F.SilkS"))
  (gr_text "7" (at 237.715 55.87 0) (layer "F.SilkS"))
  (gr_text "HPOS" (at 224.8 35 0) (layer "F.SilkS"))
  (gr_text "4" (at 237.715 48.25 0) (layer "F.SilkS"))
  (gr_text "2" (at 237.715 43.17 0) (layer "F.SilkS"))
  (gr_text "16" (at 237.715 78.73 0) (layer "F.SilkS"))
  (gr_text "26" (at 237.715 104.13 0) (layer "F.SilkS"))
  (gr_text "22" (at 237.715 93.97 0) (layer "F.SilkS"))
  (gr_text "ON-SCREEN DISPLAY CARD\nPCB-001-02, ASY-001-02" (at 107.2 126.7 0) (layer "F.SilkS"))
  (gr_text "6" (at 237.715 53.33 0) (layer "F.SilkS"))
  (gr_text "13" (at 237.715 71.11 0) (layer "F.SilkS"))
  (gr_text "3" (at 237.715 45.71 0) (layer "F.SilkS"))
  (gr_text "32" (at 237.715 119.37 0) (layer "F.SilkS"))
  (gr_text "ROM-001-2x" (at 196 121.8 0) (layer "F.SilkS"))
  (gr_text "1" (at 237.715 40.63 0) (layer "F.SilkS"))
  (gr_text "15" (at 237.715 76.19 0) (layer "F.SilkS"))
  (gr_text "18" (at 237.715 83.81 0) (layer "F.SilkS"))
  (gr_text "C" (at 239.62 38.09 0) (layer "F.SilkS"))
  (gr_text "10" (at 237.715 63.49 0) (layer "F.SilkS"))
  (gr_text "B" (at 242.16 121.91 0) (layer "F.SilkS"))
  (gr_text "31" (at 237.715 116.83 0) (layer "F.SilkS"))
  (gr_text "29" (at 237.715 111.75 0) (layer "F.SilkS"))
  (gr_text "VSEP" (at 214.8 75.4 0) (layer "F.SilkS"))
  (gr_text "8" (at 237.715 58.41 0) (layer "F.SilkS"))
  (gr_text "14" (at 237.715 73.65 0) (layer "F.SilkS"))
  (gr_text "© 2020 LOCKWOOD CC BY-NC-SA" (at 107.2 124.2 0) (layer "F.SilkS"))
  (gr_text "12" (at 237.715 68.57 0) (layer "F.SilkS"))
  (gr_text "27" (at 237.715 106.67 0) (layer "F.SilkS"))
  (gr_text "5" (at 237.715 50.79 0) (layer "F.SilkS"))
  (gr_text "24" (at 237.715 99.05 0) (layer "F.SilkS"))
  (gr_text "23" (at 237.715 96.51 0) (layer "F.SilkS"))
  (gr_text "C" (at 239.62 121.91 0) (layer "F.SilkS"))
  (gr_text "FONT ROM" (at 196.2 120.4 0) (layer "F.SilkS"))
  (gr_text "9" (at 237.715 60.95 0) (layer "F.SilkS"))
  (gr_text "Bend radius" (at 60 38 0) (layer "Dwgs.User"))
  (gr_text "d=3.2mm" (at 34 125 0) (layer "Dwgs.User"))
  (gr_text "Captive\npanel\nscrews" (at 80 140 0) (layer "Dwgs.User"))
  (gr_text "optional short cut" (at 37 80 90) (layer "Dwgs.User"))
  (gr_text "hole dia 2.5mm\ntap M3x0.5" (at 106 135 0) (layer "Dwgs.User"))
  (gr_text "RAF M0171-SS\nor equiv" (at 80 146 0) (layer "Dwgs.User"))
  (gr_text "d=3.2mm\nno tap" (at 34 35 0) (layer "Dwgs.User"))
  (gr_text "d=2.5mm\ntap M3x0.5" (at 62 22 0) (layer "Dwgs.User"))
  (gr_text "spacer, 5mm×ID=4mm\nattached to chassis" (at 106 139 0) (layer "Dwgs.User"))
  (gr_text "Chassis" (at 103 143 0) (layer "Dwgs.User"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 62 25) (xy 50 25))
    (height 0)
    (gr_text "12.0000 mm" (at 56 23.85 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 250 130) (xy 90 130))
    (height -1)
    (gr_text "160.0000 mm" (at 170 129.85 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 74 19) (xy 50 19))
    (height 2)
    (gr_text "24.0000 mm" (at 62 15.85 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 253 40.63) (xy 253 30))
    (height 6)
    (gr_text "10.6300 mm" (at 257.85 35.315 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 250 130) (xy 250 30))
    (height 13)
    (gr_text "100.0000 mm" (at 261.85 80 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 23 35) (xy 43 35))
    (height -2.999999)
    (gr_text "20.0000 mm" (at 33 30.850001 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 50 35) (xy 43 35))
    (height 3)
    (gr_text "7.0000 mm" (at 46.5 30.85 0) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 62 25) (xy 62 20))
    (height 4)
    (gr_text "5.0000 mm" (at 64.85 22.5 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 91) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.5) (thermal_bridge_width 0.5)
      (hatch_thickness 1) (hatch_gap 1.5) (hatch_orientation 0)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 249.555 129.54)
        (xy 90.5 129.5)
        (xy 90.5 30.5)
        (xy 249.555 30.48)
      )
    )
  )
  (zone (net 91) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 40)
        (xy 90 40)
        (xy 90 30)
        (xy 105 30)
      )
    )
  )
  (zone (net 91) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 130)
        (xy 90 130)
        (xy 90 120)
        (xy 105 120)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 40)
        (xy 90 40)
        (xy 90 30)
        (xy 105 30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 130)
        (xy 90 130)
        (xy 90 120)
        (xy 105 120)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 40)
        (xy 90 40)
        (xy 90 30)
        (xy 105 30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 130)
        (xy 90 130)
        (xy 90 120)
        (xy 105 120)
      )
    )
  )
)
