(kicad_pcb (version 20210722) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 186.25 88.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 4) (layer "F.SilkS"))
    (fp_text value "PTH-3mm" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 166.25 88.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 4) (layer "F.SilkS"))
    (fp_text value "PTH-3mm" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 170.9 97.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "1mm" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 171.8 102.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "1mm" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "1"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 166.25 111)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "NPTH-3mm" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 186.25 111)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "NPTH-3mm" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 165.5 101.25 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "LCSC N°" "C20079")
    (property "N°" "XH-2A")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J1" (at -3.75 -2 180) (layer "F.SilkS"))
    (fp_text value "XH-2A" (at 1.25 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 180 102.25 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "LCSC N°" "C269977")
    (property "N°" "NPXE21E102MF")
    (property "Sheet file" "Test.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "C1" (at -3.75 0 180) (layer "F.SilkS"))
    (fp_text value "1m25vPY_5x10x16" (at 2.5 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 162.5 85) (end 190 115) (layer "Edge.Cuts") (width 0.1) (fill none))
  (dimension (type leader) (layer "Dwgs.User")
    (pts (xy 186.96 87.96) (xy 190.64 84.1))
    (gr_text "Max Hole Violation" (at 195.68 80.93) (layer "Dwgs.User"))
    (format (units 0) (units_format 0) (precision 4) (override_value "Max Hole Violation"))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (text_frame 0) (extension_offset 0.5))
  )
  (dimension (type leader) (layer "Dwgs.User")
    (pts (xy 187.2 109.71) (xy 189.56 107.05))
    (gr_text "Max Hole Violation" (at 195.77 101.67) (layer "Dwgs.User"))
    (format (units 0) (units_format 0) (precision 4) (override_value "Max Hole Violation"))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (text_frame 0) (extension_offset 0.5))
  )
  (dimension (type leader) (layer "Dwgs.User")
    (pts (xy 167.95 100.95) (xy 170.31 98.29))
    (gr_text "PTH Violation" (at 176.52 92.91) (layer "Dwgs.User"))
    (format (units 0) (units_format 0) (precision 4) (override_value "PTH Violation"))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (text_frame 0) (extension_offset 0.5))
  )
  (dimension (type leader) (layer "Dwgs.User")
    (pts (xy 168.47 111.15) (xy 173.05 116.98))
    (gr_text "NPTH Violation" (at 183.34 117.01) (layer "Dwgs.User"))
    (format (units 0) (units_format 0) (precision 4) (override_value "NPTH Violation"))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (text_frame 0) (extension_offset 0.5))
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.5 114.5)
        (xy 163 114.5)
        (xy 163 85.5)
        (xy 189.5 85.5)
      )
    )
  )
)
