(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "envboard")
    (date "2020-11-29")
    (rev "4")
    (comment 1 "sonnichsen")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./GERBER")
    )
  )
  (net 0 "")
  (net 1 "MCLR")
  (net 2 "PGD")
  (net 3 "PGC")
  (net 4 "+3V3")
  (net 5 "GND")
  (net 6 "Net-(U4-Pad4)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(C16-Pad2)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(J2-Pad3)")
  (net 12 "Net-(U4-Pad1)")
  (net 13 "Net-(U4-Pad3)")
  (net 14 "Net-(U4-Pad11)")
  (net 15 "Net-(U4-Pad14)")
  (net 16 "Net-(U4-Pad18)")
  (net 17 "Net-(U4-Pad19)")
  (net 18 "Net-(U4-Pad20)")
  (net 19 "Net-(U4-Pad21)")
  (net 20 "Net-(U4-Pad22)")
  (net 21 "Net-(U4-Pad23)")
  (net 22 "Net-(U4-Pad24)")
  (net 23 "Net-(U4-Pad25)")
  (net 24 "Net-(U4-Pad28)")
  (net 25 "Net-(U4-Pad29)")
  (net 26 "Net-(U4-Pad32)")
  (net 27 "Net-(U4-Pad33)")
  (net 28 "Net-(U4-Pad34)")
  (net 29 "Net-(U4-Pad35)")
  (net 30 "Net-(U4-Pad39)")
  (net 31 "Net-(U4-Pad40)")
  (net 32 "Net-(U4-Pad41)")
  (net 33 "Net-(U4-Pad42)")
  (net 34 "Net-(U4-Pad43)")
  (net 35 "Net-(U4-Pad44)")
  (net 36 "Net-(U4-Pad47)")
  (net 37 "Net-(U4-Pad48)")
  (net 38 "Net-(U4-Pad60)")
  (net 39 "Net-(U4-Pad61)")
  (net 40 "Net-(U4-Pad63)")
  (net 41 "Net-(U4-Pad64)")
  (net 42 "Net-(U4-Pad66)")
  (net 43 "Net-(U4-Pad67)")
  (net 44 "Net-(U4-Pad68)")
  (net 45 "Net-(U4-Pad69)")
  (net 46 "Net-(U4-Pad70)")
  (net 47 "Net-(U4-Pad71)")
  (net 48 "Net-(U4-Pad72)")
  (net 49 "Net-(U4-Pad73)")
  (net 50 "Net-(U4-Pad74)")
  (net 51 "Net-(U4-Pad78)")
  (net 52 "Net-(U4-Pad79)")
  (net 53 "Net-(U4-Pad80)")
  (net 54 "Net-(U4-Pad81)")
  (net 55 "Net-(U4-Pad82)")
  (net 56 "Net-(U4-Pad83)")
  (net 57 "Net-(U4-Pad84)")
  (net 58 "Net-(U4-Pad87)")
  (net 59 "Net-(U4-Pad88)")
  (net 60 "Net-(U4-Pad89)")
  (net 61 "Net-(U4-Pad90)")
  (net 62 "Net-(U4-Pad91)")
  (net 63 "Net-(U4-Pad92)")
  (net 64 "Net-(U4-Pad93)")
  (net 65 "Net-(U4-Pad94)")
  (net 66 "Net-(U4-Pad95)")
  (net 67 "Net-(U4-Pad96)")
  (net 68 "Net-(U4-Pad97)")
  (net 69 "Net-(U4-Pad98)")
  (net 70 "Net-(U4-Pad99)")
  (net 71 "Net-(U4-Pad100)")
  (net 72 "Net-(C2-Pad1)")
  (net 73 "Net-(C2-Pad2)")
  (net 74 "Net-(U1-Pad8)")
  (net 75 "Net-(U1-Pad10)")
  (net 76 "Net-(C19-Pad2)")
  (net 77 "Net-(C20-Pad1)")
  (net 78 "PT5")
  (net 79 "PR5")
  (net 80 "Net-(U4-Pad17)")
  (net 81 "Net-(U4-Pad38)")
  (net 82 "Net-(D1-Pad1)")
  (net 83 "Net-(U4-Pad8)")
  (net 84 "Net-(U4-Pad9)")
  (net 85 "Net-(U4-Pad58)")
  (net 86 "Net-(U4-Pad59)")
  (net 87 "+5V")
  (net 88 "Net-(D2-Pad1)")
  (net 89 "Net-(C11-Pad1)")
  (net 90 "Net-(C11-Pad2)")
  (net 91 "SCK1")
  (net 92 "Net-(R4-Pad2)")
  (net 93 "Net-(R4-Pad1)")
  (net 94 "Net-(R8-Pad2)")
  (net 95 "SDA1")
  (net 96 "SCL1")
  (net 97 "H2O")
  (net 98 "Net-(RTD1-Pad1)")
  (net 99 "Net-(H2O1-Pad2)")
  (net 100 "Net-(PIC1-Pad1)")
  (net 101 "Net-(PIC1-Pad6)")
  (net 102 "Net-(U4-Pad6)")
  (net 103 "Net-(U4-Pad7)")
  (net 104 "Net-(U1-Pad7)")
  (net 105 "Net-(U1-Pad9)")
  (net 106 "Net-(LED1-Pad1)")
  (net 107 "Net-(R12-Pad1)")
  (net 108 "Net-(BUCKTOOT(BATT)1-Pad2)")
  (net 109 "BATT")
  (net 110 "Net-(C76-Pad1)")
  (net 111 "LED")
  (net 112 "BUCK")
  (net 113 "Net-(R76-Pad1)")
  (net 114 "Net-(M1-Pad1)")
  (net 115 "Net-(M1-Pad2)")
  (net 116 "Net-(M1-Pad3)")
  (net 117 "Net-(M1-Pad4)")
  (net 118 "Net-(M2-Pad4)")
  (net 119 "Net-(M2-Pad3)")
  (net 120 "Net-(M2-Pad2)")
  (net 121 "Net-(M2-Pad1)")
  (net 122 "Net-(M5-Pad1)")
  (net 123 "Net-(M5-Pad2)")
  (net 124 "Net-(M5-Pad3)")
  (net 125 "Net-(M5-Pad4)")
  (net 126 "\\CS")
  (net 127 "Net-(U4-Pad10)")
  (net 128 "Net-(U4-Pad12)")
  (net 129 "Net-(Q1-Pad3)")
  (net 130 "Net-(U6-Pad20)")
  (net 131 "MISO")
  (net 132 "MOSI")
  (net 133 "\\DRDY")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (at 130.937 58.801 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Reference" "PIC1" (at 2.921 10.16 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x06" (at 2.286 5.842 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(PIC1-Pad1)")
    )
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3")
    )
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "PGD")
    )
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "PGC")
    )
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(PIC1-Pad6)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:post_small" (layer "F.Cu")
    (at 184.912 93.98 180)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "GND1" (at 0 -2.54 0) (layer "F.SilkS"))
    (property "Value" "TestPoint" (at 0 2.54 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 3.556 3.556) (drill 1.6764) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
  )
  (footprint "whoi:post_small" (layer "F.Cu")
    (at 179.2224 94.3483)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "+3.3V2" (at 0 -2.54 0) (layer "F.SilkS"))
    (property "Value" "TestPoint" (at 0 2.54 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.6764) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3")
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 119.9769 55.4609)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Reference" "J2" (at 2.9591 -0.0889 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x03" (at 0 7.85 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pad2)")
    )
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pad3)")
    )
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:403D" (layer "F.Cu")
    (at 175.26 77.216 180)
    (property "Reference" "D1" (at -4.445 0.254 -90) (layer "F.SilkS"))
    (property "Value" "MBRA130" (at 0 -2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -2 0 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(D1-Pad1)")
    )
    (pad "2" smd rect (at 2 0 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "BATT")
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-263-3_TabPin2" (layer "F.Cu")
    (at 174.9171 62.5094 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (property "Reference" "U2" (at 0 -6.65 90) (layer "F.SilkS"))
    (property "Value" "LM1084-3.3" (at 0 6.65 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers "F.Paste"))
    (pad "1" smd rect (at -5.775 -2.54 90) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "2" smd rect (at -5.775 0 90) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3")
    )
    (pad "2" smd rect (at 3.375 0 90) (size 9.4 10.8) (layers "F.Cu" "F.Mask")
      (net 4 "+3V3")
    )
    (pad "3" smd rect (at -5.775 2.54 90) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(D1-Pad1)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:403D" (layer "F.Cu")
    (at 164.465 104.648 90)
    (property "Reference" "D2" (at 0 2.5 90) (layer "F.SilkS"))
    (property "Value" "MBRA130" (at 0 -2.5 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (pad "1" smd rect (at -2 0 90) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D2-Pad1)")
    )
    (pad "2" smd rect (at 2 0 90) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "BATT")
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-263-3_TabPin2" (layer "F.Cu")
    (at 178.616 104.013)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (property "Reference" "U3" (at 1.4065 6.6802 0) (layer "F.SilkS"))
    (property "Value" "LM1084-5.0" (at 0 6.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers "F.Paste"))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers "F.Paste"))
    (pad "1" smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "2" smd rect (at -5.775 0) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "+5V")
    )
    (pad "2" smd rect (at 3.375 0) (size 9.4 10.8) (layers "F.Cu" "F.Mask")
      (net 87 "+5V")
    )
    (pad "3" smd rect (at -5.775 2.54) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D2-Pad1)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 161.330999 56.043001 -90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Reference" "U7" (at 2.856999 0.230999 180) (layer "F.SilkS"))
    (property "Value" "TL331" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(H2O1-Pad2)")
    )
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "3" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(R8-Pad2)")
    )
    (pad "4" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "H2O")
    )
    (pad "5" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 125.61316 69.64172 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Reference" "U1" (at 3.09372 6.21284 90) (layer "F.SilkS"))
    (property "Value" "MAX3232CSE" (at 0 5.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(C2-Pad1)")
    )
    (pad "2" smd roundrect (at -2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(C20-Pad1)")
    )
    (pad "3" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C2-Pad2)")
    )
    (pad "4" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C4-Pad1)")
    )
    (pad "5" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)")
    )
    (pad "6" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(C19-Pad2)")
    )
    (pad "7" smd roundrect (at -2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(U1-Pad7)")
    )
    (pad "8" smd roundrect (at -2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(U1-Pad8)")
    )
    (pad "9" smd roundrect (at 2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(U1-Pad9)")
    )
    (pad "10" smd roundrect (at 2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U1-Pad10)")
    )
    (pad "11" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "PT5")
    )
    (pad "12" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "PR5")
    )
    (pad "13" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad2)")
    )
    (pad "14" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J2-Pad3)")
    )
    (pad "15" smd roundrect (at 2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "16" smd roundrect (at 2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 120.6627 130.5687 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Reference" "J1" (at 0 5.08 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 109 "BATT")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (at 146.812 128.642099 -90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Reference" "LED1" (at 0.770901 6.096 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x02" (at 4.385 4.81 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 2.77 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "+5V")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 158.1755 127.8271 180)
    (descr "FE Package; 16-Lead Plastic TSSOP (4.4mm); Exposed Pad Variation BB; (see Linear Technology 1956f.pdf)")
    (tags "SSOP 0.65")
    (property "Reference" "U9" (at 0 -3.55 0) (layer "F.SilkS"))
    (property "Value" "LT3083" (at 0 3.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.775 -2.275 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "2" smd rect (at -2.775 -1.625 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "3" smd rect (at -2.775 -0.975 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "4" smd rect (at -2.775 -0.325 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "5" smd rect (at -2.775 0.325 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "6" smd rect (at -2.775 0.975 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "7" smd rect (at -2.775 1.625 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(Q1-Pad3)")
    )
    (pad "8" smd rect (at -2.775 2.275 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "9" smd rect (at 2.775 2.275 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "10" smd rect (at 2.775 1.625 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "+5V")
    )
    (pad "11" smd rect (at 2.775 0.975 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "+5V")
    )
    (pad "12" smd rect (at 2.775 0.325 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (pad "13" smd rect (at 2.775 -0.325 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (pad "14" smd rect (at 2.775 -0.975 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (pad "15" smd rect (at 2.775 -1.625 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (pad "16" smd rect (at 2.775 -2.275 180) (size 1.05 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "17" smd rect (at -0.735 -1.3425 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at -0.735 -0.4475 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at -0.735 0.4475 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at -0.735 1.3425 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at 0.735 -1.3425 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at 0.735 -0.4475 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at 0.735 0.4475 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (pad "17" smd rect (at 0.735 1.3425 180) (size 1.47 0.895) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_paste_margin_ratio -0.2)
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (at 121.92 109.855 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Reference" "BUCKTOOT(BATT)1" (at -3.556 0.635 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x02" (at 4.385 4.81 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 2.77 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 108 "Net-(BUCKTOOT(BATT)1-Pad2)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at 132.977001 108.404999 90)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Reference" "U75" (at 3.756999 2.150999 90) (layer "F.SilkS"))
    (property "Value" "TPS22810" (at 0 2.9 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "BATT")
    )
    (pad "2" smd rect (at -1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "3" smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "BUCK")
    )
    (pad "4" smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "Net-(C76-Pad1)")
    )
    (pad "5" smd rect (at 1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "Net-(R76-Pad1)")
    )
    (pad "6" smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "Net-(BUCKTOOT(BATT)1-Pad2)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 160.02 47.498 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Reference" "H2O1" (at 0.127 -2.794 90) (layer "F.SilkS"))
    (property "Value" "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(H2O1-Pad2)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 141.6 95.1 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Reference" "HUM1" (at 0 -2.33 90) (layer "F.SilkS"))
    (property "Value" "SPARKSi7021" (at 0 9.95 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3")
    )
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 95 "SDA1")
    )
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 96 "SCL1")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:post_small" (layer "F.Cu")
    (at 144.145 112.395)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "BATT1" (at 0 -2.54 0) (layer "F.SilkS"))
    (property "Value" "TestPoint" (at 0 2.54 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.6764) (layers "*.Cu" "*.Mask")
      (net 109 "BATT")
    )
  )
  (footprint "whoi:post_small" (layer "F.Cu")
    (at 153.924 118.872)
    (descr "Wire solder connection")
    (tags "connector")
    (property "Reference" "5V1" (at 0 -2.54 0) (layer "F.SilkS"))
    (property "Value" "TestPoint" (at 0 2.54 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.6764) (layers "*.Cu" "*.Mask")
      (net 87 "+5V")
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 120.904 76.454)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C2" (at 0 1.524 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(C2-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C2-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.126 69.85 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C20" (at -3.23088 0.254 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(C20-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 125.476 76.454)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C4" (at 0 1.524 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C4-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 129.54 76.454 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C19" (at 0 -1.43 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(C19-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 121.60264 64.01816)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C5" (at 5.14336 0.24384 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.398 67.183 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C1" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "MCLR")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 150.8608 57.912 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C13" (at 0 -1.651 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.573 64.77 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C14" (at 4.064 0.0762 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.6238 70.231 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C15" (at 0 1.4478 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.6238 74.102 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C17" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 152.019 81.534 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C18" (at 0 -1.43 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.398 75.184 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R1" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "MCLR")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.398 71.247 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R2" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "470" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(PIC1-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "MCLR")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.652 109.728 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R75" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "BUCK")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.588 104.14 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R76" (at 0 1.524 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R76-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(BUCKTOOT(BATT)1-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 129.54 110.744 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "C75" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "BATT")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.652 104.648 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "C76" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "0.01uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(C76-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 129.54 106.172 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "C77" (at -1.016 1.524 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(BUCKTOOT(BATT)1-Pad2)")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 164.846 61.849 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C12" (at -2.399 -0.635 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 120.142 80.8355)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C9" (at 0 -1.43 0) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 125 96.175 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C11" (at 0.125 -1.6 90) (layer "F.SilkS"))
    (property "Value" "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(C11-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(C11-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.0625 85.598 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R4" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "4K" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R4-Pad1)")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(R4-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.4295 85.852)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R5" (at 0.127 1.778 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "SCK1")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.493 83.693)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R6" (at 0 -1.5875 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "MISO")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 165.227 55.88 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R7" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "1M" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(H2O1-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 160.782 52.197 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R8" (at 0 -1.43 0) (layer "F.SilkS"))
    (property "Value" "100K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R8-Pad2)")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 156.845 55.88 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R9" (at 0 -1.43 90) (layer "F.SilkS"))
    (property "Value" "100K" (at 0 1.43 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R8-Pad2)")
    )
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 145.8 89.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R10" (at -0.125 -1.5 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "SDA1")
    )
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 150.1 89.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R11" (at 0 1.4 0) (layer "F.SilkS"))
    (property "Value" "10K" (at 0 1.43 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "SCL1")
    )
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 170.561 73.533 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C3" (at 0 -1.82 0) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 4 "+3V3")
    )
    (pad "2" smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 165.608 75.692 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C6" (at 0 -1.82 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 109 "BATT")
    )
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 164.465 94.361 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C7" (at 0 -1.82 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 109 "BATT")
    )
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 168.529 98.425 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C8" (at 0 -1.82 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 87 "+5V")
    )
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 165.354 67.821 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C16" (at 0 -1.82 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 9 "Net-(C16-Pad2)")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 151.892 124.714 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Reference" "C21" (at 0 -1.82 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0 1.82 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 87 "+5V")
    )
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:PIC24" (layer "F.Cu")
    (at 151.8158 69.342 -90)
    (descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "Reference" "U4" (at 0 -9.35 90) (layer "F.SilkS"))
    (property "Value" "PIC24" (at 0 9.35 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -7.9165 -6 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U4-Pad1)")
    )
    (pad "2" smd roundrect (at -7.9165 -5.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "3" smd roundrect (at -7.9165 -5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U4-Pad3)")
    )
    (pad "4" smd roundrect (at -7.9165 -4.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U4-Pad4)")
    )
    (pad "5" smd roundrect (at -7.9165 -4 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "H2O")
    )
    (pad "6" smd roundrect (at -7.9165 -3.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(U4-Pad6)")
    )
    (pad "7" smd roundrect (at -7.9165 -3 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(U4-Pad7)")
    )
    (pad "8" smd roundrect (at -7.9165 -2.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U4-Pad8)")
    )
    (pad "9" smd roundrect (at -7.9165 -2 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(U4-Pad9)")
    )
    (pad "10" smd roundrect (at -7.9165 -1.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(U4-Pad10)")
    )
    (pad "11" smd roundrect (at -7.9165 -1 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U4-Pad11)")
    )
    (pad "12" smd roundrect (at -7.9165 -0.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(U4-Pad12)")
    )
    (pad "13" smd roundrect (at -7.9165 0 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "MCLR")
    )
    (pad "14" smd roundrect (at -7.9165 0.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U4-Pad14)")
    )
    (pad "15" smd roundrect (at -7.9165 1 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "16" smd roundrect (at -7.9165 1.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "17" smd roundrect (at -7.9165 2 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(U4-Pad17)")
    )
    (pad "18" smd roundrect (at -7.9165 2.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U4-Pad18)")
    )
    (pad "19" smd roundrect (at -7.9165 3 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U4-Pad19)")
    )
    (pad "20" smd roundrect (at -7.9165 3.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U4-Pad20)")
    )
    (pad "21" smd roundrect (at -7.9165 4 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U4-Pad21)")
    )
    (pad "22" smd roundrect (at -7.9165 4.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U4-Pad22)")
    )
    (pad "23" smd roundrect (at -7.9165 5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U4-Pad23)")
    )
    (pad "24" smd roundrect (at -7.9165 5.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U4-Pad24)")
    )
    (pad "25" smd roundrect (at -7.9165 6 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U4-Pad25)")
    )
    (pad "26" smd roundrect (at -6 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "PGC")
    )
    (pad "27" smd roundrect (at -5.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "PGD")
    )
    (pad "28" smd roundrect (at -5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U4-Pad28)")
    )
    (pad "29" smd roundrect (at -4.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U4-Pad29)")
    )
    (pad "30" smd roundrect (at -4 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "31" smd roundrect (at -3.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "32" smd roundrect (at -3 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U4-Pad32)")
    )
    (pad "33" smd roundrect (at -2.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U4-Pad33)")
    )
    (pad "34" smd roundrect (at -2 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U4-Pad34)")
    )
    (pad "35" smd roundrect (at -1.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U4-Pad35)")
    )
    (pad "36" smd roundrect (at -1 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "37" smd roundrect (at -0.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "38" smd roundrect (at 0 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(U4-Pad38)")
    )
    (pad "39" smd roundrect (at 0.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U4-Pad39)")
    )
    (pad "40" smd roundrect (at 1 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U4-Pad40)")
    )
    (pad "41" smd roundrect (at 1.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U4-Pad41)")
    )
    (pad "42" smd roundrect (at 2 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U4-Pad42)")
    )
    (pad "43" smd roundrect (at 2.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U4-Pad43)")
    )
    (pad "44" smd roundrect (at 3 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(U4-Pad44)")
    )
    (pad "45" smd roundrect (at 3.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "46" smd roundrect (at 4 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "47" smd roundrect (at 4.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(U4-Pad47)")
    )
    (pad "48" smd roundrect (at 5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(U4-Pad48)")
    )
    (pad "49" smd roundrect (at 5.5 8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "\\DRDY")
    )
    (pad "50" smd roundrect (at 6 8.001 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "\\CS")
    )
    (pad "51" smd roundrect (at 8.0435 6 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "PT5")
    )
    (pad "52" smd roundrect (at 8.0435 5.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "PR5")
    )
    (pad "53" smd roundrect (at 8.0435 5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "MOSI")
    )
    (pad "54" smd roundrect (at 8.0435 4.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "MISO")
    )
    (pad "55" smd roundrect (at 8.0435 4 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "SCK1")
    )
    (pad "56" smd roundrect (at 8.0435 3.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "SDA1")
    )
    (pad "57" smd roundrect (at 8.0435 3 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "SCL1")
    )
    (pad "58" smd roundrect (at 8.0435 2.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(U4-Pad58)")
    )
    (pad "59" smd roundrect (at 8.0435 2 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(U4-Pad59)")
    )
    (pad "60" smd roundrect (at 8.0435 1.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(U4-Pad60)")
    )
    (pad "61" smd roundrect (at 8.0435 1 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U4-Pad61)")
    )
    (pad "62" smd roundrect (at 8.0435 0.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "63" smd roundrect (at 8.0435 0 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(U4-Pad63)")
    )
    (pad "64" smd roundrect (at 8.0435 -0.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(U4-Pad64)")
    )
    (pad "65" smd roundrect (at 8.0435 -1 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "66" smd roundrect (at 8.0435 -1.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(U4-Pad66)")
    )
    (pad "67" smd roundrect (at 8.0435 -2 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(U4-Pad67)")
    )
    (pad "68" smd roundrect (at 8.0435 -2.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(U4-Pad68)")
    )
    (pad "69" smd roundrect (at 8.0435 -3 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(U4-Pad69)")
    )
    (pad "70" smd roundrect (at 8.0435 -3.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U4-Pad70)")
    )
    (pad "71" smd roundrect (at 8.0435 -4 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(U4-Pad71)")
    )
    (pad "72" smd roundrect (at 8.0435 -4.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(U4-Pad72)")
    )
    (pad "73" smd roundrect (at 8.0435 -5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(U4-Pad73)")
    )
    (pad "74" smd roundrect (at 8.0435 -5.5 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(U4-Pad74)")
    )
    (pad "75" smd roundrect (at 8.0435 -6 270) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "76" smd roundrect (at 6 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "BUCK")
    )
    (pad "77" smd roundrect (at 5.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "LED")
    )
    (pad "78" smd roundrect (at 5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(U4-Pad78)")
    )
    (pad "79" smd roundrect (at 4.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(U4-Pad79)")
    )
    (pad "80" smd roundrect (at 4 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(U4-Pad80)")
    )
    (pad "81" smd roundrect (at 3.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U4-Pad81)")
    )
    (pad "82" smd roundrect (at 3 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(U4-Pad82)")
    )
    (pad "83" smd roundrect (at 2.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U4-Pad83)")
    )
    (pad "84" smd roundrect (at 2 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(U4-Pad84)")
    )
    (pad "85" smd roundrect (at 1.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C16-Pad2)")
    )
    (pad "86" smd roundrect (at 1 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "87" smd roundrect (at 0.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(U4-Pad87)")
    )
    (pad "88" smd roundrect (at 0 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(U4-Pad88)")
    )
    (pad "89" smd roundrect (at -0.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(U4-Pad89)")
    )
    (pad "90" smd roundrect (at -1 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(U4-Pad90)")
    )
    (pad "91" smd roundrect (at -1.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U4-Pad91)")
    )
    (pad "92" smd roundrect (at -2 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(U4-Pad92)")
    )
    (pad "93" smd roundrect (at -2.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(U4-Pad93)")
    )
    (pad "94" smd roundrect (at -3 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(U4-Pad94)")
    )
    (pad "95" smd roundrect (at -3.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(U4-Pad95)")
    )
    (pad "96" smd roundrect (at -4 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(U4-Pad96)")
    )
    (pad "97" smd roundrect (at -4.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(U4-Pad97)")
    )
    (pad "98" smd roundrect (at -5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(U4-Pad98)")
    )
    (pad "99" smd roundrect (at -5.5 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(U4-Pad99)")
    )
    (pad "100" smd roundrect (at -6 -8.0435 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(U4-Pad100)")
    )
    (model "${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (at 165.481 130.2131)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R12" (at -0.127 1.9304 0) (layer "F.SilkS"))
    (property "Value" "0.5ohms" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173904348)
      (net 107 "Net-(R12-Pad1)")
    )
    (pad "2" smd roundrect (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173904348)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 165.4025 126.6571)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Reference" "R13" (at 0 -1.65 0) (layer "F.SilkS"))
    (property "Value" "15K" (at 0 1.65 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083325)
      (net 129 "Net-(Q1-Pad3)")
    )
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083325)
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (at 121.285 98.425 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Reference" "RTD1" (at 4.385 -2.27 0) (layer "F.SilkS"))
    (property "Value" "Conn_01x03" (at 4.385 7.35 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 2.77 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(RTD1-Pad1)")
    )
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(C11-Pad2)")
    )
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(C11-Pad1)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 171.958 128.5875 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q2" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "DMG3406L" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "LED")
    )
    (pad "2" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "3" smd rect (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(LED1-Pad1)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 172.0215 123.1265 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Reference" "Q1" (at 0 -2.5 0) (layer "F.SilkS"))
    (property "Value" "DMG3406L" (at 0 2.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "LED")
    )
    (pad "2" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND")
    )
    (pad "3" smd rect (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(Q1-Pad3)")
    )
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3266W_Vertical" (layer "F.Cu")
    (at 166.3065 118.491)
    (descr "Potentiometer, vertical, Bourns 3266W, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266W")
    (property "Reference" "RV1" (at -2.54 -2.27 0) (layer "F.SilkS"))
    (property "Value" "50K" (at -2.54 4.73 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at -3.175 1.23 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 129 "Net-(Q1-Pad3)")
    )
    (pad "2" thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 129 "Net-(Q1-Pad3)")
    )
    (pad "3" thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND")
    )
    (model "${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "whoi:MAX31865" (layer "F.Cu")
    (at 127.127 85.5345)
    (descr "SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (property "Reference" "U6" (at 0 -4.55 0) (layer "F.SilkS"))
    (property "Value" "MAX31865xAP" (at 0 4.55 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.5 -2.925) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "\\DRDY")
    )
    (pad "2" smd roundrect (at -3.5 -2.275) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "3" smd roundrect (at -3.5 -1.625) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3")
    )
    (pad "4" smd roundrect (at -3.5 -0.975) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R4-Pad1)")
    )
    (pad "5" smd roundrect (at -3.5 -0.325) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R4-Pad1)")
    )
    (pad "6" smd roundrect (at -3.5 0.325) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(R4-Pad2)")
    )
    (pad "7" smd roundrect (at -3.5 0.975) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(R4-Pad2)")
    )
    (pad "8" smd roundrect (at -3.5 1.625) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(RTD1-Pad1)")
    )
    (pad "9" smd roundrect (at -3.5 2.275) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(RTD1-Pad1)")
    )
    (pad "10" smd roundrect (at -3.5 2.925) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(C11-Pad2)")
    )
    (pad "11" smd roundrect (at 3.5 2.925) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(C11-Pad1)")
    )
    (pad "12" smd roundrect (at 3.5 2.275) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(C11-Pad1)")
    )
    (pad "13" smd roundrect (at 3.5 1.625) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "14" smd roundrect (at 3.5 0.975) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "MOSI")
    )
    (pad "15" smd roundrect (at 3.5 0.325) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "SCK1")
    )
    (pad "16" smd roundrect (at 3.5 -0.325) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "\\CS")
    )
    (pad "17" smd roundrect (at 3.5 -0.975) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "MISO")
    )
    (pad "18" smd roundrect (at 3.5 -1.625) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "19" smd roundrect (at 3.5 -2.275) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND")
    )
    (pad "20" smd roundrect (at 3.5 -2.925) (size 1.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(U6-Pad20)")
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_5.3x7.2mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "B.Cu")
    (at 184.722 53.68386 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "h4" (at 0 4.2 0) (layer "B.SilkS") hide)
    (property "Value" "MountingHole_3.2mm_M3" (at 0 -4.2 0) (layer "B.Fab") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "B.Cu")
    (at 137.9947 53.69656 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "h3" (at 0 4.2 0) (layer "B.SilkS") hide)
    (property "Value" "MountingHole_3.2mm_M3" (at 0 -4.2 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "B.Cu")
    (at 138.0709 120.4299 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "h1" (at 0 4.2 0) (layer "B.SilkS") hide)
    (property "Value" "MountingHole_3.2mm_M3" (at 0 -4.2 0) (layer "B.Fab") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "B.Cu")
    (at 184.722 120.36386 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "h2" (at 0 4.2 0) (layer "B.SilkS") hide)
    (property "Value" "MountingHole_3.2mm_M3" (at 0 -4.2 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" locked (layer "B.Cu")
    (at 120.5357 121.4247)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (property "Reference" "M1" (at 1.27 2.33 0) (layer "B.SilkS") hide)
    (property "Value" "Conn_02x02_Odd_Even" (at 1.27 -4.87 0) (layer "B.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.27 -1.27 -90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(M1-Pad1)")
    )
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "Net-(M1-Pad2)")
    )
    (pad "3" thru_hole oval locked (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(M1-Pad3)")
    )
    (pad "4" thru_hole oval locked (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(M1-Pad4)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" locked (layer "B.Cu")
    (at 121.0437 50.3047)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (property "Reference" "M2" (at 1.27 2.33 0) (layer "B.SilkS") hide)
    (property "Value" "Conn_02x02_Odd_Even" (at 1.27 -4.87 0) (layer "B.Fab") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.27 -1.27 -90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 121 "Net-(M2-Pad1)")
    )
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 120 "Net-(M2-Pad2)")
    )
    (pad "3" thru_hole oval locked (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(M2-Pad3)")
    )
    (pad "4" thru_hole oval locked (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 118 "Net-(M2-Pad4)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" locked (layer "B.Cu")
    (at 177.1015 86.4997)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (property "Reference" "M5" (at 1.27 2.33 0) (layer "B.SilkS"))
    (property "Value" "Conn_02x02_Odd_Even" (at 1.27 -4.87 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 1.27 -1.27 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 122 "Net-(M5-Pad1)")
    )
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 123 "Net-(M5-Pad2)")
    )
    (pad "3" thru_hole oval locked (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 124 "Net-(M5-Pad3)")
    )
    (pad "4" thru_hole oval locked (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 125 "Net-(M5-Pad4)")
    )
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 188.595 43.18) (end 188.595 133.985)
    (layer "Edge.Cuts"))
  (gr_line (start 116.84 133.985) (end 188.595 133.985)
    (layer "Edge.Cuts"))
  (gr_line (start 116.8109 42.9768) (end 188.595 43.18)
    (layer "Edge.Cuts"))
  (gr_line (start 116.84 133.985) (end 116.8109 42.9768)
    (layer "Edge.Cuts"))
  (gr_text "Envboard rev4\nSonnichsen 12/01/2020" (at 177.546 47.117 0) (layer "B.SilkS"))
  (gr_text "-->" (at 123.9393 60.8838 180) (layer "F.SilkS"))
  (gr_text "BATT" (at 122.301 127.3556 0) (layer "F.SilkS"))
  (gr_text "-" (at 119.126 126.7206 0) (layer "F.SilkS"))
  (gr_text "+" (at 124.968 127 0) (layer "F.SilkS"))
  (gr_text "5V" (at 183.769 111.9505 180) (layer "F.SilkS"))
  (gr_text "(-)" (at 121.92 113.792 180) (layer "F.SilkS"))
  (gr_text "+" (at 121.92 104.267 90) (layer "F.SilkS"))
  (gr_text "+" (at 142.748 125.603 90) (layer "F.SilkS"))
  (gr_text "(-)" (at 147.828 125.476 180) (layer "F.SilkS"))
  (gr_text "-->" (at 123.9266 58.2168 0) (layer "F.SilkS"))
  (gr_text "3.3V" (at 182.626 62.484 90) (layer "F.SilkS"))
  (gr_text "RS232" (at 126.873 58.7121 90) (layer "F.SilkS"))
  (gr_text "Envboard rev4\nSonnichsen 12/01/2020" (at 178.308 46.736 0) (layer "F.SilkS"))
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.3 43.4)
        (xy 188.4 133.8)
        (xy 117 133.8)
        (xy 117 43.2)
      )
    )
  )
  (zone (net 4) (net_name "+3V3") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.3 43.4)
        (xy 188.4 133.8)
        (xy 117 133.8)
        (xy 117 43.2)
      )
    )
  )
)
