(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/ThisIsNot_a_NoName_net")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J3-Pad4)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J3-Pad1)")
  (footprint "digikey-footprints:PinHeader_1x4_P2.54mm_Drill1.02mm" (layer "F.Cu")
    (at 133.62 68.79)
    (descr "http://www.molex.com/pdm_docs/sd/022232031_sd.pdf")
    (property "Reference" "J1" (at 4.33 -4.56 0) (layer "F.SilkS"))
    (property "Value" "0022232041" (at 4.08 4.52 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "CONN HEADER VERT 4POS 2.54MM" (at 133.62 68.79 0) (layer "F.Fab") hide)
    (property "Category" "Connectors, Interconnects" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Datasheet_Link" "https://www.molex.com/pdm_docs/sd/022232041_sd.pdf" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Detail_Page" "/product-detail/en/molex/0022232041/WM4202-ND/26671" (at 0 0 0) (layer "F.Fab") hide)
    (property "Digi-Key_PN" "WM4202-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Family" "Rectangular Connectors - Headers, Male Pins" (at 0 0 0) (layer "F.Fab") hide)
    (property "MPN" "0022232041" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Molex" (at 0 0 0) (layer "F.Fab") hide)
    (property "Status" "Active" (at 0 0 0) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 4.17 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.02 2.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J3-Pad4)")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 2.02 2.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J3-Pad1)")
    )
    (pad "3" thru_hole circle (at 5.08 0) (size 2.02 2.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pad3)")
    )
    (pad "4" thru_hole circle (at 7.62 0) (size 2.02 2.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J3-Pad4)")
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (at 137.87 81.99)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Reference" "H1" (at 0 -3.8 0) (layer "F.SilkS") hide)
    (property "Value" "MountingHole" (at 0 3.8 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Comment_sch" "M3x5" (at 0 0 0) (layer "F.Fab") hide)
    (sheetfile "MB Expander.kicad_sch")
    (attr exclude_from_pos_files)
    (fp_text user "${REFERENCE}" (at 0.3 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.6) (clearance 1.7)
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right" (layer "F.Cu")
    (at 128.24 75.1)
    (descr "surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right")
    (property "Reference" "J3" (at 0 -8.68 0) (layer "F.SilkS"))
    (property "Value" "0022232041" (at 0 8.68 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "CONN HEADER VERT 4POS 2.54MM" (at 128.24 75.1 0) (layer "F.Fab") hide)
    (property "Category" "Connectors, Interconnects" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Datasheet_Link" "https://www.molex.com/pdm_docs/sd/022232041_sd.pdf" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Detail_Page" "/product-detail/en/molex/0022232041/WM4202-ND/26671" (at 0 0 0) (layer "F.Fab") hide)
    (property "Digi-Key_PN" "WM4202-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Family" "Rectangular Connectors - Headers, Male Pins" (at 0 0 0) (layer "F.Fab") hide)
    (property "MPN" "0022232041" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Molex" (at 0 0 0) (layer "F.Fab") hide)
    (property "Status" "Active" (at 0 0 0) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.655 -6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J3-Pad1)")
    )
    (pad "2" smd rect (at -1.655 -3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J3-Pad2)")
    )
    (pad "3" smd rect (at 1.655 -1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J3-Pad3)")
    )
    (pad "4" smd rect (at -1.655 1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J3-Pad4)")
    )
    (pad "5" smd rect (at 1.655 3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at -1.655 6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "qli-footprints:MountingHole_M3_wKeepout" (layer "F.Cu")
    (at 138.74 75.22)
    (property "Reference" "REF**" (at 0.5 4.5 0) (layer "F.SilkS"))
    (property "Value" "MountingHole_M3_wKeepout" (at 0 -0.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 0.5 4.5 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 1.6) (clearance 1.7)
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right" (layer "F.Cu")
    (at 147.16 75.63)
    (descr "surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right")
    (property "Reference" "J2" (at 0 -8.68 0) (layer "F.SilkS"))
    (property "Value" "0022232041" (at 0 8.68 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "CONN HEADER VERT 4POS 2.54MM" (at 147.16 75.63 0) (layer "F.Fab") hide)
    (property "Category" "Connectors, Interconnects" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Datasheet_Link" "https://www.molex.com/pdm_docs/sd/022232041_sd.pdf" (at 0 0 0) (layer "F.Fab") hide)
    (property "DK_Detail_Page" "/product-detail/en/molex/0022232041/WM4202-ND/26671" (at 0 0 0) (layer "F.Fab") hide)
    (property "Digi-Key_PN" "WM4202-ND" (at 0 0 0) (layer "F.Fab") hide)
    (property "Family" "Rectangular Connectors - Headers, Male Pins" (at 0 0 0) (layer "F.Fab") hide)
    (property "MPN" "0022232041" (at 0 0 0) (layer "F.Fab") hide)
    (property "Manufacturer" "Molex" (at 0 0 0) (layer "F.Fab") hide)
    (property "Status" "Active" (at 0 0 0) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.655 -6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/ThisIsNot_a_NoName_net")
    )
    (pad "2" smd rect (at -1.655 -3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J2-Pad2)")
    )
    (pad "3" smd rect (at 1.655 -1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J2-Pad3)")
    )
    (pad "4" smd rect (at -1.655 1.27) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J3-Pad4)")
    )
    (pad "5" smd rect (at 1.655 3.81) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at -1.655 6.35) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 119.21 61.32) (end 154.59 87.08)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "REF**" (at 134.32 64.77 0) (layer "F.SilkS"))
  (gr_text "HeaderPin_2x2_P4.2_Drill1.4mm" (at 135.040459 80.679711 0) (layer "F.Fab"))
  (zone (net 1) (net_name "/ThisIsNot_a_NoName_net") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.31 58.54)
        (xy 159.69 90.53)
        (xy 111.68 91.56)
        (xy 115.96 53.56)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J3-Pad3)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.4))
    (min_thickness 0.21) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.63 85.62)
        (xy 124.15 86.21)
        (xy 128.98 71.03)
        (xy 130.67 70.19)
        (xy 135.36 71.48)
      )
    )
  )
)
