(kicad_pcb (version 20210722) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "signal")
  (footprint "Housings_DIP:DIP-14_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 6105426B)
    (at 154.305 74.93)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -5.22) (layer "F.SilkS"))
    (fp_text value "DIP-14_W7.62mm_LongPads" (at 0 -3.72) (layer "F.Fab"))
    (fp_rect (start 2.286 0.127) (end 5.334 14.732) (layer "Edge.Cuts") (width 0.05) (fill none))
    (pad "1" thru_hole oval locked (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "signal"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "signal"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 78.105 50.165) (end 228.6 130.81) (layer "Edge.Cuts") (width 0.05) (fill none))
)
