(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "HomeControl Temperature/Humidity Sensor Interface")
		(date "2020-11-23")
		(rev "1.0")
		(company "WorldInOne M.Straub")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "Mechanical.2")
		(19 "Cmts.User" user "Mechanical.1")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 150 100)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755557f)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros yes)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Manufacture/Gerber/JLCPCB/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-Pad2)")
	(net 2 "GND")
	(net 3 "Net-(C14-Pad1)")
	(net 4 "Net-(C15-Pad1)")
	(net 5 "Net-(D12-Pad1)")
	(net 6 "/5V ")
	(net 7 "Net-(IC2-Pad1)")
	(net 8 "Net-(L1-Pad2)")
	(net 9 "Net-(L2-Pad2)")
	(net 10 "Net-(L3-Pad2)")
	(net 11 "Net-(L4-Pad2)")
	(net 12 "/230V & general interface/230V1")
	(net 13 "Net-(L5-Pad2)")
	(net 14 "Net-(L6-Pad2)")
	(net 15 "Net-(R13-Pad2)")
	(net 16 "Net-(R17-Pad2)")
	(net 17 "/AM2315 sensors I2C interface/S0SDA")
	(net 18 "/AM2315 sensors I2C interface/S0SCL")
	(net 19 "/AM2315 sensors I2C interface/S1SDA")
	(net 20 "Net-(R18-Pad2)")
	(net 21 "/AM2315 sensors I2C interface/S1SCL")
	(net 22 "/AM2315 sensors I2C interface/S2SDA")
	(net 23 "Net-(R19-Pad2)")
	(net 24 "Net-(R20-Pad2)")
	(net 25 "Net-(IC1-Pad1)")
	(net 26 "/AM2315 sensors I2C interface/S2SCL")
	(net 27 "no_connect_(IC1-Pad2)")
	(net 28 "/SCL")
	(net 29 "/SDA")
	(net 30 "/AM2315 sensors I2C interface/S3SDA")
	(net 31 "/AM2315 sensors I2C interface/S3SCL")
	(net 32 "/AM2315 sensors I2C interface/S4SDA")
	(net 33 "Net-(P11-Pad1)")
	(net 34 "Net-(P11-Pad2)")
	(net 35 "Net-(P12-Pad1)")
	(net 36 "Net-(P12-Pad2)")
	(net 37 "no_connect_(IC1-Pad3)")
	(net 38 "no_connect_(IC2-Pad2)")
	(net 39 "/230V & general interface/230V2")
	(net 40 "Net-(IC2-Pad4)")
	(net 41 "no_connect_(IC2-Pad3)")
	(net 42 "Net-(R22-Pad2)")
	(net 43 "Net-(R23-Pad2)")
	(net 44 "/AM2315 sensors I2C interface/S4SCL")
	(net 45 "Net-(P13-Pad1)")
	(net 46 "Net-(P13-Pad2)")
	(net 47 "Net-(P14-Pad1)")
	(net 48 "/AM2315 sensors I2C interface/S5SDA")
	(net 49 "Net-(FH1-Pad1)")
	(net 50 "/AM2315 sensors I2C interface/S5SCL")
	(net 51 "Net-(R24-Pad2)")
	(net 52 "Net-(P14-Pad2)")
	(net 53 "no_connect_(U13-Pad17)")
	(net 54 "no_connect_(U13-Pad18)")
	(net 55 "no_connect_(U13-Pad19)")
	(net 56 "no_connect_(U13-Pad20)")
	(net 57 "Net-(D2-Pad2)")
	(net 58 "Net-(D13-Pad1)")
	(net 59 "Net-(D11-Pad1)")
	(net 60 "/12V")
	(net 61 "Net-(D14-Pad1)")
	(net 62 "Net-(D9-Pad2)")
	(net 63 "Net-(D12-Pad2)")
	(net 64 "Net-(R14-Pad2)")
	(net 65 "Net-(R15-Pad2)")
	(net 66 "Net-(R21-Pad2)")
	(net 67 "Net-(IC1-Pad4)")
	(net 68 "Net-(R16-Pad2)")
	(net 69 "/5VMCU")
	(net 70 "/NIORESET")
	(net 71 "Net-(D14-Pad2)")
	(net 72 "Net-(P9-Pad1)")
	(net 73 "/230V & general interface/AUX")
	(net 74 "/230V & general interface/DOOR")
	(net 75 "/230V & general interface/ZWANG")
	(net 76 "/230V & general interface/BTP6")
	(net 77 "/230V & general interface/ZUAB")
	(net 78 "/230V & general interface/ENTFON")
	(net 79 "Net-(R37-Pad2)")
	(net 80 "Net-(P9-Pad2)")
	(net 81 "Net-(P10-Pad1)")
	(net 82 "Net-(P10-Pad2)")
	(net 83 "Net-(D10-Pad2)")
	(net 84 "Net-(D11-Pad2)")
	(net 85 "Net-(R26-Pad1)")
	(net 86 "Net-(D13-Pad2)")
	(net 87 "Net-(R27-Pad1)")
	(net 88 "/NIOINT")
	(net 89 "/230V & general interface/BTP5")
	(net 90 "/230V & general interface/BTP4")
	(net 91 "/230V & general interface/BTP3")
	(net 92 "Net-(R28-Pad1)")
	(net 93 "/230V & general interface/BTP2")
	(net 94 "Net-(R30-Pad1)")
	(net 95 "no_connect_(U18-Pad4)")
	(net 96 "Net-(R29-Pad1)")
	(net 97 "Net-(R31-Pad1)")
	(net 98 "Net-(R32-Pad1)")
	(net 99 "Net-(R33-Pad1)")
	(net 100 "no_connect_(U18-Pad5)")
	(net 101 "no_connect_(J1-Pad8)")
	(net 102 "no_connect_(J1-Pad7)")
	(net 103 "/230V & general interface/BTP1")
	(net 104 "/230V & general interface/BTL6")
	(net 105 "/230V & general interface/BTL3")
	(net 106 "/230V & general interface/BTL4")
	(net 107 "/230V & general interface/BTL1")
	(net 108 "no_connect_(J1-PadGA)")
	(net 109 "no_connect_(J1-PadYA)")
	(net 110 "/230V & general interface/BTL7")
	(net 111 "/230V & general interface/ENTFRH")
	(net 112 "/230V & general interface/BTL5")
	(net 113 "Net-(D3-Pad1)")
	(net 114 "Net-(R36-Pad2)")
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 200.8505 111.73968 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 0 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 312.59018 -89.11082 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 312.59018 -89.11082 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 312.59018 -89.11082 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 312.59018 -89.11082 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "Net-(D10-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.216 90.4748 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 1.5875 270)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 113.7412 294.6908 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 113.7412 294.6908 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 113.7412 294.6908 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 113.7412 294.6908 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Net-(R32-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/230V & general interface/BTP3")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 182.626 89.378 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 272.004 -93.248 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 272.004 -93.248 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 272.004 -93.248 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 272.004 -93.248 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Net-(R28-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/230V & general interface/BTP1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 203.708 71.58736 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D1"
			(at -3.302 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 407.416 143.17472 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_DIP:DIP-8_W7.62mm_Socketed"
		(layer "F.Cu")
		(at 173.504422 118.538283 90)
		(descr "8-lead dip package, row spacing 7.62 mm (300 mils), socketed")
		(tags "dil dip 2.54 300")
		(property "Reference" "IC1"
			(at 3.628683 -2.277835 90)
			(layer "F.SilkS")
		)
		(property "Value" "HCPL-3760"
			(at 0 -3.72 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(IC1-Pad1)")
			(pinfunction "AC+")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "no_connect_(IC1-Pad2)")
			(pinfunction "DC+")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "no_connect_(IC1-Pad3)")
			(pinfunction "DC-")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(IC1-Pad4)")
			(pinfunction "AC-")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/230V & general interface/230V1")
			(pinfunction "Vo")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/5V ")
			(pinfunction "VCC")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Sockets_DIP.3dshapes/Socket_DIP8.stp"
			(offset (xyz 3.81 -3.81 3.81))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 90))
		)
		(model "${KICAD6_3DMODEL_DIR}/Housings_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset (xyz 0 0 3.5))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 120.108696 107.66645)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q4"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "/230V & general interface/AUX")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D12-Pad1)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 115 135.04025 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P9"
			(at -6.3715 5.842 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(P9-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(P9-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 155.6385 70.358 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L1"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 225.9965 -85.2805 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(L1-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 141.6685 70.5485 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L6"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 212.217 -71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(L6-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 168.7345 73.406 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.301 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 337.469 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 337.469 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 337.469 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 337.469 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 337.469 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 112.791 73.5815 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.301 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 225.582 147.163 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 225.582 147.163 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 225.582 147.163 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 225.582 147.163 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 225.582 147.163 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 189.687865 108.441002)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at -0.015 -1.7145 0)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 126.619 73.5965 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.3495 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 253.238 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 253.238 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 253.238 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 253.238 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 253.238 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SMA_Standard"
		(layer "F.Cu")
		(at 119.507 94.0435 90)
		(descr "Diode SMA")
		(tags "Diode SMA")
		(property "Reference" "D4"
			(at -4.2545 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "SS34"
			(at 0 4.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.99898 0 90)
			(size 2.49936 1.80086)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.99898 0 90)
			(size 2.49936 1.80086)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(zone_connect 2)
			(thermal_bridge_width 0.4064)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(locked yes)
		(layer "F.Cu")
		(at 132.9944 64.5 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P3"
			(at -6.0325 -4.29768 0)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/AM2315 sensors I2C interface/S2SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/AM2315 sensors I2C interface/S2SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(L5-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 125.883858 84.5185)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -2.54 -0.0065 270)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/5VMCU")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_DIP:DIP-8_W7.62mm_Socketed"
		(layer "F.Cu")
		(at 175.4505 92.85224 -90)
		(descr "8-lead dip package, row spacing 7.62 mm (300 mils), socketed")
		(tags "dil dip 2.54 300")
		(property "Reference" "U15"
			(at 3.69824 9.8425 270)
			(layer "F.SilkS")
		)
		(property "Value" "LTV-827C"
			(at 0 -3.72 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "OrderNo" "OrderNo"
			(at 82.59826 268.30274 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 82.59826 268.30274 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "Net-(R27-Pad1)")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/230V & general interface/BTP4")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "Net-(R26-Pad1)")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/230V & general interface/BTP3")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "/230V & general interface/BTL6")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/230V & general interface/BTL3")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Sockets_DIP.3dshapes/Socket_DIP8.stp"
			(offset (xyz 3.81 -3.81 3.81))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 90))
		)
		(model "${KICAD6_3DMODEL_DIR}/Housings_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset (xyz 0 0 3.5))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 104.9655 70.612 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U1"
			(at -2.2225 2.8575 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/AM2315 sensors I2C interface/S0SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/AM2315 sensors I2C interface/S0SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/AM2315 sensors I2C interface/S0SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/AM2315 sensors I2C interface/S0SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 159.0675 91.53144 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at -2.906 -0.015 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 318.135 183.06288 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 318.135 183.06288 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 318.135 183.06288 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 318.135 183.06288 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 186.7385 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/230V & general interface/BTL1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_95"
		(layer "F.Cu")
		(at 126.03099 94.615 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at -2.9845 -0.1905 0)
			(layer "F.SilkS")
		)
		(property "Value" "22µ"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 220.64599 -31.41599 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 220.64599 -31.41599 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "25V"
			(at 220.64599 -31.41599 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 220.64599 -31.41599 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 220.64599 -31.41599 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 60 "/12V")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 158.691796 106.3962 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D8"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 317.383592 212.7924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(D14-Pad1)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 101.981 70.5485 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 172.5295 -31.4325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 172.5295 -31.4325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 172.5295 -31.4325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 172.5295 -31.4325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/AM2315 sensors I2C interface/S0SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 150.182296 107.79345)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q5"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "/230V & general interface/ZWANG")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(D14-Pad1)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 113.547796 106.2692 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D5"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 227.095592 212.5384 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Net-(D11-Pad1)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 94 140)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "MH3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MHNP_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 1.4)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 122.047 70.5335 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 51.5135 192.5805 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 51.5135 192.5805 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 51.5135 192.5805 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 51.5135 192.5805 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/AM2315 sensors I2C interface/S1SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 108.0135 70.5485 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.5875 90)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 37.465 178.562 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 37.465 178.562 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 37.465 178.562 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 37.465 178.562 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/AM2315 sensors I2C interface/S0SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 132.9055 76.185)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U9"
			(at 0 3.4925 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/AM2315 sensors I2C interface/S2SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(R17-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(R18-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/AM2315 sensors I2C interface/S2SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 125.899858 86.9315 180)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L7"
			(at 2.6195 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 251.799716 173.863 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 180)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 180)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/5VMCU")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 113.7285 70.5335 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L4"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 184.262 -43.195 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(L4-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 150.241 70.5485 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 79.6925 220.7895 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 79.6925 220.7895 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 79.6925 220.7895 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 79.6925 220.7895 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/AM2315 sensors I2C interface/S3SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 132.969 70.597 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U3"
			(at -2.2225 2.794 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/AM2315 sensors I2C interface/S2SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/AM2315 sensors I2C interface/S2SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/AM2315 sensors I2C interface/S2SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/AM2315 sensors I2C interface/S2SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 175.006 70.612 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U6"
			(at -2.2225 3.1115 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/AM2315 sensors I2C interface/S5SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/AM2315 sensors I2C interface/S5SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/AM2315 sensors I2C interface/S5SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/AM2315 sensors I2C interface/S5SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 206 140)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "MH4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MHNP_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 1.4)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 113.7285 76.439 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2.87504 -0.0635 270)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 37.2895 190.1675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 37.2895 190.1675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 37.2895 190.1675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 37.2895 190.1675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(R15-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_DIP:DIP-8_W7.62mm_Socketed"
		(layer "F.Cu")
		(at 200.0885 92.7862 -90)
		(descr "8-lead dip package, row spacing 7.62 mm (300 mils), socketed")
		(tags "dil dip 2.54 300")
		(property "Reference" "U14"
			(at 3.69824 9.8425 270)
			(layer "F.SilkS")
		)
		(property "Value" "LTV-827C"
			(at 0 -3.72 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "OrderNo" "OrderNo"
			(at 107.3023 292.8747 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 107.3023 292.8747 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "Net-(R31-Pad1)")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/230V & general interface/BTP2")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "Net-(R30-Pad1)")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/230V & general interface/BTP4")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/230V & general interface/BTL7")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/230V & general interface/BTL5")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Sockets_DIP.3dshapes/Socket_DIP8.stp"
			(offset (xyz 3.81 -3.81 3.81))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 90))
		)
		(model "${KICAD6_3DMODEL_DIR}/Housings_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset (xyz 0 0 3.5))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_MELF_MMB-0207"
		(layer "F.Cu")
		(at 190.789032 124.55144 -90)
		(descr "Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf")
		(tags "MELF Resistor")
		(property "Reference" "R55"
			(at -2.6416 -2.615165 270)
			(layer "F.SilkS")
		)
		(property "Value" "82K"
			(at 0 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "MELF0207"
			(at 66.237592 315.340472 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "1W"
			(at 66.237592 315.340472 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 66.237592 315.340472 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 66.237592 315.340472 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(IC2-Pad1)")
		)
		(pad "2" smd rect
			(at 2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(P14-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MELF_MMB-0207.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 171.8945 70.5485 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -2.4765 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 242.443 -101.346 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 242.443 -101.346 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 242.443 -101.346 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 242.443 -101.346 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/AM2315 sensors I2C interface/S5SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 186.182 75.41768 90)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 0 -2.4765 270)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "/230V & general interface/ENTFRH")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-Pad2)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 150.893496 111.63115 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 0.0231 1.5748 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 39.262346 262.524646 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 39.262346 262.524646 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 39.262346 262.524646 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 39.262346 262.524646 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(D14-Pad2)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 123.613896 110.00325 -90)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D12"
			(at 2.794 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-G"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D12-Pad1)")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "Net-(D12-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 135.205071 107.91025)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q6"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/230V & general interface/ZUAB")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D13-Pad1)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 195.0085 89.41816 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 284.42666 -105.59034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 284.42666 -105.59034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 284.42666 -105.59034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 284.42666 -105.59034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Net-(R30-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/230V & general interface/BTP6")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 147.0025 76.2)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U10"
			(at 1.5875 3.51028 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/AM2315 sensors I2C interface/S3SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(R19-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(R20-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/AM2315 sensors I2C interface/S3SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 141.6835 76.454 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 1.6025 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 65.2295 218.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 65.2295 218.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 65.2295 218.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 65.2295 218.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(R19-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:Relais_G5NB"
		(layer "F.Cu")
		(at 113.611296 118.2072 -90)
		(property "Reference" "RL3"
			(at 0.779 -4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "G5NB-5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(D11-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 2.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(P9-Pad1)")
		)
		(pad "3" thru_hole circle
			(at 9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(P9-Pad2)")
		)
		(pad "4" thru_hole circle
			(at -9.25 -2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/g5nb-e.stp"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Resistor_SMD:R_MELF_MMB-0207"
		(layer "F.Cu")
		(at 198.171835 124.55144 -90)
		(descr "Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf")
		(tags "MELF Resistor")
		(property "Reference" "R56"
			(at -2.6416 -2.615165 270)
			(layer "F.SilkS")
		)
		(property "Value" "82K"
			(at 0 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "MELF0207"
			(at 73.620395 322.723275 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "1W"
			(at 73.620395 322.723275 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 73.620395 322.723275 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 73.620395 322.723275 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(IC2-Pad4)")
		)
		(pad "2" smd rect
			(at 2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(P14-Pad1)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MELF_MMB-0207.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 169.672 76.581 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 93.091 246.253 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 93.091 246.253 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 93.091 246.253 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 93.091 246.253 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(R23-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:Relais_G5NB"
		(layer "F.Cu")
		(at 128.724296 118.2072 -90)
		(property "Reference" "RL4"
			(at 0.779 -4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "G5NB-5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D12-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 2.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "Net-(P10-Pad1)")
		)
		(pad "3" thru_hole circle
			(at 9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Net-(P10-Pad2)")
		)
		(pad "4" thru_hole circle
			(at -9.25 -2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/g5nb-e.stp"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_95"
		(layer "F.Cu")
		(at 123.23699 94.615 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -2.9845 -0.012 0)
			(layer "F.SilkS")
		)
		(property "Value" "22µ"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 217.85199 -28.62199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 217.85199 -28.62199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "25V"
			(at 217.85199 -28.62199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 217.85199 -28.62199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 217.85199 -28.62199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 60 "/12V")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:Relais_G5NB"
		(layer "F.Cu")
		(at 143.769296 118.2072 -90)
		(property "Reference" "RL5"
			(at 0.779 -4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "G5NB-5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(D13-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 2.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(P11-Pad1)")
		)
		(pad "3" thru_hole circle
			(at 9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(P11-Pad2)")
		)
		(pad "4" thru_hole circle
			(at -9.25 -2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/g5nb-e.stp"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 137.20699 97.7265 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at -2.4765 0.0635 90)
			(layer "F.SilkS")
		)
		(property "Value" "27K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 274.41398 195.453 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 274.41398 195.453 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 274.41398 195.453 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 274.41398 195.453 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C15-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Net-(R36-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(locked yes)
		(layer "F.Cu")
		(at 175.006 64.516 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P6"
			(at -7.874 3.29692 90)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/AM2315 sensors I2C interface/S5SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/AM2315 sensors I2C interface/S5SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(L2-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 159.0675 93.71076 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at -2.921 -0.0635 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 318.135 187.42152 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 318.135 187.42152 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 318.135 187.42152 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 318.135 187.42152 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/SCL")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 160 135.04025 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P12"
			(at -6.3715 5.842 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(P12-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(P12-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 104.9655 76.2)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U7"
			(at -0.0635 3.429 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/AM2315 sensors I2C interface/S0SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(R13-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "Net-(R14-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/AM2315 sensors I2C interface/S0SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 166.0525 76.3905 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 3.048 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 89.662 242.443 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 89.662 242.443 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 89.662 242.443 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 89.662 242.443 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(R22-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(locked yes)
		(layer "F.Cu")
		(at 147.0152 64.516 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P4"
			(at -6.0325 -4.29768 0)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/AM2315 sensors I2C interface/S3SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/AM2315 sensors I2C interface/S3SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(L6-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(locked yes)
		(layer "F.Cu")
		(at 118.9912 64.516 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P2"
			(at -6.0325 -4.29768 0)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/AM2315 sensors I2C interface/S1SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/AM2315 sensors I2C interface/S1SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(L4-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Symbol:KiCad-Logo2_5mm_SilkScreen"
		(locked yes)
		(layer "F.Cu")
		(at 205.8035 121.24944 90)
		(descr "KiCad Logo")
		(tags "Logo KiCad")
		(property "Reference" "REF**"
			(at 0 -5.08 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KiCad-Logo2_5mm_SilkScreen"
			(at 0 5.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 186.182 84.26704 90)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at 2.50952 -0.0635 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "/230V & general interface/ENTFON")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0 90)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(D2-Pad2)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 181.6585 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/230V & general interface/BTL4")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 109.7915 76.454 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 2.921 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 33.3375 186.2455 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 33.3375 186.2455 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 33.3375 186.2455 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 33.3375 186.2455 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(R14-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 194.041 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/230V & general interface/BTL7")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-2-5.0"
		(locked yes)
		(layer "F.Cu")
		(at 98.933 87.884 90)
		(property "Reference" "P7"
			(at 6.19252 0.0635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-2-5.0"
			(at 2.54 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 90)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(FH1-Pad1)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_KF128-5.0-2.stp"
			(offset (xyz 0 0 5))
			(scale (xyz 1 1.3 1))
			(rotate (xyz 0 0 180))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 164.084 70.5485 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 93.5355 234.6325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 93.5355 234.6325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 93.5355 234.6325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 93.5355 234.6325 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/AM2315 sensors I2C interface/S4SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:SIP-1A5"
		(layer "F.Cu")
		(at 198.882 75.6158)
		(property "Reference" "RL1"
			(at 9.017 3.5848 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SIP-1A5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -7.62 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/230V & general interface/BTP1")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-Pad2)")
		)
		(pad "3" thru_hole circle
			(at 2.54 -0.0635)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/5V ")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "Net-(R32-Pad1)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Relays_ThroughHole.3dshapes/SIP-1A5.STEP"
			(offset (xyz 0 0 1.5))
			(scale (xyz 1.33 1.33 1.33))
			(rotate (xyz -90 0 0))
		)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/SIP-1A5.STEP"
			(offset (xyz 0 0 1.5))
			(scale (xyz 1.3 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 154.432 101.10724 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 2.44348 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 53.32476 255.53924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 53.32476 255.53924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 53.32476 255.53924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 53.32476 255.53924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 53.32476 255.53924 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 105.704596 111.67965 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0 1.5979 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at -5.975054 217.384246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at -5.975054 217.384246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at -5.975054 217.384246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at -5.975054 217.384246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Net-(D11-Pad2)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 124.0155 76.439 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 3.048 -0.0635 270)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 47.5765 200.4545 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 47.5765 200.4545 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 47.5765 200.4545 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 47.5765 200.4545 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(R16-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SSOP:TSSOP-24_4.4x7.8mm_Pitch0.65mm"
		(layer "F.Cu")
		(at 148.209 88.59827 -90)
		(descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U13"
			(at 0.48969 -5.0165 90)
			(layer "F.SilkS")
		)
		(property "Value" "PCA9548A"
			(at 0 4.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.85 -3.575 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A0")
		)
		(pad "2" smd rect
			(at -2.85 -2.925 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A1")
		)
		(pad "3" smd rect
			(at -2.85 -2.275 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "/NIORESET")
			(pinfunction "~RESET")
		)
		(pad "4" smd rect
			(at -2.85 -1.625 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(R13-Pad2)")
			(pinfunction "SD0")
		)
		(pad "5" smd rect
			(at -2.85 -0.975 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "Net-(R14-Pad2)")
			(pinfunction "SC0")
		)
		(pad "6" smd rect
			(at -2.85 -0.325 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(R15-Pad2)")
			(pinfunction "SD1")
		)
		(pad "7" smd rect
			(at -2.85 0.325 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(R16-Pad2)")
			(pinfunction "SC1")
		)
		(pad "8" smd rect
			(at -2.85 0.975 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(R17-Pad2)")
			(pinfunction "SD2")
		)
		(pad "9" smd rect
			(at -2.85 1.625 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(R18-Pad2)")
			(pinfunction "SC2")
		)
		(pad "10" smd rect
			(at -2.85 2.275 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(R19-Pad2)")
			(pinfunction "SD3")
		)
		(pad "11" smd rect
			(at -2.85 2.925 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(R20-Pad2)")
			(pinfunction "SC3")
		)
		(pad "12" smd rect
			(at -2.85 3.575 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "13" smd rect
			(at 2.85 3.575 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(R21-Pad2)")
			(pinfunction "SD4")
		)
		(pad "14" smd rect
			(at 2.85 2.925 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(R22-Pad2)")
			(pinfunction "SC4")
		)
		(pad "15" smd rect
			(at 2.85 2.275 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(R23-Pad2)")
			(pinfunction "SD5")
		)
		(pad "16" smd rect
			(at 2.85 1.625 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(R24-Pad2)")
			(pinfunction "SC5")
		)
		(pad "17" smd rect
			(at 2.85 0.975 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "no_connect_(U13-Pad17)")
			(pinfunction "SD6")
		)
		(pad "18" smd rect
			(at 2.85 0.325 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "no_connect_(U13-Pad18)")
			(pinfunction "SC6")
		)
		(pad "19" smd rect
			(at 2.85 -0.325 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "no_connect_(U13-Pad19)")
			(pinfunction "SD7")
		)
		(pad "20" smd rect
			(at 2.85 -0.975 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "no_connect_(U13-Pad20)")
			(pinfunction "SC7")
		)
		(pad "21" smd rect
			(at 2.85 -1.625 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A2")
		)
		(pad "22" smd rect
			(at 2.85 -2.275 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/SCL")
			(pinfunction "SCL")
		)
		(pad "23" smd rect
			(at 2.85 -2.925 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/SDA")
			(pinfunction "SDA")
		)
		(pad "24" smd rect
			(at 2.85 -3.575 270)
			(size 1.1 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VCC")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SSOP_TSSOP.3dshapes/TSSOP-24_4.4x7.8mm_Pitch0.65mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_95"
		(layer "F.Cu")
		(at 136.52049 88.3315 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -2.924 0.012 0)
			(layer "F.SilkS")
		)
		(property "Value" "22µ"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 48.18899 224.85199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 48.18899 224.85199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "25V"
			(at 48.18899 224.85199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 48.18899 224.85199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 48.18899 224.85199 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 270)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 1.4 0 270)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_MELF_MMB-0207"
		(layer "F.Cu")
		(at 173.609 124.5333 -90)
		(descr "Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf")
		(tags "MELF Resistor")
		(property "Reference" "R53"
			(at -2.6416 -2.615165 270)
			(layer "F.SilkS")
		)
		(property "Value" "82K"
			(at 0 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "MELF0207"
			(at 49.0757 298.1423 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "1W"
			(at 49.0757 298.1423 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 49.0757 298.1423 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 49.0757 298.1423 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(IC1-Pad1)")
		)
		(pad "2" smd rect
			(at 2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(P13-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MELF_MMB-0207.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 145 135.04025 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P11"
			(at -6.3715 5.842 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(P11-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(P11-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Housings_DIP:DIP-8_W7.62mm_Socketed"
		(layer "F.Cu")
		(at 190.618835 118.538283 90)
		(descr "8-lead dip package, row spacing 7.62 mm (300 mils), socketed")
		(tags "dil dip 2.54 300")
		(property "Reference" "IC2"
			(at 3.628683 -2.277835 90)
			(layer "F.SilkS")
		)
		(property "Value" "HCPL-3760"
			(at 0 -3.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(IC2-Pad1)")
			(pinfunction "AC+")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "no_connect_(IC2-Pad2)")
			(pinfunction "DC+")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "no_connect_(IC2-Pad3)")
			(pinfunction "DC-")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(IC2-Pad4)")
			(pinfunction "AC-")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/230V & general interface/230V2")
			(pinfunction "Vo")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/5V ")
			(pinfunction "VCC")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Sockets_DIP.3dshapes/Socket_DIP8.stp"
			(offset (xyz 3.81 -3.81 3.81))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 90))
		)
		(model "${KICAD6_3DMODEL_DIR}/Housings_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset (xyz 0 0 3.5))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 118.9355 70.597 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U2"
			(at -2.22525 3.1115 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/AM2315 sensors I2C interface/S1SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/AM2315 sensors I2C interface/S1SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/AM2315 sensors I2C interface/S1SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/AM2315 sensors I2C interface/S1SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Fuse_Holders_and_Fuses:Fuseholder5x20_horizontal_open_inline_1"
		(layer "F.Cu")
		(at 111.4425 92.3925 -90)
		(property "Reference" "FH1"
			(at -7.6581 -5.1181 270)
			(layer "F.SilkS")
		)
		(property "Value" "FC5X20"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -10.4 0 270)
			(size 2.5 2.5)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(FH1-Pad1)")
		)
		(pad "1" thru_hole circle
			(at -5.1 0 270)
			(size 2.5 2.5)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(FH1-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 5.1 0 270)
			(size 2.5 2.5)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(pad "2" thru_hole circle
			(at 10.4 0 270)
			(size 2.5 2.5)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
			(polygon
				(pts
					(xy 107.8425 88.1925) (xy 107.8425 81.0925) (xy 115.0425 81.0925) (xy 115.0425 88.1925)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
			(polygon
				(pts
					(xy 107.8425 103.6925) (xy 107.8425 96.5925) (xy 115.0425 96.5925) (xy 115.0425 103.6925)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Fuse_Holders_and_Fuses.3dshapes/Clips FH-100 with fuse 5x20.STEP"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 -90))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 130 135.04025 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P10"
			(at -6.3715 5.842 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "Net-(P10-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Net-(P10-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 154.432 91.4654)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -0.4445 1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 108.577096 110.00325 -90)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D11"
			(at 2.8067 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-G"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Net-(D11-Pad1)")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "Net-(D11-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 175.4505 89.378 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 264.8285 -86.0725 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 264.8285 -86.0725 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 264.8285 -86.0725 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 264.8285 -86.0725 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Net-(R27-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/230V & general interface/BTP1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 138.09599 100.6475 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.8N"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 37.44849 238.74349 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 37.44849 238.74349 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 37.44849 238.74349 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 37.44849 238.74349 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 37.44849 238.74349 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C15-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 200.0885 89.41816 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "560E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 289.50666 -110.67034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 289.50666 -110.67034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 289.50666 -110.67034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 289.50666 -110.67034 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "Net-(R31-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/230V & general interface/BTP6")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 127.74549 100.711 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 3.048 -0.9525 0)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 255.49098 201.422 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 255.49098 201.422 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 255.49098 201.422 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 255.49098 201.422 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 255.49098 201.422 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C14-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 131.36499 100.711)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0.6985 1.5875 0)
			(layer "F.SilkS")
		)
		(property "Value" "9.53K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "1%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Net-(R37-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 160.9725 70.612 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U5"
			(at -2.2225 2.7305 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/AM2315 sensors I2C interface/S4SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/AM2315 sensors I2C interface/S4SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/AM2315 sensors I2C interface/S4SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/AM2315 sensors I2C interface/S4SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:Relais_G5NB"
		(layer "F.Cu")
		(at 158.691796 118.2072 -90)
		(property "Reference" "RL6"
			(at 0.779 -4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "G5NB-5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(D14-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 2.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(P12-Pad1)")
		)
		(pad "3" thru_hole circle
			(at 9.25 2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(P12-Pad2)")
		)
		(pad "4" thru_hole circle
			(at -9.25 -2.35 270)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/g5nb-e.stp"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Connectors:RJ45_LEDs_Shield"
		(layer "F.Cu")
		(at 199.517 61.28512 180)
		(tags "RJ45")
		(property "Reference" "J1"
			(at -2.667 -6.20776 90)
			(layer "F.SilkS")
		)
		(property "Value" "RJ45_LEDs_Shield"
			(at 6.35 4.064 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 0.3)
		)
		(pad "" np_thru_hole circle
			(at 12.7 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 0.3)
		)
		(pad "1" thru_hole circle
			(at 9.906 -2.54 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/230V & general interface/BTP1")
		)
		(pad "2" thru_hole circle
			(at 8.89 -4.318 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/230V & general interface/BTP2")
			(thermal_bridge_width 0.4064)
		)
		(pad "3" thru_hole circle
			(at 7.874 -2.54 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/230V & general interface/BTP3")
		)
		(pad "4" thru_hole circle
			(at 6.858 -4.318 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/230V & general interface/BTP4")
		)
		(pad "5" thru_hole circle
			(at 5.842 -2.54 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/230V & general interface/BTP5")
			(thermal_bridge_width 0.4064)
		)
		(pad "6" thru_hole circle
			(at 4.826 -4.318 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/230V & general interface/BTP6")
		)
		(pad "7" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "no_connect_(J1-Pad7)")
		)
		(pad "8" thru_hole circle
			(at 2.794 -4.318 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "no_connect_(J1-Pad8)")
			(thermal_bridge_width 0.4064)
		)
		(pad "GA" thru_hole circle
			(at 10.922 -9.144 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "no_connect_(J1-PadGA)")
		)
		(pad "GK" thru_hole circle
			(at 13.208 -9.144 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "Shld" thru_hole circle
			(at -1.778 -3.429 180)
			(size 2.5 2.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Shield")
		)
		(pad "Shld" thru_hole circle
			(at 14.478 -3.429 180)
			(size 2.5 2.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Shield")
		)
		(pad "YA" thru_hole circle
			(at -0.508 -9.144 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "no_connect_(J1-PadYA)")
		)
		(pad "YK" thru_hole circle
			(at 1.778 -9.144 180)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "E:/Repository_local/KiCad/3Dmodels/Connect.3dshapes/RJ45_LEDs_Shield.wrl"
			(offset (xyz 6.349999905 2.539999962 6.349999905))
			(scale (xyz 0.393 0.393 0.393))
			(rotate (xyz 180 0 90))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 183.10098 108.6358)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D9"
			(at 0.09652 -1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-Y"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 180)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/230V & general interface/230V1")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 180)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D9-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 153.560496 109.95245 -90)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D14"
			(at 2.82448 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-G"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(D14-Pad1)")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(D14-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 184.15 111.73968 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0 1.7145 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 295.88968 -72.41032 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 295.88968 -72.41032 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 295.88968 -72.41032 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 295.88968 -72.41032 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D9-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 129.9845 70.5335 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -2.4765 -0.0635 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 200.518 -59.451 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 200.518 -59.451 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 200.518 -59.451 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 200.518 -59.451 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/AM2315 sensors I2C interface/S2SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 118.9355 76.185)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U8"
			(at 0 3.429 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/AM2315 sensors I2C interface/S1SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(R15-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(R16-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/AM2315 sensors I2C interface/S1SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_60"
		(layer "F.Cu")
		(at 172.547322 108.321622)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -0.03 -1.6256 0)
			(layer "F.SilkS")
		)
		(property "Value" "100N"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 127.6985 76.439 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 51.2595 204.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 51.2595 204.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 51.2595 204.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 51.2595 204.1375 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(R17-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 104.970296 107.66645)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q3"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.15 -0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/230V & general interface/DOOR")
			(pinfunction "G")
		)
		(pad "2" smd rect
			(at -1.15 0.95)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "S")
		)
		(pad "3" smd rect
			(at 1.15 0)
			(size 1 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Net-(D11-Pad1)")
			(pinfunction "D")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 138.701496 109.98547 -90)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D13"
			(at 2.82448 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-G"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D13-Pad1)")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 90)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(D13-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(locked yes)
		(layer "F.Cu")
		(at 160.9852 64.516 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P5"
			(at -6.0325 -4.29768 0)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/AM2315 sensors I2C interface/S4SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/AM2315 sensors I2C interface/S4SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(L1-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 115.951 70.5335 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.413 -0.0635 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 186.4845 -45.4175 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 186.4845 -45.4175 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 186.4845 -45.4175 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 186.4845 -45.4175 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/AM2315 sensors I2C interface/S1SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Relays_THT:SIP-1A5"
		(layer "F.Cu")
		(at 198.882 84.26704)
		(property "Reference" "RL2"
			(at 8.5725 3.56616 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SIP-1A5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -7.62 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/230V & general interface/BTP1")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(D2-Pad2)")
		)
		(pad "3" thru_hole circle
			(at 2.54 -0.0635)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/5V ")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "Net-(R33-Pad1)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Relays_ThroughHole.3dshapes/SIP-1A5.STEP"
			(offset (xyz 0 0 1.5))
			(scale (xyz 1.33 1.33 1.33))
			(rotate (xyz -90 0 0))
		)
		(model "${KICAD6_3DMODEL_DIR}/Relays_ThroughHole.3dshapes/SIP-1A5.STEP"
			(offset (xyz 0 0 1.5))
			(scale (xyz 1.3 1 1))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Housings_DIP:DIP-8_W7.62mm_Socketed"
		(layer "F.Cu")
		(at 187.706 92.85224 -90)
		(descr "8-lead dip package, row spacing 7.62 mm (300 mils), socketed")
		(tags "dil dip 2.54 300")
		(property "Reference" "U16"
			(at 3.69824 9.8425 270)
			(layer "F.SilkS")
		)
		(property "Value" "LTV-827C"
			(at 0 -3.72 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "OrderNo" "OrderNo"
			(at 94.85376 280.55824 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 94.85376 280.55824 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "Net-(R29-Pad1)")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/230V & general interface/BTP2")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "Net-(R28-Pad1)")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/230V & general interface/BTP5")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "/230V & general interface/BTL4")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/230V & general interface/BTL1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Sockets_DIP.3dshapes/Socket_DIP8.stp"
			(offset (xyz 3.81 -3.81 3.81))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 90))
		)
		(model "${KICAD6_3DMODEL_DIR}/Housings_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset (xyz 0 0 3.5))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 155.6385 76.454 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 1.4605 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 79.1845 232.0925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 79.1845 232.0925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 79.1845 232.0925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 79.1845 232.0925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(R21-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_MELF_MMB-0207"
		(layer "F.Cu")
		(at 181.187922 124.5333 -90)
		(descr "Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf")
		(tags "MELF Resistor")
		(property "Reference" "R54"
			(at -2.6416 -2.615165 270)
			(layer "F.SilkS")
		)
		(property "Value" "82K"
			(at 0 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "MELF0207"
			(at 56.654622 305.721222 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "1W"
			(at 56.654622 305.721222 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 56.654622 305.721222 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 56.654622 305.721222 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(IC1-Pad4)")
		)
		(pad "2" smd rect
			(at 2.45 0 270)
			(size 2.1 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "Net-(P13-Pad1)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MELF_MMB-0207.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 99.6315 70.612 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L3"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 170.2435 -29.0195 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(L3-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 206.5655 90.4748 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.651 270)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 116.0907 297.0403 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 116.0907 297.0403 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 116.0907 297.0403 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 116.0907 297.0403 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "Net-(R33-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/230V & general interface/BTP2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:KF128-4-3.5"
		(layer "F.Cu")
		(at 105.0036 64.516 180)
		(descr "Terminal block, 3.5mm pitch, 4 pin, KF128 series")
		(property "Reference" "P1"
			(at -6.0325 -4.29768 0)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-4-3.5"
			(at 0 -0.0635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at -5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at -1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/AM2315 sensors I2C interface/S0SCL")
		)
		(pad "3" thru_hole circle
			(at 1.75 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/AM2315 sensors I2C interface/S0SDA")
		)
		(pad "4" thru_hole circle
			(at 5.25 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(L3-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl"
			(offset (xyz -5.25 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm_PowerPAD"
		(layer "F.Cu")
		(at 131.42149 96.604)
		(descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U17"
			(at -4.946 2.329 0)
			(layer "F.SilkS")
		)
		(property "Value" "AOZ3015"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "PGND")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "VIN")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "AGND")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(C14-Pad1)")
			(pinfunction "VCC")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(R37-Pad2)")
			(pinfunction "FB")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "Net-(R36-Pad2)")
			(pinfunction "CMP")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "EN")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VOUT")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.4 3.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(D3-Pad1)")
			(pinfunction "LX")
			(solder_paste_margin_ratio -0.2)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 143.769296 106.3327 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D7"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 287.538592 212.6654 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D13-Pad1)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 138.1125 76.439 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 2.9845 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 61.6735 214.5515 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 61.6735 214.5515 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 61.6735 214.5515 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 61.6735 214.5515 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(R18-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 128.724296 106.2692 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D6"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 257.448592 212.5384 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/12V")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D12-Pad1)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "LEDs:LED_0805"
		(layer "F.Cu")
		(at 199.771 108.6358)
		(descr "LED 0805 smd package")
		(tags "LED 0805 SMD")
		(property "Reference" "D10"
			(at 0.09652 -1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED0805-Y"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.04902 0 180)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/230V & general interface/230V2")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.04902 0 180)
			(size 1.19888 1.19888)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "Net-(D10-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 169.672 70.358 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L2"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 240.03 -99.314 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(L2-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_95"
		(layer "F.Cu")
		(at 139.30249 88.3315 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -2.924 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22µ"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 50.97099 227.63399 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 50.97099 227.63399 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "25V"
			(at 50.97099 227.63399 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 50.97099 227.63399 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 50.97099 227.63399 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 270)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 1.4 0 270)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 187.706 89.378 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 277.084 -98.328 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 277.084 -98.328 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 277.084 -98.328 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 277.084 -98.328 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "Net-(R29-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/230V & general interface/BTP1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 160.909 76.2)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U11"
			(at 0 3.4925 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/AM2315 sensors I2C interface/S4SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(R21-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(R22-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/AM2315 sensors I2C interface/S4SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 143.891 70.5485 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -2.4765 -0.0635 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 214.4395 -73.3425 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 214.4395 -73.3425 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 214.4395 -73.3425 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 214.4395 -73.3425 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/AM2315 sensors I2C interface/S3SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 180.0225 76.3905 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 2.921 -0.0635 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 103.632 256.413 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 103.632 256.413 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 103.632 256.413 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 103.632 256.413 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(R24-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.2075 70.5335 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.7145 90)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 65.674 206.741 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 65.674 206.741 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 65.674 206.741 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 65.674 206.741 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/AM2315 sensors I2C interface/S2SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 140.731 73.5965 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2375 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 281.462 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 281.462 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 281.462 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 281.462 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 281.462 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SOD-323"
		(layer "F.Cu")
		(at 200.025 80.17256 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D2"
			(at -3.4925 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WS"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 400.05 160.34512 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.35 0 180)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(D2-Pad2)")
			(pinfunction "A")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 98.679 73.5965 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.398 0.0635 270)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 197.358 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 197.358 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 197.358 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 197.358 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 197.358 147.193 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 193.531365 108.441362)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -0.015 -1.71486 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/230V & general interface/230V2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 170.3705 89.378 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 259.7485 -80.9925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 259.7485 -80.9925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 259.7485 -80.9925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 259.7485 -80.9925 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "Net-(R26-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/230V & general interface/BTP6")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_95"
		(layer "F.Cu")
		(at 154.7495 73.406 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 2.286 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µ"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 309.499 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 309.499 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 309.499 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 309.499 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 309.499 146.812 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Cap_SMD.3dshapes/CAPC2012x95.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 147.0025 70.612 90)
		(descr "6-pin SOT-23 package")
		(tags "SOT-23-6")
		(property "Reference" "U4"
			(at -2.2225 3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.9 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/AM2315 sensors I2C interface/S3SDA")
			(pinfunction "IO1")
		)
		(pad "2" smd rect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "3" smd rect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/AM2315 sensors I2C interface/S3SCL")
			(pinfunction "IO2")
		)
		(pad "4" smd rect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/AM2315 sensors I2C interface/S3SCL")
			(pinfunction "IO2")
		)
		(pad "5" smd rect
			(at 1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VBUS")
		)
		(pad "6" smd rect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/AM2315 sensors I2C interface/S3SDA")
			(pinfunction "IO1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_TO_SOT.3dshapes/SOT-23-6.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 194.425335 135.00136 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P14"
			(at -6.8453 5.81696 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(P14-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(P14-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_95"
		(layer "F.Cu")
		(at 125.566358 89.4715)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -2.9845 -0.0635 270)
			(layer "F.SilkS")
		)
		(property "Value" "22µ"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "25V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "CK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 69 "/5VMCU")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 159.0675 89.35212)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 2.906 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/NIORESET")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 178.1175 70.5485 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -1.778 -2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 107.569 248.666 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 107.569 248.666 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 107.569 248.666 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 107.569 248.666 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/AM2315 sensors I2C interface/S5SCL")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 206 59.946)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "MH2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MHNP_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 1.4)
		)
		(embedded_fonts no)
	)
	(footprint "Inductors_SMD:Inductor_0630"
		(layer "F.Cu")
		(at 131.42849 89.7255 90)
		(property "Reference" "L8"
			(at 4.699 0.065 180)
			(layer "F.SilkS")
		)
		(property "Value" "10µ"
			(at -0.0635 4.2545 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0630"
			(at 221.15399 -41.70299 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 221.15399 -41.70299 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "L"
			(at 221.15399 -41.70299 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.8 0 90)
			(size 1.9 3.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(D3-Pad1)")
		)
		(pad "2" smd rect
			(at 2.8 0 90)
			(size 1.9 3.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_SMD_CDRH127.STEP"
			(offset (xyz -3.3 3.3 0))
			(scale (xyz 0.56 0.56 0.56))
			(rotate (xyz -90 0 0))
		)
	)
	(footprint "Terminal_Blocks:Terminal_Block_KF128_7.5mm-2pol"
		(layer "F.Cu")
		(at 177.355634 135.001421 180)
		(descr "Screw terminal block, pitch 7.5 mm")
		(property "Reference" "P13"
			(at 6.41 5.835161 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "KF128-7.5-2"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(P13-Pad1)")
			(pinfunction "P1")
		)
		(pad "2" thru_hole circle
			(at 3.75 0 180)
			(size 3.5 3.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(P13-Pad2)")
			(pinfunction "P2")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Terminal_Block.3dshapes/terminal_blocks_a-tb500-ti02.stp"
			(offset (xyz 0 -5.5 0))
			(scale (xyz 1.5 1 1))
			(rotate (xyz -90 0 180))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 176.174922 108.296222)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0 -1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/230V & general interface/230V1")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 152.146 76.3905 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 2.92354 0.3175 270)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 75.7555 228.5365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 75.7555 228.5365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 75.7555 228.5365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 75.7555 228.5365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(R20-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 199.106 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/230V & general interface/BTL5")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 135.04799 100.711)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 1.5875 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "1%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Net-(R37-Pad2)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Inductors_SMD:INDC2012X110"
		(layer "F.Cu")
		(at 127.6985 70.5335 90)
		(descr "Resistor,Chip;2.00mm L X 1.25mm W X 0.60mm H")
		(property "Reference" "L5"
			(at 0 -1.7145 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 198.232 -57.165 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
		)
		(pad "2" smd rect
			(at 1 0 90)
			(size 0.95 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(L5-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductors_SMD.3dshapes/L_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.870696 111.65655 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at -0.0277 1.5748 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 9.214146 232.527246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 9.214146 232.527246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 9.214146 232.527246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 9.214146 232.527246 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D12-Pad2)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 157.7975 70.5485 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -2.4765 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "680E"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 228.346 -87.249 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 228.346 -87.249 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 228.346 -87.249 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 228.346 -87.249 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/AM2315 sensors I2C interface/S4SDA")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Connectors:IDC_Header_Straight_8pins"
		(layer "F.Cu")
		(at 96.8375 111.3155 90)
		(descr "8 pins through hole IDC header")
		(tags "IDC header socket VASCH")
		(property "Reference" "P8"
			(at 9.81202 0.0635 180)
			(layer "F.SilkS")
		)
		(property "Value" "IDCMV-4-2"
			(at 1.27 6.493 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "P1")
		)
		(pad "2" thru_hole oval
			(at -3.81 -1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "P2")
		)
		(pad "3" thru_hole oval
			(at -1.27 1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/SCL")
			(pinfunction "P3")
		)
		(pad "4" thru_hole oval
			(at -1.27 -1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/SDA")
			(pinfunction "P4")
		)
		(pad "5" thru_hole oval
			(at 1.27 1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/NIORESET")
			(pinfunction "P5")
		)
		(pad "6" thru_hole oval
			(at 1.27 -1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/NIOINT")
			(pinfunction "P6")
		)
		(pad "7" thru_hole oval
			(at 3.81 1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/5VMCU")
			(pinfunction "P7")
		)
		(pad "8" thru_hole oval
			(at 3.81 -1.27 90)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/5VMCU")
			(pinfunction "P8")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x04_P2.54mm_Vertical.step"
			(offset (xyz -3.81 -1.27 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 -90))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 174.483 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/230V & general interface/BTL3")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 169.403 103.48468)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 1.71704 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/230V & general interface/BTL6")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.6315 76.454 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 23.1775 176.0855 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 23.1775 176.0855 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 23.1775 176.0855 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 23.1775 176.0855 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/5V ")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(R13-Pad2)")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Diodes_SMD:SMA_Standard"
		(layer "F.Cu")
		(at 138.92149 92.71)
		(descr "Diode SMA")
		(tags "Diode SMA")
		(property "Reference" "D3"
			(at -0.04699 2.78384 180)
			(layer "F.SilkS")
		)
		(property "Value" "SS34"
			(at 0 4.3 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.99898 0)
			(size 2.49936 1.80086)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(D3-Pad1)")
			(pinfunction "K")
		)
		(pad "2" smd rect
			(at 1.99898 0)
			(size 2.49936 1.80086)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(zone_connect 2)
			(thermal_bridge_width 0.4064)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 175.006 76.2)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U12"
			(at 0 3.4925 0)
			(layer "F.SilkS")
		)
		(property "Value" "P82B715"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "AM2315 sensors I2C interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.sensors_io.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/AM2315 sensors I2C interface/S5SDA")
			(pinfunction "Lx")
		)
		(pad "3" smd rect
			(at -2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(R23-Pad2)")
			(pinfunction "Sx")
		)
		(pad "4" smd rect
			(at -2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
		)
		(pad "5" smd rect
			(at 2.7 1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.7 0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(R24-Pad2)")
			(pinfunction "Sy")
		)
		(pad "7" smd rect
			(at 2.7 -0.635)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/AM2315 sensors I2C interface/S5SCL")
			(pinfunction "Ly")
		)
		(pad "8" smd rect
			(at 2.7 -1.905)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "Vcc")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 135.958296 111.65655 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0 1.5748 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "0805"
			(at 24.301746 247.614846 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "P_or_V" "_"
			(at 24.301746 247.614846 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "_"
			(at 24.301746 247.614846 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "WIO_Prefix" "R"
			(at 24.301746 247.614846 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(D13-Pad2)")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/12V")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistors_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "Housings_SSOP:SSOP-24_5.3x8.2mm_Pitch0.65mm"
		(layer "F.Cu")
		(at 148.209 97.87128 -90)
		(descr "24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U18"
			(at 0 -5.25 270)
			(layer "F.SilkS")
		)
		(property "Value" "PCF8575"
			(at 0 5.25 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "230V & general interface")
		(sheetfile "E:\\Projects_local\\020.HomeControl\\Hardware\\020.02.010.0221\\020.02.010.0221.230V_actuators&presence.kicad_sch")
		(clearance 0.1778)
		(attr smd)
		(pad "1" smd rect
			(at -3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "/NIOINT")
			(pinfunction "~INT")
		)
		(pad "2" smd rect
			(at -3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A1")
		)
		(pad "3" smd rect
			(at -3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A2")
		)
		(pad "4" smd rect
			(at -3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "no_connect_(U18-Pad4)")
			(pinfunction "IO0_0")
		)
		(pad "5" smd rect
			(at -3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "no_connect_(U18-Pad5)")
			(pinfunction "IO0_1")
		)
		(pad "6" smd rect
			(at -3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/230V & general interface/BTL5")
			(pinfunction "IO0_2")
		)
		(pad "7" smd rect
			(at -3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "/230V & general interface/BTL7")
			(pinfunction "IO0_3")
		)
		(pad "8" smd rect
			(at -3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/230V & general interface/BTL1")
			(pinfunction "IO0_4")
		)
		(pad "9" smd rect
			(at -3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "/230V & general interface/BTL4")
			(pinfunction "IO0_5")
		)
		(pad "10" smd rect
			(at -3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "/230V & general interface/BTL3")
			(pinfunction "IO0_6")
		)
		(pad "11" smd rect
			(at -3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "/230V & general interface/BTL6")
			(pinfunction "IO0_7")
		)
		(pad "12" smd rect
			(at -3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
		)
		(pad "13" smd rect
			(at 3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/230V & general interface/DOOR")
			(pinfunction "IO1_0")
		)
		(pad "14" smd rect
			(at 3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "/230V & general interface/AUX")
			(pinfunction "IO1_1")
		)
		(pad "15" smd rect
			(at 3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/230V & general interface/ZUAB")
			(pinfunction "IO1_2")
		)
		(pad "16" smd rect
			(at 3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "/230V & general interface/ZWANG")
			(pinfunction "IO1_3")
		)
		(pad "17" smd rect
			(at 3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/230V & general interface/230V1")
			(pinfunction "IO1_4")
		)
		(pad "18" smd rect
			(at 3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/230V & general interface/230V2")
			(pinfunction "IO1_5")
		)
		(pad "19" smd rect
			(at 3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "/230V & general interface/ENTFRH")
			(pinfunction "IO1_6")
		)
		(pad "20" smd rect
			(at 3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "/230V & general interface/ENTFON")
			(pinfunction "IO1_7")
		)
		(pad "21" smd rect
			(at 3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A0")
		)
		(pad "22" smd rect
			(at 3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/SCL")
			(pinfunction "SCL")
		)
		(pad "23" smd rect
			(at 3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/SDA")
			(pinfunction "SDA")
		)
		(pad "24" smd rect
			(at 3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/5V ")
			(pinfunction "VDD")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Housings_SSOP_TSSOP.3dshapes/SSOP-24_5.3x8.2mm_Pitch0.65mm.step"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 94 60)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "MH1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MHNP_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "020.02.010.0221.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3.2)
			(layers "*.Mask")
			(clearance 1.4)
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 89.999998 59.999998)
		(mid 91.171572 57.171571)
		(end 94 56)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 93.999998 144)
		(mid 91.171571 142.828426)
		(end 90 139.999998)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 151.895296 125.38825)
		(end 153.228796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 124.278796 115.7307)
		(end 135.010296 117.1912)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 188.551585 125.37011) (xy 193.853835 125.37011) (xy 193.853835 137.99899) (xy 195.187335 137.99899)
			(xy 195.187335 125.37011) (xy 200.489585 125.37011) (xy 200.489585 123.71911) (xy 188.551585 123.71911)
			(xy 188.551585 125.37011)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 136.895296 125.38825)
		(end 138.228796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94 56)
		(end 206 56)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 144.395296 125.38825)
		(end 145.728796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210 140)
		(mid 208.828426 142.828427)
		(end 205.999998 143.999998)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 109.039296 115.7307)
		(end 119.770796 117.1912)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 114.395296 125.38825)
		(end 115.728796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 154.282546 115.70208)
		(end 165.014046 117.16258)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210 60)
		(end 210 140)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.999998 143.999998)
		(end 93.999998 144)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 171.41825 125.37011) (xy 176.7205 125.37011) (xy 176.7205 137.99899) (xy 178.054 137.99899) (xy 178.054 125.37011)
			(xy 183.35625 125.37011) (xy 183.35625 123.71911) (xy 171.41825 123.71911) (xy 171.41825 125.37011)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 139.201296 115.70208)
		(end 149.932796 117.16258)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 121.895296 125.38825)
		(end 123.228796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.000002 55.999998)
		(mid 208.828429 57.171572)
		(end 210 60)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90 140)
		(end 90 60)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 159.395296 125.38825)
		(end 160.728796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 129.395296 125.38825)
		(end 130.728796 138.01713)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "020.02.010.0221"
		(at 93.90975 71.11462 270)
		(layer "B.Cu")
	)
	(gr_text "Zu/Abluft"
		(at 145.061296 142.04375 0)
		(layer "F.SilkS")
	)
	(gr_text "Netz 2"
		(at 193.695335 142.113 0)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 104.9655 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "Türöffner"
		(at 115.030296 142.04375 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 1"
		(at 104.775 57.46475 0)
		(layer "F.SilkS")
	)
	(gr_text "500mA"
		(at 111.4425 91.6305 270)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 132.969 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 3"
		(at 132.715 57.52825 0)
		(layer "F.SilkS")
	)
	(gr_text "HC-IO V1"
		(at 97.9805 129.83464 0)
		(layer "F.SilkS")
	)
	(gr_text "Reserve"
		(at 130.016296 142.04375 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 6"
		(at 174.752 57.52825 0)
		(layer "F.SilkS")
	)
	(gr_text "Netz 1"
		(at 177.338731 142.131561 0)
		(layer "F.SilkS")
	)
	(gr_text "MCU"
		(at 91.186 111.34344 270)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 160.909 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 4"
		(at 146.685 57.52825 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 2"
		(at 118.745 57.46475 0)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 174.9425 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "Zwangsentl."
		(at 160.047296 142.04375 0)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 147.0025 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "WorldInOne M.Straub\n(C) 2021"
		(at 206.4385 103.28656 90)
		(layer "F.SilkS")
	)
	(gr_text "12VDC  GND"
		(at 91.7575 87.884 270)
		(layer "F.SilkS")
	)
	(gr_text "5V SDA SCL GND"
		(at 118.999 59.36975 0)
		(layer "F.SilkS")
	)
	(gr_text "Sensor 5"
		(at 160.782 57.52825 0)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 94 60) (xy 94 140)
		)
		(height 119.0425)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
		)
		(gr_text "80.0 mm"
			(at 213.0425 100 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 210 140) (xy 90 139.999998)
		)
		(height 11.16556)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.05)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "120.0 mm"
			(at 150 151.16556 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 206 140) (xy 94 140)
		)
		(height 9.5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "112.0 mm"
			(at 150 149.5 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 205.999998 143.999998) (xy 206 56)
		)
		(height 10)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.05)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "88.0 mm"
			(at 215.999998 99.999999 90)
			(layer "Cmts.User")
		)
	)
	(zone
		(net 6)
		(net_name "/5V ")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
		(polygon
			(pts
				(xy 140.431783 87.6935) (xy 126.24268 87.6935) (xy 126.24268 86.106) (xy 140.431783 86.106)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/12V")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
		(polygon
			(pts
				(xy 129.505853 96.4565) (xy 122.557946 96.4565) (xy 122.557946 95.504) (xy 129.505853 95.504)
			)
		)
	)
	(zone
		(net 113)
		(net_name "Net-(D3-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
		(polygon
			(pts
				(xy 138.03249 93.472) (xy 132.44449 93.472) (xy 132.50799 96.9645) (xy 130.34899 96.9645) (xy 130.34899 91.948)
				(xy 138.03249 91.948)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(name "GND")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.2032) (thermal_bridge_width 0.254))
		(polygon
			(pts
				(xy 209.667695 114.69878) (xy 102.673194 114.736206) (xy 102.669699 144.01753) (xy 89.843195 144.018)
				(xy 89.773208 55.847287) (xy 209.722417 55.877593)
			)
		)
	)
	(embedded_fonts no)
)
