(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (grid_origin 135.898082 66.20975)
    (pcbplotparams
      (layerselection 0x0001030_80000001)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(P8-Pad3)")
  (net 2 "Net-(P8-Pad4)")
  (net 3 "Net-(P8-Pad5)")
  (net 4 "Net-(P8-Pad6)")
  (net 5 "Net-(P8-Pad13)")
  (net 6 "Net-(P8-Pad14)")
  (net 7 "Net-(P8-Pad17)")
  (net 8 "Net-(P8-Pad19)")
  (net 9 "Net-(P8-Pad20)")
  (net 10 "Net-(P8-Pad21)")
  (net 11 "Net-(P8-Pad22)")
  (net 12 "Net-(P8-Pad23)")
  (net 13 "Net-(P8-Pad24)")
  (net 14 "Net-(P8-Pad25)")
  (net 15 "Net-(P8-Pad26)")
  (net 16 "Net-(P8-Pad27)")
  (net 17 "Net-(P8-Pad28)")
  (net 18 "Net-(P8-Pad29)")
  (net 19 "Net-(P8-Pad30)")
  (net 20 "Net-(P9-Pad11)")
  (net 21 "Net-(P9-Pad12)")
  (net 22 "Net-(P9-Pad13)")
  (net 23 "Net-(P9-Pad17)")
  (net 24 "Net-(P9-Pad18)")
  (net 25 "Net-(P9-Pad25)")
  (net 26 "Net-(P9-Pad27)")
  (net 27 "Net-(P9-Pad28)")
  (net 28 "Net-(P9-Pad33)")
  (net 29 "Net-(P9-Pad35)")
  (net 30 "Net-(P9-Pad36)")
  (net 31 "Net-(P9-Pad37)")
  (net 32 "Net-(P9-Pad38)")
  (net 33 "Net-(P9-Pad39)")
  (net 34 "Net-(P9-Pad40)")
  (net 35 "Net-(P9-Pad41)")
  (net 36 "Net-(P9-Pad42)")
  (net 37 "+3V3")
  (net 38 "SYS_5V")
  (net 39 "PWR_BUT")
  (net 40 "SYS_RESETN")
  (net 41 "Net-(D1-Pad4)")
  (net 42 "Net-(D1-Pad3)")
  (net 43 "Net-(D1-Pad1)")
  (net 44 "/IL1-")
  (net 45 "/IL2-")
  (net 46 "/IL3-")
  (net 47 "/IL4-")
  (net 48 "/IL5-")
  (net 49 "/IL6-")
  (net 50 "/IL7-")
  (net 51 "/plane0-")
  (net 52 "/plane1-")
  (net 53 "/plane2-")
  (net 54 "/plane3-")
  (net 55 "/plane4-")
  (net 56 "/plane5-")
  (net 57 "/plane6-")
  (net 58 "/plane7-")
  (net 59 "/plane8-")
  (net 60 "/clear-")
  (net 61 "/addr_okay-")
  (net 62 "/IL1+")
  (net 63 "/IL2+")
  (net 64 "/IL3+")
  (net 65 "/IL4+")
  (net 66 "/IL5+")
  (net 67 "/IL6+")
  (net 68 "/IL7+")
  (net 69 "/plane0+")
  (net 70 "/plane1+")
  (net 71 "/plane2+")
  (net 72 "/plane3+")
  (net 73 "/plane4+")
  (net 74 "/plane5+")
  (net 75 "/plane6+")
  (net 76 "/plane7+")
  (net 77 "/plane8+")
  (net 78 "/clear+")
  (net 79 "/addr_okay+")
  (net 80 "/sense1+")
  (net 81 "/sense2+")
  (net 82 "/sense3+")
  (net 83 "/sense4+")
  (net 84 "/sense5+")
  (net 85 "/sense6+")
  (net 86 "/sense7+")
  (net 87 "/sense8+")
  (net 88 "/sense9+")
  (net 89 "/sense10+")
  (net 90 "/sense11+")
  (net 91 "/sense12+")
  (net 92 "/sense13+")
  (net 93 "/sense14+")
  (net 94 "/sense15+")
  (net 95 "/sense16+")
  (net 96 "/sense1-")
  (net 97 "/sense2-")
  (net 98 "/sense3-")
  (net 99 "/sense4-")
  (net 100 "/sense5-")
  (net 101 "/sense6-")
  (net 102 "/sense7-")
  (net 103 "/sense8-")
  (net 104 "/sense9-")
  (net 105 "/sense10-")
  (net 106 "/sense11-")
  (net 107 "/sense12-")
  (net 108 "/sense13-")
  (net 109 "/sense14-")
  (net 110 "/sense15-")
  (net 111 "/sense16-")
  (net 112 "/sense2")
  (net 113 "/sense3")
  (net 114 "/sense5")
  (net 115 "/sense4")
  (net 116 "/IL2")
  (net 117 "/IL1")
  (net 118 "/IL4")
  (net 119 "/IL3")
  (net 120 "/sense1")
  (net 121 "/plane3")
  (net 122 "/plane4")
  (net 123 "/plane2")
  (net 124 "/b")
  (net 125 "/plane1")
  (net 126 "/sense16")
  (net 127 "/sense14")
  (net 128 "/sense15")
  (net 129 "/sense12")
  (net 130 "/sense13")
  (net 131 "/sense10")
  (net 132 "/sense11")
  (net 133 "/sense8")
  (net 134 "/sense9")
  (net 135 "/sense6")
  (net 136 "/sense7")
  (net 137 "Net-(P9-Pad5)")
  (net 138 "Net-(P9-Pad6)")
  (net 139 "/IL7")
  (net 140 "/IL5")
  (net 141 "/plane0")
  (net 142 "/plane6")
  (net 143 "/plane5")
  (net 144 "/g")
  (net 145 "/r")
  (net 146 "/IL6")
  (net 147 "/plane8")
  (net 148 "/plane7")
  (net 149 "/clear")
  (net 150 "/red")
  (net 151 "/addr_okay")
  (net 152 "Net-(P9-Pad32)")
  (net 153 "Net-(P9-Pad34)")
  (net 154 "Net-(IC5-Pad13)")
  (net 155 "/red_out")
  (net 156 "Net-(U10-Pad12)")
  (net 157 "Net-(U10-Pad10)")
  (net 158 "Net-(U10-Pad8)")
  (net 159 "Net-(U10-Pad6)")
  (net 160 "Net-(U10-Pad4)")
  (net 161 "Net-(M1-Pad19)")
  (net 162 "Net-(M1-Pad21)")
  (net 163 "Net-(M1-Pad22)")
  (net 164 "Net-(M1-Pad23)")
  (net 165 "Net-(M1-Pad24)")
  (net 166 "Net-(M1-Pad25)")
  (net 167 "Net-(M1-Pad50)")
  (net 168 "Net-(M1-Pad49)")
  (net 169 "Net-(M1-Pad48)")
  (net 170 "Net-(M1-Pad47)")
  (net 171 "Net-(M1-Pad46)")
  (net 172 "Net-(M1-Pad45)")
  (net 173 "Net-(M1-Pad44)")
  (net 174 "Net-(M2-Pad25)")
  (net 175 "Net-(M2-Pad24)")
  (net 176 "Net-(M2-Pad23)")
  (net 177 "Net-(M2-Pad22)")
  (net 178 "Net-(M2-Pad21)")
  (net 179 "Net-(M2-Pad20)")
  (net 180 "Net-(M2-Pad19)")
  (net 181 "Net-(M2-Pad18)")
  (net 182 "Net-(M2-Pad17)")
  (net 183 "Net-(M2-Pad42)")
  (net 184 "Net-(M2-Pad43)")
  (net 185 "Net-(M2-Pad44)")
  (net 186 "Net-(M2-Pad45)")
  (net 187 "Net-(M2-Pad46)")
  (net 188 "Net-(M2-Pad47)")
  (net 189 "Net-(M2-Pad48)")
  (net 190 "Net-(M2-Pad49)")
  (net 191 "Net-(M2-Pad50)")
  (net 192 "GNDD")
  (net 193 "Net-(IC5-Pad5)")
  (footprint "Socket_BeagleBone_Black:Socket_BeagleBone_Black" (layer "F.Cu")
    (at 116.3701 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (property "Reference" "P9" (at 0 -5.1 0) (layer "F.SilkS"))
    (property "Value" "BeagleBone_Black_Header" (at 0 -3.1 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 37 "+3V3")
    )
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 37 "+3V3")
    )
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 137 "Net-(P9-Pad5)")
    )
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 138 "Net-(P9-Pad6)")
    )
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 38 "SYS_5V")
    )
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 38 "SYS_5V")
    )
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 39 "PWR_BUT")
    )
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 40 "SYS_RESETN")
    )
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 20 "Net-(P9-Pad11)")
    )
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 21 "Net-(P9-Pad12)")
    )
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 22 "Net-(P9-Pad13)")
    )
    (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 139 "/IL7")
    )
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 140 "/IL5")
    )
    (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 141 "/plane0")
    )
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 23 "Net-(P9-Pad17)")
    )
    (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 24 "Net-(P9-Pad18)")
    )
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 142 "/plane6")
    )
    (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 143 "/plane5")
    )
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 144 "/g")
    )
    (pad "22" thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 145 "/r")
    )
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 146 "/IL6")
    )
    (pad "24" thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 147 "/plane8")
    )
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 25 "Net-(P9-Pad25)")
    )
    (pad "26" thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 148 "/plane7")
    )
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 26 "Net-(P9-Pad27)")
    )
    (pad "28" thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 27 "Net-(P9-Pad28)")
    )
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 149 "/clear")
    )
    (pad "30" thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 150 "/red")
    )
    (pad "31" thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 151 "/addr_okay")
    )
    (pad "32" thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 152 "Net-(P9-Pad32)")
    )
    (pad "33" thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 28 "Net-(P9-Pad33)")
    )
    (pad "34" thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 153 "Net-(P9-Pad34)")
    )
    (pad "35" thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 29 "Net-(P9-Pad35)")
    )
    (pad "36" thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 30 "Net-(P9-Pad36)")
    )
    (pad "37" thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 31 "Net-(P9-Pad37)")
    )
    (pad "38" thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 32 "Net-(P9-Pad38)")
    )
    (pad "39" thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 33 "Net-(P9-Pad39)")
    )
    (pad "40" thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 34 "Net-(P9-Pad40)")
    )
    (pad "41" thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 35 "Net-(P9-Pad41)")
    )
    (pad "42" thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 36 "Net-(P9-Pad42)")
    )
    (pad "43" thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "44" thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "45" thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "46" thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (model "${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl"
      (offset (xyz 1.269999981 -27.93999958 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "LEDs:LED_D5.0mm-4" (layer "F.Cu")
    (at 154.5971 55.9054)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (property "Reference" "D1" (at 1.905 -3.96 0) (layer "F.SilkS"))
    (property "Value" "LED_RCGB" (at 1.905 3.96 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(D1-Pad1)")
    )
    (pad "2" thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
    (pad "3" thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(D1-Pad3)")
    )
    (pad "4" thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(D1-Pad4)")
    )
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 142.6591 84.4804)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC2" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C32" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/IL5-")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/IL5+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "/IL5")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "/IL7")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/IL7+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/IL7-")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/plane0-")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/plane0+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "/plane0")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/IL6")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/IL6+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/IL6-")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 142.6591 109.7534)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC4" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C32" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/plane5-")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/plane5+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "/plane5")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "/plane7")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/plane7+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/plane7-")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/plane8-")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/plane8+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/plane8")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "/plane6")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/plane6+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/plane6-")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 154.7241 97.1804)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC7" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C31" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "/sense7")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/sense7+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "/sense7-")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "/sense5-")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/sense5+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/sense5")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "/sense6")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/sense6+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "/sense6-")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "/sense8-")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/sense8+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "/sense8")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 154.9781 71.0184)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC9" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C31" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "/sense15")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/sense15+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/sense15-")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "/sense13-")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/sense13+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/sense13")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "/sense14")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/sense14+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/sense14-")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/sense16-")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/sense16+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "/sense16")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Buttons_Switches_ThroughHole:SW_PUSH_6mm" (layer "F.Cu")
    (at 163.2331 50.9524 90)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Reference" "B2" (at 3.25 -2 90) (layer "F.SilkS"))
    (property "Value" "SW_Push" (at 3.75 6.7 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "SYS_RESETN")
    )
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "SYS_RESETN")
    )
    (model "${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0.1269999981 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 142.6591 97.1804)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC3" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C32" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/plane1-")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/plane1+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "/plane1")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/plane3")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/plane3+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/plane3-")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/plane4-")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/plane4+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "/plane4")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "/plane2")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/plane2+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/plane2-")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Measurement_Points:Measurement_Point_Round-TH_Small" (layer "F.Cu")
    (at 133.993082 125.51875)
    (descr "Measurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Measurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (property "Reference" "TP1" (at 0 -2 0) (layer "F.SilkS"))
    (property "Value" "TestPoint" (at 0 2 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 148.6281 117.8814)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C5" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 148.7551 103.5304)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C4" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 148.7551 66.4464)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 154.7241 84.4804)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC8" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C31" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "/sense11")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/sense11+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/sense11-")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "/sense9-")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/sense9+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/sense9")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/sense10")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/sense10+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "/sense10-")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "/sense12-")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/sense12+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "/sense12")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 148.2471 89.9414)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C3" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 159.9311 78.8924)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C8" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 160.4391 67.2084)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C9" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 160.8201 119.2784)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C10" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm" (layer "F.Cu")
    (at 154.9781 123.0884)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "U10" (at 0 -5.375 0) (layer "F.SilkS"))
    (property "Value" "74LVC07" (at 0 5.375 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "/red")
    )
    (pad "2" smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "/red_out")
    )
    (pad "3" smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "4" smd rect (at -2.7 0) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(U10-Pad4)")
    )
    (pad "5" smd rect (at -2.7 1.27) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "6" smd rect (at -2.7 2.54) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(U10-Pad6)")
    )
    (pad "7" smd rect (at -2.7 3.81) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "8" smd rect (at 2.7 3.81) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(U10-Pad8)")
    )
    (pad "9" smd rect (at 2.7 2.54) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "10" smd rect (at 2.7 1.27) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "Net-(U10-Pad10)")
    )
    (pad "11" smd rect (at 2.7 0) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "12" smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(U10-Pad12)")
    )
    (pad "13" smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "14" smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Buttons_Switches_ThroughHole:SW_PUSH_6mm" (layer "F.Cu")
    (at 159.2961 44.3484 -90)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Reference" "B1" (at 3.25 -2 -90) (layer "F.SilkS"))
    (property "Value" "SW_Push" (at 3.75 6.7 -90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "${REFERENCE}" (at 3.25 2.25 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
    (pad "1" thru_hole circle (at 6.5 0) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 192 "GNDD")
    )
    (pad "2" thru_hole circle (at 0 4.5) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "PWR_BUT")
    )
    (pad "2" thru_hole circle (at 6.5 4.5) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "PWR_BUT")
    )
    (model "${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0.1269999981 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Centronics-Ken:CENTRONICS-50-F" (layer "F.Cu")
    (at 130.4671 58.6994 90)
    (property "Reference" "M1" (at -12.7 6.35 90) (layer "F.SilkS"))
    (property "Value" "50-PIN-CENTRONICS-FFEMALE" (at -12.7 2.54 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "26" (at 1.524 -6.096 90) (layer "F.SilkS"))
    (fp_text user "25" (at -53.848 1.524 90) (layer "F.SilkS"))
    (fp_text user "50" (at -53.848 -5.588 90) (layer "F.SilkS"))
    (fp_text user "1" (at 1.016 2.032 90) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -63.335 -2.03 90) (size 3.45 3.45) (drill 3.45) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 11.495 -2.03 90) (size 3.45 3.45) (drill 3.45) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 44 "/IL1-")
    )
    (pad "2" thru_hole circle (at -2.16 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 45 "/IL2-")
    )
    (pad "3" thru_hole circle (at -4.32 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 46 "/IL3-")
    )
    (pad "4" thru_hole circle (at -6.48 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 47 "/IL4-")
    )
    (pad "5" thru_hole circle (at -8.64 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 48 "/IL5-")
    )
    (pad "6" thru_hole circle (at -10.8 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 49 "/IL6-")
    )
    (pad "7" thru_hole circle (at -12.96 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 50 "/IL7-")
    )
    (pad "8" thru_hole circle (at -15.12 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 51 "/plane0-")
    )
    (pad "9" thru_hole circle (at -17.28 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 52 "/plane1-")
    )
    (pad "10" thru_hole circle (at -19.44 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 53 "/plane2-")
    )
    (pad "11" thru_hole circle (at -21.6 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 54 "/plane3-")
    )
    (pad "12" thru_hole circle (at -23.76 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 55 "/plane4-")
    )
    (pad "13" thru_hole circle (at -25.92 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 56 "/plane5-")
    )
    (pad "14" thru_hole circle (at -28.08 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 57 "/plane6-")
    )
    (pad "15" thru_hole circle (at -30.24 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 58 "/plane7-")
    )
    (pad "16" thru_hole circle (at -32.4 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 59 "/plane8-")
    )
    (pad "17" thru_hole circle (at -34.56 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 60 "/clear-")
    )
    (pad "18" thru_hole circle (at -36.72 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 61 "/addr_okay-")
    )
    (pad "19" thru_hole circle (at -38.88 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 161 "Net-(M1-Pad19)")
    )
    (pad "20" thru_hole circle (at -41.04 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 155 "/red_out")
    )
    (pad "21" thru_hole circle (at -43.2 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 162 "Net-(M1-Pad21)")
    )
    (pad "22" thru_hole circle (at -45.36 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 163 "Net-(M1-Pad22)")
    )
    (pad "23" thru_hole circle (at -47.52 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 164 "Net-(M1-Pad23)")
    )
    (pad "24" thru_hole circle (at -49.68 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 165 "Net-(M1-Pad24)")
    )
    (pad "25" thru_hole circle (at -51.84 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 166 "Net-(M1-Pad25)")
    )
    (pad "26" thru_hole circle (at 0 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 62 "/IL1+")
    )
    (pad "27" thru_hole circle (at -2.16 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 63 "/IL2+")
    )
    (pad "28" thru_hole circle (at -4.32 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 64 "/IL3+")
    )
    (pad "29" thru_hole circle (at -6.48 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 65 "/IL4+")
    )
    (pad "30" thru_hole circle (at -8.64 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 66 "/IL5+")
    )
    (pad "31" thru_hole circle (at -10.8 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 67 "/IL6+")
    )
    (pad "32" thru_hole circle (at -12.96 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 68 "/IL7+")
    )
    (pad "33" thru_hole circle (at -15.12 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 69 "/plane0+")
    )
    (pad "34" thru_hole circle (at -17.28 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 70 "/plane1+")
    )
    (pad "35" thru_hole circle (at -19.44 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 71 "/plane2+")
    )
    (pad "36" thru_hole circle (at -21.6 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 72 "/plane3+")
    )
    (pad "37" thru_hole circle (at -23.76 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 73 "/plane4+")
    )
    (pad "38" thru_hole circle (at -25.92 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 74 "/plane5+")
    )
    (pad "39" thru_hole circle (at -28.08 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 75 "/plane6+")
    )
    (pad "40" thru_hole circle (at -30.24 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 76 "/plane7+")
    )
    (pad "41" thru_hole circle (at -32.4 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 77 "/plane8+")
    )
    (pad "42" thru_hole circle (at -34.56 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 78 "/clear+")
    )
    (pad "43" thru_hole circle (at -36.72 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 79 "/addr_okay+")
    )
    (pad "44" thru_hole circle (at -38.88 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 173 "Net-(M1-Pad44)")
    )
    (pad "45" thru_hole circle (at -41.04 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 172 "Net-(M1-Pad45)")
    )
    (pad "46" thru_hole circle (at -43.2 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 171 "Net-(M1-Pad46)")
    )
    (pad "47" thru_hole circle (at -45.36 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 170 "Net-(M1-Pad47)")
    )
    (pad "48" thru_hole circle (at -47.52 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 169 "Net-(M1-Pad48)")
    )
    (pad "49" thru_hole circle (at -49.68 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 168 "Net-(M1-Pad49)")
    )
    (pad "50" thru_hole circle (at -51.84 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 167 "Net-(M1-Pad50)")
    )
  )
  (footprint "Centronics-Ken:CENTRONICS-50-M" (layer "F.Cu")
    (at 178.8541 59.2074 90)
    (property "Reference" "M2" (at -12.7 6.35 90) (layer "F.SilkS"))
    (property "Value" "50-PIN-CENTRONICS-MMALE" (at -12.7 2.54 90) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (fp_text user "26" (at -53.848 -5.588 90) (layer "F.SilkS"))
    (fp_text user "50" (at 1.524 -6.096 90) (layer "F.SilkS"))
    (fp_text user "1" (at -53.848 1.524 90) (layer "F.SilkS"))
    (fp_text user "25" (at 1.016 2.032 90) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -63.335 -2.03 90) (size 3.45 3.45) (drill 3.45) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 11.495 -2.03 90) (size 3.45 3.45) (drill 3.45) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -51.84 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 80 "/sense1+")
    )
    (pad "2" thru_hole circle (at -49.68 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 81 "/sense2+")
    )
    (pad "3" thru_hole circle (at -47.52 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 82 "/sense3+")
    )
    (pad "4" thru_hole circle (at -45.36 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 83 "/sense4+")
    )
    (pad "5" thru_hole circle (at -43.2 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 84 "/sense5+")
    )
    (pad "6" thru_hole circle (at -41.04 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 85 "/sense6+")
    )
    (pad "7" thru_hole circle (at -38.88 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 86 "/sense7+")
    )
    (pad "8" thru_hole circle (at -36.72 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 87 "/sense8+")
    )
    (pad "9" thru_hole circle (at -34.56 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 88 "/sense9+")
    )
    (pad "10" thru_hole circle (at -32.4 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 89 "/sense10+")
    )
    (pad "11" thru_hole circle (at -30.24 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 90 "/sense11+")
    )
    (pad "12" thru_hole circle (at -28.08 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 91 "/sense12+")
    )
    (pad "13" thru_hole circle (at -25.92 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 92 "/sense13+")
    )
    (pad "14" thru_hole circle (at -23.76 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 93 "/sense14+")
    )
    (pad "15" thru_hole circle (at -21.6 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 94 "/sense15+")
    )
    (pad "16" thru_hole circle (at -19.44 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 95 "/sense16+")
    )
    (pad "17" thru_hole circle (at -17.28 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 182 "Net-(M2-Pad17)")
    )
    (pad "18" thru_hole circle (at -15.12 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 181 "Net-(M2-Pad18)")
    )
    (pad "19" thru_hole circle (at -12.96 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 180 "Net-(M2-Pad19)")
    )
    (pad "20" thru_hole circle (at -10.8 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 179 "Net-(M2-Pad20)")
    )
    (pad "21" thru_hole circle (at -8.64 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 178 "Net-(M2-Pad21)")
    )
    (pad "22" thru_hole circle (at -6.48 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 177 "Net-(M2-Pad22)")
    )
    (pad "23" thru_hole circle (at -4.32 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 176 "Net-(M2-Pad23)")
    )
    (pad "24" thru_hole circle (at -2.16 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 175 "Net-(M2-Pad24)")
    )
    (pad "25" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 174 "Net-(M2-Pad25)")
    )
    (pad "26" thru_hole circle (at -51.84 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 96 "/sense1-")
    )
    (pad "27" thru_hole circle (at -49.68 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 97 "/sense2-")
    )
    (pad "28" thru_hole circle (at -47.52 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 98 "/sense3-")
    )
    (pad "29" thru_hole circle (at -45.36 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 99 "/sense4-")
    )
    (pad "30" thru_hole circle (at -43.2 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 100 "/sense5-")
    )
    (pad "31" thru_hole circle (at -41.04 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 101 "/sense6-")
    )
    (pad "32" thru_hole circle (at -38.88 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 102 "/sense7-")
    )
    (pad "33" thru_hole circle (at -36.72 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 103 "/sense8-")
    )
    (pad "34" thru_hole circle (at -34.56 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 104 "/sense9-")
    )
    (pad "35" thru_hole circle (at -32.4 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 105 "/sense10-")
    )
    (pad "36" thru_hole circle (at -30.24 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 106 "/sense11-")
    )
    (pad "37" thru_hole circle (at -28.08 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 107 "/sense12-")
    )
    (pad "38" thru_hole circle (at -25.92 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 108 "/sense13-")
    )
    (pad "39" thru_hole circle (at -23.76 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 109 "/sense14-")
    )
    (pad "40" thru_hole circle (at -21.6 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 110 "/sense15-")
    )
    (pad "41" thru_hole circle (at -19.44 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 111 "/sense16-")
    )
    (pad "42" thru_hole circle (at -17.28 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 183 "Net-(M2-Pad42)")
    )
    (pad "43" thru_hole circle (at -15.12 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 184 "Net-(M2-Pad43)")
    )
    (pad "44" thru_hole circle (at -12.96 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 185 "Net-(M2-Pad44)")
    )
    (pad "45" thru_hole circle (at -10.8 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 186 "Net-(M2-Pad45)")
    )
    (pad "46" thru_hole circle (at -8.64 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 187 "Net-(M2-Pad46)")
    )
    (pad "47" thru_hole circle (at -6.48 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 188 "Net-(M2-Pad47)")
    )
    (pad "48" thru_hole circle (at -4.32 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 189 "Net-(M2-Pad48)")
    )
    (pad "49" thru_hole circle (at -2.16 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 190 "Net-(M2-Pad49)")
    )
    (pad "50" thru_hole circle (at 0 -4.06 90) (size 1.7 1.7) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 191 "Net-(M2-Pad50)")
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 142.6591 122.4534)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC5" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C32" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/clear-")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/clear+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "/clear")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "Net-(IC5-Pad5)")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/addr_okay-")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/addr_okay+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "/addr_okay")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(IC5-Pad13)")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 160.1851 91.4654)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C7" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 148.6281 78.0034)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 160.3121 105.83375)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "C6" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" ".1UF" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 142.6591 71.0184)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC1" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C32" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/IL1-")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/IL1+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/IL1")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "/IL3")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/IL3+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/IL3-")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/IL4-")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/IL4+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/IL4")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/IL2")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/IL2+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/IL2-")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "+3V3")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket_BeagleBone_Black:Socket_BeagleBone_Black" (layer "F.Cu")
    (at 164.6301 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (property "Reference" "P8" (at 0 -5.1 0) (layer "F.SilkS"))
    (property "Value" "BeagleBone_Black_Header" (at 0 -3.1 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 192 "GNDD")
    )
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "Net-(P8-Pad3)")
    )
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 2 "Net-(P8-Pad4)")
    )
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 3 "Net-(P8-Pad5)")
    )
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 4 "Net-(P8-Pad6)")
    )
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 112 "/sense2")
    )
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 113 "/sense3")
    )
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 114 "/sense5")
    )
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 115 "/sense4")
    )
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 116 "/IL2")
    )
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 117 "/IL1")
    )
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 5 "Net-(P8-Pad13)")
    )
    (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 6 "Net-(P8-Pad14)")
    )
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 118 "/IL4")
    )
    (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 119 "/IL3")
    )
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 7 "Net-(P8-Pad17)")
    )
    (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 120 "/sense1")
    )
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 8 "Net-(P8-Pad19)")
    )
    (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 9 "Net-(P8-Pad20)")
    )
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 10 "Net-(P8-Pad21)")
    )
    (pad "22" thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 11 "Net-(P8-Pad22)")
    )
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "Net-(P8-Pad23)")
    )
    (pad "24" thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "Net-(P8-Pad24)")
    )
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 14 "Net-(P8-Pad25)")
    )
    (pad "26" thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 15 "Net-(P8-Pad26)")
    )
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 16 "Net-(P8-Pad27)")
    )
    (pad "28" thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 17 "Net-(P8-Pad28)")
    )
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 18 "Net-(P8-Pad29)")
    )
    (pad "30" thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 19 "Net-(P8-Pad30)")
    )
    (pad "31" thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 121 "/plane3")
    )
    (pad "32" thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 122 "/plane4")
    )
    (pad "33" thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 123 "/plane2")
    )
    (pad "34" thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 124 "/b")
    )
    (pad "35" thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 125 "/plane1")
    )
    (pad "36" thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 126 "/sense16")
    )
    (pad "37" thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 127 "/sense14")
    )
    (pad "38" thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 128 "/sense15")
    )
    (pad "39" thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 129 "/sense12")
    )
    (pad "40" thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 130 "/sense13")
    )
    (pad "41" thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 131 "/sense10")
    )
    (pad "42" thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 132 "/sense11")
    )
    (pad "43" thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 133 "/sense8")
    )
    (pad "44" thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 134 "/sense9")
    )
    (pad "45" thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 135 "/sense6")
    )
    (pad "46" thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 136 "/sense7")
    )
    (model "${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl"
      (offset (xyz 1.269999981 -27.93999958 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer "F.Cu")
    (at 154.7241 110.1344)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (property "Reference" "IC6" (at 0 -6 0) (layer "F.SilkS"))
    (property "Value" "AM26C31" (at 0 6 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/sense4")
    )
    (pad "2" smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/sense4+")
    )
    (pad "3" smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/sense4-")
    )
    (pad "4" smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "5" smd rect (at -2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "/sense2-")
    )
    (pad "6" smd rect (at -2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/sense2+")
    )
    (pad "7" smd rect (at -2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/sense2")
    )
    (pad "8" smd rect (at -2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "9" smd rect (at 2.7 4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/sense1")
    )
    (pad "10" smd rect (at 2.7 3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/sense1+")
    )
    (pad "11" smd rect (at 2.7 1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/sense1-")
    )
    (pad "12" smd rect (at 2.7 0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "GNDD")
    )
    (pad "13" smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/sense3-")
    )
    (pad "14" smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/sense3+")
    )
    (pad "15" smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/sense3")
    )
    (pad "16" smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SYS_5V")
    )
    (model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 117.64 57.31)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "REF**" (at 0 -4.2 0) (layer "F.SilkS"))
    (property "Value" "MountingHole_3.2mm_M3" (at 0 4.2 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0.3 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 166.03 57.31)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "REF**" (at 0 -4.2 0) (layer "F.SilkS"))
    (property "Value" "MountingHole_3.2mm_M3" (at 0 4.2 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0.3 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 162.72 123.41)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "REF**" (at 0 -4.2 0) (layer "F.SilkS"))
    (property "Value" "MountingHole_3.2mm_M3" (at 0 4.2 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0.3 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Mounting_Holes:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 120.81 123.41)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Reference" "REF**" (at 0 -4.2 0) (layer "F.SilkS"))
    (property "Value" "MountingHole_3.2mm_M3" (at 0 4.2 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0.3 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 155.441082 59.91975)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "R1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "220" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/r")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(D1-Pad1)")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 155.329082 63.41575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "R2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "220" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 1.914939 1.816099 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "/b")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(D1-Pad4)")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitors_SMD:C_0603" (layer "F.Cu")
    (at 155.329082 61.63775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Reference" "R3" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "220" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr smd)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "/g")
    )
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(D1-Pad3)")
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 127.1651 129.0574) (end 184.5691 129.0574)
    (layer "Edge.Cuts"))
  (gr_arc (start 114.4651 49.0474) (mid 116.324972 44.557272) (end 120.8151 42.6974)
    (layer "Edge.Cuts"))
  (gr_line (start 184.5691 129.0574) (end 184.5691 42.8244)
    (layer "Edge.Cuts"))
  (gr_line (start 135.4201 42.6974) (end 120.8151 42.6974)
    (layer "Edge.Cuts"))
  (gr_line (start 135.4201 64.2874) (end 135.4201 42.6974)
    (layer "Edge.Cuts"))
  (gr_line (start 114.4651 49.0474) (end 114.4651 116.3574)
    (layer "Edge.Cuts"))
  (gr_line (start 153.2001 64.2874) (end 135.4201 64.2874)
    (layer "Edge.Cuts"))
  (gr_arc (start 127.1651 129.0574) (mid 118.184844 125.337656) (end 114.4651 116.3574)
    (layer "Edge.Cuts"))
  (gr_line (start 184.5691 42.8244) (end 153.2001 42.8244)
    (layer "Edge.Cuts"))
  (gr_line (start 153.2001 42.8244) (end 153.2001 64.2874)
    (layer "Edge.Cuts"))
  (gr_text "AGC rope V1.02  righto.com" (at 171.966082 127.67775 0) (layer "F.SilkS"))
  (zone (net 192) (net_name "GNDD") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.22606) (filled_areas_thickness no)
    (fill yes (thermal_gap 1.016) (thermal_bridge_width 0.2286))
    (polygon
      (pts
        (xy 184.539082 42.84175)
        (xy 184.666082 129.07475)
        (xy 107.831082 129.45575)
        (xy 112.530082 42.20675)
      )
    )
  )
  (zone (net 192) (net_name "GNDD") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.920082 42.84175)
        (xy 184.793082 129.70975)
        (xy 108.593082 130.47175)
        (xy 112.530082 42.84175)
      )
    )
  )
)
