(kicad_pcb (version 20210722) (generator pcbnew)
  (general
    (thickness 4.48)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" power)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.44) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.44) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.44) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.05)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+12V")
  (net 3 "USER2_L")
  (net 4 "USER3_L")
  (net 5 "CLK_P")
  (net 6 "CLK_N")
  (net 7 "TRIG_P")
  (net 8 "TRIG_N")
  (net 9 "TIMES_P")
  (net 10 "TIMES_N")
  (net 11 "USER1_P")
  (net 12 "USER1_N")
  (net 13 "/MP")
  (net 14 "PEG+12Vo")
  (net 15 "/12Vs")
  (net 16 "/12Vg")
  (net 17 "unconnected-(J10-Pad5)")
  (footprint "BoardIO:Molex_Mini-Fit_Jr_5569-06A1_2x03_P4.20mm_Horizontal" (layer "F.Cu")
    (tedit 60B7A0D6)
    (at 104.648 -92.695 -90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-06A1, example for new mpn: 39-29-4069, 3 Pins per row, Mounting: PCB Mounting Flange (http://www.molex.com/pdm_docs/sd/039291047_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr top entryscrew_flange")
    (property "P/N" "Molex 3929-1067")
    (property "Rating" "600V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (fp_text reference "J10" (at 4.2 -15.1 -90) (layer "F.SilkS"))
    (fp_text value "DC PWR IN" (at 4.2 8.55 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 -13.2 -90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -4.5 -4.2 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 12.9 -4.2 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask) (roundrect_rratio 0.092593)
      (net 14 "PEG+12Vo") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 4.2 0 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 14 "PEG+12Vo") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval locked (at 8.4 0 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 14 "PEG+12Vo") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval locked (at 0 5.5 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval locked (at 4.2 5.5 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J10-Pad5)") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval locked (at 8.4 5.5 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6"))
    (model "${KIPRJMOD}/BoardIO.pretty/39291067.wrl"
      (offset (xyz 4.2 13.8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 10.668 -5.8675 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "P/N" "Yageo RC0603FR-070RL")
    (property "Rating" "0.1W")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R71" (at -0.0255 2.032) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/MP"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 8.509 -91.7195 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "P/N" "Yageo RC0603FR-070RL")
    (property "Rating" "0.1W")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R72" (at -0.0255 1.651 270) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/MP"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BoardIO:LEMO-EPG.00.302.NLN" (layer "F.Cu")
    (tedit 60B81FFE)
    (at 11.746 -61.524 180)
    (descr "Triaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/4241383485754fa8adfc4e1aca22058b/EPG.00.302.NLN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPG.00.302.NLN")
    (property "Rating" "1kV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J2" (at 0 -4.6 180) (layer "F.SilkS"))
    (fp_text value "LVDS OUT" (at 0 4.6 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at -0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 7 "TRIG_P") (pinfunction "In1"))
    (pad "2" thru_hole circle locked (at 0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask)
      (net 8 "TRIG_N") (pinfunction "In2"))
    (pad "3" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPG.00.302.NLN.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "BoardIO:LEMO-EPG.00.302.NLN" (layer "F.Cu")
    (tedit 60B81FFE)
    (at 11.746 -49.024 180)
    (descr "Triaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/4241383485754fa8adfc4e1aca22058b/EPG.00.302.NLN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPG.00.302.NLN")
    (property "Rating" "1kV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J3" (at 0 -4.6 180) (layer "F.SilkS"))
    (fp_text value "LVDS OUT" (at 0 4.6 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at -0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 9 "TIMES_P") (pinfunction "In1"))
    (pad "2" thru_hole circle locked (at 0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask)
      (net 10 "TIMES_N") (pinfunction "In2"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPG.00.302.NLN.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "BoardIO:LEMO-EPL.00.250.NTN" (layer "F.Cu")
    (tedit 60B820E2)
    (at 11.746 -24.024 180)
    (descr "Coaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/c05b81de6963431aa48906be13a46183/EPL.00.250.NTN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPL.00.250.NTN")
    (property "Rating" "4A")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J5" (at 0 -4.7 180) (layer "F.SilkS"))
    (fp_text value "TTL IN" (at 0 4.7 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 3 "USER2_L") (pinfunction "In"))
    (pad "2" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPL.00.250.NTN.wrl"
      (offset (xyz -3.5 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "BoardIO:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm" (layer "F.Cu")
    (tedit 60B0211B)
    (at 102.616 -96.012 180)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP81" (at 1.27 1.905 180) (layer "F.SilkS"))
    (fp_text value "TestPoint_2Pole" (at 1.27 2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.3 -2 180) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 14 "PEG+12Vo") (pinfunction "1"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2"))
  )
  (footprint "BoardIO:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm" (layer "F.Cu")
    (tedit 60B0211B)
    (at 91.44 -94.107 180)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP82" (at 1.3 -2 180) (layer "F.SilkS"))
    (fp_text value "TestPoint_2Pole" (at 1.27 2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.3 -2 180) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "1"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2"))
  )
  (footprint "BoardIO:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm" (layer "F.Cu")
    (tedit 60B0211B)
    (at 68.834 -74.676 -90)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP5" (at 1.3 -2 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint_2Pole" (at 1.27 2 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.3 -2 -90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "USER2_L") (pinfunction "1"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2"))
  )
  (footprint "BoardIO:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm" (layer "F.Cu")
    (tedit 60B0211B)
    (at 68.834 -64.282 -90)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP6" (at 1.3 -2 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint_2Pole" (at 1.27 2 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.3 -2 -90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 "USER3_L") (pinfunction "1"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2"))
  )
  (footprint "BoardIO:PCIbracket" (layer "F.Cu")
    (tedit 60B79EBA)
    (at 0 0)
    (descr "http://www.bracket.com/downloads/brackets/pdf/94560000A.pdf")
    (property "P/N" "Gompf 9456-0000A ; McMaster-Carr 92095A181 90576A102")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (fp_text reference "H1" (at 4.4196 -5.2832) (layer "F.SilkS"))
    (fp_text value "PCIeBracket_Pads" (at 6.2992 -7.2136) (layer "F.Fab"))
    (pad "MP" thru_hole circle locked (at 8.4836 -85.3948) (size 6.4 6.4) (drill oval 3.8 3.2) (layers *.Cu *.Mask)
      (net 13 "/MP") (pinfunction "MP"))
    (pad "MP" thru_hole circle locked (at 8.4836 0) (size 6.4 6.4) (drill oval 3.8 3.2) (layers *.Cu *.Mask)
      (net 13 "/MP") (pinfunction "MP"))
    (model "${KIPRJMOD}/BoardIO.pretty/Gompf-9456-0000A.step" hide
      (offset (xyz 0 46.35 3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/M3-Nut.wrl"
      (offset (xyz 8.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/M3x8-Screw.wrl"
      (offset (xyz 8.5 0 -2.75))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/M3-Nut.wrl"
      (offset (xyz 8.5 85.3948 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/M3x8-Screw.wrl"
      (offset (xyz 8.5 85.3948 -2.75))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/Gompf-9456-0000A.wrl"
      (offset (xyz 0 46.35 3))
      (scale (xyz 394 394 394))
      (rotate (xyz 0 90 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_4x5.4" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 90.954 -97.917)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
    (tags "capacitor electrolytic")
    (property "P/N" "Nichicon UWT1C100MCL1GB")
    (property "Rating" "16V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 3.324 2.286 270) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.8 0) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 2 "+12V"))
    (pad "2" smd roundrect locked (at 1.8 0) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BoardIO:LEMO-EPG.00.302.NLN" (layer "F.Cu")
    (tedit 60B81FFE)
    (at 11.746 -36.524 180)
    (descr "Triaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/4241383485754fa8adfc4e1aca22058b/EPG.00.302.NLN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPG.00.302.NLN")
    (property "Rating" "1kV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J4" (at 0 -4.6 180) (layer "F.SilkS"))
    (fp_text value "LVDS IN" (at 0 4.6 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at -0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 11 "USER1_P") (pinfunction "In1"))
    (pad "2" thru_hole circle locked (at 0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask)
      (net 12 "USER1_N") (pinfunction "In2"))
    (pad "3" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPG.00.302.NLN.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "BoardIO:LEMO-EPG.00.302.NLN" (layer "F.Cu")
    (tedit 60B81FFE)
    (at 11.746 -74.024 180)
    (descr "Triaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/4241383485754fa8adfc4e1aca22058b/EPG.00.302.NLN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPG.00.302.NLN")
    (property "Rating" "1kV")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J1" (at 0 -4.6 180) (layer "F.SilkS"))
    (fp_text value "LVDS OUT" (at 0 4.6 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at -0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 5 "CLK_P") (pinfunction "In1"))
    (pad "2" thru_hole circle locked (at 0.6 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Paste *.Mask)
      (net 6 "CLK_N") (pinfunction "In2"))
    (pad "3" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPG.00.302.NLN.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_8x10" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 99.874 -77.597 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm")
    (tags "capacitor electrolytic")
    (property "P/N" "Nichicon UWT1C471MNL1GS")
    (property "Rating" "16V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -5.155 -4.064) (layer "F.SilkS"))
    (fp_text value "470u" (at -0.202 -2.032) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -3.25 0 180) (size 3.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 14 "PEG+12Vo"))
    (pad "2" smd roundrect locked (at 3.25 0 180) (size 3.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal" (layer "F.Cu")
    (tedit 5B0886BD)
    (at 82.224 -84.851)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (property "P/N" "CUI PJ-063AH")
    (property "Rating" "24V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr through_hole)
    (fp_text reference "J12" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "DC jack" (at 0 13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 9) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 14 "PEG+12Vo"))
    (pad "2" thru_hole oval locked (at 0 6) (size 3.3 2) (drill oval 2.3 1) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "MP" thru_hole oval locked (at -4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MountPin"))
    (pad "MP" thru_hole oval locked (at 4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MountPin"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BoardIO:Molex_878331031_2x05_P2.00mm_Horizontal" (layer "F.Cu")
    (tedit 60B7A636)
    (at 56.896 -92.202 90)
    (descr "Through hole angled Molex connector, 2x05, 2.00mm pitch, 4.2mm pin length, double rows")
    (tags "Through hole angled Molex connector THT 2x05 2.00mm double row")
    (property "P/N" "Molex 87833-1031")
    (property "Rating" "125V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (clearance 0.2)
    (fp_text reference "J11" (at 6.096 -3.302 90) (layer "F.SilkS"))
    (fp_text value "MultiSync" (at 4.1 10 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.25 4) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "CLK_P") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval locked (at 2 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "CLK_N") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval locked (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "TRIG_P") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval locked (at 2 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "TRIG_N") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval locked (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "TIMES_P") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval locked (at 2 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "TIMES_N") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval locked (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "USER1_P") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval locked (at 2 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "USER1_N") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval locked (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "USER2_L") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval locked (at 2 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "USER3_L") (pinfunction "Pin_10"))
    (model "${KIPRJMOD}/BoardIO.pretty/878331031.wrl"
      (offset (xyz 5.25 -4 3.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "BoardIO:LEMO-EPL.00.250.NTN" (layer "F.Cu")
    (tedit 60B820E2)
    (at 11.746 -11.524 180)
    (descr "Coaxial LEMO connector PCB elbow socket https://web.lemo.com/PARTSEARCH_WEB/V1.00Fw/PDF/c05b81de6963431aa48906be13a46183/EPL.00.250.NTN.pdf")
    (tags "LEMO THT Female Jack Horizontal")
    (property "P/N" "LEMO EPL.00.250.NTN")
    (property "Rating" "4A")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J6" (at -0.192 -4.412 180) (layer "F.SilkS"))
    (fp_text value "TTL IN" (at 0 4.7 180) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask) (roundrect_rratio 0.25)
      (net 4 "USER3_L") (pinfunction "In"))
    (pad "2" thru_hole circle locked (at 2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at 2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at -2.54 2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (pad "2" thru_hole circle locked (at -2.54 -2.54 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Paste *.Mask)
      (net 1 "GND") (pinfunction "Ext"))
    (model "${KIPRJMOD}/BoardIO.pretty/EPL.00.250.NTN.wrl"
      (offset (xyz -3.5 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "BoardIO:SIS1160" locked (layer "F.Cu")
    (tedit 5F8D98B5)
    (at 2.073 5)
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "exclude_from_bom" "")
    (attr exclude_from_bom)
    (fp_text reference "FID1" (at 11.6332 -0.8128) (layer "F.SilkS") hide)
    (fp_text value "BoardOutline" (at 3.302 -0.8128) (layer "F.Fab") hide)
  )
  (footprint "Symbol:WEEE-Logo_4.2x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 65.786 -49.784)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "FID3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo Trash" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "Symbol:KiCad-Logo2_5mm_Copper" (layer "F.Cu")
    (tedit 0)
    (at 48.26 -50.038)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "FID2" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "Logo KiCAD" (at 0 5.08) (layer "F.Fab") hide)
  )
  (footprint "Symbol:OSHW-Logo2_7.3x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 29.972 -49.53)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "FID4" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Licensed under CERN-OHL-W v2 or later" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "BoardIO:L_Bourns-SRU1028_10.0x10.0mm" (layer "B.Cu")
    (tedit 60B7A4CB)
    (at 91.313 -85.543 90)
    (descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
    (tags "Bourns SRU1028 SMD inductor")
    (property "P/N" "Bourns SRU1028-820Y")
    (property "Rating" "0.9A")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Primitive" "L")
    (attr smd)
    (fp_text reference "FB1" (at -4.009 4.953 270) (layer "B.SilkS"))
    (fp_text value "82u" (at 0 -6.2 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.5 0 90) (size 1.8 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/12Vs"))
    (pad "2" smd rect locked (at 4.5 0 90) (size 1.8 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "+12V"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRU1028_10.0x10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/BoardIO.pretty/SRU1028.wrl"
      (offset (xyz 0 0 0.15))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 98.536 -80.198)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "P/N" "Infineon IRLML5203TRPBF")
    (property "Rating" "30V")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "models/irlml5203.lib")
    (property "Spice_Model" "irlml5203")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "3 1 2")
    (property "Spice_Primitive" "X")
    (attr smd)
    (fp_text reference "Q1" (at 1.794 1.331) (layer "B.SilkS"))
    (fp_text value "IRLML5203" (at 0 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/12Vg") (pinfunction "G"))
    (pad "2" smd roundrect locked (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/12Vs") (pinfunction "S"))
    (pad "3" smd roundrect locked (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "PEG+12Vo") (pinfunction "D"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 98.298 -77.597)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "P/N" "Yageo RT0603FRE07100KL")
    (property "Rating" "0.1W")
    (property "Sheetfile" "BoardIO.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R73" (at -1.143 1.397) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/12Vg"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 119.38 -101.6) (end 0.127 -101.6) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 -89.535) (end 1.143 -89.535) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 1.143 -89.535) (end 1.143 -81.28) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 1.143 -81.28) (end 0.127 -81.28) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 -81.28) (end 0.127 -4.191) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 4.191) (end 0.127 4.953) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 1.143 4.191) (end 0.127 4.191) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 1.143 -4.191) (end 1.143 4.191) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 -4.191) (end 1.143 -4.191) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 20.32 -40.64) (end 25.4 -45.72) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 25.4 -45.72) (end 68.58 -45.72) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 68.58 -45.72) (end 76.2 -53.34) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 119.38 -74.93) (end 119.38 -101.6) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 116.84 -72.39) (end 119.38 -74.93) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 20.32 -3.429) (end 20.32 -40.64) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 13.843 4.953) (end 13.843 -3.429) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 13.843 -3.429) (end 20.32 -3.429) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 116.84 -72.39) (end 76.2 -72.39) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 -101.6) (end 0.127 -89.535) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 0.127 4.953) (end 13.843 4.953) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 76.2 -72.39) (end 76.2 -53.34) (layer "Edge.Cuts") (width 0.05))
  (gr_text "12V" (at 93.472 -93.218 90) (layer "F.SilkS"))
  (gr_text "USER3_L" (at 72.39 -65.806) (layer "F.SilkS"))
  (gr_text "USER2_L" (at 72.39 -76.2) (layer "F.SilkS"))
  (gr_text "+12Vo" (at 103.886 -98.806 90) (layer "F.SilkS"))
  (gr_text "SIS1160 PCI-L IO add on\nRev. 0\nIFIC (CSIC/UV) - IRIS\nCPGM - CDEIGENT/2019/011\nLicensed under CERN-OHL-W v2 or later\nhttps://ohwr.org/project/sis1160-pci-io" (at 31.623 -93.98) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.35319 -3.556)
        (xy 1.524 -3.556)
        (xy 1.524 -101.346)
        (xy 166.35319 -101.346)
      )
    )
  )
)
