(kicad_pcb (version 20210623) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "ADC12_IN14")
  (net 3 "+3V3")
  (net 4 "ADC2_IN15")
  (net 5 "ADC3_IN5")
  (net 6 "unconnected-(IC2-Pad19)")
  (net 7 "unconnected-(IC2-Pad18)")
  (net 8 "~{RESET}")
  (net 9 "Net-(C27-Pad1)")
  (net 10 "Net-(C28-Pad1)")
  (net 11 "unconnected-(IC2-Pad22)")
  (net 12 "PA15_IN_DFM")
  (net 13 "PC15_IN_PICKUP")
  (net 14 "PC13_OUT_BTS723_MV")
  (net 15 "PC14_OUT_BTS723_ALARM")
  (net 16 "ADC12_IN1")
  (net 17 "unconnected-(IC2-Pad40)")
  (net 18 "ADC12_IN2")
  (net 19 "USART2_TX")
  (net 20 "USART2_RX")
  (net 21 "SPI1_~{SS}")
  (net 22 "SPI1_SCK")
  (net 23 "SPI1_MISO")
  (net 24 "TIM1_CH1N")
  (net 25 "PB0_OUT_SM_STEP")
  (net 26 "TIM8_CH3N")
  (net 27 "ADC1_IN11")
  (net 28 "ADC1_IN5")
  (net 29 "TIM1_CH1")
  (net 30 "USART1_TX")
  (net 31 "USART1_RX")
  (net 32 "CAN1_RX")
  (net 33 "CAN1_TX")
  (net 34 "SWDIO")
  (net 35 "SWDCLK")
  (net 36 "SPI1_MOSI")
  (net 37 "CAN2_RX")
  (net 38 "CAN2_TX")
  (net 39 "PB7_OUT_SM_~{ENABLE}")
  (net 40 "PB8_OUT__LED")
  (net 41 "TIM8_CH3")
  (net 42 "Net-(IC2-Pad20)")
  (footprint "0IBF_Crystal:Crystal_SMD_5032-2Pin_5.0x3.2mm_IBF" (layer "F.Cu")
    (tedit 60FD5043)
    (at 106.07 -86.88 90)
    (descr "SMD Crystal 5x3,2mm Quantek QC5CB / Interquip SMAC-5032 angepaßte Pads IBFEEW")
    (tags "SMD crystal")
    (property "Alternative" "Abracom ABM3-10.000MHZ-D2Y-T")
    (property "Bemerkung" "")
    (property "Farnell" "2508597")
    (property "MF" "Quantek")
    (property "MPN" "QC5CB10.0000F18B23M / QC5CB10.0000F18B23R")
    (property "RS" "813-6097")
    (property "Sheetfile" "controller.kicad_sch")
    (property "Sheetname" "Controller")
    (property "digikey" "")
    (property "mouser" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.8 90) (layer "F.SilkS"))
    (fp_text value "QC5CB10.000" (at 0 2.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.82 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0 90) (size 2.2 2.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C28-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0 90) (size 2.2 2.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C27-Pad1)") (pintype "passive"))
    (model "${KICAD6_USER_LIBRARY_3D}/discrete/Crystal_SMD_5032_2pin_5x3mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "0IBF_RCL:C_1206_3216Metric" (layer "F.Cu")
    (tedit 60FD2F22)
    (at 104.47 -82.38 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Alternative" "")
    (property "Bemerkung" "")
    (property "Farnell" "")
    (property "MF" "")
    (property "MPN" "")
    (property "RS" "")
    (property "Sheetfile" "controller.kicad_sch")
    (property "Sheetname" "Controller")
    (property "digikey" "")
    (property "mouser" "")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 8 "~{RESET}") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:LQFP-48_7x7mm_P0.5mm" (layer "F.Cu")
    (tedit 5D9F72AF)
    (at 115.6 -85.1)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Alternative" "")
    (property "Bemerkung" "")
    (property "Farnell" "3648858")
    (property "MF" "ST")
    (property "MPN" "STM32G491CET6")
    (property "RS" "215-0839 / 215-0838")
    (property "Sheetfile" "controller.kicad_sch")
    (property "Sheetname" "Controller")
    (property "digikey" "497-STM32G491CET6-ND")
    (property "mouser" "511-STM32G491CET6")
    (attr smd)
    (fp_text reference "IC2" (at 0 -5.85) (layer "F.SilkS"))
    (fp_text value "STM32G491CET6" (at 0 5.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "Vbat") (pintype "input"))
    (pad "2" smd roundrect locked (at -4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "PC13_OUT_BTS723_MV") (pinfunction "PC13") (pintype "passive"))
    (pad "3" smd roundrect locked (at -4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "PC14_OUT_BTS723_ALARM") (pinfunction "PC14_OSC32") (pintype "passive"))
    (pad "4" smd roundrect locked (at -4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "PC15_IN_PICKUP") (pinfunction "PC15_OSC32") (pintype "passive"))
    (pad "5" smd roundrect locked (at -4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C27-Pad1)") (pinfunction "PF0_OSC") (pintype "passive"))
    (pad "6" smd roundrect locked (at -4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C28-Pad1)") (pinfunction "PF1_OSC") (pintype "passive"))
    (pad "7" smd roundrect locked (at -4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "~{RESET}") (pinfunction "PG10_~{RES}") (pintype "passive"))
    (pad "8" smd roundrect locked (at -4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "ADC12_IN1") (pinfunction "PA0") (pintype "passive"))
    (pad "9" smd roundrect locked (at -4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "ADC12_IN2") (pinfunction "PA1") (pintype "passive"))
    (pad "10" smd roundrect locked (at -4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "USART2_TX") (pinfunction "PA2") (pintype "passive"))
    (pad "11" smd roundrect locked (at -4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "USART2_RX") (pinfunction "PA3") (pintype "passive"))
    (pad "12" smd roundrect locked (at -4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "SPI1_~{SS}") (pinfunction "PA4") (pintype "passive"))
    (pad "13" smd roundrect locked (at -2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "SPI1_SCK") (pinfunction "PA5") (pintype "passive"))
    (pad "14" smd roundrect locked (at -2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "SPI1_MISO") (pinfunction "PA6") (pintype "passive"))
    (pad "15" smd roundrect locked (at -1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "TIM1_CH1N") (pinfunction "PA7") (pintype "passive"))
    (pad "16" smd roundrect locked (at -1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "PB0_OUT_SM_STEP") (pinfunction "PB0") (pintype "passive"))
    (pad "17" smd roundrect locked (at -0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "TIM8_CH3N") (pinfunction "PB1") (pintype "passive"))
    (pad "18" smd roundrect locked (at -0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(IC2-Pad18)") (pinfunction "PB2") (pintype "passive"))
    (pad "19" smd roundrect locked (at 0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "unconnected-(IC2-Pad19)") (pinfunction "VSSA") (pintype "input"))
    (pad "20" smd roundrect locked (at 0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(IC2-Pad20)") (pinfunction "VRef+") (pintype "input"))
    (pad "21" smd roundrect locked (at 1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(IC2-Pad20)") (pinfunction "Vdda") (pintype "input"))
    (pad "22" smd roundrect locked (at 1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "unconnected-(IC2-Pad22)") (pinfunction "PB10") (pintype "passive"))
    (pad "23" smd roundrect locked (at 2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS/GND") (pintype "input"))
    (pad "24" smd roundrect locked (at 2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "Vdd") (pintype "input"))
    (pad "25" smd roundrect locked (at 4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "ADC12_IN14") (pinfunction "PB11") (pintype "passive"))
    (pad "26" smd roundrect locked (at 4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "ADC1_IN11") (pinfunction "PB12") (pintype "passive"))
    (pad "27" smd roundrect locked (at 4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "ADC3_IN5") (pinfunction "PB13") (pintype "passive"))
    (pad "28" smd roundrect locked (at 4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "ADC1_IN5") (pinfunction "PB14") (pintype "passive"))
    (pad "29" smd roundrect locked (at 4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "ADC2_IN15") (pinfunction "PB15") (pintype "passive"))
    (pad "30" smd roundrect locked (at 4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "TIM1_CH1") (pinfunction "PA8") (pintype "passive"))
    (pad "31" smd roundrect locked (at 4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "USART1_TX") (pinfunction "PA9") (pintype "passive"))
    (pad "32" smd roundrect locked (at 4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "USART1_RX") (pinfunction "PA10") (pintype "passive"))
    (pad "33" smd roundrect locked (at 4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "CAN1_RX") (pinfunction "PA11") (pintype "passive"))
    (pad "34" smd roundrect locked (at 4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "CAN1_TX") (pinfunction "PA12") (pintype "passive"))
    (pad "35" smd roundrect locked (at 4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS/GND") (pintype "input"))
    (pad "36" smd roundrect locked (at 4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "Vdd") (pintype "input"))
    (pad "37" smd roundrect locked (at 2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "SWDIO") (pinfunction "SWDIO_PA13") (pintype "passive"))
    (pad "38" smd roundrect locked (at 2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "SWDCLK") (pinfunction "SWDCLK_PA14") (pintype "passive"))
    (pad "39" smd roundrect locked (at 1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "PA15_IN_DFM") (pinfunction "PA15") (pintype "passive"))
    (pad "40" smd roundrect locked (at 1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(IC2-Pad40)") (pinfunction "SWO_PB3") (pintype "passive"))
    (pad "41" smd roundrect locked (at 0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "SPI1_MOSI") (pinfunction "PB4") (pintype "passive"))
    (pad "42" smd roundrect locked (at 0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "CAN2_RX") (pinfunction "PB5") (pintype "passive"))
    (pad "43" smd roundrect locked (at -0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "CAN2_TX") (pinfunction "PB6") (pintype "passive"))
    (pad "44" smd roundrect locked (at -0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "PB7_OUT_SM_~{ENABLE}") (pinfunction "PB7") (pintype "passive"))
    (pad "45" smd roundrect locked (at -1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "PB8_OUT__LED") (pinfunction "Boot0_PB8") (pintype "passive"))
    (pad "46" smd roundrect locked (at -1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "TIM8_CH3") (pinfunction "PB9") (pintype "passive"))
    (pad "47" smd roundrect locked (at -2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS/GND") (pintype "input"))
    (pad "48" smd roundrect locked (at -2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "Vdd") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0IBF_RCL:C_1206_3216Metric" (layer "F.Cu")
    (tedit 60FD2F22)
    (at 101.67 -88.88 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Alternative" "")
    (property "Bemerkung" "")
    (property "Farnell" "")
    (property "MF" "")
    (property "MPN" "")
    (property "RS" "")
    (property "Sheetfile" "controller.kicad_sch")
    (property "Sheetname" "Controller")
    (property "digikey" "")
    (property "mouser" "")
    (attr smd)
    (fp_text reference "C27" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "18pF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 9 "Net-(C27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0IBF_RCL:C_1206_3216Metric" (layer "F.Cu")
    (tedit 60FD2F22)
    (at 101.67 -86.38 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Alternative" "")
    (property "Bemerkung" "")
    (property "Farnell" "")
    (property "MF" "")
    (property "MPN" "")
    (property "RS" "")
    (property "Sheetfile" "controller.kicad_sch")
    (property "Sheetname" "Controller")
    (property "digikey" "")
    (property "mouser" "")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "18pF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 10 "Net-(C28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_poly
    (pts
      (xy 0 0)
      (xy 0 -100)
      (xy 150.7 -100)
      (xy 150.7 0)
    ) (layer "Edge.Cuts") (width 0.1) (fill none))
)
