(kicad_pcb (version 20210807) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power "L2 Ground")
    (2 "In2.Cu" power "L3 PWR")
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 247.803999 54.9455)
    (pcbplotparams
      (layerselection 0x00010f8_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "LVHV_20191026/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C203-Pad1)")
  (net 3 "Net-(C205-Pad2)")
  (net 4 "Net-(C205-Pad1)")
  (net 5 "+5V")
  (net 6 "Net-(C301-Pad1)")
  (net 7 "Net-(C406-Pad2)")
  (net 8 "Net-(C406-Pad1)")
  (net 9 "Net-(C407-Pad2)")
  (net 10 "Net-(C407-Pad1)")
  (net 11 "Net-(C408-Pad2)")
  (net 12 "Net-(C408-Pad1)")
  (net 13 "Net-(C204-Pad2)")
  (net 14 "Net-(C209-Pad1)")
  (net 15 "Net-(C210-Pad1)")
  (net 16 "+3V3I")
  (net 17 "Net-(C417-Pad2)")
  (net 18 "Net-(C401-Pad1)")
  (net 19 "Net-(C402-Pad1)")
  (net 20 "Net-(C423-Pad1)")
  (net 21 "+3V8")
  (net 22 "/LowVoltage/3V0")
  (net 23 "Net-(C426-Pad1)")
  (net 24 "+3V3")
  (net 25 "Net-(C501-Pad1)")
  (net 26 "/LowVoltage/2V6")
  (net 27 "Net-(C507-Pad1)")
  (net 28 "Net-(C508-Pad1)")
  (net 29 "Net-(D201-Pad2)")
  (net 30 "Net-(D201-Pad1)")
  (net 31 "/LowVoltage/3V8_OUT")
  (net 32 "Net-(D501-Pad2)")
  (net 33 "/LowVoltage/3V0_OUT")
  (net 34 "Net-(C424-Pad2)")
  (net 35 "Net-(C427-Pad1)")
  (net 36 "Net-(C428-Pad1)")
  (net 37 "/MCU/PGC")
  (net 38 "/MCU/PGD")
  (net 39 "Net-(J501-Pad1)")
  (net 40 "/LowVoltage/1V8_OUT")
  (net 41 "/HighVoltage/HV_Ctrl")
  (net 42 "Net-(D303-Pad1)")
  (net 43 "Net-(J504-Pad2)")
  (net 44 "Net-(J504-Pad1)")
  (net 45 "Net-(J601-Pad1)")
  (net 46 "Net-(J601-Pad2)")
  (net 47 "Net-(J601-Pad3)")
  (net 48 "Net-(J601-Pad4)")
  (net 49 "Net-(J601-Pad5)")
  (net 50 "Net-(J601-Pad6)")
  (net 51 "Net-(J601-Pad7)")
  (net 52 "Net-(J601-Pad8)")
  (net 53 "Net-(C603-Pad1)")
  (net 54 "Net-(C603-Pad2)")
  (net 55 "Net-(C604-Pad1)")
  (net 56 "Net-(C604-Pad2)")
  (net 57 "Net-(C701-Pad1)")
  (net 58 "Net-(C801-Pad1)")
  (net 59 "Net-(C605-Pad1)")
  (net 60 "Net-(C605-Pad2)")
  (net 61 "Net-(C901-Pad1)")
  (net 62 "Net-(C1001-Pad1)")
  (net 63 "Net-(C1101-Pad1)")
  (net 64 "Net-(C1201-Pad1)")
  (net 65 "/LVDSConnections/BiasNet3/in_p")
  (net 66 "/LVDSConnections/BiasNet3/in_n")
  (net 67 "Net-(C606-Pad1)")
  (net 68 "Net-(C606-Pad2)")
  (net 69 "Net-(J604-Pad1)")
  (net 70 "Net-(J604-Pad2)")
  (net 71 "Net-(J604-Pad3)")
  (net 72 "Net-(J604-Pad4)")
  (net 73 "Net-(J604-Pad5)")
  (net 74 "Net-(J604-Pad6)")
  (net 75 "Net-(J604-Pad7)")
  (net 76 "Net-(J604-Pad8)")
  (net 77 "Net-(R203-Pad1)")
  (net 78 "/PowerInput/5V_Feedback")
  (net 79 "Net-(R301-Pad2)")
  (net 80 "Net-(D303-Pad2)")
  (net 81 "Net-(D304-Pad1)")
  (net 82 "Net-(D304-Pad2)")
  (net 83 "Net-(D305-Pad2)")
  (net 84 "Net-(R412-Pad1)")
  (net 85 "Net-(D306-Pad1)")
  (net 86 "Net-(D307-Pad2)")
  (net 87 "Net-(D308-Pad1)")
  (net 88 "/MCU/SCL")
  (net 89 "/MCU/SDA")
  (net 90 "+12V")
  (net 91 "Net-(D309-Pad2)")
  (net 92 "Net-(D310-Pad1)")
  (net 93 "Net-(C510-Pad1)")
  (net 94 "/PowerInput/VIN")
  (net 95 "/Alarm2")
  (net 96 "/Alarm1")
  (net 97 "Net-(C511-Pad1)")
  (net 98 "/MCU/CAN_L")
  (net 99 "/MCU/CAN_H")
  (net 100 "/Sine")
  (net 101 "Net-(D311-Pad2)")
  (net 102 "Net-(D312-Pad1)")
  (net 103 "Net-(D314-Pad1)")
  (net 104 "unconnected-(J501-Pad6)")
  (net 105 "Net-(J502-Pad2)")
  (net 106 "/HighVoltage/SW1")
  (net 107 "Net-(Q203-Pad9)")
  (net 108 "Net-(R515-Pad2)")
  (net 109 "Net-(Q301-Pad1)")
  (net 110 "/MCU/CAN_RX")
  (net 111 "/MCU/CAN_TX")
  (net 112 "Net-(R202-Pad2)")
  (net 113 "Net-(R206-Pad2)")
  (net 114 "Net-(R208-Pad2)")
  (net 115 "Net-(R210-Pad1)")
  (net 116 "/HighVoltage/HV_ON_OFF")
  (net 117 "/LowVoltage/3V8_Feedback")
  (net 118 "/LowVoltage/3V0_Feedback")
  (net 119 "/LowVoltage/2V6_Feedback")
  (net 120 "/LowVoltage/LV_EN")
  (net 121 "Net-(R415-Pad1)")
  (net 122 "unconnected-(U202-Pad7)")
  (net 123 "/HighVoltage/HV_MON")
  (net 124 "unconnected-(U501-Pad17)")
  (net 125 "unconnected-(U501-Pad18)")
  (net 126 "unconnected-(U501-Pad24)")
  (net 127 "unconnected-(U501-Pad25)")
  (net 128 "unconnected-(U503-Pad6)")
  (net 129 "unconnected-(U504-Pad5)")
  (net 130 "unconnected-(U504-Pad6)")
  (net 131 "unconnected-(U504-Pad7)")
  (net 132 "unconnected-(U601-Pad13)")
  (net 133 "unconnected-(U602-Pad13)")
  (net 134 "Net-(R505-Pad1)")
  (net 135 "unconnected-(U502-Pad1)")
  (net 136 "unconnected-(U502-Pad5)")
  (net 137 "unconnected-(U502-Pad8)")
  (net 138 "Net-(J502-Pad3)")
  (net 139 "/PowerInput/VIN_FUSED")
  (net 140 "Net-(Q203-Pad5)")
  (net 141 "Net-(C513-Pad1)")
  (net 142 "Net-(C513-Pad2)")
  (net 143 "-5V")
  (net 144 "unconnected-(U506-Pad5)")
  (net 145 "/LVDSConnections/BiasNet4/in_p")
  (net 146 "/LVDSConnections/BiasNet5/in_p")
  (net 147 "/LVDSConnections/BiasNet5/in_n")
  (net 148 "/LVDSConnections/BiasNet4/in_n")
  (net 149 "/LVDSConnections/BiasNet/in_p")
  (net 150 "/LVDSConnections/BiasNet/in_n")
  (net 151 "/LVDSConnections/BiasNet1/in_p")
  (net 152 "/LVDSConnections/BiasNet2/in_p")
  (net 153 "/LVDSConnections/BiasNet2/in_n")
  (net 154 "/LVDSConnections/BiasNet1/in_n")
  (net 155 "Net-(R505-Pad2)")
  (footprint "Capacitor_SMD:CP_Elec_6.3x5.9" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 161.508999 53.2455 90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C6, 6.3x5.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "PCE4012CT-ND")
    (property "mpn" "EEE-FC1H100P")
    (attr smd)
    (fp_text reference "C201" (at -5.842 -1.27 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.8 0 90) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.8 0 90) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D16.0mm_W5.0mm_P10.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 264.977 54.176999 90)
    (descr "C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=16.0*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 10.00mm  diameter 16.0mm width 5.0mm Capacitor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "1269PH-ND")
    (property "mpn" "S202M75Z5UU83L0R")
    (attr through_hole)
    (fp_text reference "C301" (at 5 -3.75 90) (layer "F.SilkS"))
    (fp_text value "2nF" (at 5 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D16.0mm_W5.0mm_P10.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 63.941165 57.6535 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C403" (at 0.037 1.5495 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 92.741165 57.557999 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C404" (at 0.037 1.5495 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 115.748165 62.572699 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C405" (at 0.037 1.5495) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 59.562165 54.504001)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C406" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C406-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C406-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 87.511 56.468 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C407" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C407-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C407-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 112.598665 66.951699 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C408" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C408-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C408-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 65.799665 62.4955)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C409" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 21 "+3V8") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 124.409665 67.627199 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C411" (at 3.302 -0.0635 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 26 "/LowVoltage/2V6") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 56.799665 62.4955 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C412" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 21 "+3V8") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 124.409665 62.801199 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C414" (at 3.048 0.0635 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 90) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 26 "/LowVoltage/2V6") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 90) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 135.204665 71.437199 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C417" (at -3.556 0) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C417-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 129.743665 61.166199 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C423" (at 3.3655 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C423-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 132.690165 62.674199)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C426" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C426-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 127.349665 74.2455 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C429" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/LowVoltage/1V8_OUT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 168.758999 44.9955)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "507-1191-1-ND")
    (property "mpn" "C1S 3")
    (attr smd)
    (fp_text reference "F201" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 139 "/PowerInput/VIN_FUSED") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 94 "/PowerInput/VIN") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 174.175293 44.9125 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "A98342-ND")
    (property "mpn" "282841-2")
    (attr through_hole)
    (fp_text reference "J201" (at -4.8715 5.529707 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2.54 11.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 94 "/PowerInput/VIN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole" (layer "F.Cu")
    (tedit 5B785047)
    (at 53.559665 79.397784)
    (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)")
    (tags "phoenix_contact connector MSTB_01x02_GF_5.08mm_MH")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "277-6269-ND")
    (property "mpn" "1776692")
    (attr through_hole)
    (fp_text reference "J401" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.08 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 10.16 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 31 "/LowVoltage/3V8_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole" (layer "F.Cu")
    (tedit 5B785047)
    (at 82.851665 79.397784)
    (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)")
    (tags "phoenix_contact connector MSTB_01x02_GF_5.08mm_MH")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "277-6269-ND")
    (property "mpn" "1776692")
    (attr through_hole)
    (fp_text reference "J402" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.08 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 10.16 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 33 "/LowVoltage/3V0_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole" (layer "F.Cu")
    (tedit 5B785047)
    (at 112.225332 79.397784)
    (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)")
    (tags "phoenix_contact connector MSTB_01x02_GF_5.08mm_MH")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "277-6269-ND")
    (property "mpn" "1776692")
    (attr through_hole)
    (fp_text reference "J403" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.08 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 10.16 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 40 "/LowVoltage/1V8_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole" (layer "F.Cu")
    (tedit 5B785047)
    (at 141.598999 79.397784)
    (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)")
    (tags "phoenix_contact connector MSTB_01x02_GF_5.08mm_MH")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "277-6269-ND")
    (property "mpn" "1776692")
    (attr through_hole)
    (fp_text reference "J404" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.08 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 10.16 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 40 "/LowVoltage/1V8_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:RJ45_Wuerth_615008142621_Horizontal" (layer "F.Cu")
    (tedit 5D7C03E7)
    (at 31.759998 69.088 -90)
    (descr "10/100Base-TX RJ45 ethernet connector horizontal https://katalog.we-online.de/em/datasheet/615008142621.pdf")
    (tags "RJ45 ethernet ")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "732-3163-ND")
    (property "mpn" "615008142621")
    (attr through_hole)
    (fp_text reference "J601" (at 0 -4.953 90) (layer "F.SilkS"))
    (fp_text value "RJ45" (at 7 14.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 4 -90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 8.89 -1.27) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 8.89 10.16) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 2.54 8.89) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(J601-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 7.62) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(J601-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 6.35) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(J601-Pad3)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 5.08) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(J601-Pad4)") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.54 3.81) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(J601-Pad5)") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 2.54) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(J601-Pad6)") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 2.54 1.27) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(J601-Pad7)") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(J601-Pad8)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at 5.84 -3.305) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at 5.84 12.195) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/Models/615008142621 (rev1).stp"
      (offset (xyz 9 -4.5 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "LVHV:RJ45_Wuerth_615008142621_Horizontal" (layer "F.Cu")
    (tedit 5D7C03E7)
    (at 48.466961 22.055963)
    (descr "10/100Base-TX RJ45 ethernet connector horizontal https://katalog.we-online.de/em/datasheet/615008142621.pdf")
    (tags "RJ45 ethernet ")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "732-3163-ND")
    (property "mpn" "615008142621")
    (attr through_hole)
    (fp_text reference "J603" (at 1.825039 -5.545963) (layer "F.SilkS"))
    (fp_text value "RJ45" (at 7 14.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 4 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 8.89 -1.27 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 8.89 10.16 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 2.54 8.89 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 149 "/LVDSConnections/BiasNet/in_p") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 7.62 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 150 "/LVDSConnections/BiasNet/in_n") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 6.35 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 151 "/LVDSConnections/BiasNet1/in_p") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 5.08 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 152 "/LVDSConnections/BiasNet2/in_p") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.54 3.81 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 153 "/LVDSConnections/BiasNet2/in_n") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 2.54 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 154 "/LVDSConnections/BiasNet1/in_n") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 2.54 1.27 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(C603-Pad1)") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(C604-Pad1)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at 5.84 -3.305 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at 5.84 12.195 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/Models/615008142621 (rev1).stp"
      (offset (xyz 9 -4.5 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "LVHV:RJ45_Wuerth_615008142621_Horizontal" (layer "F.Cu")
    (tedit 5D7C03E7)
    (at 205.232 69.088 -90)
    (descr "10/100Base-TX RJ45 ethernet connector horizontal https://katalog.we-online.de/em/datasheet/615008142621.pdf")
    (tags "RJ45 ethernet ")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "732-3163-ND")
    (property "mpn" "615008142621")
    (attr through_hole)
    (fp_text reference "J604" (at -3 -4.5 90) (layer "F.SilkS"))
    (fp_text value "RJ45" (at 7 14.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 4 -90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 8.89 -1.27) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 8.89 10.16) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 2.54 8.89) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(J604-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 7.62) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(J604-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 6.35) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 "Net-(J604-Pad3)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 5.08) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 "Net-(J604-Pad4)") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.54 3.81) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Net-(J604-Pad5)") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 2.54) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Net-(J604-Pad6)") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 2.54 1.27) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 "Net-(J604-Pad7)") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 76 "Net-(J604-Pad8)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at 5.84 -3.305) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at 5.84 12.195) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/Models/615008142621 (rev1).stp"
      (offset (xyz 9 -4.5 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "LVHV:L_Pulse_PA4331.332NLT" (layer "F.Cu")
    (tedit 5D7C111D)
    (at 61.299665 61.355 -90)
    (descr "Choke,Pulse Electronics, SMD,")
    (tags "Choke Pulse Electronics SMD ")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "553-3284-1-ND")
    (property "mpn" "PA4331.332NLT")
    (attr smd)
    (fp_text reference "L401" (at 0 -2.7915 90) (layer "F.SilkS"))
    (fp_text value "3u3H" (at 0 5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C406-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V8") (pinfunction "2") (pintype "passive"))
  )
  (footprint "LVHV:L_Pulse_PA4331.332NLT" (layer "F.Cu")
    (tedit 5D7C111D)
    (at 90.099665 61.259501 -90)
    (descr "Choke,Pulse Electronics, SMD,")
    (tags "Choke Pulse Electronics SMD ")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "553-3284-1-ND")
    (property "mpn" "PA4331.332NLT")
    (attr smd)
    (fp_text reference "L402" (at 0 -2.7915 90) (layer "F.SilkS"))
    (fp_text value "3u3H" (at 0 5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C407-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LowVoltage/3V0") (pinfunction "2") (pintype "passive"))
  )
  (footprint "LVHV:L_Pulse_PA4331.332NLT" (layer "F.Cu")
    (tedit 5D7C111D)
    (at 119.449665 65.214199)
    (descr "Choke,Pulse Electronics, SMD,")
    (tags "Choke Pulse Electronics SMD ")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "553-3284-1-ND")
    (property "mpn" "PA4331.332NLT")
    (attr smd)
    (fp_text reference "L403" (at 0 -2.7915) (layer "F.SilkS"))
    (fp_text value "3u3H" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.15 0) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C408-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.15 0) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/LowVoltage/2V6") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 258.152 54.2555 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A129859CT-ND")
    (property "mpn" "CRGCQ1210F100R")
    (attr smd)
    (fp_text reference "R301" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 79 "Net-(R301-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 269.494 75.7555 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "RHM1090CT-ND")
    (property "mpn" "KTR25JZPF2004")
    (attr smd)
    (fp_text reference "R302" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "2M" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 91 "Net-(D309-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 255.143 75.7555 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "RHM1041CT-ND")
    (property "mpn" "KTR25JZPF1005")
    (attr smd)
    (fp_text reference "R303" (at -2.794 2.54) (layer "F.SilkS"))
    (fp_text value "10M" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 91 "Net-(D309-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 92 "Net-(D310-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 240.919 75.7555 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "RHM1090CT-ND")
    (property "mpn" "KTR25JZPF2004")
    (attr smd)
    (fp_text reference "R304" (at -2.794 2.54) (layer "F.SilkS"))
    (fp_text value "2M" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 92 "Net-(D310-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 101 "Net-(D311-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 226.19 75.819 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "RHM1041CT-ND")
    (property "mpn" "KTR25JZPF1005")
    (attr smd)
    (fp_text reference "R305" (at -2.794 2.54) (layer "F.SilkS"))
    (fp_text value "10M" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 101 "Net-(D311-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 102 "Net-(D312-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 214.122 63.7555 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "RHM1090CT-ND")
    (property "mpn" "KTR25JZPF2004")
    (attr smd)
    (fp_text reference "R306" (at -2.794 2.54) (layer "F.SilkS"))
    (fp_text value "2M" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 102 "Net-(D312-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 57.262165 58.7455 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A109969CT-ND")
    (property "mpn" "RP73PF1J35R7BTDF")
    (attr smd)
    (fp_text reference "R401" (at 0.762 2.54 45) (layer "F.SilkS"))
    (fp_text value "39k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V8") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "/LowVoltage/3V8_Feedback") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 56.512165 56.4955 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R402" (at 0.762 2.54 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "/LowVoltage/3V8_Feedback") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 86.114 60.024 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A102246CT-ND")
    (property "mpn" "CPF0603F25K5C1")
    (attr smd)
    (fp_text reference "R403" (at 0.762 2.3495 135) (layer "F.SilkS"))
    (fp_text value "29k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LowVoltage/3V0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/LowVoltage/3V0_Feedback") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 82.685 60.024 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R404" (at 0.889 2.3495 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "/LowVoltage/3V0_Feedback") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 120.599665 68.516199 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "RNCP0603FTD24K9CT-ND")
    (property "mpn" "RNCP0603FTD24K9")
    (attr smd)
    (fp_text reference "R405" (at 0 -1.43 -90) (layer "F.SilkS"))
    (fp_text value "24k9" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/LowVoltage/2V6") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "/LowVoltage/2V6_Feedback") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 120.599665 71.564199 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R406" (at 0.889 2.4765 45) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "/LowVoltage/2V6_Feedback") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 128.092665 61.166199 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R409" (at 3.3655 0 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/LowVoltage/2V6") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 135.204665 69.849699)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R412" (at 3.6195 -0.0635) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(R412-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/LowVoltage/2V6") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 195.461 61.976999 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "A126330CT-ND")
    (property "mpn" "CRG0603J100R")
    (attr smd)
    (fp_text reference "R601" (at 3.39183 -0.049019 90) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(J604-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(J604-Pad8)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 61.299665 57.341001 90)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "296-37301-1-ND")
    (property "mpn" "TPS562200DDCT")
    (attr smd)
    (fp_text reference "U401" (at 4.0425 1.651 90) (layer "F.SilkS"))
    (fp_text value "TPS562200" (at 0 2.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C406-Pad1)") (pinfunction "SW") (pintype "output"))
    (pad "3" smd rect locked (at -1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/LowVoltage/3V8_Feedback") (pinfunction "VFB") (pintype "input"))
    (pad "5" smd rect locked (at 1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/LowVoltage/LV_EN") (pinfunction "EN") (pintype "input"))
    (pad "6" smd rect locked (at 1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C406-Pad2)") (pinfunction "VBST") (pintype "input"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 90.099665 57.2455 90)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "296-37301-1-ND")
    (property "mpn" "TPS562200DDCT")
    (attr smd)
    (fp_text reference "U402" (at 4.0425 1.651 90) (layer "F.SilkS"))
    (fp_text value "TPS562200" (at 0 2.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C407-Pad1)") (pinfunction "SW") (pintype "output"))
    (pad "3" smd rect locked (at -1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/LowVoltage/3V0_Feedback") (pinfunction "VFB") (pintype "input"))
    (pad "5" smd rect locked (at 1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/LowVoltage/LV_EN") (pinfunction "EN") (pintype "input"))
    (pad "6" smd rect locked (at 1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C407-Pad2)") (pinfunction "VBST") (pintype "input"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 115.435665 65.214199 180)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "296-37301-1-ND")
    (property "mpn" "TPS562200DDCT")
    (attr smd)
    (fp_text reference "U403" (at 4.2965 1.143) (layer "F.SilkS"))
    (fp_text value "TPS562200" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C408-Pad1)") (pinfunction "SW") (pintype "output"))
    (pad "3" smd rect locked (at -1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "/LowVoltage/2V6_Feedback") (pinfunction "VFB") (pintype "input"))
    (pad "5" smd rect locked (at 1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/LowVoltage/LV_EN") (pinfunction "EN") (pintype "input"))
    (pad "6" smd rect locked (at 1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C408-Pad2)") (pinfunction "VBST") (pintype "input"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm" (layer "F.Cu")
    (tedit 5C56E16F)
    (at 129.997665 67.754199 90)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "ADP7158ARDZ-1.8-R7CT-ND")
    (property "mpn" "ADP7158ARDZ-1.8-R7")
    (attr smd)
    (fp_text reference "U406" (at 1.587199 3.708067 270) (layer "F.SilkS"))
    (fp_text value "ADP7158ARDZ-1.8" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/LowVoltage/1V8_OUT") (pinfunction "VOUT") (pintype "power_out"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/LowVoltage/1V8_OUT") (pinfunction "VOUT_SENSE") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C417-Pad2)") (pinfunction "BYP") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(R412-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "5" smd roundrect locked (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C426-Pad1)") (pinfunction "REF_SENSE") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C426-Pad1)") (pinfunction "REF") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C423-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/LowVoltage/2V6") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" smd roundrect locked (at 0 0 90) (size 2.29 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.10917)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 200.66 62.103 -90)
    (descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "FIN1104MTCXCT-ND")
    (property "mpn" "FIN1104MTCX")
    (attr smd)
    (fp_text reference "U601" (at -1.905 -5.08 90) (layer "F.SilkS"))
    (fp_text value "FIN1104" (at 0 4.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.85 -3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.85 -2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -2.85 -2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/LVDSConnections/BiasNet3/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "4" smd rect locked (at -2.85 -1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/LVDSConnections/BiasNet3/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "5" smd rect locked (at -2.85 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/LVDSConnections/BiasNet4/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "6" smd rect locked (at -2.85 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "/LVDSConnections/BiasNet4/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "7" smd rect locked (at -2.85 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/LVDSConnections/BiasNet5/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "8" smd rect locked (at -2.85 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/LVDSConnections/BiasNet5/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "9" smd rect locked (at -2.85 1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(J604-Pad7)") (pinfunction "RI+") (pintype "input"))
    (pad "10" smd rect locked (at -2.85 2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(J604-Pad8)") (pinfunction "RI-") (pintype "input"))
    (pad "11" smd rect locked (at -2.85 2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "EN") (pintype "input"))
    (pad "12" smd rect locked (at -2.85 3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "13" smd rect locked (at 2.85 3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(U601-Pad13)") (pinfunction "VBB") (pintype "output+no_connect"))
    (pad "14" smd rect locked (at 2.85 2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" smd rect locked (at 2.85 2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(C606-Pad2)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "16" smd rect locked (at 2.85 1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(C605-Pad2)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "17" smd rect locked (at 2.85 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(J604-Pad4)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "18" smd rect locked (at 2.85 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(J604-Pad5)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "19" smd rect locked (at 2.85 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(J604-Pad6)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "20" smd rect locked (at 2.85 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(J604-Pad3)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "21" smd rect locked (at 2.85 -1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(J604-Pad1)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "22" smd rect locked (at 2.85 -2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(J604-Pad2)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "23" smd rect locked (at 2.85 -2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{EN}") (pintype "input"))
    (pad "24" smd rect locked (at 2.85 -3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "VCC") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-8" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 255.588999 46.2555 90)
    (descr "8-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_8_05-08-1637.pdf")
    (tags "TSOT-23-8")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "LTC2631ACTS8-HZ12#TRMPBFCT-ND")
    (property "mpn" "LTC2631ACTS8-HZ12#TRMPBF")
    (attr smd)
    (fp_text reference "U503" (at -0.000001 2.729001 90) (layer "F.SilkS"))
    (fp_text value "LTC2631-HZ" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.31 -0.97 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5V") (pinfunction "CA1/REF_SEL") (pintype "input"))
    (pad "2" smd rect locked (at -1.31 -0.33 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/MCU/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "3" smd rect locked (at -1.31 0.33 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/MCU/SDA") (pinfunction "SDA") (pintype "input"))
    (pad "4" smd rect locked (at -1.31 0.97 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.31 0.97 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd rect locked (at 1.31 0.33 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "unconnected-(U503-Pad6)") (pinfunction "REF") (pintype "power_in+no_connect"))
    (pad "7" smd rect locked (at 1.31 -0.33 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HighVoltage/HV_Ctrl") (pinfunction "OUTA") (pintype "output"))
    (pad "8" smd rect locked (at 1.31 -0.97 90) (size 1.22 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 111.5695 17.0815 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R501" (at 3.683 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J501-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 146.947 39.704 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P2.00KHCT-ND")
    (property "mpn" "ERJ-3EKF2001V")
    (attr smd)
    (fp_text reference "R506" (at -0.0635 -2.2225 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(J502-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric_Castellated" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 105.7275 12.8905)
    (descr "Diode SMD 0805 (2012 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode castellated")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "VEMD1060X01CT-ND")
    (property "mpn" "VEMD1060X01")
    (attr smd)
    (fp_text reference "D501" (at 0 -1.6) (layer "F.SilkS"))
    (fp_text value "D_Photo" (at 0 1.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9625 0) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9625 0) (size 1.325 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 32 "Net-(D501-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:L_Pulse_PA4331.332NLT" (layer "F.Cu")
    (tedit 5D7C111D)
    (at 174.7775 66.675 -90)
    (descr "Choke,Pulse Electronics, SMD,")
    (tags "Choke Pulse Electronics SMD ")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "553-3284-1-ND")
    (property "mpn" "PA4331.332NLT")
    (attr smd)
    (fp_text reference "L201" (at 0 -2.7915 -270) (layer "F.SilkS"))
    (fp_text value "3u3H" (at 0 5 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C205-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.15 0 270) (size 0.8 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5V") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 174.8205 61.529 180)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "296-37301-1-ND")
    (property "mpn" "TPS562200DDCT")
    (attr smd)
    (fp_text reference "U201" (at -0.028 2.5195 180) (layer "F.SilkS"))
    (fp_text value "TPS562200" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C205-Pad1)") (pinfunction "SW") (pintype "output"))
    (pad "3" smd rect locked (at -1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/PowerInput/5V_Feedback") (pinfunction "VFB") (pintype "input"))
    (pad "5" smd rect locked (at 1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(R203-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "6" smd rect locked (at 1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C205-Pad2)") (pinfunction "VBST") (pintype "input"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 123.101 16.6685 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R413" (at 0.4825 1.524) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/LowVoltage/LV_EN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 175.258999 58.2455)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R203" (at 3.56 -0.093999) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "+12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5C97300E)
    (at 129.6035 24.1615 90)
    (descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "DSPIC33EV256GM102-I/SO-ND")
    (property "mpn" "DSPIC33EV256GM102-I/SO")
    (attr smd)
    (fp_text reference "U501" (at 0 -9.9 90) (layer "F.SilkS"))
    (fp_text value "DSPIC33EV256GM102" (at 0 9.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.65 -8.255 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J501-Pad1)") (pinfunction "~{MCLR}") (pintype "input"))
    (pad "2" smd roundrect locked (at -4.65 -6.985 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/LowVoltage/3V8_OUT") (pinfunction "AN0/VREF+/CN2/RA0") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -4.65 -5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D501-Pad2)") (pinfunction "AN1/VREF-/CN3/RA1") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -4.65 -4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/LowVoltage/3V0_OUT") (pinfunction "PGED1/AN2/C2IN-/RP0/CN4/RB0") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -4.65 -3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/LowVoltage/1V8_OUT") (pinfunction "PGEC1/AN3/C2IN+/RP1/CN5/RB1") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -4.65 -1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/MCU/PGC") (pinfunction "AN4/C1IN-/RP2/CN6/RB2") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -4.65 -0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/MCU/PGD") (pinfunction "AN5/C1IN+/RP3/CN7/RB3") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -4.65 0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect locked (at -4.65 1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C507-Pad1)") (pinfunction "OSC1/CLKI/CN30/RA2") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -4.65 3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C508-Pad1)") (pinfunction "OSC2/CLKO/CN29/PMA0/RA3") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at -4.65 4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J504-Pad1)") (pinfunction "SOSCI/RP4/CN1/PMBE/RB4") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at -4.65 5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "/HighVoltage/HV_ON_OFF") (pinfunction "SOSCO/T1CK/CN0/PMA1/RA4") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -4.65 6.985 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "14" smd roundrect locked (at -4.65 8.255 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/MCU/SDA") (pinfunction "PGED3/ASDA1/RP5/CN27/PMD7/RB5") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at 4.65 8.255 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/MCU/SCL") (pinfunction "PGEC3/ASCL1/RP6/CN24/PMD6/RB6") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at 4.65 6.985 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(R505-Pad1)") (pinfunction "INT0/RP7/CN23/PMD5/RB7") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at 4.65 5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "unconnected-(U501-Pad17)") (pinfunction "TCK/PWM2H1/SCL1/RP8/CN22/PMD4/RB8") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect locked (at 4.65 4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "unconnected-(U501-Pad18)") (pinfunction "TDO/PWM2L1/SDA1/RP9/CN21/PMD3/RB9") (pintype "bidirectional+no_connect"))
    (pad "19" smd roundrect locked (at 4.65 3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "20" smd roundrect locked (at 4.65 1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(C501-Pad1)") (pinfunction "VCAP") (pintype "passive"))
    (pad "21" smd roundrect locked (at 4.65 0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J504-Pad2)") (pinfunction "PGED2/TDI/PWM1H3/RP10/CN16/PMD2/RB10") (pintype "bidirectional"))
    (pad "22" smd roundrect locked (at 4.65 -0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/MCU/CAN_TX") (pinfunction "PGEC2/TMS/PWM1L3/RP11/CN15/PMD1/RB11") (pintype "bidirectional"))
    (pad "23" smd roundrect locked (at 4.65 -1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/MCU/CAN_RX") (pinfunction "PWM1H2/RP12/CN14/PMD0/RB12") (pintype "bidirectional"))
    (pad "24" smd roundrect locked (at 4.65 -3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "unconnected-(U501-Pad24)") (pinfunction "PWM1L2/RP13/CN13/PMRD/RB13") (pintype "bidirectional+no_connect"))
    (pad "25" smd roundrect locked (at 4.65 -4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "unconnected-(U501-Pad25)") (pinfunction "PWM1H1/RTCC/RP14/CN12/PMWR/RB14") (pintype "bidirectional+no_connect"))
    (pad "26" smd roundrect locked (at 4.65 -5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/LowVoltage/LV_EN") (pinfunction "PWM1L1/RP15/CN11/PMCS1/RB15") (pintype "bidirectional"))
    (pad "27" smd roundrect locked (at 4.65 -6.985 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "AVSS") (pintype "power_in"))
    (pad "28" smd roundrect locked (at 4.65 -8.255 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "AVDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 156.091 53.166 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C202" (at 0.3835 1.4785 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_HC49-SD" (layer "F.Cu")
    (tedit 5A1AD52C)
    (at 132.1435 34.621)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "XC1272CT-ND")
    (property "mpn" "ECS-80-32-5PX-TR")
    (attr smd)
    (fp_text reference "Y501" (at 0 -3.55) (layer "F.SilkS"))
    (fp_text value "Crystal" (at 0 3.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -4.25 0) (size 4.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(C507-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.25 0) (size 4.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(C508-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 174.7775 64.135 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C205" (at -3.373 0.0455) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C205-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C205-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 178.758999 68.706999 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C206" (at 2.921 -0.635 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 171.008999 68.7455 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C207" (at 2.921 29.294334 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 132.3975 16.6685)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C501" (at -3.556 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 137.376 31.1465)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C502" (at 3.7845 0) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 252.984 46.7555 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C506" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 123.5785 34.621 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "399-14498-1-ND")
    (property "mpn" "C0603C200K4GAC7867")
    (attr smd)
    (fp_text reference "C507" (at 3.627 -0.2085) (layer "F.SilkS"))
    (fp_text value "20pF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C507-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 140.825 34.621)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "399-14498-1-ND")
    (property "mpn" "C0603C200K4GAC7867")
    (attr smd)
    (fp_text reference "C508" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "20pF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C508-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 119.4435 18.7005 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C503" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 152.027 39.704 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P2.00KHCT-ND")
    (property "mpn" "ERJ-3EKF2001V")
    (attr smd)
    (fp_text reference "R507" (at 0.5715 1.9685 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(J502-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 132.0875 38.5125)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "A129724CT-ND")
    (property "mpn" "CRGCQ0603F1M0")
    (attr smd)
    (fp_text reference "R508" (at -0.071 1.524) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C507-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C508-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 169.595999 60.520999 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R205" (at 3.7645 0.0455) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/PowerInput/5V_Feedback") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 109.9225 12.103 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R502" (at 3.5305 -0.004 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D501-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 172.008999 61.283 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "311-54.9KHRCT-ND")
    (property "mpn" "RC0603FR-0754K9L")
    (attr smd)
    (fp_text reference "R204" (at -0.0815 1.4425 90) (layer "F.SilkS"))
    (fp_text value "54k9" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/PowerInput/5V_Feedback") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 205.817 64.262 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C602" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPST_Omron-G5Q-1A" (layer "F.Cu")
    (tedit 5AE38B4B)
    (at 281.25 25.5 180)
    (descr "Relay SPST-NO Omron Serie G5Q, http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5q.pdf")
    (tags "Relay SPST-NO Omron Serie G5Q")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "Z223-ND")
    (property "mpn" "G5Q-1A4 DC12")
    (attr through_hole)
    (fp_text reference "K201" (at 9.5 -10.5 180) (layer "F.SilkS"))
    (fp_text value "G5Q-1A4 DC12" (at 8.8 3 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9.6 -4.5) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 90 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 90 "+12V") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 17.78 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(D201-Pad2)") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 -7.62) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 106 "/HighVoltage/SW1") (pintype "passive"))
    (model "${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPST_Omron-G5Q-1A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/Models/G5Q_1A4.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LVHV:RJ45_Wuerth_615008142621_Horizontal" (layer "F.Cu")
    (tedit 5D7C03E7)
    (at 173.23498 22.055963)
    (descr "10/100Base-TX RJ45 ethernet connector horizontal https://katalog.we-online.de/em/datasheet/615008142621.pdf")
    (tags "RJ45 ethernet ")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "732-3163-ND")
    (property "mpn" "615008142621")
    (attr through_hole)
    (fp_text reference "J602" (at -3.30898 10.837037 90) (layer "F.SilkS"))
    (fp_text value "RJ45" (at 7 14.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 4 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 8.89 -1.27 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 8.89 10.16 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect locked (at 2.54 8.89 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 65 "/LVDSConnections/BiasNet3/in_p") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 7.62 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 "/LVDSConnections/BiasNet3/in_n") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 6.35 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 145 "/LVDSConnections/BiasNet4/in_p") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 5.08 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 146 "/LVDSConnections/BiasNet5/in_p") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.54 3.81 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 147 "/LVDSConnections/BiasNet5/in_n") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 2.54 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 148 "/LVDSConnections/BiasNet4/in_n") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 2.54 1.27 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(C605-Pad1)") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 "Net-(C606-Pad1)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at 5.84 -3.305 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at 5.84 12.195 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/Models/615008142621 (rev1).stp"
      (offset (xyz 9 -4.5 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 162.433 16.2815 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C511" (at 3.7845 0 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 173.538001 12.793 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "277-1106-ND")
    (property "mpn" "1757242")
    (attr through_hole)
    (fp_text reference "J506" (at 2.54 -3.2 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 2.54 11.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 99 "/MCU/CAN_H") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 98 "/MCU/CAN_L") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 159.385 15.494 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P60.4DBCT-ND")
    (property "mpn" "ERA-3AEB60R4V")
    (attr smd)
    (fp_text reference "R513" (at 0.508 -1.524) (layer "F.SilkS"))
    (fp_text value "60R4" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/MCU/CAN_L") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 165.735 15.494 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P60.4DBCT-ND")
    (property "mpn" "ERA-3AEB60R4V")
    (attr smd)
    (fp_text reference "R514" (at -0.508 -1.524) (layer "F.SilkS"))
    (fp_text value "60R4" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/MCU/CAN_H") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(C511-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 94.849665 62.4955)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C410" (at 2.9845 -0.0635 90) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 22 "/LowVoltage/3V0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 85.349665 62.4955 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "1276-3395-1-ND")
    (property "mpn" "CL32B226MOJNNNE")
    (attr smd)
    (fp_text reference "C413" (at 3.2385 0.0635 90) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 22 "/LowVoltage/3V0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7)
    (at 256.908999 41.12)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "1N5819HW-FDICT-ND")
    (property "mpn" "1N5819HW-7-F")
    (attr smd)
    (fp_text reference "D301" (at -0.254 2.032) (layer "F.SilkS"))
    (fp_text value "1N5819" (at 0 2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HighVoltage/HV_Ctrl") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_10x7.7" (layer "F.Cu")
    (tedit 5BCA39D1)
    (at 234.203999 22.5455 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 10.0x7.7mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "493-3956-1-ND")
    (property "mpn" "UCL1V151MCL6GS")
    (attr smd)
    (fp_text reference "C203" (at 0 -6.2) (layer "F.SilkS"))
    (fp_text value "150uF" (at 0 6.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.35 0 180) (size 4.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.131579)
      (net 2 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 4.35 0 180) (size 4.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.131579)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_10x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7)
    (at 256.803999 24.7455)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "1N5819HW-FDICT-ND")
    (property "mpn" "1N5819HW-7-F")
    (attr smd)
    (fp_text reference "D201" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "1N5819" (at 0 2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(D201-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(D201-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 260.403999 23.9455 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R201" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D201-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 250.603999 24.7455)
    (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "507-1758-1-ND")
    (property "mpn" "0ZCG0030FF2C")
    (attr smd)
    (fp_text reference "F202" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "Polyfuse" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "Net-(D201-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 241.9265 45.466)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C509" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 231.1315 45.466 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C510" (at 0.065 1.397) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(C510-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5C97300E)
    (at 236.5925 47.371)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "480-5704-1-ND")
    (property "mpn" "HIH6030-021-001")
    (attr smd)
    (fp_text reference "U504" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "HIH6030-21" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(C510-Pad1)") (pinfunction "VCORE") (pintype "output"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/MCU/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/MCU/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "unconnected-(U504-Pad5)") (pinfunction "AL_H") (pintype "output+no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "unconnected-(U504-Pad6)") (pinfunction "AL_L") (pintype "output+no_connect"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "unconnected-(U504-Pad7)") (pinfunction "NC") (pintype "no_connect"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 31.377 64.189499 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C601" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 26.186001 62.182999 -90)
    (descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "FIN1104MTCXCT-ND")
    (property "mpn" "FIN1104MTCX")
    (attr smd)
    (fp_text reference "U602" (at -2.031999 -5.444999 -270) (layer "F.SilkS"))
    (fp_text value "FIN1104" (at 0 4.95 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.85 -3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.85 -2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -2.85 -2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "/LVDSConnections/BiasNet/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "4" smd rect locked (at -2.85 -1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "/LVDSConnections/BiasNet/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "5" smd rect locked (at -2.85 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "/LVDSConnections/BiasNet1/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "6" smd rect locked (at -2.85 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "/LVDSConnections/BiasNet1/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "7" smd rect locked (at -2.85 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/LVDSConnections/BiasNet2/in_n") (pinfunction "RI-") (pintype "input"))
    (pad "8" smd rect locked (at -2.85 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "/LVDSConnections/BiasNet2/in_p") (pinfunction "RI+") (pintype "input"))
    (pad "9" smd rect locked (at -2.85 1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(J601-Pad7)") (pinfunction "RI+") (pintype "input"))
    (pad "10" smd rect locked (at -2.85 2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(J601-Pad8)") (pinfunction "RI-") (pintype "input"))
    (pad "11" smd rect locked (at -2.85 2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "EN") (pintype "input"))
    (pad "12" smd rect locked (at -2.85 3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "13" smd rect locked (at 2.85 3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "unconnected-(U602-Pad13)") (pinfunction "VBB") (pintype "output+no_connect"))
    (pad "14" smd rect locked (at 2.85 2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" smd rect locked (at 2.85 2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(C604-Pad2)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "16" smd rect locked (at 2.85 1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(C603-Pad2)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "17" smd rect locked (at 2.85 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(J601-Pad4)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "18" smd rect locked (at 2.85 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(J601-Pad5)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "19" smd rect locked (at 2.85 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(J601-Pad6)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "20" smd rect locked (at 2.85 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(J601-Pad3)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "21" smd rect locked (at 2.85 -1.625 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J601-Pad1)") (pinfunction "DO+") (pintype "tri_state"))
    (pad "22" smd rect locked (at 2.85 -2.275 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(J601-Pad2)") (pinfunction "DO-") (pintype "tri_state"))
    (pad "23" smd rect locked (at 2.85 -2.925 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{EN}") (pintype "input"))
    (pad "24" smd rect locked (at 2.85 -3.575 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3I") (pinfunction "VCC") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 20.963 62.437 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "A126330CT-ND")
    (property "mpn" "CRG0603J100R")
    (attr smd)
    (fp_text reference "R605" (at 3.7085 0 90) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J601-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J601-Pad8)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A42D)
    (at 108.9025 15.8365)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "S5481-ND")
    (property "mpn" "PPPC061LGBN-RC")
    (attr through_hole)
    (fp_text reference "J501" (at -7.366 -2.565) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Female" (at -4.38 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.775 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J501-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/MCU/PGD") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/MCU/PGC") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "unconnected-(J501-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 36.576 27.432 180)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "lvhv.kicad_sch")
    (property "Sheetname" "")
    (property "digikey" "A98342-ND")
    (property "mpn" "282841-2")
    (attr through_hole)
    (fp_text reference "J101" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 96 "/Alarm1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 95 "/Alarm2") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 31.496 35.433)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "lvhv.kicad_sch")
    (property "Sheetname" "")
    (property "digikey" "A98342-ND")
    (property "mpn" "282841-2")
    (attr through_hole)
    (fp_text reference "J102" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 95 "/Alarm2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 96 "/Alarm1") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:Davis_Shop_25mm" locked (layer "F.Cu")
    (tedit 581A4233)
    (at 64.508999 42.9955)
    (attr through_hole)
    (fp_text reference "Davis_Shop_25mm" (at 0 -10.944808) (layer "F.SilkS") hide)
    (fp_text value "LOGO***" (at 0 10.944808) (layer "F.SilkS") hide)
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 20.574 27.432 180)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "lvhv.kicad_sch")
    (property "Sheetname" "")
    (property "digikey" "A98342-ND")
    (property "mpn" "282841-2")
    (attr through_hole)
    (fp_text reference "J103" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 100 "/Sine") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5B785047)
    (at 15.494 35.433)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (property "Sheetfile" "lvhv.kicad_sch")
    (property "Sheetname" "")
    (property "digikey" "A98342-ND")
    (property "mpn" "282841-2")
    (attr through_hole)
    (fp_text reference "J104" (at 2.54 -3.2) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2.54 11.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.3) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 100 "/Sine") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 147.96 24.21 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C512" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 158.46 25.4975 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P300LCT-ND")
    (property "mpn" "ERJ-2RKF3000X")
    (attr smd)
    (fp_text reference "R515" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "300R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(R515-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5C97300E)
    (at 152.52 24.37)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "MCP2561-E/SN-ND")
    (property "mpn" "MCP2561-E/SN")
    (attr smd)
    (fp_text reference "U505" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "MCP2561-E-SN" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/MCU/CAN_TX") (pinfunction "TXD") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/MCU/CAN_RX") (pinfunction "RXD") (pintype "output"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(R515-Pad2)") (pinfunction "SPLIT") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/MCU/CAN_L") (pinfunction "CANL") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/MCU/CAN_H") (pinfunction "CANH") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "STBY") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 37.219 53.293)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R702" (at 3.5645 0.076) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(C701-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 260.152 65.7555 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D305" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(D303-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(D305-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:L_Bourns_SRP5015" (layer "F.Cu")
    (tedit 60FAF71E)
    (at 84.849665 67.2455 180)
    (descr "Bourns SRP5015 series SMD inductor")
    (tags "Bourns SRP5015 SMD inductor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "SRP5015TA-R20YCT-ND")
    (property "mpn" "SRP5015TA-R20Y")
    (attr smd)
    (fp_text reference "L405" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "200nH" (at 0 4.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.1 0 180) (size 2 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 19 "Net-(C402-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.1 0 180) (size 2 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 33 "/LowVoltage/3V0_OUT") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRP2313AA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 30.107 50.245)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet1")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R802" (at 3.8765 -1.352) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C801-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 149.487 39.704 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "DMN601DWKDICT-ND")
    (property "mpn" "DMN601DWK-7")
    (attr smd)
    (fp_text reference "Q501" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "DMN601DWK-7" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.95 -0.65 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(J502-Pad3)") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect locked (at -0.95 0 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+3V3") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect locked (at -0.95 0.65 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/MCU/SCL") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect locked (at 0.95 0.65 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "Net-(J502-Pad2)") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect locked (at 0.95 0 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+3V3") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect locked (at 0.95 -0.65 180) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/MCU/SDA") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 198.7885 50.118)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet4")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R1101" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C1101-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 207.1705 54.309)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet3")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1004" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C1001-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/LVDSConnections/BiasNet3/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 230.152 63.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D304" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(D304-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(D304-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 224.0275 42.976748)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C513" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(C513-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(C513-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 20.572502 53.202234)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet2")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R901" (at -0.589001 3.014766) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C901-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 185.508999 63.958 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C209" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C209-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 30.107 48.721 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet1")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R803" (at -3.8765 1.228) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "/LVDSConnections/BiasNet1/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C801-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 15.883 53.039 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C603" (at -3.556 0 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C603-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(C603-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 163.508999 67.9955 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R414" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 163.492999 43.4955 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "311-100KHRCT-ND")
    (property "mpn" "RC0603FR-07100KL")
    (attr smd)
    (fp_text reference "R208" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "/PowerInput/VIN_FUSED") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(R208-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 197.62 52.531)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet5")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1204" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C1201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "/LVDSConnections/BiasNet5/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 94.849665 67.2455)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "490-6543-1-ND")
    (property "mpn" "GRM32ER71A476ME15L")
    (attr smd)
    (fp_text reference "C402" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 19 "Net-(C402-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 161.758999 67.9955 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R415" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(R415-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 250.152 60.2555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D310" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(D310-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(D306-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 263.652 69.518 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D309" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(D305-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(D309-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:Texas_CSD87312Q3E" (layer "F.Cu")
    (tedit 60FB3DC7)
    (at 167.210249 48.4705 -90)
    (descr "8-Lead Plastic VSON, 3x3mm Body, 0.65mm Pitch, S-PVSON-N8, http://www.ti.com/lit/ds/symlink/opa2333.pdf")
    (tags "DFN 0.65 S-PVSON-N8")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "296-35526-1-ND")
    (property "mpn" "CSD87312Q3E")
    (attr smd)
    (fp_text reference "Q203" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "CSD87312Q3E" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect locked (at -1.475 -0.975 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at -1.475 -0.6) (size 0.55 0.55) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at -1.475 -0.28625 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at -1.475 0.28625 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at -1.475 0.975 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at -0.45 -0.9 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at -0.45 0 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at -0.45 0.9 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at 0.45 -0.9 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at 0.45 0 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at 0.45 0.9 270) (size 0.7 0.7) (layers "F.Paste" "F.Mask"))
    (pad "" smd rect locked (at 1.475 -0.975 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at 1.475 -0.325 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at 1.475 0.325 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "" smd rect locked (at 1.475 0.975 270) (size 0.55 0.34) (layers "F.Paste")
      (solder_paste_margin -0.05))
    (pad "1" smd rect locked (at -1.475 -0.89625 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 139 "/PowerInput/VIN_FUSED") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "2" smd rect locked (at -1.475 -0.29875 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 139 "/PowerInput/VIN_FUSED") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "3" smd rect locked (at -1.475 0.29875 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 139 "/PowerInput/VIN_FUSED") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "4" smd rect locked (at -1.475 0.89625 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 139 "/PowerInput/VIN_FUSED") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "5" smd rect locked (at 1.475 0.975 270) (size 0.65 0.44) (layers "F.Cu" "F.Mask")
      (net 140 "Net-(Q203-Pad5)") (pinfunction "G") (pintype "input") (solder_paste_margin -0.05))
    (pad "6" smd rect locked (at 1.475 0.29875 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 90 "+12V") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "7" smd rect locked (at 1.475 -0.29875 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 90 "+12V") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "8" smd rect locked (at 1.475 -0.89625 270) (size 0.65 0.5975) (layers "F.Cu" "F.Mask")
      (net 90 "+12V") (pinfunction "D") (pintype "passive") (solder_paste_margin -0.05))
    (pad "9" smd rect locked (at -0.59 -1.575 270) (size 0.3 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(Q203-Pad9)") (pinfunction "S") (pintype "passive") (solder_paste_margin -0.05))
    (pad "9" smd rect locked (at -0.59 1.575 270) (size 0.3 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(Q203-Pad9)") (pinfunction "S") (pintype "passive") (solder_paste_margin -0.05))
    (pad "9" smd rect locked (at 0 0 270) (size 1.9 2.8) (layers "F.Cu" "F.Mask")
      (net 107 "Net-(Q203-Pad9)") (pinfunction "S") (pintype "passive"))
    (pad "9" smd rect locked (at 0.59 -1.575 270) (size 0.3 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(Q203-Pad9)") (pinfunction "S") (pintype "passive") (solder_paste_margin -0.05))
    (pad "9" smd rect locked (at 0.59 1.575 270) (size 0.3 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(Q203-Pad9)") (pinfunction "S") (pintype "passive") (solder_paste_margin -0.05))
    (model "${KISYS3DMOD}/Package_SON.3dshapes/Texas_S-PVSON-N8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 154.008999 72.9955 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C430" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 276.25 38.62)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R307" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "/HighVoltage/HV_ON_OFF") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Net-(Q301-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 37.219 54.817)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C701" (at 3.5645 0.076) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(C701-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 227.5275 46.226748)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C505" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 187.008999 75.708 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C204" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C204-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 23.620501 53.202234)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet2")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R902" (at 3.362999 0.014766) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C901-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 214.152 58.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "353-3SMAJ5946B-TPCT-ND")
    (property "mpn" "3SMAJ5946B-TP")
    (attr smd)
    (fp_text reference "D316" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "75V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "Net-(D312-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 207.1705 57.357)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet3")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C1001" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C1001-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 204.1225 54.309)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet3")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1003" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/LVDSConnections/BiasNet3/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C1001-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 20.572501 51.678234)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet2")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R903" (at -0.589001 3.014766) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "/LVDSConnections/BiasNet2/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C901-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 187.008999 63.933 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C210" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C210-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 258.152 60.2555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D303" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(D303-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(D303-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 175.508999 78.252784 -90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "732-2705-ND")
    (property "mpn" "61900419521")
    (attr through_hole)
    (fp_text reference "J502" (at 4.385 -2.27 90) (layer "F.SilkS"))
    (fp_text value "61900419521" (at 4.385 9.89 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(J502-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J502-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 198.7885 48.594 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet4")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1104" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C1101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "/LVDSConnections/BiasNet4/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm" (layer "F.Cu")
    (tedit 5C56E16F)
    (at 156.893999 67.9705 90)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "ADP7158ARDZ-1.8-R7CT-ND")
    (property "mpn" "ADP7158ARDZ-1.8-R7")
    (attr smd)
    (fp_text reference "U405" (at 0 -3.4 90) (layer "F.SilkS"))
    (fp_text value "ADP7158ARDZ-3.3" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "+3V3") (pinfunction "VOUT_SENSE") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(C424-Pad2)") (pinfunction "BYP") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(R415-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "5" smd roundrect locked (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C428-Pad1)") (pinfunction "REF_SENSE") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C428-Pad1)") (pinfunction "REF") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C427-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" smd roundrect locked (at 0 0 90) (size 2.29 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.10917)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 281.25 37.62 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "2156-MMBTA42-ND")
    (property "mpn" "MMBTA42")
    (attr smd)
    (fp_text reference "Q301" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "MMBTA42" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "Net-(Q301-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/HighVoltage/SW1") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 65.799665 67.2455)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "490-6543-1-ND")
    (property "mpn" "GRM32ER71A476ME15L")
    (attr smd)
    (fp_text reference "C401" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 18 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 34.171 53.293)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R701" (at -0.7875 3.124) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(C701-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 30.107 51.769)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet1")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C801" (at 3.8765 -1.476) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C801-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 242.152 60.2555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "353-3SMAJ5946B-TPCT-ND")
    (property "mpn" "3SMAJ5946B-TP")
    (attr smd)
    (fp_text reference "D315" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "75V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(D311-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(D314-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 269.822 81.018)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "353-3SMAJ5946B-TPCT-ND")
    (property "mpn" "3SMAJ5946B-TP")
    (attr smd)
    (fp_text reference "D313" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "75V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(D309-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C301-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:Caddock_USVD_HVD" (layer "F.Cu")
    (tedit 60F9D886)
    (at 247.803999 54.9455 180)
    (descr "Precision HV Resistor Divider")
    (tags "R")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "683-HVD5-A50M-050-05-ND")
    (property "mpn" "HVD5-A50M-050-05")
    (attr through_hole)
    (fp_text reference "RN301" (at 17.78 -2.4) (layer "F.SilkS"))
    (fp_text value "HVD5-A50M" (at 17.78 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 16.51 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 2.54 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 27.94 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 123 "/HighVoltage/HV_MON") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 30.48 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 123 "/HighVoltage/HV_MON") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 35.56 0 180) (size 1.7526 1.7526) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP14.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm" (layer "F.Cu")
    (tedit 5C56E16F)
    (at 186.373999 69.683 90)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "ADP7158ARDZ-1.8-R7CT-ND")
    (property "mpn" "ADP7158ARDZ-1.8-R7")
    (attr smd)
    (fp_text reference "U203" (at 0 -3.4 90) (layer "F.SilkS"))
    (fp_text value "ADP7158ARDZ-3.3" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 -0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.57 0.75 90) (size 0.92 1.21) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pinfunction "VOUT") (pintype "power_out"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pinfunction "VOUT_SENSE") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C204-Pad2)") (pinfunction "BYP") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(R210-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "5" smd roundrect locked (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C210-Pad1)") (pinfunction "REF_SENSE") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C210-Pad1)") (pinfunction "REF") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C209-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" smd roundrect locked (at 0 0 90) (size 2.29 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.10917)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:L_Bourns_SRP5015" (layer "F.Cu")
    (tedit 60FAF71E)
    (at 55.449665 67.2455 180)
    (descr "Bourns SRP5015 series SMD inductor")
    (tags "Bourns SRP5015 SMD inductor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "SRP5015TA-R20YCT-ND")
    (property "mpn" "SRP5015TA-R20Y")
    (attr smd)
    (fp_text reference "L404" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "200nH" (at 0 4.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.1 0 180) (size 2 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 18 "Net-(C401-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.1 0 180) (size 2 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 31 "/LowVoltage/3V8_OUT") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRP2313AA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 254.152 63.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D306" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(D306-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(D303-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 27.059 50.245)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet1")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R801" (at -3.4755 -0.088) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C801-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 90.099665 65.9955 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "P17684CT-ND")
    (property "mpn" "ERJ-8BSFR20V")
    (attr smd)
    (fp_text reference "R408" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "0R2" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 22 "/LowVoltage/3V0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 19 "Net-(C402-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 157.508999 73.4955 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C424" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(C424-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 194.572 52.531)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet5")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1203" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "/LVDSConnections/BiasNet5/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C1201-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 37.219 51.769)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R704" (at 3.5645 0.076) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(C701-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "/LVDSConnections/BiasNet/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 212.977 49.513749 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R509" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(R505-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "/HighVoltage/HV_MON") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 23.620501 51.678234)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet2")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R904" (at 3.362999 0.014766) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C901-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "/LVDSConnections/BiasNet2/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 238.152 63.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D311" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D307-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(D311-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 212.977 46.440248 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R505" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(R505-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(R505-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 222.152 63.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D312" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "Net-(D312-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(D308-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 224.0275 46.226748 180)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "ADM8828ARTZ-REEL7CT-ND")
    (property "mpn" "ADM8828ARTZ-REEL7")
    (attr smd)
    (fp_text reference "U506" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "ADM8828" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "-5V") (pinfunction "VOUT") (pintype "power_out"))
    (pad "2" smd rect locked (at -1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5V") (pinfunction "V+") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(C513-Pad2)") (pinfunction "CAP-") (pintype "input"))
    (pad "4" smd rect locked (at 1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(U506-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd rect locked (at 1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(C513-Pad1)") (pinfunction "CAP+") (pintype "input"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 158.758999 62.2455 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C428" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C428-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMB" (layer "F.Cu")
    (tedit 58645DF3)
    (at 268.152 20.2555 180)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "S1KB-FDICT-ND")
    (property "mpn" "S1KB-13-F")
    (attr smd)
    (fp_text reference "D302" (at 0 -3) (layer "F.SilkS"))
    (fp_text value "S1KB-13-F" (at 0 3.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.15 0 180) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.15 0 180) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(D201-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 215.326499 41.926748 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C504" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 216.748999 46.676748 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "296-48157-1-ND")
    (property "mpn" "OPA196IDR")
    (attr smd)
    (fp_text reference "U502" (at 3.5385 -3.771999 90) (layer "F.SilkS"))
    (fp_text value "OPA196IDR" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "unconnected-(U502-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(R505-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "-5V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "unconnected-(U502-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(R505-Pad1)") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "unconnected-(U502-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 201.8365 51.642)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet4")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C1101" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C1101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 34.171 51.769)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R703" (at -0.7875 3.124) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "/LVDSConnections/BiasNet/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(C701-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 84.349665 73.4955)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "490-6543-1-ND")
    (property "mpn" "GRM32ER71A476ME15L")
    (attr smd)
    (fp_text reference "C416" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 33 "/LowVoltage/3V0_OUT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 160.258999 46.2455 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "311-20.0KHRCT-ND")
    (property "mpn" "RC0603FR-0720KL")
    (attr smd)
    (fp_text reference "R206" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(R202-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R206-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 220.49 48.481248 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C515" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 143.357499 27.1925 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P2.00KHCT-ND")
    (property "mpn" "ERJ-3EKF2001V")
    (attr smd)
    (fp_text reference "R503" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/MCU/SCL") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 234.152 60.2555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D307" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(D304-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D307-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 17.407 53.039 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C604" (at -3.556 0 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(C604-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C604-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 190.258999 71.208 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R210" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(R210-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 201.8365 48.594 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet4")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R1103" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "/LVDSConnections/BiasNet4/in_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C1101-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 190.889 56.849 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C606" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(C606-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(C606-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 207.1705 55.833)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet3")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R1002" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C1001-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 201.8365 50.118)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet4")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R1102" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C1101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 140 27.707999 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "P2.00KHCT-ND")
    (property "mpn" "ERJ-3EKF2001V")
    (attr smd)
    (fp_text reference "R504" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/MCU/SDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 182.758999 64.9955 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C418" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:DFN-8-1EP_2x3mm_P0.5mm_EP0.61x2.2mm" (layer "F.Cu")
    (tedit 60FB4F8E)
    (at 160.258999 43.4955 90)
    (descr "DDB Package; 8-Lead Plastic DFN (3mm x 2mm) (see Linear Technology DFN_8_05-08-1702.pdf)")
    (tags "DFN 0.5")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "LTC4365IDDB#TRPBFCT-ND")
    (property "mpn" "LTC4365IDDB#TRPBF")
    (attr smd)
    (fp_text reference "U202" (at 0 -2.55 90) (layer "F.SilkS"))
    (fp_text value "LTC4365IDDB" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect locked (at 0 -0.734 90) (size 0.5 0.59) (layers "F.Paste"))
    (pad "" smd rect locked (at 0 0 90) (size 0.5 0.59) (layers "F.Paste"))
    (pad "" smd rect locked (at 0 0.734 90) (size 0.5 0.59) (layers "F.Paste"))
    (pad "1" smd rect locked (at -0.925 -0.75 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_width 0.254) (thermal_gap 0.254))
    (pad "2" smd rect locked (at -0.925 -0.25 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "Net-(R206-Pad2)") (pinfunction "OV") (pintype "input"))
    (pad "3" smd rect locked (at -0.925 0.25 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "Net-(R202-Pad2)") (pinfunction "UV") (pintype "input"))
    (pad "4" smd rect locked (at -0.925 0.75 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "/PowerInput/VIN_FUSED") (pinfunction "Vin") (pintype "power_in"))
    (pad "5" smd rect locked (at 0.925 0.75 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "Net-(Q203-Pad5)") (pinfunction "GATE") (pintype "output"))
    (pad "6" smd rect locked (at 0.925 0.25 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "+12V") (pinfunction "Vout") (pintype "input"))
    (pad "7" smd rect locked (at 0.925 -0.25 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "unconnected-(U202-Pad7)") (pinfunction "~{FAULT}") (pintype "open_collector+no_connect"))
    (pad "8" smd rect locked (at 0.925 -0.75 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(R208-Pad2)") (pinfunction "~{SHDN}") (pintype "input"))
    (pad "9" smd rect locked (at 0 0 90) (size 0.61 2.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_2x3mm_P0.5mm_EP0.61x2.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 194.5465 54.055)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet5")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R1201" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C1201-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 27.059 48.721 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet1")
    (property "digikey" "A109983CT-ND")
    (property "mpn" "RP73PF1J49R9BTDF")
    (attr smd)
    (fp_text reference "R804" (at 3.4755 0.028) (layer "F.SilkS"))
    (fp_text value "49R9" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C801-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "/LVDSConnections/BiasNet1/in_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 153.008999 63.9955 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C208" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 197.5945 55.579)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet5")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C1201" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C1201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 157.258998 46.2455 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "311-42.2KHRCT-ND")
    (property "mpn" "RC0603FR-0742K2L")
    (attr smd)
    (fp_text reference "R207" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "42k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R206-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 184.508999 75.683 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C211" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 204.1225 55.833)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet3")
    (property "digikey" "A102203CT-ND")
    (property "mpn" "CPF0603F10KC1")
    (attr smd)
    (fp_text reference "R1001" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3I") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C1001-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 190.258999 67.933 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "A130103CT-ND")
    (property "mpn" "CRGCQ0603J100K")
    (attr smd)
    (fp_text reference "R209" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 23.646003 54.726234)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet2")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C901" (at 3.362999 0.014766) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C901-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 163.258997 46.2455 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PowerInput.kicad_sch")
    (property "Sheetname" "PowerInput")
    (property "digikey" "541-1.33MHCT-ND")
    (property "mpn" "CRCW06031M33FKEA")
    (attr smd)
    (fp_text reference "R202" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1M33" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "/PowerInput/VIN_FUSED") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(R202-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 226.0275 49.226748)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "587-3417-1-ND")
    (property "mpn" "LMK212AB7106MG-T")
    (attr smd)
    (fp_text reference "C514" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 226.152 60.2555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "  1SMA200ZR3GCT-ND")
    (property "mpn" "1SMA200Z")
    (attr smd)
    (fp_text reference "D308" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "200V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(D308-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(D304-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 61.284364 65.9955 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "P17684CT-ND")
    (property "mpn" "ERJ-8BSFR20V")
    (attr smd)
    (fp_text reference "R407" (at 0 -1.82 -90) (layer "F.SilkS"))
    (fp_text value "0R2" (at 0 1.82 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 21 "+3V8") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 18 "Net-(C401-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 246.152 63.7555)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "353-3SMAJ5946B-TPCT-ND")
    (property "mpn" "3SMAJ5946B-TP")
    (attr smd)
    (fp_text reference "D314" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "75V" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(D314-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(D310-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 156.258999 62.2455 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "587-3352-1-ND")
    (property "mpn" "GMK107AB7105KAHT")
    (attr smd)
    (fp_text reference "C427" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C427-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 197.5945 54.055)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lvds_bias.kicad_sch")
    (property "Sheetname" "BiasNet5")
    (property "digikey" "A139482CT-ND")
    (property "mpn" "RQ73C1J5K76BTD")
    (attr smd)
    (fp_text reference "R1202" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "5k7" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C1201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 54.999665 73.4955)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LowVoltage.kicad_sch")
    (property "Sheetname" "LowVoltage")
    (property "digikey" "490-6543-1-ND")
    (property "mpn" "GRM32ER71A476ME15L")
    (attr smd)
    (fp_text reference "C415" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 31 "/LowVoltage/3V8_OUT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 189.365 56.849 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LVDS.kicad_sch")
    (property "Sheetname" "LVDSConnections")
    (property "digikey" "587-3354-1-ND")
    (property "mpn" "GMK107B7104KAHT")
    (attr smd)
    (fp_text reference "C605" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0u1F" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C605-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C605-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:TE_63951-1_1x02_P5.08mm_Drill1.45mm" (layer "B.Cu")
    (tedit 5D7C1E62)
    (at 263.652 75.7555 -90)
    (descr "CONN QC TAB 0.250 SOLDER")
    (tags "connector")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A100799CT-ND‎")
    (property "mpn" "63951-1‎")
    (attr exclude_from_pos_files)
    (fp_text reference "J301" (at -2.9845 -0.127) (layer "B.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 2.54 -3.81 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 91 "Net-(D309-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 91 "Net-(D309-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/Models/c-63951-1-s-3d.stp"
      (offset (xyz 19.685 0 6.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "LVHV:TE_63951-1_1x02_P5.08mm_Drill1.45mm" (layer "B.Cu")
    (tedit 5D7C1E62)
    (at 249.525332 75.7555 -90)
    (descr "CONN QC TAB 0.250 SOLDER")
    (tags "connector")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A100799CT-ND‎")
    (property "mpn" "63951-1‎")
    (attr exclude_from_pos_files)
    (fp_text reference "J302" (at -2.9845 -0.029668) (layer "B.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 2.54 -3.81 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 92 "Net-(D310-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 92 "Net-(D310-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/Models/c-63951-1-s-3d.stp"
      (offset (xyz 19.6088 0 6.0452))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "LVHV:TE_63951-1_1x02_P5.08mm_Drill1.45mm" (layer "B.Cu")
    (tedit 5D7C1E62)
    (at 235.398666 75.7555 -90)
    (descr "CONN QC TAB 0.250 SOLDER")
    (tags "connector")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A100799CT-ND‎")
    (property "mpn" "63951-1‎")
    (attr exclude_from_pos_files)
    (fp_text reference "J303" (at -2.9845 -0.059334) (layer "B.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 2.54 -3.81 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 101 "Net-(D311-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 101 "Net-(D311-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/Models/c-63951-1-s-3d.stp"
      (offset (xyz 19.685 0 6.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "LVHV:TE_63951-1_1x02_P5.08mm_Drill1.45mm" (layer "B.Cu")
    (tedit 5D7C1E62)
    (at 221.272 75.7555 -90)
    (descr "CONN QC TAB 0.250 SOLDER")
    (tags "connector")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A100799CT-ND‎")
    (property "mpn" "63951-1‎")
    (attr exclude_from_pos_files)
    (fp_text reference "J304" (at -2.9845 0.038) (layer "B.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 2.54 -3.81 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 102 "Net-(D312-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 102 "Net-(D312-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/Models/c-63951-1-s-3d.stp"
      (offset (xyz 19.685 0 6.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Horizontal" (layer "B.Cu")
    (tedit 5A19A41B)
    (at 130.302 3.556 90)
    (descr "Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "MCU.kicad_sch")
    (property "Sheetname" "MCU")
    (property "digikey" "S5440-ND")
    (property "mpn" "PPTC041LGBN-RC")
    (attr through_hole)
    (fp_text reference "J504" (at -4.38 2.77 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x04" (at -4.38 -5.31 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -5.775 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J504-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J504-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LVHV:EMCO_C40N.fp" (layer "B.Cu")
    (tedit 5D952EFA)
    (at 246.507 29.9605)
    (descr "EMCO_C40N.fp")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "1470-3255-ND")
    (property "mpn" "C40N")
    (attr through_hole)
    (fp_text reference "Z301" (at -19.304 -10.414 270) (layer "F.SilkS"))
    (fp_text value "C40N" (at -6.858 2.794 180) (layer "F.SilkS"))
    (fp_circle (center 2.54 8.13) (end 0.165 8.13) (layer "Edge.Cuts") (width 0.12) (fill none))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(C203-Pad1)") (pinfunction "P_IN") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at -12.7 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 6.35 3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "/HighVoltage/HV_Ctrl") (pinfunction "PrgmV") (pintype "input"))
    (pad "4" thru_hole oval locked (at 6.35 25.4 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 79 "Net-(R301-Pad2)") (pinfunction "HV_Out") (pintype "power_out"))
    (pad "5" thru_hole oval locked (at -2.54 -8.89 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "CASE") (pintype "power_in"))
  )
  (footprint "LVHV:TE_63951-1_1x02_P5.08mm_Drill1.45mm" (layer "B.Cu")
    (tedit 5D7C1E62)
    (at 277.77948 75.7555 -90)
    (descr "CONN QC TAB 0.250 SOLDER")
    (tags "connector")
    (property "Sheetfile" "HighVoltage.kicad_sch")
    (property "Sheetname" "HighVoltage")
    (property "digikey" "A100799CT-ND‎")
    (property "mpn" "63951-1‎")
    (attr exclude_from_pos_files)
    (fp_text reference "J305" (at 2.54 3.81 -90) (layer "B.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 2.54 -3.81 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 5.08 0 270) (size 3.50012 3.50012) (drill 1.45) (layers *.Cu *.Mask)
      (net 6 "Net-(C301-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/Models/c-63951-1-s-3d.stp"
      (offset (xyz 19.558 0 5.715))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_arc (start 273.05 76.2) (end 285.75 76.2) (angle 90) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 22.225 22.225) (end 0 22.225) (angle 90) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 231.775 12.7) (end 233.6038 12.7) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 276.225 63.5) (end 278.0538 63.5) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 9.525 63.5) (end 11.3538 63.5) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 223.973266 0) (end 263.525 0) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 53.975 12.7) (end 55.8038 12.7) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_arc (start 185.746267 6.351269) (end 185.746266 0) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 198.446266 38.103804) (end 211.019267 38.103804) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 217.497535 31.753804) (end 217.495 6.344927) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 223.846267 6.349999) (end 217.495 6.344927) (angle 91.0999987) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 192.096266 6.478268) (end 192.096266 31.625536) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 211.146266 31.753805) (end 217.497535 31.753804) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 198.446265 31.752535) (end 198.446266 38.103804) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 74.548999 31.748731) (end 74.549 38.1) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 87.249 31.750001) (end 93.600269 31.75) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 68.199 6.478268) (end 68.199 31.621732) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.949001 6.35) (end 93.597734 6.344928) (angle 91.0999987) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 93.600269 31.75) (end 93.597734 6.344928) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 74.549 38.1) (end 87.122001 38.1) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 61.849001 6.351269) (end 61.849 0) (angle 91.14576302) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 142.875 12.7) (end 144.7038 12.7) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_arc (start 12.7 76.2) (end 12.7 88.9) (angle 90) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 22.225 0) (end 61.849 0) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 285.75 22.225) (end 285.75 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 273.05 88.9) (end 12.7 88.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 76.2) (end 0 22.225) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 100.076 0.000001) (end 185.746266 0) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 263.525 22.225) (end 263.525 0) (angle 90) (layer "Edge.Cuts") (width 0.1))
  (gr_text "+1V8" (at 132.099665 82.4455 90) (layer "F.SilkS"))
  (gr_text "+1V8" (at 102.099665 82.4455 90) (layer "F.SilkS"))
  (gr_text "+3V0" (at 72.349665 82.296 90) (layer "F.SilkS"))
  (gr_text "I2C" (at 149.258999 70.2455) (layer "F.SilkS"))
  (gr_text "+3K7V" (at 259.08 81.7245 90) (layer "F.SilkS"))
  (gr_text "+2K2V" (at 244.094 81.5975 90) (layer "F.SilkS"))
  (gr_text "+1K8V" (at 231.394 81.788 90) (layer "F.SilkS"))
  (gr_text "+300V" (at 217.17 81.5975 90) (layer "F.SilkS"))
  (gr_text "ALARM - THRU" (at 42.926 31.369 90) (layer "F.SilkS"))
  (gr_text "+4KV" (at 273.685 81.661 90) (layer "F.SilkS"))
  (gr_text "CAN" (at 164.084 10.287 90) (layer "F.SilkS"))
  (gr_text "L" (at 168.021 7.62 90) (layer "F.SilkS"))
  (gr_text "H" (at 168.021 12.827 90) (layer "F.SilkS"))
  (gr_text "GND" (at 166.116 40.005) (layer "F.SilkS"))
  (gr_text "SINE - THRU" (at 9.017 31.496 90) (layer "F.SilkS"))
  (gr_text "3.3V" (at 44.849665 69.2455) (layer "F.SilkS"))
  (gr_text "+12V" (at 174.758999 51.2455) (layer "F.SilkS"))
  (gr_text "DANGER\nHIGH VOLTAGE" (at 244.758999 94.9955) (layer "F.SilkS"))
  (gr_text "2.5V" (at 89.868165 58.437 270) (layer "F.SilkS"))
  (gr_text "Low V" (at 127.0425 5.53275) (layer "F.SilkS"))
  (gr_text "LVHV Control\n20210722" (at 51.473344 50.9965) (layer "F.SilkS"))
  (gr_text "+3V8" (at 42.258999 82.9455 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 217.551 22.225) (xy 285.75 22.225))
    (height -35.052)
    (gr_text "2.6850  in" (at 251.6505 -13.977) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 269.748 88.9) (xy 269.748 0))
    (height 47.625)
    (gr_text "3.5000  in" (at 316.223 44.45 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 14.986 12.553732) (xy 14.986 114.153732))
    (height 47.625)
    (gr_text "4.0000  in" (at -33.789 63.353732 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 53.975 22.225) (xy 0 22.225))
    (height 38.862)
    (gr_text "2.1250  in" (at 26.9875 -17.787) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 68.21 22.225) (xy 0 22.225))
    (height 55.109672)
    (gr_text "2.6854  in" (at 34.105 -34.034672) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 192.151 22.098) (xy 217.551 22.098))
    (height -34.925)
    (gr_text "1.0000  in" (at 204.851 -13.977) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 363.711 12.525) (xy 77.961 12.525))
    (height -46.865244)
    (gr_text "11.2500  in" (at 220.836 58.240244) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 53.975 0) (xy 53.975 12.7))
    (height 67.818)
    (gr_text "0.5000  in" (at -14.993 6.35 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 65.095 38.098732) (xy 65.095 -0.001268))
    (height 9.865)
    (gr_text "1.5000  in" (at 73.81 19.048732 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 285.75 63.498732) (xy 276.225 63.5))
    (height 6.602732)
    (gr_text "0.3750  in" (at 280.986468 55.746634 0.007627406613) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 214.011735 51.601329)
        (xy 295.93654 51.280008)
        (xy 296.362 102.126)
        (xy 214.066 102.126)
        (xy 214.066 76.853)
        (xy 214.122 76.79228)
        (xy 214.122 69.003721)
        (xy 213.968193 69.020679)
      )
    )
  )
  (zone (net 33) (net_name "/LowVoltage/3V0_OUT") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 84.849665 69.9955)
        (xy 84.849665 64.4955)
        (xy 80.099665 64.4955)
        (xy 80.099665 76.9955)
        (xy 80.099665 81.9955)
        (xy 84.599665 81.9955)
        (xy 84.650099 76.263199)
        (xy 84.349665 74.9955)
        (xy 84.349665 71.2455)
      )
    )
  )
  (zone (net 40) (net_name "/LowVoltage/1V8_OUT") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 127.099665 75.9955)
        (xy 109.915206 76.046555)
        (xy 110.008793 82.961786)
        (xy 144.058517 82.991895)
        (xy 144.077197 75.952967)
        (xy 130.345792 75.99551)
        (xy 130.349665 68.6492)
        (xy 127.095104 68.739767)
      )
    )
  )
  (zone (net 5) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 136.271 28.035)
        (xy 144.145 28.035)
        (xy 144.145 20.034)
        (xy 136.525 20.034)
      )
    )
  )
  (zone (net 5) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 185.094695 65.090192)
        (xy 166.762329 65.126768)
        (xy 166.758999 68.74642)
        (xy 185.10914 68.732611)
      )
    )
  )
  (zone (net 139) (net_name "/PowerInput/VIN_FUSED") (layer "F.Cu") (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 168.758999 47.2455)
        (xy 162.058999 47.2455)
        (xy 162.058999 42.9955)
        (xy 168.758999 42.9955)
      )
    )
  )
  (zone (net 90) (net_name "+12V") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 177.634596 49.495498)
        (xy 177.634596 42.072256)
        (xy 183.444 42.072256)
        (xy 183.444 59.093921)
        (xy 150.755744 59.028304)
        (xy 150.755744 54.436)
        (xy 117.745488 54.427954)
        (xy 117.737 63.330802)
        (xy 115.832 63.351316)
        (xy 115.832 54.436)
        (xy 96.274 54.436)
        (xy 96.274 59.693)
        (xy 90.592614 59.693)
        (xy 90.592614 57.493)
        (xy 94.475221 57.493)
        (xy 94.475221 54.436)
        (xy 68.588 54.436)
        (xy 68.588 59.693)
        (xy 61.7835 59.693)
        (xy 61.7835 57.893)
        (xy 65.865559 57.893)
        (xy 65.865559 50.405254)
        (xy 154.694 50.405254)
        (xy 154.694035 53.228488)
        (xy 166.509008 53.234887)
        (xy 166.509004 49.495495)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F.Cu" "In1.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 288.544 -1.524)
        (xy -2.159 -1.524)
        (xy -2.159 105.283)
        (xy 288.671 105.283)
      )
    )
  )
  (zone (net 5) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 155.758999 66.7455)
        (xy 150.258999 66.7455)
        (xy 150.258999 63.9955)
        (xy 155.758999 63.9955)
      )
    )
  )
  (zone (net 31) (net_name "/LowVoltage/3V8_OUT") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 55.577799 69.980791)
        (xy 55.577799 64.480791)
        (xy 50.827799 64.480791)
        (xy 50.827799 76.980791)
        (xy 50.827799 81.980791)
        (xy 55.327799 81.980791)
        (xy 55.378233 76.24849)
        (xy 55.077799 74.980791)
        (xy 55.077799 71.230791)
      )
    )
  )
  (zone (net 94) (net_name "/PowerInput/VIN") (layer "F.Cu") (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 177.419 42.545)
        (xy 177.419 49.213)
        (xy 168.823 49.213)
        (xy 168.823 42.545)
      )
    )
  )
  (zone (net 16) (net_name "+3V3I") (layer "F.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.373999 75.693)
        (xy 181.5835 75.693)
        (xy 181.5835 71.828)
        (xy 186.373999 71.828)
      )
    )
  )
  (zone (net 16) (net_name "+3V3I") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 292.1835 106.893)
        (xy -3.4165 106.893)
        (xy -3.4165 -2.707)
        (xy 292.1835 -2.707)
      )
    )
  )
  (zone (net 5) (net_name "+5V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 166.759363 68.63384)
        (xy 166.758999 66.7455)
        (xy 150.258999 66.7455)
        (xy 150.258999 63.9955)
        (xy 166.889 63.9955)
        (xy 166.889 26.592)
        (xy 136.271 26.338)
        (xy 136.271 21.427207)
        (xy 170 21.502793)
        (xy 170 49.75)
        (xy 183.65 49.75)
        (xy 183.65 41.35)
        (xy 254 41.35)
        (xy 254 49.15)
        (xy 187.25 49.15)
        (xy 187.25 54)
        (xy 170 54)
        (xy 170 68.644414)
      )
    )
  )
  (zone (net 90) (net_name "+12V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 285.5 41.15)
        (xy 183.476 41.15)
        (xy 183.476 49.5)
        (xy 177.75 49.5)
        (xy 177.75 38)
        (xy 211.5 38)
        (xy 211.5 12.75)
        (xy 285.5 12.75)
      )
    )
  )
)
