(kicad_pcb (version 20210824) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J1-Pad1)")
  (net 2 "unconnected-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "unconnected-(J1-Pad4)")
  (net 5 "unconnected-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "unconnected-(J1-Pad7)")
  (net 8 "unconnected-(J1-Pad8)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 133.87 100.395)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "asdf_DRC_THThole_5.99.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x08" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_4020_10251Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 133.41 106.76 180)
    (descr "Resistor SMD 4020 (10251 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://datasheet.octopart.com/HVC0603T5004FET-Ohmite-datasheet-26699797.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "asdf_DRC_THThole_5.99.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 7.5 4.49) (layer "B.SilkS"))
    (fp_text value "2k2" (at 0 -3.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.8125 0 180) (size 1.475 5.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.169492)
      (net 3 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 4.8125 0 180) (size 1.475 5.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.169492)
      (net 6 "Net-(J1-Pad6)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_4020_10251Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 115 95) (end 150 95) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150 125) (end 115 125) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115 125) (end 115 95) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150 95) (end 150 125) (layer "Edge.Cuts") (width 0.1))
)
