(kicad_pcb (version 20220815) (generator pcbnew)
  (general
    (thickness 0)
  )
  (paper "A4")
  (title_block
    (rev "1")
    (company "Kicad Demo")
  )
  (layers
    (0 "F.Cu" signal "top_copper")
    (31 "B.Cu" signal "bottom_copper")
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001030_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (footprint "Diode_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (at 134.62 72.39 180)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "sonde xilinx.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.47 180) (layer "F.SilkS") hide)
    (fp_text value "BAT46" (at 3.81 2.47 180) (layer "F.Fab") hide)
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 119.5 69.1) (end 137.3 80.8)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 1) (net_name "Net-(D1-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.5 77.3)
        (xy 132.8 77)
        (xy 132.9 77.8)
        (xy 134.2 77.7)
        (xy 134.6 77.2)
        (xy 133.1 79.9)
        (xy 128.6 79.4)
        (xy 130.8 76.4)
      )
    )
    (polygon
      (pts
        (xy 131.962958 77.241665)
        (xy 132.01481 77.562503)
        (xy 132.754165 77.357194)
        (xy 132.622685 77.072469)
      )
    )
  )
  (zone (net 1) (net_name "Net-(D1-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.09101 76.812004)
        (xy 133.962002 76.812004)
        (xy 133.962002 74.636898)
        (xy 137.09101 74.636898)
      )
    )
  )
)
