(kicad_pcb
	(version 20240922)
	(generator "pcbnew")
	(generator_version "8.99")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top Layer")
		(4 "In1.Cu" signal "Inner 1")
		(6 "In2.Cu" signal "Inner 2")
		(2 "B.Cu" signal "Bottom Layer")
		(13 "F.Paste" user "Top Paste")
		(15 "B.Paste" user "Bottom Paste")
		(5 "F.SilkS" user "Top Overlay")
		(7 "B.SilkS" user "Bottom Overlay")
		(1 "F.Mask" user "Top Solder")
		(3 "B.Mask" user "Bottom Solder")
		(17 "Dwgs.User" user "Mechanical 10")
		(23 "Eco2.User" user "Mechanical 11")
		(35 "F.Fab" user "Mechanical 12")
		(33 "B.Fab" user "Mechanical 13")
		(39 "User.1" auxiliary "Mechanical 1")
		(41 "User.2" auxiliary "Mechanical 2")
		(43 "User.3" auxiliary "Mechanical 3")
		(45 "User.4" auxiliary "Mechanical 4")
		(47 "User.5" auxiliary "Mechanical 5")
		(49 "User.6" auxiliary "Mechanical 6")
		(51 "User.7" auxiliary "Mechanical 7")
		(53 "User.8" auxiliary "Mechanical 8")
		(55 "User.9" auxiliary "Mechanical 9")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 139.0396 112.0521)
		(grid_origin 139.0396 112.0521)
		(pcbplotparams
			(layerselection 0x55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(footprint ""
		(layer "F.Cu")
		(at 141.9606 108.3691)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "3" thru_hole rect
			(at 0 0)
			(size 0.762 0.762)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(padstack
				(mode custom)
				(layer "F.Cu"
					(shape rect)
					(size 0.762 0.762)
				)
				(layer "In1.Cu"
					(shape rect)
					(size 1.016 1.016)
				)
				(layer "In2.Cu"
					(shape rect)
					(size 1.27 -1.27)
				)
				(layer "B.Cu"
					(shape rect)
					(size 1.524 1.524)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.5956 101.6381)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 3.048 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape oval)
					(size 1.27 1.27)
				)
				(layer "B.Cu"
					(shape oval)
					(size 2.54 1.016)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 152.6286 101.8921)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "2" thru_hole rect
			(at 0 0)
			(size 0.762 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape roundrect)
					(size 1.016 1.016)
					(roundrect_rratio 0.25)
					(chamfer_ratio 0.25)
					(chamfer top_left top_right bottom_left bottom_right)
				)
				(layer "B.Cu"
					(shape roundrect)
					(size 1.27 0.635)
					(roundrect_rratio 0.25)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 151.1046 108.6231)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "4" thru_hole rect
			(at 0 0)
			(size 0.762 0.762)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(padstack
				(mode custom)
				(layer "F.Cu"
					(shape rect)
					(size 0.762 0.762)
				)
				(layer "In1.Cu"
					(shape rect)
					(size 1.016 1.016)
				)
				(layer "In2.Cu"
					(shape rect)
					(size 1.27 -1.27)
				)
				(layer "B.Cu"
					(shape rect)
					(size 1.524 1.524)
				)
			)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 139.0396 97.9551)
		(end 157.9626 97.9551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.9626 97.9551)
		(end 157.9626 112.0521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.0396 112.0521)
		(end 139.0396 97.9551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.9626 112.0521)
		(end 139.0396 112.0521)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
