(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(footprint "Connector_JAE:JAE_LY20-18P-DLT1_2x09_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 152 83)
		(descr "Molex LY 20 series connector, LY20-18P-DLT1, 9 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator")
		(tags "connector JAE  top entry")
		(property "Reference" "J2"
			(at 3.2 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "JAE_LY20-18P-DLT1_2x09_P2.00mm_Horizontal"
			(at 3.2 19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JAE:JAE_LY20-18P-DLT1_2x09_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.2 17.1 0)
			(layer "F.Fab")
		)
		(pad "a1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
		)
		(pad "a2" thru_hole trapezoid
			(at 0 2)
			(size 1.3 1.1)
			(rect_delta 0.2 0)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "a3" thru_hole roundrect
			(at 0 4)
			(size 1 1.2)
			(drill oval 0.4 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.16)
		)
		(pad "a4" thru_hole roundrect
			(at 0 6)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.3)
			(chamfer bottom_left bottom_right)
		)
		(pad "a5" thru_hole oval
			(at 0 8)
			(size 2 1.2)
			(drill 0.8
				(offset -0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "a6" thru_hole circle
			(at 0 10)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "a7" thru_hole circle
			(at 0 12)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "a8" thru_hole circle
			(at 0 14)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "a9" thru_hole circle
			(at 0 16)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b1" thru_hole oval
			(at 2 0)
			(size 2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b2" thru_hole trapezoid
			(at 2 2)
			(size 1.2 1.2)
			(rect_delta 0 0.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b3" thru_hole roundrect
			(at 2 4)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left)
		)
		(pad "b4" thru_hole roundrect
			(at 2 6)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.22)
			(chamfer_ratio 0.21)
			(chamfer top_left bottom_left)
		)
		(pad "b5" thru_hole roundrect
			(at 2 8)
			(size 1.2 1.2)
			(drill 0.8
				(offset 0.1 -0.15)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left)
		)
		(pad "b6" thru_hole circle
			(at 2 10)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b7" thru_hole circle
			(at 2 12)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b8" thru_hole circle
			(at 2 14)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "b9" thru_hole circle
			(at 2 16)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_LY20-18P-DLT1_2x09_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Samtec:Samtec_LSHM-105-xx.x-x-DV-S_2x05-1SH_P0.50mm_Vertical"
		(layer "F.Cu")
		(at 139 91 90)
		(descr "Molex LSHM 0.50 mm Razor Beam High-Speed Hermaphroditic Terminal/Socket Strip, LSHM-105-xx.x-x-DV-S, 5 Pins per row (http://suddendocs.samtec.com/prints/lshm-1xx-xx.x-x-dv-a-x-x-tr-footprint.pdf), generated with kicad-footprint-generator")
		(tags "connector Samtec  side entry")
		(property "Reference" "J1"
			(at 0 -3.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Samtec_LSHM-105-xx.x-x-DV-S_2x05-1SH_P0.50mm_Vertical"
			(at 0 3.8 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Samtec:Samtec_LSHM-105-xx.x-x-DV-S_2x05-1SH_P0.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.25 -0.85 90)
			(size 1.45 1.45)
			(drill 1.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.25 -0.85 90)
			(size 1.45 1.45)
			(drill 1.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1 -1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at -1 1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "3" smd rect
			(at -0.5 -1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at -0.5 1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at 0 -1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 0 1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "7" smd rect
			(at 0.5 -1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at 0.5 1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "9" smd rect
			(at 1 -1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "10" smd rect
			(at 1 1.85 90)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "SH" thru_hole circle
			(at -3.725 1.15 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "SH" thru_hole circle
			(at 3.725 1.15 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Samtec.3dshapes/Samtec_LSHM-105-xx.x-x-DV-S_2x05-1SH_P0.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
