(kicad_pcb (version 20210904) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 5.000000)
      (dashed_line_gap_ratio 3.000000)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+5V")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "/USB_D+")
  (net 5 "/USB_D-")
  (footprint "misc:USB_Micro-B" (layer "F.Cu")
    (tedit 61126B8C)
    (at 119.6 114 -90)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd allow_soldermask_bridges)
    (fp_text reference "J1" (at 0 -3.45 -90) (layer "F.SilkS"))
    (fp_text value "USB_B_Mini" (at 0 4.8 -90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.3009 -1.56254) (size 1.35 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V"))
    (pad "2" smd rect locked (at -0.6509 -1.56254) (size 1.35 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/USB_D-"))
    (pad "3" smd rect locked (at -0.0009 -1.56254) (size 1.35 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/USB_D+"))
    (pad "4" smd rect locked (at 0.6491 -1.56254) (size 1.35 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-Pad4)") (zone_connect 1) (thermal_bridge_width 1) (thermal_gap 0.2))
    (pad "5" smd rect locked (at 1.2991 -1.56254) (size 1.35 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (zone_connect 2))
    (pad "6" smd rect locked (at -3.75 1.15 270) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "6" smd rect locked (at 3.75 1.15 270) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "Connectors_Samtec:MECF-30-0_-L-DV_Edge" (layer "F.Cu")
    (tedit 61350C5C)
    (at 137.0584 131.4704)
    (descr "Highspeed card edge connector for PCB's with 30 contacts (polarized)")
    (tags "conn samtec card-edge high-speed")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "J1" (at 0 -2.3368) (layer "F.SilkS"))
    (fp_text value "MECF-30-0_-L-DV_Edge" (at 0 -3.81) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "F.Fab") hide)
    (pad "1" smd rect (at -18.405 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -18.405 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "3" smd rect (at -17.135 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at -17.135 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd rect (at -15.865 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at -15.865 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "7" smd rect (at -14.595 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "8" smd rect (at -14.595 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "9" smd rect (at -13.325 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "10" smd rect (at -13.325 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "11" smd rect (at -12.055 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "12" smd rect (at -12.055 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "13" smd rect (at -10.785 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "14" smd rect (at -10.785 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "15" smd rect (at -9.515 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "16" smd rect (at -9.515 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "17" smd rect (at -8.245 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "18" smd rect (at -8.245 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "19" smd rect (at -6.975 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "20" smd rect (at -6.975 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "23" smd rect (at -4.435 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "24" smd rect (at -4.435 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "25" smd rect (at -3.165 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "26" smd rect (at -3.165 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "27" smd rect (at -1.895 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "28" smd rect (at -1.895 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "29" smd rect (at -0.625 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "30" smd rect (at -0.625 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "31" smd rect (at 0.645 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "32" smd rect (at 0.645 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "33" smd rect (at 1.915 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "34" smd rect (at 1.915 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "35" smd rect (at 3.185 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "36" smd rect (at 3.185 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "37" smd rect (at 4.455 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "38" smd rect (at 4.455 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "39" smd rect (at 5.725 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "40" smd rect (at 5.725 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "41" smd rect (at 6.995 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "42" smd rect (at 6.995 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "43" smd rect (at 8.265 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "44" smd rect (at 8.265 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "45" smd rect (at 9.535 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "46" smd rect (at 9.535 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "47" smd rect (at 10.805 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "48" smd rect (at 10.805 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "49" smd rect (at 12.075 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "50" smd rect (at 12.075 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "51" smd rect (at 13.345 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "52" smd rect (at 13.345 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "53" smd rect (at 14.615 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "54" smd rect (at 14.615 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "55" smd rect (at 15.885 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "56" smd rect (at 15.885 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "57" smd rect (at 17.155 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "58" smd rect (at 17.155 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "59" smd rect (at 18.425 2.5) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "60" smd rect (at 18.425 2.5) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "Connectors_Samtec:MECF-05-0_-L-DV_Edge" (layer "F.Cu")
    (tedit 61350FA5)
    (at 152.4 106.0196 90)
    (descr "Highspeed card edge connector for PCB's with 05 contacts (polarized)")
    (tags "conn samtec card-edge high-speed")
    (attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
    (fp_text reference "J2" (at 0 -1.7272 90) (layer "F.SilkS"))
    (fp_text value "MECF-05-0_-L-DV_Edge" (at 0 -3.81 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.53 2.5 90) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -2.53 2.5 90) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd rect (at 0.01 2.5 90) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 0.01 2.5 90) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "7" smd rect (at 1.28 2.5 90) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "8" smd rect (at 1.28 2.5 90) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "9" smd rect (at 2.55 2.5 90) (size 0.56 4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "10" smd rect (at 2.55 2.5 90) (size 0.56 4) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (gr_line (start 157 98) (end 117 98)
    (layer "Edge.Cuts"))
  (gr_line (start 117 136) (end 157 136)
    (layer "Edge.Cuts"))
  (gr_line (start 117 98) (end 117 136)
    (layer "Edge.Cuts"))
  (gr_line (start 157 136) (end 157 98)
    (layer "Edge.Cuts"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 157 98) (xy 157 136))
    (height -1.9)
    (gr_text "38.0000  mm" (at 157.75 117 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 157 136) (xy 117 136))
    (height -1.3)
    (gr_text "40.0000  mm" (at 137 136.15) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 117 98)
        (xy 157 98)
        (xy 157 136)
        (xy 117 136)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 117 98)
        (xy 157 98)
        (xy 157 136)
        (xy 117 136)
      )
    )
  )
)
