(kicad_pcb
	(version 20240225)
	(generator "pcbnew")
	(generator_version "8.99")
	(general
		(thickness 0.2)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user "0.2mm_Polymid_Stiffener")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.11)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00713fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "P-${PROJECT_NUMBER}_${PROJECT_NAME}_${PROJECT_VERSION}_ID${PROJECT_ID}_FAB_OUTPUT")
		)
	)
	(net 0 "")
	(net 1 "/OUT_CAM0_SCL")
	(net 2 "GND")
	(net 3 "/SYNC_ZRGB")
	(footprint "Don-Con:FFC_Pads_01x22_P0.5mm_3mm-stiffener"
		(layer "F.Cu")
		(at 66.42 53.84)
		(property "Reference" "J?"
			(at 5.08 0.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "Vision_Module"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "16" smd rect
			(at 1.45 2.25)
			(size 2.5 0.25)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 2)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 1.45 2.75)
			(size 2.5 0.25)
			(layers "F.Cu")
			(net 3 "/SYNC_ZRGB")
			(pinfunction "Pin_17")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 2)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd rect
			(at 1.45 3.75)
			(size 2.5 0.25)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 2)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd rect
			(at 1.45 4.25)
			(size 2.5 0.25)
			(layers "F.Cu")
			(net 1 "/OUT_CAM0_SCL")
			(pinfunction "Pin_20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 2)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(gr_rect
		(start 62.82 49.49)
		(end 73.01 62.64)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "/OUT_CAM0_SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 69.37702 58.062083) (xy 69.351139 57.965492) (xy 69.12 57.965) (xy 67.869035 58.090258) (xy 69.12 58.151436)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/SYNC_ZRGB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 69.379867 56.553161) (xy 69.341599 56.460774) (xy 67.872416 56.465) (xy 67.869077 56.590382)
				(xy 69.12 56.645625)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 66.395255 57.695389) (xy 66.456131 57.774725) (xy 67.871046 57.715) (xy 67.870793 57.589392)
				(xy 66.62 57.589837)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 66.393659 56.299416) (xy 66.443659 56.386017) (xy 67.878815 56.215) (xy 67.870866 56.0895) (xy 66.62 56.180723)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/SYNC_ZRGB")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 66.364554 56.701366) (xy 66.390436 56.797958) (xy 67.875233 56.715) (xy 67.870965 56.589742)
				(xy 66.62 56.59798)
			)
		)
	)
)
