(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Test1")
  (net 2 "Test2")
  (net 3 "Test3")
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (at 153.75 83.55 180)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (property "Reference" "REF**" (at 0 2.54 0) (layer "B.SilkS"))
    (property "Value" "SolderWirePad_1x01_SMD_1x2mm" (at 0 -2.54 0) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Test3")
    )
  )
  (footprint "NetTie:NetTie-2_SMD_Pad0.5mm" (layer "B.Cu")
    (at 155.35 85.75 -90)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (property "Reference" "NT2" (at 0 1.2 90) (layer "B.SilkS") hide)
    (property "Value" "Net-Tie_2" (at 0 -1.2 90) (layer "B.Fab"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "Net tie, 2 pins" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "exclude_from_bom" "" (at 0 0 0) (layer "B.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (net_tie_pad_groups "1, 2")
    (pad "1" smd circle (at -0.5 0 270) (size 0.5 0.5) (layers "B.Cu")
      (net 1 "Test1") (pinfunction "1") (pintype "passive")
    )
    (pad "2" smd circle (at 0.5 0 270) (size 0.5 0.5) (layers "B.Cu")
      (net 2 "Test2") (pinfunction "2") (pintype "passive")
    )
  )
  (gr_rect (start 139.573 79.375) (end 163.957 93.091)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Otherwise" (at 155.194 89.281 0) (layer "B.Cu" knockout))
  (gr_text "What" (at 156.718 84.455 0) (layer "B.Cu"))
  (zone (net 2) (net_name "Test2") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.637 84.582)
        (xy 147.955 84.582)
        (xy 147.955 91.694)
        (xy 143.637 91.694)
      )
    )
  )
  (zone (net 3) (net_name "Test3") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 157.4 82.05)
        (xy 157.4 88.1)
        (xy 152.7 88.1)
        (xy 152.7 82.05)
      )
    )
  )
  (zone (net 3) (net_name "Test3") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.385 89.154)
        (xy 150.241 89.154)
        (xy 150.241 91.313)
        (xy 159.385 91.313)
      )
    )
  )
)
