(module Potentiometer_Single_Vertical (layer F.Cu) (tedit 5F79F6D8)
  (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
  (tags "potentiometer vertical 9mm single")
  (fp_text reference REF** (at 6.71 -4.64 180) (layer F.SilkS))
  (fp_text value Potentiometer_Single_Vertical (at 0 9.86 180) (layer F.Fab))
  (fp_text user %R (at 7.62 2.54) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad "" thru_hole oval (at 7.5 7.3 90) (size 2.72 4) (drill oval 1.1 2.2) (layers *.Cu *.Mask))
  (pad "" thru_hole oval (at 7.5 -2.3 90) (size 2.72 4) (drill oval 1.1 2.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
