(footprint "C2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Condensateur = 2 pas")
	(tags "C")
	(property "Reference" "REF**"
		(at -11.5 -15.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "R"
		(at -13.4 14 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" connect custom
		(at -11.081 -0.025 90)
		(size 1.397 1.397)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.5)
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance convexhull)
			(anchor rect)
		)
		(primitives
			(gr_line
				(start 6 1.9)
				(end 6 13.9)
				(width 2)
			)
			(gr_line
				(start -6 1.9)
				(end -6 13.9)
				(width 2)
			)
			(gr_line
				(start 0 -0.1)
				(end 0 18)
				(width 2)
			)
			(gr_arc
				(start -9.9 7.9)
				(mid -0.049149 -0.19988)
				(end 9.880067 7.803745)
				(width 2)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" connect custom
		(at 10.509 -0.025 270)
		(size 3 3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_line
				(start 3 0.5)
				(end 3 17)
				(width 2)
			)
			(gr_line
				(start -3 0.5)
				(end -3 17)
				(width 2)
			)
			(gr_arc
				(start -9.9 7.9)
				(mid -1.506614 -0.086997)
				(end 8.869415 5.068492)
				(width 2)
			)
			(gr_arc
				(start -15 7.9)
				(mid 0.011791 -5.232741)
				(end 15.003099 7.923378)
				(width 2)
			)
			(gr_line
				(start 0 0)
				(end 0 -5)
				(width 2)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "discret/capa_2pas_5x5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
