(footprint "DIP-14__300_ELL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14 pins DIL package, elliptical pads")
	(tags "DIL")
	(property "Reference" "REF**"
		(at -5.08 -1.27 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIP-14_300_ELL"
		(at 5.88 13.872 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole board_only)
	(pad "1" thru_hole rect
		(at -8.2 3.8)
		(size 1.5748 2.286)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole oval
		(at -5.08 3.81)
		(size 1.5748 2.286)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "3" thru_hole trapezoid
		(at -7.62 -3.81)
		(size 1.5748 2.286)
		(rect_delta 0 1)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "4" thru_hole oval
		(at -5.08 -3.81 30)
		(size 1.5748 2.286)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "5" connect custom
		(at 8 10)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance convexhull)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center 0 -10)
				(end 2.5 -10)
				(width 1)
				(fill no)
			)
			(gr_circle
				(center 0 -10)
				(end 5 -10)
				(width 1)
				(fill no)
			)
			(gr_circle
				(center 0 -10)
				(end 7.5 -10)
				(width 1)
				(fill no)
			)
			(gr_circle
				(center 0 -10)
				(end 10 -10)
				(width 1)
				(fill no)
			)
			(gr_line
				(start 0 0)
				(end 0 -7.5)
				(width 1)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "dil/dil_14.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
