(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "C"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C? C_????_* C_???? SMD*_c Capacitor*"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_1"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 2.032 0 0)
		)
		(property "Value" "CONN_1"
			(at 0 1.397 0)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 -1.27 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_1_0_1")
		(symbol "CONN_1_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "CP"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "cap capacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP_*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECC83"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.302 7.874 0)
		)
		(property "Value" "ECC83"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" "VALVE-NOVAL_P"
			(at 10.16 -8.89 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "ECC83_0_1")
		(symbol "ECC83_1_0")
		(symbol "ECC83_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "7")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "8")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "ECC83_2_0")
		(symbol "ECC83_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "ECC83_3_1"
			(pin input line
				(at -2.54 -11.43 90)
				(length 5.08)
				(name "F1")
				(number "4")
			)
			(pin input line
				(at 0 -11.43 90)
				(length 5.08)
				(name "F2")
				(number "9")
			)
			(pin input line
				(at 2.54 -11.43 90)
				(length 5.08)
				(name "F1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -6.35 0)
		)
		(property "Value" "GND"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_* Resistor_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
)
