(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Hybrid Switched capacitor converter, 28 to 700 V")
		(date "2023-05-02")
		(company "U.S. Department of Energy, Office of Scientific and Technical Information")
		(comment 1 "https://www.osti.gov/servlets/purl/1497233")
	)
	(lib_symbols
		(symbol "DIODE_1"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "DIODE_1"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode, anode on pin 1, for simulation only!"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "D"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "DIODE_1_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy 1.27 0) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "DIODE_1_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "K")
					(number "2")
				)
			)
		)
		(symbol "DIODE_2"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "DIODE_2"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode, anode on pin 1, for simulation only!"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "D"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "DIODE_2_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy 1.27 0) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "DIODE_2_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "K")
					(number "2")
				)
			)
		)
		(symbol "DIODE_3"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "DIODE_3"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode, anode on pin 1, for simulation only!"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "D"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "DIODE_3_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy 1.27 0) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "DIODE_3_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "K")
					(number "2")
				)
			)
		)
		(symbol "DIODE_4"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "DIODE_4"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode, anode on pin 1, for simulation only!"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "D"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "DIODE_4_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy 1.27 0) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "DIODE_4_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "K")
					(number "2")
				)
			)
		)
		(symbol "DIODE_5"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "DIODE_5"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode, anode on pin 1, for simulation only!"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "D"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "DIODE_5_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27) (xy 1.27 0) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "DIODE_5_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "K")
					(number "2")
				)
			)
		)
		(symbol "Device:C_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "capacitor cap"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_Small_0_1"
				(polyline
					(pts
						(xy -1.524 -0.508) (xy 1.524 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.524 0.508) (xy 1.524 0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 2.032)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.032)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:L_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 0.762 1.016 0)
			)
			(property "Value" "L_Small"
				(at 0.762 -1.016 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_Small_0_1"
				(arc
					(start 0 -2.032)
					(mid 0.5058 -1.524)
					(end 0 -1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.016)
					(mid 0.5058 -0.508)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.5058 0.508)
					(end 0 1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.016)
					(mid 0.5058 1.524)
					(end 0 2.032)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.508)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.508)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:Q_NMOS_GDS"
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.27 0)
			)
			(property "Value" "Q_NMOS_GDS"
				(at 5.08 -1.27 0)
			)
			(property "Footprint" ""
				(at 5.08 2.54 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "N-MOSFET transistor, gate/drain/source"
				(at 0 0 0)
			)
			(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
				(at 0 0 0)
			)
			(symbol "Q_NMOS_GDS_0_1"
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.778) (xy 3.302 -1.778) (xy 3.302 1.778) (xy 0.762 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 0) (xy 2.032 0.381) (xy 2.032 -0.381) (xy 1.016 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 2.921 0.381) (xy 3.683 0.381) (xy 3.81 0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 0.381) (xy 2.921 -0.254) (xy 3.683 -0.254) (xy 3.302 0.381)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
			)
			(symbol "Q_NMOS_GDS_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D")
					(number "2")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S")
					(number "3")
				)
			)
		)
		(symbol "Device:R_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 0.762 0.508 0)
			)
			(property "Value" "R_Small"
				(at 0.762 -1.016 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "R resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_Small_0_1"
				(rectangle
					(start -0.762 1.778)
					(end 0.762 -1.778)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.762)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.762)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Simulation_SPICE:VPULSE"
			(pin_numbers hide)
			(pin_names
				(offset 0.0254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "V"
				(at 2.54 2.54 0)
			)
			(property "Value" "VPULSE"
				(at 2.54 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Voltage source, pulse"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "V"
				(at 0 0 0)
			)
			(property "Spice_Model" "pulse(0 1 2n 2n 2n 50n 100n)"
				(at 2.54 -2.54 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "VPULSE_0_0"
				(polyline
					(pts
						(xy -2.032 -0.762) (xy -1.397 -0.762) (xy -1.143 0.762) (xy -0.127 0.762) (xy 0.127 -0.762) (xy 1.143 -0.762)
						(xy 1.397 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 0 1.905 0)
				)
			)
			(symbol "VPULSE_0_1"
				(circle
					(center 0 0)
					(radius 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "VPULSE_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "pspice:0"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#GND"
				(at 0 -2.54 0)
			)
			(property "Value" "0"
				(at 0 -1.778 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "0V reference potential for simulation"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "0_0_1"
				(polyline
					(pts
						(xy -1.27 0) (xy 0 -1.27) (xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "0_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 0) hide
					(name "0")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 217.932 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 134.112 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.992 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.992 84.328)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 176.022 108.204)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 84.328)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 233.172 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.454 108.204)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.454 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.142 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.142 108.204)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.574 108.204)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 176.022 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.574 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 134.112 84.328)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 105.156 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 229.87 108.204) (xy 220.726 108.204)
		)
	)
	(wire
		(pts
			(xy 68.072 129.286) (xy 68.072 134.366)
		)
	)
	(wire
		(pts
			(xy 233.172 104.648) (xy 233.172 108.712)
		)
	)
	(wire
		(pts
			(xy 120.142 108.204) (xy 133.35 108.204)
		)
	)
	(wire
		(pts
			(xy 229.87 96.52) (xy 229.87 108.204)
		)
	)
	(wire
		(pts
			(xy 81.28 102.362) (xy 97.536 102.362)
		)
	)
	(wire
		(pts
			(xy 147.574 96.52) (xy 147.574 108.204)
		)
	)
	(wire
		(pts
			(xy 147.574 96.52) (xy 151.638 96.52)
		)
	)
	(wire
		(pts
			(xy 166.878 108.204) (xy 176.022 108.204)
		)
	)
	(wire
		(pts
			(xy 217.932 84.328) (xy 217.932 96.52)
		)
	)
	(wire
		(pts
			(xy 229.87 96.52) (xy 233.172 96.52)
		)
	)
	(wire
		(pts
			(xy 162.56 84.328) (xy 162.56 96.52)
		)
	)
	(wire
		(pts
			(xy 147.574 108.204) (xy 161.798 108.204)
		)
	)
	(wire
		(pts
			(xy 162.56 84.328) (xy 172.72 84.328)
		)
	)
	(wire
		(pts
			(xy 242.57 96.52) (xy 242.57 99.314)
		)
	)
	(wire
		(pts
			(xy 242.57 104.394) (xy 242.57 108.712)
		)
	)
	(wire
		(pts
			(xy 177.8 84.328) (xy 189.992 84.328)
		)
	)
	(wire
		(pts
			(xy 176.022 108.204) (xy 189.23 108.204)
		)
	)
	(wire
		(pts
			(xy 189.992 96.52) (xy 193.802 96.52)
		)
	)
	(wire
		(pts
			(xy 203.454 96.52) (xy 207.518 96.52)
		)
	)
	(wire
		(pts
			(xy 187.706 96.52) (xy 189.992 96.52)
		)
	)
	(wire
		(pts
			(xy 176.022 96.52) (xy 180.086 96.52)
		)
	)
	(wire
		(pts
			(xy 131.572 96.52) (xy 134.112 96.52)
		)
	)
	(wire
		(pts
			(xy 145.542 96.52) (xy 147.574 96.52)
		)
	)
	(wire
		(pts
			(xy 120.142 108.204) (xy 120.142 111.252)
		)
	)
	(wire
		(pts
			(xy 84.836 96.52) (xy 86.614 96.52)
		)
	)
	(wire
		(pts
			(xy 120.142 116.332) (xy 120.142 120.396)
		)
	)
	(wire
		(pts
			(xy 227.838 96.52) (xy 229.87 96.52)
		)
	)
	(wire
		(pts
			(xy 91.694 96.52) (xy 105.156 96.52)
		)
	)
	(wire
		(pts
			(xy 189.992 84.328) (xy 200.152 84.328)
		)
	)
	(wire
		(pts
			(xy 162.56 96.52) (xy 166.37 96.52)
		)
	)
	(wire
		(pts
			(xy 134.112 96.52) (xy 137.922 96.52)
		)
	)
	(wire
		(pts
			(xy 149.352 84.328) (xy 162.56 84.328)
		)
	)
	(wire
		(pts
			(xy 138.43 108.204) (xy 147.574 108.204)
		)
	)
	(wire
		(pts
			(xy 134.112 84.328) (xy 134.112 96.52)
		)
	)
	(wire
		(pts
			(xy 68.072 96.52) (xy 79.756 96.52)
		)
	)
	(wire
		(pts
			(xy 173.99 96.52) (xy 176.022 96.52)
		)
	)
	(wire
		(pts
			(xy 121.92 84.328) (xy 134.112 84.328)
		)
	)
	(wire
		(pts
			(xy 189.992 84.328) (xy 189.992 96.52)
		)
	)
	(wire
		(pts
			(xy 159.258 96.52) (xy 162.56 96.52)
		)
	)
	(wire
		(pts
			(xy 68.072 119.126) (xy 68.072 96.52)
		)
	)
	(wire
		(pts
			(xy 105.156 96.52) (xy 105.156 97.282)
		)
	)
	(wire
		(pts
			(xy 205.232 84.328) (xy 217.932 84.328)
		)
	)
	(wire
		(pts
			(xy 176.022 96.52) (xy 176.022 108.204)
		)
	)
	(wire
		(pts
			(xy 116.586 96.52) (xy 120.142 96.52)
		)
	)
	(wire
		(pts
			(xy 215.138 96.52) (xy 217.932 96.52)
		)
	)
	(wire
		(pts
			(xy 105.156 84.328) (xy 116.84 84.328)
		)
	)
	(wire
		(pts
			(xy 203.454 108.204) (xy 215.646 108.204)
		)
	)
	(wire
		(pts
			(xy 134.112 84.328) (xy 144.272 84.328)
		)
	)
	(wire
		(pts
			(xy 105.156 84.328) (xy 105.156 96.52)
		)
	)
	(wire
		(pts
			(xy 81.28 120.396) (xy 81.28 123.444)
		)
	)
	(wire
		(pts
			(xy 217.932 96.52) (xy 220.218 96.52)
		)
	)
	(wire
		(pts
			(xy 201.422 96.52) (xy 203.454 96.52)
		)
	)
	(wire
		(pts
			(xy 105.156 107.442) (xy 105.156 112.522)
		)
	)
	(wire
		(pts
			(xy 120.142 96.52) (xy 123.952 96.52)
		)
	)
	(wire
		(pts
			(xy 81.28 110.236) (xy 81.28 102.362)
		)
	)
	(wire
		(pts
			(xy 233.172 96.52) (xy 233.172 99.568)
		)
	)
	(wire
		(pts
			(xy 233.172 96.52) (xy 242.57 96.52)
		)
	)
	(wire
		(pts
			(xy 120.142 96.52) (xy 120.142 108.204)
		)
	)
	(wire
		(pts
			(xy 194.31 108.204) (xy 203.454 108.204)
		)
	)
	(wire
		(pts
			(xy 105.156 96.52) (xy 108.966 96.52)
		)
	)
	(wire
		(pts
			(xy 203.454 96.52) (xy 203.454 108.204)
		)
	)
	(text "Power supply is ramped\nto reduce initial current surge"
		(exclude_from_sim no)
		(at 72.39 132.588 0)
	)
	(text "Hybrid switched capacitor converter HSCC\n28 V to 700 V\nhttps://www.osti.gov/servlets/purl/1497233"
		(exclude_from_sim no)
		(at 65.786 81.534 0)
	)
	(text ".tran 200n 120m\n.option chgtol=1e-11 reltol=0.01 method=gear\n"
		(exclude_from_sim no)
		(at 148.59 164.592 0)
	)
	(label "pwr"
		(at 69.342 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d4"
		(at 165.1 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d6"
		(at 192.532 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d7"
		(at 204.47 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d5"
		(at 177.038 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d2"
		(at 136.652 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d8"
		(at 219.456 96.52 0)
		(fields_autoplaced yes)
	)
	(label "g"
		(at 86.106 102.362 0)
		(fields_autoplaced yes)
	)
	(label "d"
		(at 101.6 96.52 0)
		(fields_autoplaced yes)
	)
	(label "out"
		(at 236.982 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d3"
		(at 148.59 96.52 0)
		(fields_autoplaced yes)
	)
	(label "d1"
		(at 122.428 96.52 0)
		(fields_autoplaced yes)
	)
	(symbol
		(lib_name "DIODE_5")
		(lib_id "Simulation_SPICE:DIODE")
		(at 127.762 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 127.762 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 127.762 92.71 0)
		)
		(property "Footprint" ""
			(at 127.762 96.52 0)
		)
		(property "Datasheet" "~"
			(at 127.762 96.52 0)
		)
		(property "Description" ""
			(at 127.762 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 127.762 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 127.762 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_4")
		(lib_id "Simulation_SPICE:DIODE")
		(at 197.612 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D7"
			(at 197.612 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 197.612 92.71 0)
		)
		(property "Footprint" ""
			(at 197.612 96.52 0)
		)
		(property "Datasheet" "~"
			(at 197.612 96.52 0)
		)
		(property "Description" ""
			(at 197.612 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 197.612 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 197.612 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 146.812 84.328 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C4"
			(at 146.8183 77.47 90)
		)
		(property "Value" "1u"
			(at 146.8183 80.01 90)
		)
		(property "Footprint" ""
			(at 146.812 84.328 0)
		)
		(property "Datasheet" "~"
			(at 146.812 84.328 0)
		)
		(property "Description" ""
			(at 146.812 84.328 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_4")
		(lib_id "Simulation_SPICE:DIODE")
		(at 170.18 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D5"
			(at 170.18 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 170.18 92.71 0)
		)
		(property "Footprint" ""
			(at 170.18 96.52 0)
		)
		(property "Datasheet" "~"
			(at 170.18 96.52 0)
		)
		(property "Description" ""
			(at 170.18 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 170.18 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 170.18 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 164.338 108.204 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C5"
			(at 164.3443 101.6 90)
		)
		(property "Value" "1u"
			(at 164.3443 104.14 90)
		)
		(property "Footprint" ""
			(at 164.338 108.204 0)
		)
		(property "Datasheet" "~"
			(at 164.338 108.204 0)
		)
		(property "Description" ""
			(at 164.338 108.204 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_3")
		(lib_id "Simulation_SPICE:DIODE")
		(at 183.896 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D6"
			(at 183.896 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 183.896 92.71 0)
		)
		(property "Footprint" ""
			(at 183.896 96.52 0)
		)
		(property "Datasheet" "~"
			(at 183.896 96.52 0)
		)
		(property "Description" ""
			(at 183.896 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 183.896 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 183.896 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 119.38 84.328 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 119.3863 77.47 90)
		)
		(property "Value" "1u"
			(at 119.3863 80.01 90)
		)
		(property "Footprint" ""
			(at 119.38 84.328 0)
		)
		(property "Datasheet" "~"
			(at 119.38 84.328 0)
		)
		(property "Description" ""
			(at 119.38 84.328 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 242.57 108.712 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND06"
			(at 242.57 111.252 0)
		)
		(property "Value" "0"
			(at 242.57 106.172 0)
		)
		(property "Footprint" ""
			(at 242.57 108.712 0)
		)
		(property "Datasheet" "~"
			(at 242.57 108.712 0)
		)
		(property "Description" ""
			(at 242.57 108.712 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_2")
		(lib_id "Simulation_SPICE:DIODE")
		(at 224.028 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D9"
			(at 224.028 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 224.028 92.71 0)
		)
		(property "Footprint" ""
			(at 224.028 96.52 0)
		)
		(property "Datasheet" "~"
			(at 224.028 96.52 0)
		)
		(property "Description" ""
			(at 224.028 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 224.028 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 224.028 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 135.89 108.204 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 135.8963 101.6 90)
		)
		(property "Value" "1u"
			(at 135.8963 104.14 90)
		)
		(property "Footprint" ""
			(at 135.89 108.204 0)
		)
		(property "Datasheet" "~"
			(at 135.89 108.204 0)
		)
		(property "Description" ""
			(at 135.89 108.204 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_1")
		(lib_id "Simulation_SPICE:DIODE")
		(at 112.776 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 112.776 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 112.776 92.71 0)
		)
		(property "Footprint" ""
			(at 112.776 96.52 0)
		)
		(property "Datasheet" "~"
			(at 112.776 96.52 0)
		)
		(property "Description" ""
			(at 112.776 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 112.776 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 112.776 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_3")
		(lib_id "Simulation_SPICE:DIODE")
		(at 211.328 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D8"
			(at 211.328 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 211.328 92.71 0)
		)
		(property "Footprint" ""
			(at 211.328 96.52 0)
		)
		(property "Datasheet" "~"
			(at 211.328 96.52 0)
		)
		(property "Description" ""
			(at 211.328 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 211.328 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 211.328 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 218.186 108.204 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 218.1923 101.6 90)
		)
		(property "Value" "1u"
			(at 218.1923 104.14 90)
		)
		(property "Footprint" ""
			(at 218.186 108.204 0)
		)
		(property "Datasheet" "~"
			(at 218.186 108.204 0)
		)
		(property "Description" ""
			(at 218.186 108.204 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 89.154 96.52 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RESR1"
			(at 89.154 90.17 90)
		)
		(property "Value" "230m"
			(at 89.154 92.71 90)
		)
		(property "Footprint" ""
			(at 89.154 96.52 0)
		)
		(property "Datasheet" "~"
			(at 89.154 96.52 0)
		)
		(property "Description" ""
			(at 89.154 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "RESR1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 242.57 101.854 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 245.11 100.5839 0)
		)
		(property "Value" "R = 'TIME > 70m ? 10k : 25k'"
			(at 213.614 113.284 0)
		)
		(property "Footprint" ""
			(at 242.57 101.854 0)
		)
		(property "Datasheet" "~"
			(at 242.57 101.854 0)
		)
		(property "Description" ""
			(at 242.57 101.854 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 233.172 108.712 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND05"
			(at 233.172 111.252 0)
		)
		(property "Value" "0"
			(at 233.172 106.172 0)
		)
		(property "Footprint" ""
			(at 233.172 108.712 0)
		)
		(property "Datasheet" "~"
			(at 233.172 108.712 0)
		)
		(property "Description" ""
			(at 233.172 108.712 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L_Small")
		(at 82.296 96.52 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L1"
			(at 82.296 91.44 90)
		)
		(property "Value" "22u"
			(at 82.296 93.98 90)
		)
		(property "Footprint" ""
			(at 82.296 96.52 0)
		)
		(property "Datasheet" "~"
			(at 82.296 96.52 0)
		)
		(property "Description" ""
			(at 82.296 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Q_NMOS_GDS")
		(at 102.616 102.362 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 108.204 101.0919 0)
		)
		(property "Value" "GS-065-018"
			(at 108.204 103.6319 0)
		)
		(property "Footprint" ""
			(at 107.696 99.822 0)
		)
		(property "Datasheet" "~"
			(at 102.616 102.362 0)
		)
		(property "Description" ""
			(at 102.616 102.362 0)
		)
		(property "Sim.Library" "GaN_PSpice_GS-065-018-2-L_L1V3P3.lib"
			(at 102.616 102.362 0)
		)
		(property "Sim.Name" "GaN_PSpice_GS-065-018-2-L_L1V3P3"
			(at 102.616 102.362 0)
		)
		(property "Sim.Pins" "1=1 2=2 3=3 3=4"
			(at 102.616 102.362 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Simulation_SPICE:VPULSE")
		(at 68.072 124.206 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "V1"
			(at 72.39 121.4761 0)
		)
		(property "Value" "VPULSE"
			(at 72.39 124.0161 0)
		)
		(property "Footprint" ""
			(at 68.072 124.206 0)
		)
		(property "Datasheet" "~"
			(at 68.072 124.206 0)
		)
		(property "Description" ""
			(at 68.072 124.206 0)
		)
		(property "Sim.Device" "V"
			(at 68.072 124.206 0)
		)
		(property "Sim.Type" "PULSE"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=28 td=1m tr=2m tf=1m tw=1 per=1"
			(at 72.39 126.5561 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "V1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 175.26 84.328 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C6"
			(at 175.2663 77.47 90)
		)
		(property "Value" "1u"
			(at 175.2663 80.01 90)
		)
		(property "Footprint" ""
			(at 175.26 84.328 0)
		)
		(property "Datasheet" "~"
			(at 175.26 84.328 0)
		)
		(property "Description" ""
			(at 175.26 84.328 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 120.142 113.792 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 123.444 112.5282 0)
		)
		(property "Value" "1u"
			(at 123.444 115.0682 0)
		)
		(property "Footprint" ""
			(at 120.142 113.792 0)
		)
		(property "Datasheet" "~"
			(at 120.142 113.792 0)
		)
		(property "Description" ""
			(at 120.142 113.792 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 120.142 120.396 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND04"
			(at 120.142 122.936 0)
		)
		(property "Value" "0"
			(at 120.142 117.856 0)
		)
		(property "Footprint" ""
			(at 120.142 120.396 0)
		)
		(property "Datasheet" "~"
			(at 120.142 120.396 0)
		)
		(property "Description" ""
			(at 120.142 120.396 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 81.28 123.444 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND02"
			(at 81.28 125.984 0)
		)
		(property "Value" "0"
			(at 81.28 120.904 0)
		)
		(property "Footprint" ""
			(at 81.28 123.444 0)
		)
		(property "Datasheet" "~"
			(at 81.28 123.444 0)
		)
		(property "Description" ""
			(at 81.28 123.444 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 191.77 108.204 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C7"
			(at 191.7763 101.6 90)
		)
		(property "Value" "1u"
			(at 191.7763 104.14 90)
		)
		(property "Footprint" ""
			(at 191.77 108.204 0)
		)
		(property "Datasheet" "~"
			(at 191.77 108.204 0)
		)
		(property "Description" ""
			(at 191.77 108.204 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_4")
		(lib_id "Simulation_SPICE:DIODE")
		(at 141.732 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D3"
			(at 141.732 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 141.732 92.71 0)
		)
		(property "Footprint" ""
			(at 141.732 96.52 0)
		)
		(property "Datasheet" "~"
			(at 141.732 96.52 0)
		)
		(property "Description" ""
			(at 141.732 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 141.732 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 141.732 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Simulation_SPICE:VPULSE")
		(at 81.28 115.316 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "V2"
			(at 85.09 112.5861 0)
		)
		(property "Value" "VPULSE"
			(at 85.09 115.1261 0)
		)
		(property "Footprint" ""
			(at 81.28 115.316 0)
		)
		(property "Datasheet" "~"
			(at 81.28 115.316 0)
		)
		(property "Description" ""
			(at 81.28 115.316 0)
		)
		(property "Sim.Device" "V"
			(at 81.28 115.316 0)
		)
		(property "Sim.Type" "PULSE"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=6 td=1m tr=20n tf=20n tw=2u per=4u"
			(at 85.09 117.6661 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "V2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 105.156 112.522 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND03"
			(at 105.156 115.062 0)
		)
		(property "Value" "0"
			(at 105.156 109.982 0)
		)
		(property "Footprint" ""
			(at 105.156 112.522 0)
		)
		(property "Datasheet" "~"
			(at 105.156 112.522 0)
		)
		(property "Description" ""
			(at 105.156 112.522 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "DIODE_3")
		(lib_id "Simulation_SPICE:DIODE")
		(at 155.448 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D4"
			(at 155.448 90.17 0)
		)
		(property "Value" "STPSC5H12D"
			(at 155.448 92.71 0)
		)
		(property "Footprint" ""
			(at 155.448 96.52 0)
		)
		(property "Datasheet" "~"
			(at 155.448 96.52 0)
		)
		(property "Description" ""
			(at 155.448 96.52 0)
		)
		(property "Sim.Library" "ST_SILICON_CARBIDE_SCHOTTKY_V9.LIB"
			(at 155.448 96.52 0)
		)
		(property "Sim.Name" "STPSC5H12D"
			(at 155.448 96.52 0)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 233.172 102.108 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C10"
			(at 236.22 100.8442 0)
		)
		(property "Value" "1u"
			(at 236.22 103.3842 0)
		)
		(property "Footprint" ""
			(at 233.172 102.108 0)
		)
		(property "Datasheet" "~"
			(at 233.172 102.108 0)
		)
		(property "Description" ""
			(at 233.172 102.108 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 202.692 84.328 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C8"
			(at 202.6983 77.47 90)
		)
		(property "Value" "1u"
			(at 202.6983 80.01 90)
		)
		(property "Footprint" ""
			(at 202.692 84.328 0)
		)
		(property "Datasheet" "~"
			(at 202.692 84.328 0)
		)
		(property "Description" ""
			(at 202.692 84.328 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pspice:0")
		(at 68.072 134.366 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#GND01"
			(at 68.072 136.906 0)
		)
		(property "Value" "0"
			(at 68.072 131.826 0)
		)
		(property "Footprint" ""
			(at 68.072 134.366 0)
		)
		(property "Datasheet" "~"
			(at 68.072 134.366 0)
		)
		(property "Description" ""
			(at 68.072 134.366 0)
		)
		(pin "1")
		(instances
			(project "HSCConverter4_load"
				(path
					(reference "#GND01")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)