(footprint "CP_Elec_6.3x11_Board_Edge_Mirrored"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3 5.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "330uF 10V"
		(at -0.7 -6 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" "Not Populated"
		(at 155 -80 0)
		(layer "B.Fab")
		(hide yes)
	)
	(property "exclude_from_bom" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0.95 -5.95 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" connect roundrect
		(at 1.25 2.25 180)
		(size 1.5 4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.333)
	)
	(pad "2" connect roundrect
		(at -1.25 2.25 180)
		(size 1.5 4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.333)
	)
	(embedded_fonts no)
	(model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Radial_D6.3mm_H11.0mm_P2.50mm.wrl"
		(offset
			(xyz 1.25 0 0.35)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -180 0)
		)
	)
)
