(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "VME P0 connector fanout + mechanics")
	)
	(lib_symbols
		(symbol "HARTING:HARTING_17_25_095_2102"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 3.81 1.27 0)
			)
			(property "Value" "HARTING_17_25_095_2102"
				(at 0 -52.705 0)
			)
			(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
				(at 0 -54.61 0)
			)
			(property "Datasheet" ""
				(at 0 -56.515 0)
			)
			(property "Description" "HAR-BUS HM Type B19"
				(at 3.81 -0.762 0)
			)
			(property "Part Number" "HARTING_17_25_095_2102"
				(at 0 -58.42 0)
			)
			(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
				(at 0 -60.325 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -62.23 0)
			)
			(property "Comment" " "
				(at 0 -64.135 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -66.04 0)
			)
			(property "Component Type" "Standard"
				(at 0 -67.945 0)
			)
			(property "PackageDescription" " "
				(at 0 -69.85 0)
			)
			(property "Pin Count" "105"
				(at 0 -71.755 0)
			)
			(property "Case" " "
				(at 0 -73.66 0)
			)
			(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
				(at 0 -75.565 0)
			)
			(property "Footprint Ref" "HARTING_17 25 095 2102"
				(at 0 -77.47 0)
			)
			(property "Family" "HAR-BUS HM Type B19"
				(at 0 -79.375 0)
			)
			(property "Mounted" "Yes"
				(at 0 -81.28 0)
			)
			(property "Socket" "No"
				(at 0 -83.185 0)
			)
			(property "SMD" "No"
				(at 0 -85.09 0)
			)
			(property "PressFit" "Yes"
				(at 0 -86.995 0)
			)
			(property "Sense" "No"
				(at 0 -88.9 0)
			)
			(property "Sense Comment" " "
				(at 0 -90.805 0)
			)
			(property "Status" "None"
				(at 0 -92.71 0)
			)
			(property "Status Comment" " "
				(at 0 -94.615 0)
			)
			(property "SCEM" " "
				(at 0 -96.52 0)
			)
			(property "Device" " "
				(at 0 -98.425 0)
			)
			(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
				(at 0 -100.33 0)
			)
			(property "Manufacturer" "HARTING"
				(at 0 -102.235 0)
			)
			(property "Manufacturer Part Number" "17 25 095 2102"
				(at 0 -104.14 0)
			)
			(property "ComponentHeight" "7.57mm"
				(at 0 -106.045 0)
			)
			(property "HelpURL" ""
				(at 0 -107.95 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -109.855 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -111.76 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -113.665 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -115.57 0)
			)
			(property "Author" "CERN DEM JMW"
				(at 0 -117.475 0)
			)
			(property "CreateDate" "05/28/08 00:00:00"
				(at 0 -119.38 0)
			)
			(property "LatestRevisionDate" "06/18/14 00:00:00"
				(at 0 -121.285 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -123.19 0)
			)
			(property "Library Name" "HARTING"
				(at 0 -125.095 0)
			)
			(property "Footprint Library" "HARTING THD"
				(at 0 -127 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -128.905 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "HARTING_17_25_095_2102_1_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -38.1) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -40.64) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -43.18) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -45.72) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -48.26) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -25.4) (xy 2.54 -25.8064) (xy 3.1242 -26.162) (xy 3.81 -26.162)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -27.94) (xy 2.54 -28.3464) (xy 3.1242 -28.702) (xy 3.81 -28.702)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -30.48) (xy 2.54 -30.8864) (xy 3.1242 -31.242) (xy 3.81 -31.242)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -33.02) (xy 2.54 -33.4264) (xy 3.1242 -33.782) (xy 3.81 -33.782)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -35.56) (xy 2.54 -35.9664) (xy 3.1242 -36.322) (xy 3.81 -36.322)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -38.1) (xy 2.54 -38.5064) (xy 3.1242 -38.862) (xy 3.81 -38.862)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -40.64) (xy 2.54 -41.0464) (xy 3.1242 -41.402) (xy 3.81 -41.402)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -43.18) (xy 2.54 -43.5864) (xy 3.1242 -43.942) (xy 3.81 -43.942)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -45.72) (xy 2.54 -46.1264) (xy 3.1242 -46.482) (xy 3.81 -46.482)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -48.26) (xy 2.54 -48.6664) (xy 3.1242 -49.022) (xy 3.81 -49.022)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -24.638) (xy 3.1242 -24.638) (xy 2.54 -24.9936) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -27.178) (xy 3.1242 -27.178) (xy 2.54 -27.5336) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -29.718) (xy 3.1242 -29.718) (xy 2.54 -30.0736) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -32.258) (xy 3.1242 -32.258) (xy 2.54 -32.6136) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -34.798) (xy 3.1242 -34.798) (xy 2.54 -35.1536) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -37.338) (xy 3.1242 -37.338) (xy 2.54 -37.6936) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -39.878) (xy 3.1242 -39.878) (xy 2.54 -40.2336) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -42.418) (xy 3.1242 -42.418) (xy 2.54 -42.7736) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -44.958) (xy 3.1242 -44.958) (xy 2.54 -45.3136) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -47.498) (xy 3.1242 -47.498) (xy 2.54 -47.8536) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "A1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "A2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "A3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "A4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "A5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "A6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "A7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "A8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "A9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "A10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "A11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "A12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "A13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "A14")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "A15")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "16")
					(number "A16")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "A17")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "18")
					(number "A18")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "A19")
				)
			)
			(symbol "HARTING_17_25_095_2102_2_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -38.1) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -40.64) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -43.18) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -45.72) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -48.26) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -25.4) (xy 2.54 -25.8064) (xy 3.1242 -26.162) (xy 3.81 -26.162)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -27.94) (xy 2.54 -28.3464) (xy 3.1242 -28.702) (xy 3.81 -28.702)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -30.48) (xy 2.54 -30.8864) (xy 3.1242 -31.242) (xy 3.81 -31.242)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -33.02) (xy 2.54 -33.4264) (xy 3.1242 -33.782) (xy 3.81 -33.782)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -35.56) (xy 2.54 -35.9664) (xy 3.1242 -36.322) (xy 3.81 -36.322)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -38.1) (xy 2.54 -38.5064) (xy 3.1242 -38.862) (xy 3.81 -38.862)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -40.64) (xy 2.54 -41.0464) (xy 3.1242 -41.402) (xy 3.81 -41.402)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -43.18) (xy 2.54 -43.5864) (xy 3.1242 -43.942) (xy 3.81 -43.942)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -45.72) (xy 2.54 -46.1264) (xy 3.1242 -46.482) (xy 3.81 -46.482)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -48.26) (xy 2.54 -48.6664) (xy 3.1242 -49.022) (xy 3.81 -49.022)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -24.638) (xy 3.1242 -24.638) (xy 2.54 -24.9936) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -27.178) (xy 3.1242 -27.178) (xy 2.54 -27.5336) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -29.718) (xy 3.1242 -29.718) (xy 2.54 -30.0736) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -32.258) (xy 3.1242 -32.258) (xy 2.54 -32.6136) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -34.798) (xy 3.1242 -34.798) (xy 2.54 -35.1536) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -37.338) (xy 3.1242 -37.338) (xy 2.54 -37.6936) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -39.878) (xy 3.1242 -39.878) (xy 2.54 -40.2336) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -42.418) (xy 3.1242 -42.418) (xy 2.54 -42.7736) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -44.958) (xy 3.1242 -44.958) (xy 2.54 -45.3136) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -47.498) (xy 3.1242 -47.498) (xy 2.54 -47.8536) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "B1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "B2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "B3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "B4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "B5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "B6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "B7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "B8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "B9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "B10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "B11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "B12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "B13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "B14")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "B15")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "16")
					(number "B16")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "B17")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "18")
					(number "B18")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "B19")
				)
			)
			(symbol "HARTING_17_25_095_2102_3_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -38.1) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -40.64) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -43.18) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -45.72) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -48.26) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -25.4) (xy 2.54 -25.8064) (xy 3.1242 -26.162) (xy 3.81 -26.162)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -27.94) (xy 2.54 -28.3464) (xy 3.1242 -28.702) (xy 3.81 -28.702)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -30.48) (xy 2.54 -30.8864) (xy 3.1242 -31.242) (xy 3.81 -31.242)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -33.02) (xy 2.54 -33.4264) (xy 3.1242 -33.782) (xy 3.81 -33.782)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -35.56) (xy 2.54 -35.9664) (xy 3.1242 -36.322) (xy 3.81 -36.322)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -38.1) (xy 2.54 -38.5064) (xy 3.1242 -38.862) (xy 3.81 -38.862)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -40.64) (xy 2.54 -41.0464) (xy 3.1242 -41.402) (xy 3.81 -41.402)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -43.18) (xy 2.54 -43.5864) (xy 3.1242 -43.942) (xy 3.81 -43.942)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -45.72) (xy 2.54 -46.1264) (xy 3.1242 -46.482) (xy 3.81 -46.482)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -48.26) (xy 2.54 -48.6664) (xy 3.1242 -49.022) (xy 3.81 -49.022)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -24.638) (xy 3.1242 -24.638) (xy 2.54 -24.9936) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -27.178) (xy 3.1242 -27.178) (xy 2.54 -27.5336) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -29.718) (xy 3.1242 -29.718) (xy 2.54 -30.0736) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -32.258) (xy 3.1242 -32.258) (xy 2.54 -32.6136) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -34.798) (xy 3.1242 -34.798) (xy 2.54 -35.1536) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -37.338) (xy 3.1242 -37.338) (xy 2.54 -37.6936) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -39.878) (xy 3.1242 -39.878) (xy 2.54 -40.2336) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -42.418) (xy 3.1242 -42.418) (xy 2.54 -42.7736) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -44.958) (xy 3.1242 -44.958) (xy 2.54 -45.3136) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -47.498) (xy 3.1242 -47.498) (xy 2.54 -47.8536) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "C1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "C2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "C3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "C4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "C5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "C6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "C7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "C8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "C9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "C10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "C11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "C12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "C13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "C14")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "C15")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "16")
					(number "C16")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "C17")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "18")
					(number "C18")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "C19")
				)
			)
			(symbol "HARTING_17_25_095_2102_4_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -38.1) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -40.64) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -43.18) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -45.72) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -48.26) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -25.4) (xy 2.54 -25.8064) (xy 3.1242 -26.162) (xy 3.81 -26.162)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -27.94) (xy 2.54 -28.3464) (xy 3.1242 -28.702) (xy 3.81 -28.702)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -30.48) (xy 2.54 -30.8864) (xy 3.1242 -31.242) (xy 3.81 -31.242)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -33.02) (xy 2.54 -33.4264) (xy 3.1242 -33.782) (xy 3.81 -33.782)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -35.56) (xy 2.54 -35.9664) (xy 3.1242 -36.322) (xy 3.81 -36.322)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -38.1) (xy 2.54 -38.5064) (xy 3.1242 -38.862) (xy 3.81 -38.862)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -40.64) (xy 2.54 -41.0464) (xy 3.1242 -41.402) (xy 3.81 -41.402)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -43.18) (xy 2.54 -43.5864) (xy 3.1242 -43.942) (xy 3.81 -43.942)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -45.72) (xy 2.54 -46.1264) (xy 3.1242 -46.482) (xy 3.81 -46.482)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -48.26) (xy 2.54 -48.6664) (xy 3.1242 -49.022) (xy 3.81 -49.022)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -24.638) (xy 3.1242 -24.638) (xy 2.54 -24.9936) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -27.178) (xy 3.1242 -27.178) (xy 2.54 -27.5336) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -29.718) (xy 3.1242 -29.718) (xy 2.54 -30.0736) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -32.258) (xy 3.1242 -32.258) (xy 2.54 -32.6136) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -34.798) (xy 3.1242 -34.798) (xy 2.54 -35.1536) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -37.338) (xy 3.1242 -37.338) (xy 2.54 -37.6936) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -39.878) (xy 3.1242 -39.878) (xy 2.54 -40.2336) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -42.418) (xy 3.1242 -42.418) (xy 2.54 -42.7736) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -44.958) (xy 3.1242 -44.958) (xy 2.54 -45.3136) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -47.498) (xy 3.1242 -47.498) (xy 2.54 -47.8536) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "D1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "D2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "D3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "D4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "D5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "D6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "D7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "D8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "D9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "D10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "D11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "D12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "D13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "D14")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "D15")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "16")
					(number "D16")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "D17")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "18")
					(number "D18")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "D19")
				)
			)
			(symbol "HARTING_17_25_095_2102_5_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -38.1) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -40.64) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -43.18) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -45.72) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -48.26) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -25.4) (xy 2.54 -25.8064) (xy 3.1242 -26.162) (xy 3.81 -26.162)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -27.94) (xy 2.54 -28.3464) (xy 3.1242 -28.702) (xy 3.81 -28.702)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -30.48) (xy 2.54 -30.8864) (xy 3.1242 -31.242) (xy 3.81 -31.242)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -33.02) (xy 2.54 -33.4264) (xy 3.1242 -33.782) (xy 3.81 -33.782)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -35.56) (xy 2.54 -35.9664) (xy 3.1242 -36.322) (xy 3.81 -36.322)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -38.1) (xy 2.54 -38.5064) (xy 3.1242 -38.862) (xy 3.81 -38.862)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -40.64) (xy 2.54 -41.0464) (xy 3.1242 -41.402) (xy 3.81 -41.402)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -43.18) (xy 2.54 -43.5864) (xy 3.1242 -43.942) (xy 3.81 -43.942)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -45.72) (xy 2.54 -46.1264) (xy 3.1242 -46.482) (xy 3.81 -46.482)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -48.26) (xy 2.54 -48.6664) (xy 3.1242 -49.022) (xy 3.81 -49.022)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -24.638) (xy 3.1242 -24.638) (xy 2.54 -24.9936) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -27.178) (xy 3.1242 -27.178) (xy 2.54 -27.5336) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -29.718) (xy 3.1242 -29.718) (xy 2.54 -30.0736) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -32.258) (xy 3.1242 -32.258) (xy 2.54 -32.6136) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -34.798) (xy 3.1242 -34.798) (xy 2.54 -35.1536) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -37.338) (xy 3.1242 -37.338) (xy 2.54 -37.6936) (xy 2.54 -38.1)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -39.878) (xy 3.1242 -39.878) (xy 2.54 -40.2336) (xy 2.54 -40.64)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -42.418) (xy 3.1242 -42.418) (xy 2.54 -42.7736) (xy 2.54 -43.18)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -44.958) (xy 3.1242 -44.958) (xy 2.54 -45.3136) (xy 2.54 -45.72)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -47.498) (xy 3.1242 -47.498) (xy 2.54 -47.8536) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "E1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "E2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "E3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "E4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "E5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "E6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "E7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "E8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "E9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "E10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "E11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "E12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "E13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "E14")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "E15")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "16")
					(number "E16")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "E17")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "18")
					(number "E18")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "E19")
				)
			)
			(symbol "HARTING_17_25_095_2102_6_1"
				(rectangle
					(start 0 -50.8)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 -48.26)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -2.54)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -7.62) (xy 0 -7.62)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -7.62)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -12.7) (xy 0 -12.7)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -12.7)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -17.78) (xy 0 -17.78)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -17.78)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -22.86) (xy 0 -22.86)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -22.86)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -27.94) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -27.94)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -33.02) (xy 0 -33.02)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -33.02)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -38.1) (xy 0 -38.1)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -38.1)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -43.18) (xy 0 -43.18)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -43.18)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -48.26) (xy 0 -48.26)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -48.26)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -1.27) (xy 6.35 -1.27)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.54 -2.54)
					(mid 2.912 -1.642)
					(end 3.81 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.81 -49.53)
					(mid 2.912 -49.158)
					(end 2.54 -48.26)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -49.53) (xy 6.35 -49.53)
					)
					(fill
						(type none)
					)
				)
				(text "Shield"
					(at 4.826 -25.4 900)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "F1")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "F3")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "F5")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "F7")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "F9")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "F11")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "F13")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "15")
					(number "F15")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "17")
					(number "F17")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "19")
					(number "F19")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "FIXME: row F is missing, importer fup?"
		(exclude_from_sim no)
		(at 191.516 119.38 0)
	)
	(text "VME P0"
		(exclude_from_sim no)
		(at 212.852 104.14 0)
	)
	(junction
		(at 106.68 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 127 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 295.91 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 337.82 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 275.59 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 64.77 165.1)
	)
	(no_connect
		(at 64.77 167.64)
	)
	(no_connect
		(at 64.77 154.94)
	)
	(no_connect
		(at 170.18 168.91)
	)
	(no_connect
		(at 208.28 151.13)
	)
	(no_connect
		(at 208.28 173.99)
	)
	(no_connect
		(at 208.28 143.51)
	)
	(no_connect
		(at 105.41 153.67)
	)
	(no_connect
		(at 208.28 128.27)
	)
	(no_connect
		(at 208.28 148.59)
	)
	(no_connect
		(at 170.18 148.59)
	)
	(no_connect
		(at 208.28 163.83)
	)
	(no_connect
		(at 208.28 130.81)
	)
	(no_connect
		(at 170.18 156.21)
	)
	(no_connect
		(at 64.77 147.32)
	)
	(no_connect
		(at 170.18 158.75)
	)
	(no_connect
		(at 208.28 153.67)
	)
	(no_connect
		(at 64.77 152.4)
	)
	(no_connect
		(at 64.77 172.72)
	)
	(no_connect
		(at 64.77 157.48)
	)
	(no_connect
		(at 274.32 153.67)
	)
	(no_connect
		(at 208.28 140.97)
	)
	(no_connect
		(at 170.18 153.67)
	)
	(no_connect
		(at 170.18 173.99)
	)
	(no_connect
		(at 208.28 158.75)
	)
	(no_connect
		(at 105.41 148.59)
	)
	(no_connect
		(at 170.18 163.83)
	)
	(no_connect
		(at 170.18 166.37)
	)
	(no_connect
		(at 208.28 138.43)
	)
	(no_connect
		(at 208.28 168.91)
	)
	(no_connect
		(at 208.28 161.29)
	)
	(no_connect
		(at 208.28 166.37)
	)
	(no_connect
		(at 208.28 135.89)
	)
	(no_connect
		(at 64.77 149.86)
	)
	(no_connect
		(at 105.41 151.13)
	)
	(no_connect
		(at 274.32 151.13)
	)
	(no_connect
		(at 64.77 160.02)
	)
	(no_connect
		(at 170.18 171.45)
	)
	(no_connect
		(at 170.18 151.13)
	)
	(no_connect
		(at 208.28 156.21)
	)
	(no_connect
		(at 170.18 161.29)
	)
	(no_connect
		(at 208.28 171.45)
	)
	(no_connect
		(at 64.77 170.18)
	)
	(no_connect
		(at 208.28 146.05)
	)
	(no_connect
		(at 208.28 133.35)
	)
	(no_connect
		(at 274.32 148.59)
	)
	(no_connect
		(at 64.77 162.56)
	)
	(bus_entry
		(at 83.82 144.78)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 135.89)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 130.81)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 146.05)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 146.05)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 143.51)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 133.35)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 128.27)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 146.05)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 138.43)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 130.81)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 137.16)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 130.81)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 128.27)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 139.7)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 143.51)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 142.24)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 129.54)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 143.51)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 138.43)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 140.97)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 135.89)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 124.46 140.97)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 132.08)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 138.43)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 134.62)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 140.97)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 83.82 127)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 128.27)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 133.35)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 293.37 135.89)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 189.23 133.35)
		(size 2.54 -2.54)
	)
	(wire
		(pts
			(xy 337.82 134.62) (xy 337.82 139.7)
		)
	)
	(bus
		(pts
			(xy 191.77 128.27) (xy 191.77 130.81)
		)
	)
	(bus
		(pts
			(xy 127 140.97) (xy 127 143.51)
		)
	)
	(wire
		(pts
			(xy 337.82 154.94) (xy 337.82 160.02)
		)
	)
	(wire
		(pts
			(xy 64.77 139.7) (xy 83.82 139.7)
		)
	)
	(bus
		(pts
			(xy 191.77 138.43) (xy 191.77 140.97)
		)
	)
	(bus
		(pts
			(xy 295.91 140.97) (xy 295.91 138.43)
		)
	)
	(bus
		(pts
			(xy 295.91 130.81) (xy 295.91 128.27)
		)
	)
	(wire
		(pts
			(xy 274.32 168.91) (xy 297.18 168.91)
		)
	)
	(bus
		(pts
			(xy 86.36 139.7) (xy 86.36 142.24)
		)
	)
	(bus
		(pts
			(xy 295.91 138.43) (xy 295.91 135.89)
		)
	)
	(wire
		(pts
			(xy 105.41 156.21) (xy 128.27 156.21)
		)
	)
	(wire
		(pts
			(xy 105.41 130.81) (xy 124.46 130.81)
		)
	)
	(wire
		(pts
			(xy 105.41 171.45) (xy 128.27 171.45)
		)
	)
	(bus
		(pts
			(xy 127 128.27) (xy 127 130.81)
		)
	)
	(wire
		(pts
			(xy 274.32 158.75) (xy 297.18 158.75)
		)
	)
	(bus
		(pts
			(xy 127 123.19) (xy 127 125.73)
		)
	)
	(bus
		(pts
			(xy 191.77 140.97) (xy 191.77 143.51)
		)
	)
	(wire
		(pts
			(xy 64.77 144.78) (xy 83.82 144.78)
		)
	)
	(bus
		(pts
			(xy 127 125.73) (xy 127 128.27)
		)
	)
	(bus
		(pts
			(xy 127 123.19) (xy 86.36 123.19)
		)
	)
	(wire
		(pts
			(xy 337.82 165.1) (xy 337.82 170.18)
		)
	)
	(wire
		(pts
			(xy 274.32 130.81) (xy 293.37 130.81)
		)
	)
	(wire
		(pts
			(xy 64.77 132.08) (xy 83.82 132.08)
		)
	)
	(bus
		(pts
			(xy 127 138.43) (xy 127 140.97)
		)
	)
	(wire
		(pts
			(xy 274.32 163.83) (xy 275.59 163.83)
		)
	)
	(bus
		(pts
			(xy 295.91 143.51) (xy 295.91 140.97)
		)
	)
	(bus
		(pts
			(xy 127 133.35) (xy 127 135.89)
		)
	)
	(wire
		(pts
			(xy 105.41 143.51) (xy 124.46 143.51)
		)
	)
	(wire
		(pts
			(xy 105.41 161.29) (xy 128.27 161.29)
		)
	)
	(wire
		(pts
			(xy 170.18 146.05) (xy 189.23 146.05)
		)
	)
	(wire
		(pts
			(xy 274.32 166.37) (xy 297.18 166.37)
		)
	)
	(wire
		(pts
			(xy 337.82 129.54) (xy 337.82 134.62)
		)
	)
	(wire
		(pts
			(xy 274.32 156.21) (xy 297.18 156.21)
		)
	)
	(wire
		(pts
			(xy 106.68 163.83) (xy 106.68 173.99)
		)
	)
	(bus
		(pts
			(xy 86.36 134.62) (xy 86.36 137.16)
		)
	)
	(bus
		(pts
			(xy 86.36 123.19) (xy 86.36 124.46)
		)
	)
	(wire
		(pts
			(xy 274.32 140.97) (xy 293.37 140.97)
		)
	)
	(wire
		(pts
			(xy 105.41 146.05) (xy 124.46 146.05)
		)
	)
	(wire
		(pts
			(xy 337.82 144.78) (xy 337.82 149.86)
		)
	)
	(wire
		(pts
			(xy 105.41 140.97) (xy 124.46 140.97)
		)
	)
	(wire
		(pts
			(xy 274.32 135.89) (xy 293.37 135.89)
		)
	)
	(wire
		(pts
			(xy 170.18 138.43) (xy 189.23 138.43)
		)
	)
	(wire
		(pts
			(xy 337.82 139.7) (xy 337.82 144.78)
		)
	)
	(wire
		(pts
			(xy 105.41 166.37) (xy 128.27 166.37)
		)
	)
	(wire
		(pts
			(xy 105.41 168.91) (xy 128.27 168.91)
		)
	)
	(bus
		(pts
			(xy 86.36 137.16) (xy 86.36 139.7)
		)
	)
	(wire
		(pts
			(xy 170.18 143.51) (xy 189.23 143.51)
		)
	)
	(bus
		(pts
			(xy 295.91 135.89) (xy 295.91 133.35)
		)
	)
	(wire
		(pts
			(xy 275.59 163.83) (xy 275.59 173.99)
		)
	)
	(bus
		(pts
			(xy 191.77 125.73) (xy 191.77 128.27)
		)
	)
	(bus
		(pts
			(xy 191.77 133.35) (xy 191.77 135.89)
		)
	)
	(wire
		(pts
			(xy 337.82 149.86) (xy 337.82 154.94)
		)
	)
	(bus
		(pts
			(xy 191.77 123.19) (xy 191.77 125.73)
		)
	)
	(wire
		(pts
			(xy 105.41 158.75) (xy 128.27 158.75)
		)
	)
	(bus
		(pts
			(xy 295.91 125.73) (xy 295.91 123.19)
		)
	)
	(bus
		(pts
			(xy 295.91 133.35) (xy 295.91 130.81)
		)
	)
	(bus
		(pts
			(xy 191.77 130.81) (xy 191.77 133.35)
		)
	)
	(wire
		(pts
			(xy 105.41 133.35) (xy 124.46 133.35)
		)
	)
	(bus
		(pts
			(xy 295.91 128.27) (xy 295.91 125.73)
		)
	)
	(bus
		(pts
			(xy 86.36 129.54) (xy 86.36 132.08)
		)
	)
	(wire
		(pts
			(xy 170.18 135.89) (xy 189.23 135.89)
		)
	)
	(wire
		(pts
			(xy 274.32 128.27) (xy 293.37 128.27)
		)
	)
	(wire
		(pts
			(xy 64.77 137.16) (xy 83.82 137.16)
		)
	)
	(bus
		(pts
			(xy 191.77 135.89) (xy 191.77 138.43)
		)
	)
	(wire
		(pts
			(xy 105.41 138.43) (xy 124.46 138.43)
		)
	)
	(wire
		(pts
			(xy 274.32 138.43) (xy 293.37 138.43)
		)
	)
	(wire
		(pts
			(xy 274.32 143.51) (xy 293.37 143.51)
		)
	)
	(wire
		(pts
			(xy 274.32 173.99) (xy 275.59 173.99)
		)
	)
	(wire
		(pts
			(xy 64.77 127) (xy 83.82 127)
		)
	)
	(wire
		(pts
			(xy 274.32 133.35) (xy 293.37 133.35)
		)
	)
	(bus
		(pts
			(xy 86.36 132.08) (xy 86.36 134.62)
		)
	)
	(bus
		(pts
			(xy 86.36 124.46) (xy 86.36 127)
		)
	)
	(wire
		(pts
			(xy 274.32 161.29) (xy 297.18 161.29)
		)
	)
	(bus
		(pts
			(xy 127 130.81) (xy 127 133.35)
		)
	)
	(bus
		(pts
			(xy 191.77 123.19) (xy 127 123.19)
		)
	)
	(wire
		(pts
			(xy 64.77 129.54) (xy 83.82 129.54)
		)
	)
	(bus
		(pts
			(xy 127 135.89) (xy 127 138.43)
		)
	)
	(wire
		(pts
			(xy 105.41 128.27) (xy 124.46 128.27)
		)
	)
	(wire
		(pts
			(xy 274.32 171.45) (xy 297.18 171.45)
		)
	)
	(wire
		(pts
			(xy 337.82 170.18) (xy 337.82 175.26)
		)
	)
	(wire
		(pts
			(xy 105.41 163.83) (xy 106.68 163.83)
		)
	)
	(wire
		(pts
			(xy 170.18 128.27) (xy 189.23 128.27)
		)
	)
	(wire
		(pts
			(xy 337.82 160.02) (xy 337.82 165.1)
		)
	)
	(wire
		(pts
			(xy 337.82 175.26) (xy 337.82 181.61)
		)
	)
	(bus
		(pts
			(xy 86.36 127) (xy 86.36 129.54)
		)
	)
	(wire
		(pts
			(xy 64.77 142.24) (xy 83.82 142.24)
		)
	)
	(wire
		(pts
			(xy 274.32 146.05) (xy 293.37 146.05)
		)
	)
	(wire
		(pts
			(xy 170.18 140.97) (xy 189.23 140.97)
		)
	)
	(wire
		(pts
			(xy 105.41 173.99) (xy 106.68 173.99)
		)
	)
	(bus
		(pts
			(xy 295.91 123.19) (xy 191.77 123.19)
		)
	)
	(wire
		(pts
			(xy 64.77 134.62) (xy 83.82 134.62)
		)
	)
	(wire
		(pts
			(xy 170.18 130.81) (xy 189.23 130.81)
		)
	)
	(wire
		(pts
			(xy 105.41 135.89) (xy 124.46 135.89)
		)
	)
	(wire
		(pts
			(xy 275.59 173.99) (xy 275.59 180.34)
		)
	)
	(wire
		(pts
			(xy 170.18 133.35) (xy 189.23 133.35)
		)
	)
	(wire
		(pts
			(xy 106.68 173.99) (xy 106.68 180.34)
		)
	)
	(bus
		(pts
			(xy 295.91 123.19) (xy 355.6 123.19)
		)
	)
	(label "LVDS_TURNCLK1_N"
		(at 107.95 158.75 0)
	)
	(label "HWBYTE.L1_2"
		(at 67.31 132.08 0)
	)
	(label "LVDS_BUNCHCLK1_N"
		(at 107.95 168.91 0)
	)
	(label "HWBYTE.L2_3"
		(at 172.72 135.89 0)
	)
	(label "HWBYTE.H2_4"
		(at 276.86 138.43 0)
	)
	(label "HWBYTE.H2_7"
		(at 276.86 146.05 0)
	)
	(label "HWBYTE.H2_0"
		(at 276.86 128.27 0)
	)
	(label "HWBYTE.H1_3"
		(at 107.95 135.89 0)
	)
	(label "{HWBYTE}"
		(at 331.47 123.19 0)
	)
	(label "HWBYTE.H1_5"
		(at 107.95 140.97 0)
	)
	(label "HWBYTE.L2_1"
		(at 172.72 130.81 0)
	)
	(label "LVDS_TURNCLK1_P"
		(at 107.95 156.21 0)
	)
	(label "LVDS_BUNCHCLK2_P"
		(at 276.86 166.37 0)
	)
	(label "LVDS_BUNCHCLK1_P"
		(at 107.95 166.37 0)
	)
	(label "HWBYTE.L2_6"
		(at 172.72 143.51 0)
	)
	(label "HWBYTE.H2_5"
		(at 276.86 140.97 0)
	)
	(label "TTL_TURNCLK2"
		(at 276.86 161.29 0)
	)
	(label "HWBYTE.L1_6"
		(at 67.31 142.24 0)
	)
	(label "HWBYTE.L1_4"
		(at 67.31 137.16 0)
	)
	(label "HWBYTE.L1_1"
		(at 67.31 129.54 0)
	)
	(label "HWBYTE.L1_0"
		(at 67.31 127 0)
	)
	(label "HWBYTE.H2_3"
		(at 276.86 135.89 0)
	)
	(label "HWBYTE.H2_6"
		(at 276.86 143.51 0)
	)
	(label "HWBYTE.H1_2"
		(at 107.95 133.35 0)
	)
	(label "HWBYTE.H2_2"
		(at 276.86 133.35 0)
	)
	(label "HWBYTE.L2_7"
		(at 172.72 146.05 0)
	)
	(label "HWBYTE.H1_1"
		(at 107.95 130.81 0)
	)
	(label "HWBYTE.H1_6"
		(at 107.95 143.51 0)
	)
	(label "LVDS_BUNCHCLK2_N"
		(at 276.86 168.91 0)
	)
	(label "HWBYTE.H1_7"
		(at 107.95 146.05 0)
	)
	(label "HWBYTE.H1_4"
		(at 107.95 138.43 0)
	)
	(label "HWBYTE.L2_0"
		(at 172.72 128.27 0)
	)
	(label "TTL_TURNCLK1"
		(at 107.95 161.29 0)
	)
	(label "TTL_BUNCHCLK1"
		(at 107.95 171.45 0)
	)
	(label "TTL_BUNCHCLK2"
		(at 276.86 171.45 0)
	)
	(label "LVDS_TURNCLK2_P"
		(at 276.86 156.21 0)
	)
	(label "LVDS_TURNCLK2_N"
		(at 276.86 158.75 0)
	)
	(label "HWBYTE.H2_1"
		(at 276.86 130.81 0)
	)
	(label "HWBYTE.L2_2"
		(at 172.72 133.35 0)
	)
	(label "HWBYTE.L1_5"
		(at 67.31 139.7 0)
	)
	(label "HWBYTE.L1_3"
		(at 67.31 134.62 0)
	)
	(label "HWBYTE.H1_0"
		(at 107.95 128.27 0)
	)
	(label "HWBYTE.L2_4"
		(at 172.72 138.43 0)
	)
	(label "HWBYTE.L2_5"
		(at 172.72 140.97 0)
	)
	(label "HWBYTE.L1_7"
		(at 67.31 144.78 0)
	)
	(hierarchical_label "LVDS_TURNCLK1_N"
		(shape input)
		(at 128.27 158.75 0)
	)
	(hierarchical_label "TTL_TURNCLK2"
		(shape input)
		(at 297.18 161.29 0)
	)
	(hierarchical_label "LVDS_TURNCLK2_P"
		(shape input)
		(at 297.18 156.21 0)
	)
	(hierarchical_label "TTL_TURNCLK1"
		(shape input)
		(at 128.27 161.29 0)
	)
	(hierarchical_label "LVDS_BUNCHCLK2_P"
		(shape input)
		(at 297.18 166.37 0)
	)
	(hierarchical_label "{HWBYTE}"
		(shape bidirectional)
		(at 355.6 123.19 0)
	)
	(hierarchical_label "LVDS_BUNCHCLK2_N"
		(shape input)
		(at 297.18 168.91 0)
	)
	(hierarchical_label "TTL_BUNCHCLK2"
		(shape input)
		(at 297.18 171.45 0)
	)
	(hierarchical_label "LVDS_TURNCLK1_P"
		(shape input)
		(at 128.27 156.21 0)
	)
	(hierarchical_label "LVDS_BUNCHCLK1_P"
		(shape input)
		(at 128.27 166.37 0)
	)
	(hierarchical_label "TTL_BUNCHCLK1"
		(shape input)
		(at 128.27 171.45 0)
	)
	(hierarchical_label "LVDS_BUNCHCLK1_N"
		(shape input)
		(at 128.27 168.91 0)
	)
	(hierarchical_label "LVDS_TURNCLK2_N"
		(shape input)
		(at 297.18 158.75 0)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 100.33 176.53 180)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 96.5835 123.19 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 100.33 123.825 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 100.33 121.92 0)
		)
		(property "Datasheet" ""
			(at 100.33 120.015 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 96.52 175.768 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 100.33 118.11 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 100.33 116.205 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 100.33 114.3 0)
		)
		(property "Comment" " "
			(at 100.33 112.395 0)
		)
		(property "Component Kind" "Standard"
			(at 100.33 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 100.33 108.585 0)
		)
		(property "PackageDescription" " "
			(at 100.33 106.68 0)
		)
		(property "Pin Count" "105"
			(at 100.33 104.775 0)
		)
		(property "Case" " "
			(at 100.33 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 100.33 100.965 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 100.33 99.06 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 100.33 97.155 0)
		)
		(property "Mounted" "Yes"
			(at 100.33 95.25 0)
		)
		(property "Socket" "No"
			(at 100.33 93.345 0)
		)
		(property "SMD" "No"
			(at 100.33 91.44 0)
		)
		(property "PressFit" "Yes"
			(at 100.33 89.535 0)
		)
		(property "Sense" "No"
			(at 100.33 87.63 0)
		)
		(property "Sense Comment" " "
			(at 100.33 85.725 0)
		)
		(property "Status" "None"
			(at 100.33 83.82 0)
		)
		(property "Status Comment" " "
			(at 100.33 81.915 0)
		)
		(property "SCEM" " "
			(at 100.33 80.01 0)
		)
		(property "Device" " "
			(at 100.33 78.105 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 100.33 76.2 0)
		)
		(property "Manufacturer" "HARTING"
			(at 100.33 74.295 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 100.33 72.39 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 100.33 70.485 0)
		)
		(property "HelpURL" ""
			(at 100.33 68.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 100.33 66.675 0)
		)
		(property "ComponentLink1Description" " "
			(at 100.33 64.77 0)
		)
		(property "ComponentLink2URL" " "
			(at 100.33 62.865 0)
		)
		(property "ComponentLink2Description" " "
			(at 100.33 60.96 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 100.33 59.055 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 100.33 57.15 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 100.33 55.245 0)
		)
		(property "Database Table Name" "Connectors"
			(at 100.33 53.34 0)
		)
		(property "Library Name" "HARTING"
			(at 100.33 51.435 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 100.33 49.53 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 100.33 47.625 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 165.1 176.53 180)
		(unit 4)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 161.3535 123.19 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 165.1 123.825 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 165.1 121.92 0)
		)
		(property "Datasheet" ""
			(at 165.1 120.015 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 161.29 175.768 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 165.1 118.11 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 165.1 116.205 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 165.1 114.3 0)
		)
		(property "Comment" " "
			(at 165.1 112.395 0)
		)
		(property "Component Kind" "Standard"
			(at 165.1 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 165.1 108.585 0)
		)
		(property "PackageDescription" " "
			(at 165.1 106.68 0)
		)
		(property "Pin Count" "105"
			(at 165.1 104.775 0)
		)
		(property "Case" " "
			(at 165.1 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 165.1 100.965 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 165.1 99.06 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 165.1 97.155 0)
		)
		(property "Mounted" "Yes"
			(at 165.1 95.25 0)
		)
		(property "Socket" "No"
			(at 165.1 93.345 0)
		)
		(property "SMD" "No"
			(at 165.1 91.44 0)
		)
		(property "PressFit" "Yes"
			(at 165.1 89.535 0)
		)
		(property "Sense" "No"
			(at 165.1 87.63 0)
		)
		(property "Sense Comment" " "
			(at 165.1 85.725 0)
		)
		(property "Status" "None"
			(at 165.1 83.82 0)
		)
		(property "Status Comment" " "
			(at 165.1 81.915 0)
		)
		(property "SCEM" " "
			(at 165.1 80.01 0)
		)
		(property "Device" " "
			(at 165.1 78.105 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 165.1 76.2 0)
		)
		(property "Manufacturer" "HARTING"
			(at 165.1 74.295 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 165.1 72.39 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 165.1 70.485 0)
		)
		(property "HelpURL" ""
			(at 165.1 68.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 165.1 66.675 0)
		)
		(property "ComponentLink1Description" " "
			(at 165.1 64.77 0)
		)
		(property "ComponentLink2URL" " "
			(at 165.1 62.865 0)
		)
		(property "ComponentLink2Description" " "
			(at 165.1 60.96 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 165.1 59.055 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 165.1 57.15 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 165.1 55.245 0)
		)
		(property "Database Table Name" "Connectors"
			(at 165.1 53.34 0)
		)
		(property "Library Name" "HARTING"
			(at 165.1 51.435 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 165.1 49.53 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 165.1 47.625 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 4)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 275.59 180.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0689"
			(at 275.59 186.69 0)
		)
		(property "Value" "GND"
			(at 275.59 185.42 0)
		)
		(property "Footprint" ""
			(at 275.59 180.34 0)
		)
		(property "Datasheet" ""
			(at 275.59 180.34 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 275.59 180.34 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0689")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 106.68 180.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0688"
			(at 106.68 186.69 0)
		)
		(property "Value" "GND"
			(at 106.68 185.42 0)
		)
		(property "Footprint" ""
			(at 106.68 180.34 0)
		)
		(property "Datasheet" ""
			(at 106.68 180.34 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 106.68 180.34 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0688")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 269.24 176.53 180)
		(unit 5)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 265.4935 123.19 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 269.24 123.825 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 269.24 121.92 0)
		)
		(property "Datasheet" ""
			(at 269.24 120.015 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 265.43 175.768 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 269.24 118.11 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 269.24 116.205 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 269.24 114.3 0)
		)
		(property "Comment" " "
			(at 269.24 112.395 0)
		)
		(property "Component Kind" "Standard"
			(at 269.24 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 269.24 108.585 0)
		)
		(property "PackageDescription" " "
			(at 269.24 106.68 0)
		)
		(property "Pin Count" "105"
			(at 269.24 104.775 0)
		)
		(property "Case" " "
			(at 269.24 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 269.24 100.965 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 269.24 99.06 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 269.24 97.155 0)
		)
		(property "Mounted" "Yes"
			(at 269.24 95.25 0)
		)
		(property "Socket" "No"
			(at 269.24 93.345 0)
		)
		(property "SMD" "No"
			(at 269.24 91.44 0)
		)
		(property "PressFit" "Yes"
			(at 269.24 89.535 0)
		)
		(property "Sense" "No"
			(at 269.24 87.63 0)
		)
		(property "Sense Comment" " "
			(at 269.24 85.725 0)
		)
		(property "Status" "None"
			(at 269.24 83.82 0)
		)
		(property "Status Comment" " "
			(at 269.24 81.915 0)
		)
		(property "SCEM" " "
			(at 269.24 80.01 0)
		)
		(property "Device" " "
			(at 269.24 78.105 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 269.24 76.2 0)
		)
		(property "Manufacturer" "HARTING"
			(at 269.24 74.295 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 269.24 72.39 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 269.24 70.485 0)
		)
		(property "HelpURL" ""
			(at 269.24 68.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 269.24 66.675 0)
		)
		(property "ComponentLink1Description" " "
			(at 269.24 64.77 0)
		)
		(property "ComponentLink2URL" " "
			(at 269.24 62.865 0)
		)
		(property "ComponentLink2Description" " "
			(at 269.24 60.96 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 269.24 59.055 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 269.24 57.15 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 269.24 55.245 0)
		)
		(property "Database Table Name" "Connectors"
			(at 269.24 53.34 0)
		)
		(property "Library Name" "HARTING"
			(at 269.24 51.435 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 269.24 49.53 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 269.24 47.625 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 5)
				)
			)
		)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 203.2 176.53 180)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 199.4535 123.19 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 203.2 123.825 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 203.2 121.92 0)
		)
		(property "Datasheet" ""
			(at 203.2 120.015 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 199.39 175.768 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 203.2 118.11 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 203.2 116.205 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 203.2 114.3 0)
		)
		(property "Comment" " "
			(at 203.2 112.395 0)
		)
		(property "Component Kind" "Standard"
			(at 203.2 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 203.2 108.585 0)
		)
		(property "PackageDescription" " "
			(at 203.2 106.68 0)
		)
		(property "Pin Count" "105"
			(at 203.2 104.775 0)
		)
		(property "Case" " "
			(at 203.2 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 203.2 100.965 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 203.2 99.06 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 203.2 97.155 0)
		)
		(property "Mounted" "Yes"
			(at 203.2 95.25 0)
		)
		(property "Socket" "No"
			(at 203.2 93.345 0)
		)
		(property "SMD" "No"
			(at 203.2 91.44 0)
		)
		(property "PressFit" "Yes"
			(at 203.2 89.535 0)
		)
		(property "Sense" "No"
			(at 203.2 87.63 0)
		)
		(property "Sense Comment" " "
			(at 203.2 85.725 0)
		)
		(property "Status" "None"
			(at 203.2 83.82 0)
		)
		(property "Status Comment" " "
			(at 203.2 81.915 0)
		)
		(property "SCEM" " "
			(at 203.2 80.01 0)
		)
		(property "Device" " "
			(at 203.2 78.105 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 203.2 76.2 0)
		)
		(property "Manufacturer" "HARTING"
			(at 203.2 74.295 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 203.2 72.39 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 203.2 70.485 0)
		)
		(property "HelpURL" ""
			(at 203.2 68.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 203.2 66.675 0)
		)
		(property "ComponentLink1Description" " "
			(at 203.2 64.77 0)
		)
		(property "ComponentLink2URL" " "
			(at 203.2 62.865 0)
		)
		(property "ComponentLink2Description" " "
			(at 203.2 60.96 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 203.2 59.055 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 203.2 57.15 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 203.2 55.245 0)
		)
		(property "Database Table Name" "Connectors"
			(at 203.2 53.34 0)
		)
		(property "Library Name" "HARTING"
			(at 203.2 51.435 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 203.2 49.53 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 203.2 47.625 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 332.74 177.8 180)
		(unit 6)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 328.9935 124.46 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 332.74 125.095 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 332.74 123.19 0)
		)
		(property "Datasheet" ""
			(at 332.74 121.285 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 328.93 177.038 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 332.74 119.38 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 332.74 117.475 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 332.74 115.57 0)
		)
		(property "Comment" " "
			(at 332.74 113.665 0)
		)
		(property "Component Kind" "Standard"
			(at 332.74 111.76 0)
		)
		(property "Component Type" "Standard"
			(at 332.74 109.855 0)
		)
		(property "PackageDescription" " "
			(at 332.74 107.95 0)
		)
		(property "Pin Count" "105"
			(at 332.74 106.045 0)
		)
		(property "Case" " "
			(at 332.74 104.14 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 332.74 102.235 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 332.74 100.33 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 332.74 98.425 0)
		)
		(property "Mounted" "Yes"
			(at 332.74 96.52 0)
		)
		(property "Socket" "No"
			(at 332.74 94.615 0)
		)
		(property "SMD" "No"
			(at 332.74 92.71 0)
		)
		(property "PressFit" "Yes"
			(at 332.74 90.805 0)
		)
		(property "Sense" "No"
			(at 332.74 88.9 0)
		)
		(property "Sense Comment" " "
			(at 332.74 86.995 0)
		)
		(property "Status" "None"
			(at 332.74 85.09 0)
		)
		(property "Status Comment" " "
			(at 332.74 83.185 0)
		)
		(property "SCEM" " "
			(at 332.74 81.28 0)
		)
		(property "Device" " "
			(at 332.74 79.375 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 332.74 77.47 0)
		)
		(property "Manufacturer" "HARTING"
			(at 332.74 75.565 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 332.74 73.66 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 332.74 71.755 0)
		)
		(property "HelpURL" ""
			(at 332.74 69.85 0)
		)
		(property "ComponentLink1URL" " "
			(at 332.74 67.945 0)
		)
		(property "ComponentLink1Description" " "
			(at 332.74 66.04 0)
		)
		(property "ComponentLink2URL" " "
			(at 332.74 64.135 0)
		)
		(property "ComponentLink2Description" " "
			(at 332.74 62.23 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 332.74 60.325 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 332.74 58.42 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 332.74 56.515 0)
		)
		(property "Database Table Name" "Connectors"
			(at 332.74 54.61 0)
		)
		(property "Library Name" "HARTING"
			(at 332.74 52.705 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 332.74 50.8 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 332.74 48.895 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 6)
				)
			)
		)
	)
	(symbol
		(lib_id "HARTING:HARTING_17_25_095_2102")
		(at 59.69 175.26 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J15"
			(at 55.9435 121.92 0)
		)
		(property "Value" "HARTING_17_25_095_2102"
			(at 59.69 122.555 0)
		)
		(property "Footprint" "HARTING THD:HARTING_17 25 095 2102"
			(at 59.69 120.65 0)
		)
		(property "Datasheet" ""
			(at 59.69 118.745 0)
		)
		(property "Description" "HAR-BUS HM Type B19"
			(at 55.88 174.498 0)
		)
		(property "Part Number" "HARTING_17_25_095_2102"
			(at 59.69 116.84 0)
		)
		(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
			(at 59.69 114.935 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 59.69 113.03 0)
		)
		(property "Comment" " "
			(at 59.69 111.125 0)
		)
		(property "Component Kind" "Standard"
			(at 59.69 109.22 0)
		)
		(property "Component Type" "Standard"
			(at 59.69 107.315 0)
		)
		(property "PackageDescription" " "
			(at 59.69 105.41 0)
		)
		(property "Pin Count" "105"
			(at 59.69 103.505 0)
		)
		(property "Case" " "
			(at 59.69 101.6 0)
		)
		(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
			(at 59.69 99.695 0)
		)
		(property "Footprint Ref" "HARTING_17 25 095 2102"
			(at 59.69 97.79 0)
		)
		(property "Family" "HAR-BUS HM Type B19"
			(at 59.69 95.885 0)
		)
		(property "Mounted" "Yes"
			(at 59.69 93.98 0)
		)
		(property "Socket" "No"
			(at 59.69 92.075 0)
		)
		(property "SMD" "No"
			(at 59.69 90.17 0)
		)
		(property "PressFit" "Yes"
			(at 59.69 88.265 0)
		)
		(property "Sense" "No"
			(at 59.69 86.36 0)
		)
		(property "Sense Comment" " "
			(at 59.69 84.455 0)
		)
		(property "Status" "None"
			(at 59.69 82.55 0)
		)
		(property "Status Comment" " "
			(at 59.69 80.645 0)
		)
		(property "SCEM" " "
			(at 59.69 78.74 0)
		)
		(property "Device" " "
			(at 59.69 76.835 0)
		)
		(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
			(at 59.69 74.93 0)
		)
		(property "Manufacturer" "HARTING"
			(at 59.69 73.025 0)
		)
		(property "Manufacturer Part Number" "17 25 095 2102"
			(at 59.69 71.12 0)
		)
		(property "ComponentHeight" "7.57mm"
			(at 59.69 69.215 0)
		)
		(property "HelpURL" ""
			(at 59.69 67.31 0)
		)
		(property "ComponentLink1URL" " "
			(at 59.69 65.405 0)
		)
		(property "ComponentLink1Description" " "
			(at 59.69 63.5 0)
		)
		(property "ComponentLink2URL" " "
			(at 59.69 61.595 0)
		)
		(property "ComponentLink2Description" " "
			(at 59.69 59.69 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 59.69 57.785 0)
		)
		(property "CreateDate" "05/28/08 00:00:00"
			(at 59.69 55.88 0)
		)
		(property "LatestRevisionDate" "06/18/14 00:00:00"
			(at 59.69 53.975 0)
		)
		(property "Database Table Name" "Connectors"
			(at 59.69 52.07 0)
		)
		(property "Library Name" "HARTING"
			(at 59.69 50.165 0)
		)
		(property "Footprint Library" "HARTING THD"
			(at 59.69 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 59.69 46.355 0)
		)
		(pin "A15")
		(pin "B4")
		(pin "D3")
		(pin "A19")
		(pin "B10")
		(pin "A4")
		(pin "C18")
		(pin "A3")
		(pin "E14")
		(pin "D11")
		(pin "C13")
		(pin "E7")
		(pin "D1")
		(pin "C12")
		(pin "F9")
		(pin "D10")
		(pin "A16")
		(pin "B16")
		(pin "C2")
		(pin "B15")
		(pin "E9")
		(pin "C19")
		(pin "B14")
		(pin "F7")
		(pin "B12")
		(pin "F5")
		(pin "E16")
		(pin "A13")
		(pin "A9")
		(pin "D8")
		(pin "A8")
		(pin "E18")
		(pin "C4")
		(pin "B8")
		(pin "C3")
		(pin "D6")
		(pin "B5")
		(pin "C17")
		(pin "D19")
		(pin "C8")
		(pin "C16")
		(pin "E1")
		(pin "E17")
		(pin "E15")
		(pin "B13")
		(pin "B18")
		(pin "A18")
		(pin "A11")
		(pin "D18")
		(pin "C14")
		(pin "C5")
		(pin "A2")
		(pin "C7")
		(pin "C6")
		(pin "E11")
		(pin "A1")
		(pin "A10")
		(pin "D15")
		(pin "E12")
		(pin "E8")
		(pin "E6")
		(pin "C9")
		(pin "A5")
		(pin "D9")
		(pin "B17")
		(pin "C15")
		(pin "A17")
		(pin "C11")
		(pin "E10")
		(pin "D12")
		(pin "D13")
		(pin "F3")
		(pin "D16")
		(pin "D14")
		(pin "F13")
		(pin "E13")
		(pin "F15")
		(pin "B11")
		(pin "F19")
		(pin "D2")
		(pin "A14")
		(pin "F17")
		(pin "B6")
		(pin "D17")
		(pin "A6")
		(pin "D4")
		(pin "B2")
		(pin "B7")
		(pin "E3")
		(pin "E4")
		(pin "E2")
		(pin "D5")
		(pin "B3")
		(pin "C10")
		(pin "B1")
		(pin "E5")
		(pin "D7")
		(pin "A12")
		(pin "F1")
		(pin "F11")
		(pin "A7")
		(pin "B9")
		(pin "B19")
		(pin "E19")
		(pin "C1")
		(instances
			(project "vme-wren"
				(path
					(reference "J15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 337.82 181.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01123"
			(at 337.82 187.96 0)
		)
		(property "Value" "GND"
			(at 337.82 186.69 0)
		)
		(property "Footprint" ""
			(at 337.82 181.61 0)
		)
		(property "Datasheet" ""
			(at 337.82 181.61 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 337.82 181.61 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01123")
					(unit 1)
				)
			)
		)
	)
)
